> GPRS Schema Statistics
> The GPRS schema provides the following types of statistics:

> • | Counter: A counter records incremental data cumulatively and rolls over when the counter limit is reached. The limit depends upon the counter data type.

> • | Gauge: A gauge statistic indicates a single value representative of a single instance. This type is often used to track particular events in time.

> Important: The format string syntax is described by Schema Format String Syntax in the Bulk Statistics Overview chapter.
> Important: Unless otherwise indicated, all statistics are counters. For statistics with the Int32 data type, the roll-over to zero limit is 4,294,967,295. For statistics with the Int64 data type, the roll-over to zero limit is 18,446,744,073,709,551,615. All counter statistics are cumulative and reset only by one of the following methods: roll-over (as described above), after a system restart, or after a clear command is performed. All statistics are considered standards-based unless otherwise noted. All Data Type values with an * have had values increased from Int32 to Int64 in releases 9.0 and higher.
> The following variables are supported:
> GPRS Service Schema Statistics

> Statistic | Description | Data Type
> vpnname | The name of the context configured on the system that is currently facilitating the GPRS service. This is a stat key variable. | String
> vpnid | The identification number of the context configured on the system that is currently facilitating the GPRS service. This is an internal reference number. This is a stat key variable. | Int32
> servname | The name of the GPRS service configured on the system for which the statistics are displayed. This is a stat key variable. | String
> nse-id | The network service entity identifier in this GPRS service. This is a stat key variable. | Int32
> ns-num-bytes-rvcd | This statistics has been obsoleted. | Int32
> ns-num-bytes-sent | This statistics has been obsoleted. | Int32
> ns-num-nsvc-failed | This statistics has been obsoleted. | Int32
> ns-num-nsvc-congest | This statistics has been obsoleted. | Int32
> ns-num-unit-data-msg-rcvd | This statistics has been obsoleted. | Int32
> ns-num-unit-data-msg-sent | This statistics has been obsoleted. | Int32
> ns-num-alive-pdu-rcvd | This statistics has been obsoleted. | Int32
> ns-num-alive-pdu-sent | This statistics has been obsoleted. | Int32
> ns-num-alive-ack-pdu-rcvd | This statistics has been obsoleted. | Int32
> ns-num-alive-ack-pdu-sent | This statistics has been obsoleted. | Int32
> ns-num-block-pdu-rcvd | This statistics has been obsoleted. | Int32
> ns-num-block-pdu-sent | This statistics has been obsoleted. | Int32
> ns-num-block-ack-pdu-rcvd | This statistics has been obsoleted. | Int32
> ns-num-block-ack-pdu-sent | This statistics has been obsoleted. | Int32
> ns-num-unblock-pdu-rcvd | This statistics has been obsoleted. | Int32
> ns-num-unblock-pdu-sent | This statistics has been obsoleted. | Int32
> ns-num-unblock-ack-pdu-rcvd | This statistics has been obsoleted. | Int32
> ns-num-unblock-ack-pdu-sent | This statistics has been obsoleted. | Int32
> ns-num-reset-pdu-rcvd | This statistics has been obsoleted. | Int32
> ns-num-reset-pdu-sent | This statistics has been obsoleted. | Int32
> ns-num-reset-ack-pdu-rcvd | This statistics has been obsoleted. | Int32
> ns-num-reset-ack-pdu-sent | This statistics has been obsoleted. | Int32
> ns-num-status-pdu-rcvd | This statistics has been obsoleted. | Int32
> ns-num-status-pdu-sent | This statistics has been obsoleted. | Int32
> num-sns-size-rcvd | Total number of sequence number space (SNS) size messages received by the network service entity. | Int32
> num-sns-size-ack-sent | Total number of ACK messages sent for sequence number space (SNS) size by the network service entity. | Int32
> num-sns-size-fail-rcvd-unknown-nse | Total number of SNS size messages failed due to unknown network service entity. | Int32
> num-sns-config-rcvd | Total number of sequence number space (SNS) configuration messages received by the network service entity. | Int32
> num-sns-config-sent | Total number of sequence number space (SNS) configuration messages sent by the network service entity. | Int32
> num-sns-config-ack-sent | Total number of sequence number space (SNS) configuration ACK messages sent by the network service entity. | Int32
> num-sns-config-ack-rcvd | Total number of sequence number space (SNS) configuration ACK messages received by the network service entity. | Int32
> sns-config-fail-rcv-pdu-not-compat-state | Total number of sequence number space (SNS) configuration messages failed as received packet data unit was not compatible with the message state in network service entity. | Int32
> sns-config-fail-sent-pdu-not-compat-state | Total number of sequence number space (SNS) configuration messages failed as sent packet data unit was not compatible with the message state in network service entity. | Int32
> sns-config-fail-rcv-inval-ipv4-endpt | Total number of sequence number space (SNS) configuration messages failed due to invalid IPv4 address of endpoint in received message. | Int32
> sns-config-fail-sent-inval-ipv4-endpt | Total number of sequence number space (SNS) configuration messages failed due to invalid IPv4 address of endpoint in sent message. | Int32
> sns-config-fail-rcv-inval-ipv6-endpt | Total number of sequence number space (SNS) configuration messages failed due to invalid IPv6 address of endpoint in received message. | Int32
> sns-config-fail-sent-inval-ipv6-endpt | Total number of sequence number space (SNS) configuration messages failed due to invalid IPv6 address of endpoint in sent message. | Int32
> sns-config-fail-rcv-prot-err-unspec | Total number of sequence number space (SNS) configuration messages failed due to unspecified protocol error in received message. | Int32
> sns-config-fail-sent-prot-err-unspec | Total number of sequence number space (SNS) configuration messages failed due to unspecified protocol error in sent message. | Int32
> sns-config-fail-rcv-inval-essential-param | Total number of sequence number space (SNS) configuration messages failed due to invalid mandatory parameters in received message. | Int32
> sns-config-fail-sent-inval-essential-param | Total number of sequence number space (SNS) configuration messages failed due to invalid mandatory parameters in sent message. | Int32
> sns-config-fail-rcv-internal-err | Total number of sequence number space (SNS) configuration messages failed due to internal error in received message. | Int32
> sns-config-fail-sent-internal-err | Total number of sequence number space (SNS) configuration messages failed due to internal error in sent message. | Int32
> sns-config-fail-rcv-inval-weight | Total number of sequence number space (SNS) configuration messages failed due to invalid weight bit in received message. | Int32
> sns-config-fail-sent-inval-weight | Total number of sequence number space (SNS) configuration messages failed due to invalid weight bit in sent message. | Int32
> sns-config-fail-sent-no-rsp-from-peer | Total number of sequence number space (SNS) configuration message failed due to no response from peer. | Int32
> num-sns-add-rcvd | Total number of SNS-ADD messages received. | Int32
> num-sns-add-sent | Total number of SNS-ADD messages sent. | Int32
> sns-add-fail-rcv-pdu-not-compat-state | Total number of ADD SNS messages failed as received packet data unit was not compatible with the message state in network service entity. | Int32
> sns-add-fail-sent-pdu-not-compat-state | Total number of ADD SNS messages failed as sent packet data unit was not compatible with the message state in network service entity. | Int32
> sns-add-fail-rcv-inval-ipv4-endpt | Total number of ADD SNS messages failed due to invalid IPv4 address of endpoint in received message. | Int32
> sns-add-fail-sent-inval-ipv4-endpt | Total number of ADD SNS messages failed due to invalid IPv4 address of endpoint in sent message. | Int32
> sns-add-fail-rcv-inval-ipv6-endpt | Total number of ADD SNS messages failed due to invalid IPv6 address of endpoint in received message. | Int32
> sns-add-fail-sent-inval-ipv6-endpt | Total number of ADD SNS messages failed due to invalid IPv6 address of endpoint in sent message. | Int32
> sns-add-fail-rcv-prot-err-unspec | Total number of ADD SNS messages failed due to unspecified protocol error in received message. | Int32
> sns-add-fail-sent-prot-err-unspec | Total number of ADD SNS messages failed due to unspecified protocol error in sent message. | Int32
> sns-add-fail-rcv-inval-essential-param | Total number of ADD SNS messages failed due to invalid mandatory parameters in received message. | Int32
> sns-add-fail-sent-inval-essential-param | Total number of ADD SNS messages failed due to invalid mandatory parameters in sent message. | Int32
> sns-add-fail-rcv-internal-err | Total number of ADD SNS messages failed due to internal error in received message. | Int32
> sns-add-fail-sent-internal-err | Total number of ADD SNS messages failed due to internal error in sent message. | Int32
> sns-add-fail-rcv-inval-weight | Total number of ADD SNS messages failed due to invalid weight bit in received message. | Int32
> sns-add-fail-sent-inval-weight | Total number of ADD SNS messages failed due to invalid weight bit in sent message. | Int32
> sns-add-fail-sent-no-rsp-from-peer | Total number of ADD SNS messages failed due to no response from peer. | Int32
> num-sns-delete-rcvd | Total number of DELETE SNS messages received. | Int32
> num-sns-delete-sent | Total number of DELETE SNS messages sent. | Int32
> sns-delete-fail-rcv-pdu-not-compat-state | Total number of DELETE SNS messages failed as received packet data unit was not compatible with the message state in network service entity. | Int32
> sns-delete-fail-sent-pdu-not-compat-state | Total number of DELETE SNS messages failed as sent packet data unit was not compatible with the message state in network service entity. | Int32
> sns-delete-fail-rcv-unknown-ip-endpt | Total number of DELETE SNS messages failed due to unknown IP endpoint in received message. | Int32
> sns-delete-fail-sent-unknown-ip-endpt | Total number of DELETE SNS messages failed due to unknown IP address in the sent message. | Int32
> sns-delete-fail-rcv-unknown-ip-address | Total number of DELETE SNS messages failed due to invalid IP address of endpoint in received message. | Int32
> sns-delete-fail-sent-unknown-ip-address | Total number of DELETE SNS messages failed due to invalid IP address of endpoint in sent message. | Int32
> sns-delete-fail-rcv-prot-err-unspec | Total number of DELETE SNS messages failed due to unspecified protocol error in received message. | Int32
> sns-delete-fail-sent-prot-err-unspec | Total number of DELETE SNS messages failed due to unspecified protocol error in sent message. | Int32
> sns-delete-fail-rcv-inval-essential-param | Total number of DELETE SNS messages failed due to invalid mandatory parameters in received message. | Int32
> sns-delete-fail-sent-inval-essential-param | Total number of DELETE SNS messages failed due to invalid mandatory parameters in sent message. | Int32
> sns-delete-fail-rcv-internal-err | Total number of DELETE SNS messages failed due to internal error in received message. | Int32
> sns-delete-fail-sent-internal-err | Total number of DELETE SNS messages failed due to internal error in sent message. | Int32
> sns-delete-fail-sent-no-rsp-from-peer | Total number of DELETE SNS messages failed due to no response from peer. | Int32
> num-sns-cw-rcvd | Total number of SNS congestion window size messages received. | Int32
> num-sns-cw-sent | Total number of SNS congestion window size messages sent. | Int32
> sns-cw-fail-rcv-pdu-not-compat-state | Total number of SNS messages with congestion window size failed as received packet data unit was not compatible with the message state. | Int32
> sns-cw-fail-sent-pdu-not-compat-state | Total number of SNS messages with congestion window size failed as sent packet data unit was not compatible with the message state. | Int32
> sns-cw-fail-rcv-inval-weight | Total number of SNS messages with congestion window size failed due to invalid weight bit in received message. | Int32
> sns-cw-fail-sent-inval-weight | Total number of SNS messages with congestion window size failed due to invalid weight bit in sent message. | Int32
> sns-cw-fail-rcv-unknown-ip-endpt | Total number of SNS messages with congestion window size failed due to unknown IP endpoint in received message. | Int32
> sns-cw-fail-sent-unknown-ip-endpt | Total number of SNS messages with congestion window size failed due to unknown IP endpoint in sent message. | Int32
> sns-cw-fail-rcv-unknown-ip-addr | Total number of SNS messages with congestion window size failed due to unknown IP address in received message. | Int32
> sns-cw-fail-sent-unknown-ip-addr | Total number of SNS messages with congestion window size failed due to unknown IP address in sent message. | Int32
> sns-cw-fail-rcv-prot-err-unspec | Total number of SNS messages with congestion window size failed due to unspecified protocol error in received message. | Int32
> sns-cw-fail-sent-prot-err-unspec | Total number of SNS messages with congestion window size failed due to unspecified protocol error in sent message. | Int32
> sns-cw-fail-rcv-inval-essential-param | Total number of SNS messages with congestion window size failed due to invalid mandatory parameters in received message. | Int32
> sns-cw-fail-sent-inval-essential-param | Total number of SNS messages with congestion window size failed due to invalid mandatory parameters in sent message. | Int32
> sns-cw-fail-rcv-internal-err | Total number of SNS messages with congestion window size failed due to internal error in received message. | Int32
> sns-cw-fail-sent-internal-err | Total number of SNS messages with congestion window size failed due to internal error in sent message. | Int32
> sns-cw-fail-sent-no-rsp-from-peer | Total number of SNS messages with congestion window size failed due to no response from peer. | Int32
> sns-num-ack-rcvd | Total number of SNS ACK messages received. | Int32
> sns-num-ack-sent | Total number of SNS ACK messages sent. | Int32
> sns-num-unknown-msg | Total number of unknown messages received. | Int32
> sns-num-status-pdu-sent | Total number of SNS ACK messages sent. | Int32
> bssgp-total-usr-req-drop | Total number of user requests to drop base station sub-system GPRS Protocol (BSSGP) in GPRS service. | Int32
> bssgp-usr-req-drop-unknown-bvci | Total number of BSSGP user requests dropped due to unknown BSSGP virtual connection identifier (BVCI). | Int32
> bssgp-usr-req-drop-blocked-bvc | Total number of BSSGP user requests due to blocked BVC. | Int32
> bssgp-usr-req-drop-encoding-fail | Total number of BSSGP user requests dropped due to failure in encoding. | Int32
> bssgp-usr-req-drop-bvc-flow-ctrl-rvcd | Total number of BSSGP user requests dropped due to BVC flow control messages received. | Int32
> bssgp-usr-req-drop-bvc-flow-ctrl-ack-sent | Total number of BSSGP user requests dropped due to flow control ack messages sent. | Int32
> bssgp-usr-req-drop-block-rvcd | Total number of BSSGP user requests dropped due to blocked BVC BLOCK messages received. | Int32
> bssgp-usr-req-drop-block-ack-sent | Total number of BSSGP user requests dropped due to blocked BVC BLOCK ACK messages sent. | Int32
> bssgp-usr-req-drop-unblock-rcvd | Total number of BSSGP user requests dropped due to blocked BVC UNBLOCK messages received. | Int32
> bssgp-usr-req-drop-unblock-ack-sent | Total number of BSSGP user requests dropped due to blocked BVC UNBLOCK ACK messages sent. | Int32
> bssgp-usr-req-drop-bvc-reset-sent | Total number of BSSGP user requests dropped due to BVC RESET sent. | Int32
> bssgp-usr-req-drop-bvc-reset-rcvd | Total number of BSSGP user requests dropped due to BVC RESET received. | Int32
> bssgp-usr-req-drop-bvc-reset-ack-sent | Total number of BSSGP user requests dropped due to BVC RESET ACK messages sent. | Int32
> bssgp-usr-req-drop-bvc-reset-ack-rcvd | Total number of BSSGP user requests dropped due to BVC RESET ACK messages received. | Int32
> bssgp-bvc-status-msg-sent | Total number of BVC status messages sent. | Int32
> bssgp-bvc-status-msg-rcvd | Total number of BVC status messages received. | Int32
> bssgp-flush-llc-msg-sent | Total number of BSSGP FLUSH LL (Logical Link) messages sent. This is a counter type of statistic. | Int32
> bssgp-flush-llc-ack-msg-rcvd | Total number of BSSGP FLUSH LL (Logical Link) ACK messages received. This is a counter type of statistic. | Int32
> bssgp-cs-paging-msg-sent | Total number of BSSGP circuit switched (CS) paging messages sent. | Int32
> bssgp-ps-paging-msg-sent | Total number of BSSGP packet switched (PS) paging messages sent. | Int32
> bssgp-ra-cap-update-msg-rcvd | Total number of BSSGP routing area (RA) capability update messages received. | Int32
> bssgp-ra-cap-update-ack-msg-sent | Total number of BSSGP routing area (RA) capability update messages sent. | Int32
> bssgp-radio-status-msg-sent | This statistic has been obsoleted. | Int32
> bssgp-radio-status-msg-rcvd | Total number of BSSGP radio status messages received. | Int32
> bssgp-suspend-msg-rcvd | Total number of BSSGP SUSPEND messages received. | Int32
> bssgp-suspend-ack-msg-sent | Total number of BSSGP SUSPEND Acks sent. | Int32
> bssgp-suspend-nack-msg-sent | Total number of BSSGP SUSPEND NAcks sent. | Int32
> bssgp-resume-msg-rcvd | Total number of BSSGP RESUME messages received. | Int32
> bssgp-resume-ack-msg-sent | Total number of BSSGP RESUME Acks sent. | Int32
> bssgp-resume-nack-msg-sent | Total number of BSSGP RESUME NAcks sent. | Int32
> bssgp-downlink-unitdata-sent | Total number of BSSGP unit data sent in downlink direction (towards MS). | Int32
> bssgp-uplink-unitdata-rcvd | Total number of BSSGP unit data received.in uplink direction (towards network). | Int32
> bssgp-llc-pdu-discard-msg-rcvd | Total number of LLC PDU discard messages received. | Int32
> bssgp-pkt-drop-flow-ctrl-queue-full | Total number of BSSGP packets dropped due to flow control buffer was full. This is a counter type of statistic. | Int32
> bssgp-downlink-pkt-drop | Total number of BSSGP packets dropped in downlink direction. This is a counter type of statistic. | Int32
> bssgp-ms-flow-ctrl-msg-rcvd | Total number of MS flow control messages received. | Int32
> bssgp-ms-flow-ctrl-ack-msg-sent | Total number of MS flow control ack messages sent. | Int32
> bssgp-bvc-unknown-ms-status-msg-rcvd | Total number of BSSGP virtual connection (BVC) messages received with unknown MS status. This is a counter type of statistic. | Int32
> bssgp-bvc-unknown-ms-status-msg-sent | Total number of BSSGP virtual connection (BVC) messages sent for unknown MS status. This is a counter type of statistic. | Int32
> sndcp-xid-req-ms-init | Total number of MS initiated eXchange Identification (XID) indicators received. This is a counter type of statistic. | Int64*
> sndcp-xid-ind-sgsn-init | Total number of SGSN initiated eXchange Identification (XID) indicators sent. This is a counter type of statistic. | Int64*
> sndcp-npdus-ack-rcvd-ms | Total number of SNDCP network PDUs in Ack mode received from MS. This is a counter type of statistic. | Int64*
> sndcp-npdus-ack-sent-ms | Total number of SNDCP network PDUs in Ack mode sent to MS. This is a counter type of statistic. | Int64*
> sndcp-npdus-uack-rcvd-ms | Total number of SNDCP network PDUs in UnAck mode received from MS. This is a counter type of statistic. | Int64*
> sndcp-npdus-uack-sent-ms | Total number of SNDCP network PDUs in UnAck mode sent to MS. This is a counter type of statistic. | Int64*
> sndcp-bytes-ack-rcvd-ms | Description: Total number of SNDCP bytes received from MS for all subscribers at SNDCP layer using LLC Acknowledged mode of LLC operation. Triggers: Increments after the uplink data packet has passed SNDCP validations as mentioned in sections 6.7 and 6.9 of SNDCP TS 44.065. Availability: per GPRS service, per Routing Area Type: Counter | Int64*
> sndcp-bytes-ack-sent-ms | Description: Total number of SNDCP bytes sent to MS for all subscribers at SNDCP layer using LLC Acknowledged mode of LLC operation. Triggers: Increments after the uplink data packet has passed SNDCP validations as mentioned in sections 6.7 and 6.9 of SNDCP TS 44.065. Availability: per GPRS service, per Routing Area Type: Counter | Int64*
> sndcp-bytes-uack-rcvd-ms | Description: Total number of SNDCP bytes received from MS for all subscribers at SNDCP layer using LLC Un-acknowledged mode of LLC operation. Triggers: Increments after the uplink data packet has passed SNDCP validations as mentioned in sections 6.7 and 6.9 of SNDCP TS 44.065. Availability: per GPRS service, per Routing Area Type: Counter | Int64*
> sndcp-bytes-uack-sent-ms | Description: Total number of SNDCP bytes sent to MS for all subscribers at SNDCP layer using LLC Un-acknowledged mode of LLC operation. Triggers: Increments after the uplink data packet has passed SNDCP validations as mentioned in sections 6.7 and 6.9 of SNDCP TS 44.065. Availability: per GPRS service, per Routing Area Type: Counter | Int64*
> sndcp-pdu-drop-rcvd-from-llc | Total number of SNDCP PDUs dropped when received from LLC due to invalid parameter or state. | Int64*
> sndcp-inval-ref-num-rcvd-from-llc | Total number of SNDCP PDUs dropped due to invalid reference number received from LLC. | Int64*
> sndcp-npdu-sent-sgsn-irau | Total number of SNDCP network PDUs sent/transferred to other SGSNs during inter-SGSN routing area update (RAU). | Int64*
> sndcp-npdu-rcvd-sgsn-irau | Total number of SNDCP network PDUs received from other SGSNs during inter-SGSN routing area update (RAU). | Int64*
> llc-data-req-rx | Total number of LLC data requests received from the MS. | Int64*
> llc-data-cfm-tx | Total number of LLC data requests confirmation sent to the MS. | Int64*
> llc-data-ind-tx | Total number of LLC data indications sent to the MS. | Int64*
> llc-data-sent-ind-tx | Total number of LLC data sent indications sent to the MS. | Int64*
> llc-unit-data-req-rx | Total number of LLC unit data requests received from the MS. | Int64*
> llc-unit-data-ind-tx | Total number of LLC unit data indications sent to the MS. | Int64*
> llc-discarded-frames-rx | Total number of LLC discarded frames received from the MS. | Int64*
> llc-discarded-frames-tx | Total number of LLC discarded frames sent to MS. | Int64*
> llc-error-frames-rx | Total number of LLC error frames received from the MS. | Int64*
> llc-unrecog-frames-rx | Total number of LLC unrecognized frames received from the MS. | Int64*
> llc-xid-collisions | Total number of LLC exchange identifier (XID) request collisions. | Int64*
> llc-ciphering-errors | Total number of LLC ciphering errors. | Int64*
> llc-fcs-errors | Total number of LLC frame check sequence errors. | Int64*
> llc-frame-stats-octets-rcvd | Description: This proprietary statistic indicates the total number of bytes of LLC frames received from an MS. This value includes all LLC messages (data + gmm messages + other LLC messages). This stat value be compared with similar counts for other layers to check if any packets have been dropped. Triggers: Increments when the LLC layer receives a packet (can be UI frame, U frame, S frame or U frame) from lower BSSGP layer. Availability: per GRPS service Type: Counter | Int64*
> llc-frame-stats-octets-sent | Description: This proprietary statistic indicates the total number of bytes sent from the LLC layer to an MS from the SGSN. This value includes all LLC messages (data + gmm messages + other LLC messages). This stat value be compared with similar counts for other layers to check if any packets have been dropped. Triggers: Increments when the LLC layer sends a packet (can be UI frame, U frame, S frame or U frame) to the lower BSSGP layer. Availability: per GPRS service Type: Counter | Int64*
> llc-frame-stats-unack-frames-rcvd | Description: This proprietary statistic indicates the total number of unacknowledged UI frames received at the LLC layer from an MS. This value be compared with the packet count in gmm and sndcp to check if there are any packets dropped in the LLC layer. Triggers: Increments when the LLC layer receives a UI frame in unacknowledged mode from the lower BSSGP layer. Availability: per GPRS service Type: Counter | Int64*
> llc-frame-stats-unack-frames-sent | Description: This proprietary statistic indicates the total number of unacknowledged UI frames sent from the LLC to an MS. This value can be compared with the packet count in gmm and sndcp to check if there are any packets dropped in the LLC layer. Triggers: Increments when the LLC layer sends a UI frame in unacknowledged mode to the lower BSSGP layer. Availability: per GPRS service Type: Counter | Int64*
> llc-frame-stats-ui-rx | Total number of LLC frames with unnumbered information received from the MS. | Int64*
> llc-frame-stats-ui-tx | Total number of LLC frames with unnumbered information sent to the MS. This is a counter type of statistic. | Int64*
> llc-frame-stats-ui-ciph-rx | Total number of LLC frames with ciphered unnumbered information received from the MS. This is a counter type of statistic. | Int64*
> llc-frame-stats-ui-ciph-tx | Description:Total number of LLC frames with ciphered unnumbered information sent to the MS. Availability: per GPRS service. Type: Counter | Int64*
> llc-frame-stats-ui-gea1-ciph-data-frames-rx | Description: Indicates the total number of GEA1 ciphered data frames received at LLC layer; where the data frames include SNDCP sapi i.e 3,5,9 or 11). Triggers: Increments when receiving data frame ciphered with the GPRS GEA1 ciphering algorithm. Availability: per GPRS service. Type: Counter | Int64*
> llc-frame-stats-ui-gea1-ciph-data-frames-tx | Description: Indicates the total number of GEA1 ciphered data frames transmitted from the LLC layer; where the data frames include SNDCP sapi i.e 3,5,9 or 11). Triggers: Increments when transmitting data frame ciphered with the GPRS GEA1 ciphering algorithm. Availability: per GPRS service. Type: Counter | Int64*
> llc-frame-stats-ui-gea1-ciph-data-octets-rx | Description: Indicates the total number of GEA1 ciphered data bytes received at the LLC layer. Triggers: Increments when receiving a data octet ciphered with GPRS GEA1 ciphering algorithm. Availability: per GPRS service. Type: Counter | Int64*
> llc-frame-stats-ui-gea1-ciph-data-octets-tx | Description: Indicates the total number of GEA1 ciphered data bytes transmitted from the LLC layer. Triggers: Increments when transmitting a data octet ciphered with GPRS GEA1 ciphering algorithm. Availability: per GPRS service. Type: Counter | Int64*
> llc-frame-stats-ui-gea2-ciph-data-frames-rx | Description: Indicates the total number of GEA2 ciphered data frames received at LLC layer; where the data frames include SNDCP sapi i.e 3,5,9 or 11). Triggers: Increments when receiving data frame ciphered with the GPRS GEA2 ciphering algorithm. Availability: per GPRS service. Type: Counter | Int64*
> llc-frame-stats-ui-gea2-ciph-data-frames-tx | Description: Indicates the total number of GEA2 ciphered data frames trasnmitted from the LLC layer; where the data frames include SNDCP sapi i.e 3,5,9 or 11). Triggers: Increments when transmitting data frame ciphered with the GPRS GEA2 ciphering algorithm. Availability: per GPRS service. Type: Counter | Int64*
> llc-frame-stats-ui-gea2-ciph-data-octets-rx | Description: Indicates the total number of GEA2 ciphered data bytes received at the LLC layer. Triggers: Increments when receiving a data octet ciphered with GPRS GEA2 ciphering algorithm. Availability: per GPRS service. Type: Counter | Int64*
> llc-frame-stats-ui-gea2-ciph-data-octets-tx | Description: Indicates the total number of GEA2 ciphered data bytes transmitted from the LLC layer. Triggers: Increments when transmitting a data octet ciphered with GPRS GEA2 ciphering algorithm. Availability: per GPRS service. Type: Counter | Int64*
> llc-frame-stats-ui-gea3-ciph-data-frames-rx | Description: Indicates the total number of GEA3 ciphered data frames received at LLC layer; where the data frames include SNDCP sapi i.e 3,5,9 or 11). Triggers: Increments when receiving data frame ciphered with the GPRS GEA3 ciphering algorithm. Availability: per GPRS service. Type: Counter | Int64*
> llc-frame-stats-ui-gea3-ciph-data-frames-tx | Description: Indicates the total number of GEA3 ciphered data frames transmitted from the LLC layer; where the data frames include SNDCP sapi i.e 3,5,9 or 11). Triggers: Increments when trasnmitting data frame ciphered with the GPRS GEA3 ciphering algorithm. Availability: per GPRS service. Type: Counter | Int64*
> llc-frame-stats-ui-gea3-ciph-data-octets-rx | Description: Indicates the total number of GEA3 ciphered data bytes received at the LLC layer. Triggers: Increments when receiving a data octet ciphered with GPRS GEA3 ciphering algorithm. Availability: per GPRS service. Type: Counter | Int64*
> llc-frame-stats-ui-gea3-ciph-data-octets-tx | Description: Indicates the total number of GEA3 ciphered data bytes transmitted from the LLC layer. Triggers: Increments when transmitting a data octet ciphered with GPRS GEA3 ciphering algorithm. Availability: per GPRS service. Type: Counter | Int64*
> llc-frame-stats-ui-unciph-rx | Description: Total number of unciphered frames received at the LLC layer. Triggers: Increments when the incoming frame is unciphered. Availability: per GPRS service. Type: Counter | Int64*
> llc-frame-stats-ui-unciph-tx | Description: Total number of unciphered frames transmitted from the LLC layer. Triggers: Increments when the outgoing frame is unciphered. Availability: per GPRS service. Type: Counter | Int64*
> llc-frame-stats-ui-unciph-data-frames-rx | Description: Total number of unciphered data frames received at the LLC layer, where the data frames include SNDCP sapi i.e 3,5,9 or 11). Triggers: Increments when the incoming data frame is unciphered. Availability: per GPRS service. Type: Counter | Int64*
> llc-frame-stats-ui-unciph-data-frames-tx | Description: Total number of unciphered data frames transmitted at the LLC layer, where the data frames include SNDCP sapi i.e 3,5,9 or 11). Triggers: Increments when the outgoing data frame is unciphered. Availability: per GPRS service. Type: Counter | Int64*
> llc-frame-stats-ui-unciph-data-octets-rx | Description: Total number of unciphered data bytes received at the LLC layer. Triggers: Increments when receiving an unciphered data octet. Availability: per GPRS service. Type: Counter | Int64*
> llc-frame-stats-ui-unciph-data-octets-tx | Description: Total number of unciphered data bytes transmitted from the LLC layer. Triggers: Increments when transmitting an unciphered data octet. Availability: per GPRS service. Type: Counter | Int64*
> llc-frame-stats-xid-rcvd | Description: This proprietary statistic indicates the total number of XID-reset messages received from the MS. Triggers: Increments when the LLC layer receives an XID request from the lower BSSGP layer. Availability: per GPRS service. Type: Counter | Int64*
> llc-frame-stats-xid-sent | Description: This proprietary statistic indicates the total number of XID-reset messages sent to the MS. This includes responses to XIDs sent by the SGSN and SID command from the MS. This stat value can be compared with the stat value for llc-frame-stats-xid-rcvd to determine XID failures. Triggers: Increments when the LLC layer sends an XID request to the lower BSSGP layer. Availability: per GPRS service. Type: Counter | Int64*
> bytes-sent-to-bsc | Description: Stat collected on the Gn interface provides the total number of bytes of data sent by a GGSN to a specific BSC. Triggers: Increments by the number of bytes of data in the data packet whenever a data packet is sent in the downlink direction from the GGSN to a subscriber served by the particular BSC. Availability: per BSC Type: Counter | Int64
> packets-sent-to-bsc | Description: Stat collected on the Gn interface provides the total number of data packets a GGSN sent to a specific BSC. Triggers: Increments whenever a data packet is sent in the downlink direction from the GGSN to a subscriber served by the particular BSC. Availability: per BSC Type: Counter | Int64
> bytes-rcvd-from-bsc | Description: Stat collected on the Gn interface provides the total number of bytes of data received by a GGSN from a specific BSC. Triggers: Increments by the number of bytes of data in the data packet whenever a data packet is sent in the uplink direction to the GGSN from a subscriber served by the particular BSC. Availability: per BSC Type: Counter | Int64
> packets-rcvd-from-bsc | Description: Stat collected on the Gn interface provides the total number of data packets the GGSN received from a specific BSC. Triggers: Increments whenever a data packet is sent in the uplink direction to the GGSN from a subscriber served by the particular BSC. Availability: per BSC Type: Counter | Int64
> gprs-num-subs-gea0-capable | Description: This proprietary statistic indicates the total number of currently attached GPRS subscribers whose MS network capability supports GEA0 (no ciphering). Availability: per GPRS Service Type:Gauge | Int32
> gprs-num-subs-gea1-capable | Description: This proprietary statistic indicates the total number of currently attached GPRS subscribers whose MS network capability supports GEA1 encryption. Availability: per GPRS Service Type: Gauge | Int32
> gprs-num-subs-gea2-capable | Description: This proprietary statistic indicates the total number of currently attached GPRS subscribers whose MS network capability supports GEA2 encryption. Availability: per GPRS Service Type: Gauge | Int32
> gprs-num-subs-gea3-capable | Description: This proprietary statistic indicates the total number of currently attached GPRS subscribers whose MS network capability supports GEA3 encryption. Availability: per GPRS Service Type: Gauge | Int32
> gprs-num-subs-gea0-negotiated | Description: This proprietary statistic indicates the total number of currently attached GPRS subscribers who have negotiated, with the SGSN during authentication and ciphering request, to use GEA0 (no ciphering). Availability: per GPRS Service Type: Gauge | Int32
> gprs-num-subs-gea1-negotiated | Description: This proprietary statistic indicates the total number of currently attached GPRS subscribers who have negotiated, with the SGSN during authentication and ciphering request, to use GEA1 encryption. Availability: per GPRS Service Type: Gauge | Int32
> gprs-num-subs-gea2-negotiated | Description: This proprietary statistic indicates the total number of currently attached GPRS subscribers who have negotiated, with the SGSN during authentication and ciphering request, to use GEA2 encryption. Availability: per GPRS Service Type: Gauge | Int32
> gprs-num-subs-gea3-negotiated | Description: This proprietary statistic indicates the total number of currently attached GPRS subscribers who have negotiated, with the SGSN during authentication and ciphering request, to use GEA3 encryption. Availability: per GPRS Service Type: Gauge | Int32
> Important: See Bulk Statistics Overview for statistics that are common to all schema.

> ‌

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883