> Web Element Manager MIB
> The figure that follows illustrates the hierarchical structure of the management information base (MIB) for the Web Element Manager.
> MIB Textual Conventions
> starentMIB(8164).starentMIBObjects(1).starentEmsMIB(1000)
> starentMIB(8164).starentMIBObjects(1).starentEMSMIB(1000).
> starEmsMIBObjects(1)
> starentMIB(8164).starentMIBObjects(1).starentEMSMIB(1000).
> starEmsMIBObjects(1).starEmsNotifMgmt(2)

> Object: | starEmsNotifInfo

> Object ID: | enterprises.8164.1.1000.1.2.5

> Description: | A textual description of EMS notification, which potentially contains additional information (more than just the type of alarm). If the text of the message exceeds 64 bytes, the message will be truncated to 63 bytes and a '*' character will be appended to indicate the message has been truncated.

> Syntax: | DisplayString (SIZE (1..64))

> Access: | Read-only

> Object: | starEmsNotifRaisedTime

> Object ID: | enterprises.8164.1.1000.1.2.6

> Description: | This object indicates the time when this notification was generated.

> Syntax: | TimeStamp

> Access: | Read-only

> Object: | starEmsProcMonThreshold

> Object ID: | enterprises.8164.1.1000.1.2.7

> Description: | This object indicates the current threshold value of process monitoring.

> Syntax: | DisplayString (SIZE (1..10))

> Access: | Read-only

> Object: | starEmsInterfaceAddr

> Object ID: | enterprises.8164.1.1000.1.2.8

> Description: | The object indicates the Interface address of host machine where EMS server is running

> Syntax: | InetAddress

> Access: | Read-only

> Object: | starEmsInterfaceName

> Object ID: | enterprises.8164.1.1000.1.2.9

> Description: | This object indicates the interface name of host machine where EMS server is running.

> Syntax: | DisplayString (SIZE (1..64))

> Access: | Read-only

> Object: | starEmsIMGAddr

> Object ID: | enterprises.8164.1.1000.1.2.10

> Description: | The object indicates the IP address of IMG.

> Syntax: | InetAddress

> Access: | Read-only

> Object: | starEmsFtpFileName

> Object ID: | enterprises.8164.1.1000.1.2.11

> Description: | This object indicates name of the file which FTP’d and then deleted from the IMG.

> Syntax: | DisplayString (SIZE (1..64))

> Access: | Read-only

> Object: | starEmsIMGState

> Object ID: | enterprises.8164.1.1000.1.2.12

> Description: | IMG state. unreachable(0) IMG is ICMP unreachable active(1) IMG is CORBA reachable inactive(1) IMG is CORBA unreachable reachable(0) IMG is ICMP reachable

> Syntax: | INTEGER

> Access: | Read-only

> Enumeration: | unreachable(0) active(1) inactive(2) reachable(3)

> Object: | starEmsBulkStatFileXferTime

> Object ID: | enterprises.8164.1.1000.1.2.13

> Description: | The configured value of a Bulkstat file transfer in minutes.

> Syntax: | INTEGER(1..999999)

> Access: | Read-only

> Object: | starEmsXMLFtpFileName

> Object ID: | enterprises.8164.1.1000.1.2.14

> Description: | This object indicates name of the BulkStat XML file which is to be FTPed on the NMS.

> IMPORTANT: This attribute is obsolete.

> Syntax: | DisplayString (SIZE (1..256))

> Access: | Read-only

> Object: | starEmsXMLFtpDestAddr

> Object ID: | enterprises.8164.1.1000.1.2.15

> Description: | This object indicates destination IP address (NMS) for BulkStat XML file FTP.

> Syntax: | InetAddress

> Access: | Read-only

> Object: | starEmsXMLFtpDestPath

> Object ID: | enterprises.8164.1.1000.1.2.16

> Description: | This object indicates destination path where BulkStat XML file is to be FTPed.

> Syntax: | DisplayString (SIZE (1..1024))

> Access: | Read-only

> Object: | starEmsIMGPreviousState

> Object ID: | enterprises.8164.1.1000.1.2.17

> Description: | IMG state. unmanageable(0) IMG is not CORBA reachable manageable(1) IMG is CORBA reachable

> Syntax: | INTEGER

> Access: | Read-only

> Enumeration: | unmanageable(0) manageable(1)

> Object: | starEmsIMGName

> Object ID: | enterprises.8164.1.1000.1.2.18

> Description: | The object indicates the name of IMG.

> Syntax: | DisplayString (SIZE (1..64))

> Access: | Read-only

> Object: | starEmsPortMonThreshold

> Object ID: | enterprises.8164.1.1000.1.2.19

> Description: | This object indicates the configured threshold value of port monitoring.

> Syntax: | DisplayString (SIZE (1..20))

> Access: | Read-only

> Object: | starEmsPortMonCurrent

> Object ID: | enterprises.8164.1.1000.1.2.20

> Description: | This object indicates the current threshold value of port monitoring.

> Syntax: | DisplayString (SIZE (1..20))

> Access: | Read-only

> Object: | starEmsTotalPendingEvts

> Object ID: | enterprises.8164.1.1000.1.2.21

> Description: | This object indicates the no of pending events for monitor in server queue.

> Syntax: | INTEGER(1..100000)

> Access: | Read-only

> Object: | starEmsMaxLimit

> Object ID: | enterprises.8164.1.1000.1.2.22

> Description: | This object indicates the limit of server queue to store pending events.

> Syntax: | InetAddress

> Access: | Read-only

> Object: | starEmsClientAddr

> Object ID: | enterprises.8164.1.1000.1.2.23

> Description: | The object indicates the IP address of EMS Client.

> Syntax: | DisplayString (SIZE (1..256))

> Access: | Read-only

> Object: | starEmsMonOldEvtTimeStamp

> Object ID: | enterprises.8164.1.1000.1.2.24

> Description: | This object indicates the timestamp for last Monitor Pending Event.

> Syntax: | DisplayString (SIZE (1..256))

> Access: | Read-only

> Object: | starEmsMonitorType

> Object ID: | enterprises.8164.1.1000.1.2.25

> Description: | This object indicates the monitor type.

> Syntax: | INTEGER

> Access: | Read-only

> Enumeration: | protocol(0) subscriber(1)

> Object: | starEmsMonitorUserName

> Object ID: | enterprises.8164.1.1000.1.2.26

> Description: | This object indicates the User name.

> Syntax: | DisplayString (SIZE (1..64))

> Access: | Read-only

> Object: | starEmsDevicePath

> Object ID: | enterprises.8164.1.1000.1.2.27

> Description: | This object indicates the Device name.

> Syntax: | DisplayString (SIZE (1..1024))

> Access: | Read-only

> Object: | starEmsPrevHostName

> Object ID: | enterprises,8164.1.1000.1.2.28

> Description: | This object indicates the name of the previous host running EMS before failover.

> Syntax: | DisplayString (SIZE (1..64))

> Access: | Read-only

> Object: | starEmsCurrHostName

> Object ID: | enterprises,8164.1.1000.1.2.29

> Description: | This object indicates the name of the current host running EMS.

> Syntax: | DisplayString (SIZE (1..64))

> Access: | Read-only

> Object: | starEmsP2PProtocolType

> Object ID: | enterprises,8164.1.1000.1.2.30

> Description: | This object indicates the protocol type.

> Syntax: | INTEGER

> Access: | Read-only

> Enumeration: | ip(1) tcp(2) udp(3) http(4) htpps(5) ftp(6) ftpcontrol(7) ftpdata(8) wtp(9) wsp(10) dns(11) icmp(12) pop3(13) sip(14) sdp(15) smtp(16) mms(17) filetransfer(18) rtp(19) rtsp(20) imap(21) totalp2p(22) p2punknown(23) p2pskype(24) p2pbittorrent(25) p2pedonkey(26) p2pmsn(27) p2pyahoo(28) p2pporb(29) p2pfasttrack(30) p2pslingbox(31) p2pvcast(32) p2pgnutella(33)

> Object: | starEmsP2PProtocolVal

> Object ID: | enterprises,8164.1.1000.1.2.31

> Description: | This object indicates the protocol value.

> Syntax: | INTEGER

> Access: | Read-only

> Enumeration: | uplinkbytes(0) downlinkbytes(1) totalbytes(2) uplinkpkts(3) downlinkpkts(4) totalpkts(5) uplinkbytespercent(6) downlinkbytespercent(7) totalbytespercent(8) uplinkpktspercent(9) downlinkpktspercent(10) totalpktspercent(11)

> Object: | starEmsSyslogLoggedTime

> Object ID: | enterprises,8164.1.1000.1.2.32

> Description: | This object indicates the logged time for the syslog message.

> Syntax: | TimeStamp

> Access: | Read-only

> Object: | starEmsSyslogFacility

> Object ID: | enterprises,8164.1.1000.1.2.33

> Description: | This object indicates the facility of syslog message.

> Syntax: | DisplayString (SIZE (1..64))

> Access: | Read-only

> Object: | starEmsSyslogPriority

> Object ID: | enterprises,8164.1.1000.1.2.34

> Description: | This object indicates the syslog message priority.

> Syntax: | DisplayString (SIZE (1..64))

> Access: | Read-only

> Object: | starEmsSyslogHostName

> Object ID: | enterprises,8164.1.1000.1.2.35

> Description: | This object indicates the hostname.

> Syntax: | DisplayString (SIZE (1..64))

> Access: | Read-only

> Object: | starEmsSyslogKeyword

> Object ID: | enterprises,8164.1.1000.1.2.36

> Description: | This object indicates the keywords detected in the syslog message.

> Syntax: | DisplayString (SIZE (1..64))

> Access: | Read-only

> Object: | starEmsSyslogMessage

> Object ID: | enterprises,8164.1.1000.1.2.37

> Description: | This object indicates the syslog message contents.

> Syntax: | DisplayString (SIZE (1..1024))

> Access: | Read-only

> Object: | starEmsSyslogFilePath

> Object ID: | enterprises,8164.1.1000.1.2.38

> Description: | This object indicates the syslog message file path.

> Syntax: | DisplayString (SIZE (1..1024))

> Access: | Read-only

> Object: | starEmsDBName

> Object ID: | enterprises,8164.1.1000.1.2.39

> Description: | This object indicates the database name.

> Syntax: | DisplayString (SIZE (1..1024))

> Access: | Read-only

> Object: | starEmsBulkstatCounter

> Object ID: | enterprises,8164.1.1000.1.2.40

> Description: | This object indicates the bulkstat counter name.

> Syntax: | DisplayString (SIZE (1..1024))

> Access: | Read-only

> Object: | starEmsBulkStatRecordDetails

> Object ID: | enterprises,8164.1.1000.1.2.41

> Description: | This object indicates the bulkstat record detail information.

> Syntax: | DisplayString (SIZE (1..1024))

> Access: | Read-only

> Object: | starEmsBulkStatRecordTime

> Object ID: | enterprises,8164.1.1000.1.2.42

> Description: | This object indicates the bulkstat record time

> Syntax: | TimeStamp

> Access: | Read-only

> Object: | starEmsBulkStatThreshold

> Object ID: | enterprises,8164.1.1000.1.2.43

> Description: | This object indicates the configured threshold value of the bulkstat counter.

> Syntax: | INTEGER(0..100000)

> Access: | Read-only

> Object: | starEmsbulkStatCurrent

> Object ID: | enterprises,8164.1.1000.1.2.44

> Description: | This object indicates the current threshold (delta) value of the bulkstat counter.

> Syntax: | INTEGER(0..100000)

> Access: | Read-only

> Object: | starEMSCFMcrdbsHostAddress

> Object ID: | enterprises,8164.1.1000.1.2.45

> Description: | MCRDBS IP address

> Syntax: | InetAddress

> Access: | Read-Only

> Object: | starEMSCFDbType

> Object ID: | enterprises,8164.1.1000.1.2.46

> Description: | Type sfmdb(1) Starent Format Master DataBase. sfmdbinc(2) Starent Format Master DataBase Incremental. optcmdb(6) Optmized Customer Master DataBase. optcmdbinc(7) Optmized Customer Master DataBase Incremental. optcmbldb(14) Optmized Customer Master Blacklist DataBase sfunkdb(5) Starent format unknown URL database

> Syntax: | INTEGER { sfmdb(1), sfmdbinc(2), optcmdb(6), optcmdbinc(7), optcmbldb(14) sfunkdb(5)

> Access: | Read-Only

> Object: | starEmsCFSourceDbFileName

> Object ID: | enterprises,8164.1.1000.1.2.47

> Description: | This object indicates name of the file whose SFTP/Conversion is failed.

> Syntax: | Displaystring (SIZE(1..64))

> Access: | Read-Only

> Object: | starEMSCFCdpHostAddress

> Object ID: | enterprises,8164.1.1000.1.2.48

> Description: | CDP IP Address

> Syntax: | InetAddress

> Access: | Read-Only

> Object: | starEMSCFFromDbType

> Object ID: | enterprises,8164.1.1000.1.2.49

> Description: | Type. sfmdb(1) Starent Format Master DataBase. sfmdbinc(2) Starent Format Master DataBase Incremental . blacklist(10) Blacklist DataBase. sfmbldb(11) Starent Format Master Blacklist DataBase.

> Syntax: | INTEGER sfmdb(1), sfmdbinc(2), blacklist(10), sfmbldb(11)

> Access: | Read-Only

> Object: | starEMSCFToDbType

> Object ID: | enterprises,8164.1.1000.1.2.50

> Description: | Databases Type optcmdb(6) Optmized Customer Master DataBase. optcmdbinc(7) Optmized Customer Master DataBase Incremental. sfmbldb(11) Starent Format Master Blacklist DataBase. optcmbldb(14) Optmized Customer Master Blacklist DataBase.

> Syntax: | INTEGER optcmdb(6), optcmdbinc(7), sfmbldb(11), optcmbldb(14)

> Access: | Read-Only

> Object: | starEMSCFDestDbName

> Object ID: | enterprises,8164.1.1000.1.2.51

> Description: | This object indicates the name of the destination file, used to specify the destination file created after conversion.

> Syntax: | DisplayString (SIZE(1..64)

> Access: | Read-Only

> Object: | starEMSCFFtpHostInfo

> Object ID: | enterprises,8164.1.1000.1.2.52

> Description: | FTP host IP address

> Syntax: | DisplayString (SIZE(1..64))

> Access: | Read-Only

> Object: | starEMSBulkstatCounterValue

> Object ID: | enterprises,8164.1.1000.1.2.53.

> Description: | Bulkstat counter current value

> Syntax: | Integer (0..100000)

> Access: | Read-Only

> Object: | starLESSNotifRaisedTime

> Object ID: | enterprises,8164.1.1000.1.2.54.

> Description: | This object indicates the time when this notification was generated. This will be current system's time in seconds.

> Syntax: | Integer32

> Access: | accessible-for-notify

> Object: | starLESSNotifInfo

> Object ID: | enterprises,8164.1.1000.1.2.55.

> Description: | A textual description of Less notification, which contains additional information (more than the type of alarm).

> Description: | If the text of the message exceeds 64 bytes, the message be truncated to 63 bytes and a '*' character will be appended to indicate the message has been truncated.

> Syntax: | DisplayString (SIZE (1..64))

> Access: | accessible-for-notify

> Object: | starLESSInstance

> Object ID: | enterprises,8164.1.1000.1.2.56.

> Description: | L-ESS Application Instance no.

> Syntax: | Integer32

> Access: | accessible-for-notify

> Object: | starLESSNodeName

> Object ID: | enterprises,8164.1.1000.1.2.57.

> Description: | L-ESS Application node name.

> Syntax: | DisplayString (SIZE (1..64))

> Access: | accessible-for-notify

> Object: | starLESSApplicationType

> Object ID: | enterprises,8164.1.1000.1.2.58.

> Description: | “L-ESS Application Type (pull / push / transfer). Pull (1) is L-ESS Pull application Push (2) is L-ESS Push application Transfer (3) is L-ESS Transfer application”

> Syntax: | INTEGER unknown(0) pull(1) push(2) transfer(3)

> Access: | accessible-for-notify

> Object: | starLESSThreshInt

> Object ID: | enterprises,8164.1.1000.1.2.59.

> Description: | This object indicates configured value of a thresholded parameter.

> Syntax: | Integer32

> Access: | accessible-for-notify

> Object: | starLESSThreshMeasuredInt

> Object ID: | enterprises,8164.1.1000.1.2.60.

> Description: | This object indicates measured value of a thresholded parameter.

> Syntax: | Integer32

> Access: | accessible-for-notify

> Object: | starLESSRuleBaseName

> Object ID: | enterprises,8164.1.1000.1.2.61.

> Description: | The object indicates the name of the rulebase present in filename.

> Syntax: | DisplayString (SIZE (1..64))

> Access: | accessible-for-notify

> Object: | starLESSSTXName

> Object ID: | enterprises,8164.1.1000.1.2.62.

> Description: | The object indicates the name of the STX.

> Syntax: | DisplayString (SIZE (1..64))

> Access: | accessible-for-notify

> Object: | starLESSStartofMissedRange

> Object ID: | enterprises,8164.1.1000.1.2.63.

> Description: | Begining of the range within which L-ESS has missed files.

> Syntax: | DisplayString (SIZE (1..15))

> Access: | accessible-for-notify

> Object: | starLESSEndofMissedRange

> Object ID: | enterprises,8164.1.1000.1.2.64.

> Description: | End of the range within which L-ESS has missed files.

> Syntax: | DisplayString (SIZE (1..15))

> Access: | accessible-for-notify

> Object: | starLESSFileType

> Object ID: | enterprises,8164.1.1000.1.2.65.

> Description: | The object indicates the name of the rulebase present in filename.

> Syntax: | DisplayString (SIZE (1..3)

> Access: | accessible-for-notify

> Object: | starLESSRemoteHostName

> Object ID: | enterprises,8164.1.1000.1.2.66.

> Description: | The object indicates the name of the STX.

> Syntax: | DisplayString (SIZE (1..64))

> Access: | accessible-for-notify

> Object: | starLESSApplicationStart

> Object ID: | enterprises,8164.1.1000.1.2.67.

> Description: | L-ESS application has started.

> Objects: | starLESSNotifRaisedTime starLESSNodeName starLESSInstance starLESSApplicationTyp

> Object: | starLESSApplicationReStart

> Object ID: | enterprises,8164.1.1000.1.2.68.

> Description: | L-ESS application has restarted.

> Objects: | starLESSNotifRaisedTime starLESSNodeName starLESSInstance starLESSApplicationType

> Object: | starLESSApplicationStop

> Object ID: | enterprises,8164.1.1000.1.2.69.

> Description: | L-ESS application has stopped.

> Objects: | starLESSNotifRaisedTime starLESSNodeName starLESSApplicationType starLESSNotifInfo

> Object: | starLESSApplicationTerminated

> Object ID: | enterprises,8164.1.1000.1.2.70.

> Description: | L-ESS application has been terminated.

> Objects: | starLESSNotifRaisedTime starLESSNodeName starLESSInstance starLESSApplicationType

> Object: | starLESSPullIntervalMissed

> Object ID: | enterprises,8164.1.1000.1.2.71.

> Description: | L-ESS application has missed pull interval.

> Objects: | starLESSNotifRaisedTime starLESSNodeName starLESSInstance

> Object: | starLESSThreshDiskUsage

> Object ID: | enterprises,8164.1.1000.1.2.72.

> Description: | Total Disk space used is beyond configured threshold. Probable Cause: This is a user configurable threshold.

> Objects: | starLESSNotifRaisedTime starLESSNodeName starLESSThreshMeasuredInt starLESSThreshInt

> Object: | starLESSThreshClearDiskUsage

> Object ID: | enterprises,8164.1.1000.1.2.73.

> Description: | Total disk used is now below configured threshold.Threshold condition is now clear.

> Objects: | starLESSNotifRaisedTime starLESSNodeName starLESSInstance starLESSRuleBaseName starLESSFileType starLESSSTXName starLESSStartofMissedRange starLESSEndofMissedRange starLESSNotifInfo

> Object: | starLESSRemoteConnectionFail

> Object ID: | enterprises,8164.1.1000.1.2.74.

> Description: | L-ESS application is unable to set up the connection with remote host. Probable Cause:No route to host, Authentication failure,HostUnrechable etc. Clear Condition: When LESS is able to setup the connection with remote host. Condition Clear Alarm: Clear alarm for this notification is starRemoteConnectionEstablished."

> Object: | starLESSRemoteConnectionEstablished

> Object ID: | enterprises,8164.1.1000.1.2.75.

> Description: | L-ESS application is now able to set up the connection with remote host. Probable Cause:Connection established with remote host ."

> Objects: | starLESSNotifRaisedTime starLESSNodeName starLESSInstance starLESSApplicationType starLESSRemoteHostName

> Object: | starLESSFileTransferFail

> Object ID: | enterprises,8164.1.1000.1.2.76.

> Description: | L-ESS application is failing to transfer file. Probable Cause:This trap could be raised if pull or push process when it fails to transfer files continuously. Reasons of this failure could be network error, Disk space unavailable at destination, Destination directory unavaialble.etc.

> Objects: | starLESSNotifRaisedTime starLESSNodeName starLESSInstance starLESSApplicationType starLESSRemoteHostName starLESSFileType starLESSNotifInfo

> Object: | starLESSFileTransferComplete

> Object ID: | enterprises,8164.1.1000.1.2.77.

> Description: | L-ESS application is now able to transfer file. Probable Cause: The problems due to which LESS was unable to transfer file have resolved and pull or push process has now restarted file transfer.

> Objects: | starLESSNotifRaisedTime starLESSNodeName starLESSInstance starLESSApplicationType starLESSRemoteHostName starLESSFileType

> Object: | starLESSThreshPendingFiles

> Object ID: | enterprises,8164.1.1000.1.2.78.

> Description: | Total pending files for this host are beyond configured threshold. Probable Cause: This is a user configurable threshold. The starLESSThreshPendingFiles notification will be generated by pull or push process when the total number of files pending for transfer in source directory are beyond configured threshold. Clear Condition: When number of pending files at source directory falls below configured threshold. Condition Clear Alarm: Clear alarm for this notification is starLESSThreshClearPendingFiles.

> Objects: | starLESSNotifRaisedTime starLESSNodeName starLESSInstance starLESSApplicationType starLESSSTXName starLESSFileType starLESSThreshMeasuredInt starLESSThreshInt

> Object: | starLESSThreshClearPendingFiles

> Object ID: | enterprises,8164.1.1000.1.2.79.

> Description: | Total pending files for this host are now below configured threshold. Probable Cause: This is a user configurable threshold. The starLESSThreshPendingFiles notification will be generated by pull or push process when the total number of files pending for transfer in source directory falls below configured threshold.

> Objects: | starLESSNotifRaisedTime starLESSNodeName starLESSInstance starLESSApplicationType starLESSSTXName starLESSFileType starLESSThreshMeasuredInt starLESSThreshInt

> Object: | starLESSNewHostFound

> Object ID: | enterprises,8164.1.1000.1.2.80.

> Description: | L-ESS Transfer process has detected addition of host. Probable Cause: Operator has added host in L-ESS from which files should be transferred to destination.

> Objects: | starLESSNotifRaisedTime starLESSNodeName starLESSInstance starLESSApplicationType starLESSSTXName

> Object: | starLESSHostRemoved

> Object ID: | enterprises,8164.1.1000.1.2.81.

> Description: | L-ESS Transfer process has detected removal of existing host. Probable Cause: Operator has removed existing host in L-ESS from which L-ESS was already transferring files to destination.

> Objects: | starLESSNotifRaisedTime starLESSNodeName starLESSInstance starLESSApplicationType starLESSSTXName

> Object: | starLESSMIBCompliance

> Object ID: | enterprises,8164.1.1000.1.2.82.

> Description: | The compliance statements for entities which implement the STARNET LESS MIB.

> Object: | starLESSNotifMgmtGroup

> Object ID: | enterprises,8164.1.1000.1.2.83.

> Description: | A collection of objects related with notification management on LESS.

> Objects: | starLESSNotifRaisedTime starLESSNotifInfo starLESSInstance starLESSNodeName starLESSApplicationType starLESSThreshMeasuredInt starLESSThreshInt starLESSRuleBaseName starLESSSTXName starLESSStartofMissedRange starLESSEndofMissedRange starLESSFileType starLESSRemoteHostName

> Object: | starLESSNotifGroup

> Object ID: | enterprises,8164.1.1000.1.2.84.

> Description: | A collection of notifications.

> Objects: | starLESSApplicationStart starLESSApplicationReStart starLESSApplicationStop starLESSApplicationTerminated starLESSPullIntervalMissed starLESSThreshDiskUsage starLESSThreshClearDiskUsage starLESSFileMissed starLESSRemoteConnectionFail starLESSRemoteConnectionEstablished starLESSFileTransferFail starLESSFileTransferComplete starLESSThreshPendingFiles starLESSThreshClearPendingFiles starLESSNewHostFound starLESSHostRemoved

> starentMIB(8164).starentMIBObjects(1).starentEMSMIB(1000).
> starEmsTraps(2)

> Object: | starEmsFmEmailFailed

> Object ID: | enterprises.8164.1.1000.2.3

> Description: | This notification is generated when EMS fault management module email notification failure has occurred.

> Objects: | starEmsNotifRaisedTime starEmsNotifInfo

> Object: | starEmsFmScriptFailed

> Object ID: | enterprises.8164.1.1000.2.4

> Description: | This notification is generated when EMS fault management module script execution failure has occurred.

> Objects: | starEmsNotifRaisedTime starEmsNotifInfo

> Object: | starEmsFmSyslogFailed

> Object ID: | enterprises.8164.1.1000.2.5

> Description: | This notification is generated when EMS fault management module syslog message logging failure has occurred.

> Objects: | starEmsNotifRaisedTime starEmsNotifInfo

> Object: | starEmsWebServerProcStart

> Object ID: | enterprises.8164.1.1000.2.6

> Description: | This notification is generated by EMS Process Monitoring when EMS web server process comes up.

> Objects: | starEmsNotifRaisedTime

> Object: | starEmsWebServerProcStop

> Object ID: | enterprises.8164.1.1000.2.7

> Description: | This notification is generated by EMS Process Monitoring when EMS web server process goes down.

> Objects: | starEmsNotifRaisedTime

> Object: | starEmsWebServerProcCPUUsageOverLimit

> Object ID: | enterprises.8164.1.1000.2.8

> Description: | This notification is generated by EMS Process Monitoring when EMS web server process CPU usage threshold is exceeded. The starEmsThreshold varbind indicates current EMS web server process cpu usage value in percentage.

> Objects: | starEmsNotifRaisedTime starEmsProcMonThreshold

> Object: | starEmsWebServerProcCPUUsageNormal

> Object ID: | enterprises.8164.1.1000.2.9

> Description: | This notification is generated by EMS Process Monitoring when EMS web server process cpu usage threshold comes to normal value. The starEmsThreshold varbind indicates current EMS web server process cpu usage value in percentage.

> Objects: | starEmsNotifRaisedTime starEmsProcMonThreshold

> Object: | starEmsDataBaseProcStart

> Object ID: | enterprises.8164.1.1000.2.10

> Description: | This notification is generated by EMS Process Monitoring when EMS data base process comes up.

> Objects: | starEmsNotifRaisedTime

> Object: | starEmsDataBaseProcStop

> Object ID: | enterprises.8164.1.1000.2.11

> Description: | This notification is generated by EMS Process Monitoring when EMS data base process goes down.

> Objects: | starEmsNotifRaisedTime

> Object: | starEmsDataBaseProcCPUUsageOverLimit

> Object ID: | enterprises.8164.1.1000.2.12

> Description: | This notification is generated by EMS Process Monitoring when EMS data base process cpu usage threshold is exceeded. The starEmsThreshold varbind indicates current EMS data base process cpu usage value in percentage.

> Objects: | starEmsNotifRaisedTime starEmsProcMonThreshold

> Object: | starEmsDataBaseProcCPUUsageNormal

> Object ID: | enterprises.8164.1.1000.2.13

> Description: | This notification is generated by EMS Process Monitoring when EMS data base process cpu usage threshold comes to normal value. The starEmsThreshold varbind indicates current EMS data base process cpu usage value in percentage.

> Objects: | starEmsNotifRaisedTime starEmsProcMonThreshold

> Object: | starEmsServerProcStart

> Object ID: | enterprises.8164.1.1000.2.14

> Description: | This notification is generated by EMS Process Monitoring when EMS server process comes up.

> Objects: | starEmsNotifRaisedTime

> Object: | starEmsServerProcStop

> Object ID: | enterprises.8164.1.1000.2.15

> Description: | This notification is generated by EMS Process Monitoring when EMS server process goes down.

> Objects: | starEmsNotifRaisedTime

> Object: | starEmsServerProcCPUUsageOverLimit

> Object ID: | enterprises.8164.1.1000.2.16

> Description: | This notification is generated by EMS Process Monitoring when EMS server process cpu usage threshold is exceeded. The starEmsThreshold varbind indicates current EMS server process cpu usage value in percentage.

> Objects: | starEmsNotifRaisedTime starEmsProcMonThreshold

> Object: | starEmsServerProcCPUUsageNormal

> Object ID: | enterprises.8164.1.1000.2.17

> Description: | This notification is generated by EMS Process Monitoring when EMS server process cpu usage threshold comes to normal value. The starEmsThreshold varbind indicates current EMS server process cpu usage value in percentage.

> Objects: | starEmsNotifRaisedTime starEmsProcMonThreshold

> Object: | starEmsScriptServerProcStart

> Object ID: | enterprises.8164.1.1000.2.18

> Description: | This notification is generated by EMS Process Monitoring when EMS script server process comes up.

> Objects: | starEmsNotifRaisedTime

> Object: | starEmsScriptServerProcStop

> Object ID: | enterprises.8164.1.1000.2.19

> Description: | This notification is generated by EMS Process Monitoring when EMS script server process goes down.

> Objects: | starEmsNotifRaisedTime

> Object: | starEmsScriptServerProcCPUUsageOverLimit

> Object ID: | enterprises.8164.1.1000.2.20

> Description: | This notification is generated by EMS Process Monitoring when EMS script server process cpu usage threshold is exceeded. The starEmsThreshold varbind indicates current EMS script server process cpu usage value in percentage.

> Objects: | starEmsNotifRaisedTime starEmsProcMonThreshold

> Object: | starEmsScriptServerProcCPUUsageNormal

> Object ID: | enterprises.8164.1.1000.2.21

> Description: | This notification is generated by EMS Process Monitoring when EMS script server process cpu usage threshold comes to normal value. The starEmsThreshold varbind indicates current EMS script server process cpu usage value in percentage.

> Objects: | starEmsNotifRaisedTime starEmsProcMonThreshold

> Object: | starEmsServerDirAccessible

> Object ID: | enterprises.8164.1.1000.2.22

> Description: | This notification is generated by EMS Process Monitoring when EMS server directory becomes accessible.

> Objects: | starEmsNotifRaisedTime

> Object: | starEmsServerDirNonAccessible

> Object ID: | enterprises.8164.1.1000.2.23

> Description: | This notification is generated by EMS Process Monitoring when EMS server directory is not accessible.

> Objects: | starEmsNotifRaisedTime

> Object: | starEmsServerDirUsageOverLimit

> Object ID: | enterprises.8164.1.1000.2.24

> Description: | This notification is generated by EMS Process Monitoring when EMS server directory size usage threshold is exceeded. The starEmsThreshold varbind indicates current EMS server directory size usage value in percentage.

> Objects: | starEmsNotifRaisedTime starEmsProcMonThreshold

> Object: | starEmsServerDirUsageNormal

> Object ID: | enterprises.8164.1.1000.2.25

> Description: | This notification is generated by EMS Process Monitoring when EMS server directory size usage threshold is comes to normal value. The starEmsThreshold varbind indicates current EMS server directory size usage value in percentage.

> Objects: | starEmsNotifRaisedTime starEmsProcMonThreshold

> Object: | starEmsDataBaseDirAccessible

> Object ID: | enterprises.8164.1.1000.2.26

> Description: | This notification is generated by EMS Process Monitoring when EMS data base directory becomes accessible.

> Objects: | starEmsNotifRaisedTime

> Object: | starEmsDataBaseDirNonAccessible

> Object ID: | enterprises.8164.1.1000.2.27

> Description: | This notification is generated by EMS Process Monitoring when EMS data base directory is not accessible.

> Objects: | starEmsNotifRaisedTime

> Object: | starEmsDataBaseDirUsageOverLimit

> Object ID: | enterprises.8164.1.1000.2.28

> Description: | This notification is generated by EMS Process Monitoring when EMS data base directory size usage threshold is exceeded. The starEmsThreshold varbind indicates current EMS data base directory size value in percentage.

> Objects: | starEmsNotifRaisedTime starEmsProcMonThreshold

> Object: | starEmsDataBaseDirUsageNormal

> Object ID: | enterprises.8164.1.1000.2.29

> Description: | This notification is generated by EMS Process Monitoring when EMS data base directory size usage threshold comes to normal value. The starEmsThreshold varbind indicates current EMS data base directory size usage value in percentage.

> Objects: | starEmsNotifRaisedTime starEmsProcMonThreshold

> Object: | starEmsFTPDirAccessible

> Object ID: | enterprises.8164.1.1000.2.30

> Description: | This notification is generated by EMS Process Monitoring when EMS FTP directory becomes accessible.

> Objects: | starEmsNotifRaisedTime

> Object: | starEmsFTPDirNonAccessible

> Object ID: | enterprises.8164.1.1000.2.31

> Description: | This notification is generated by EMS Process Monitoring when EMS FTP directory is not accessible.

> Objects: | starEmsNotifRaisedTime

> Object: | starEmsFTPDirUsageOverLimit

> Object ID: | enterprises.8164.1.1000.2.32

> Description: | This notification is generated by EMS Process Monitoring when EMS FTP directory usage threshold is exceeded. The starEmsThreshold varbind indicates current EMS FTP directory usage value in percentage.

> Objects: | starEmsNotifRaisedTime starEmsProcMonThreshold

> Object: | starEmsFTPDirUsageNormal

> Object ID: | enterprises.8164.1.1000.2.33

> Description: | This notification is generated by EMS Process Monitoring when EMS FTP directory size usage threshold is comes to normal value. The starEmsThreshold varbind indicates current EMS FTP directory size usage value in percentage.

> Objects: | starEmsNotifRaisedTime starEmsProcMonThreshold

> Object: | starEmsBlkArchDirAccessible

> Object ID: | enterprises.8164.1.1000.2.34

> Description: | This notification is generated by EMS Process Monitoring when EMS bulk archive directory becomes accessible.

> Objects: | starEmsNotifRaisedTime

> Object: | starEmsBlkArchDirNonAccessible

> Object ID: | enterprises.8164.1.1000.2.35

> Description: | This notification is generated by EMS Process Monitoring when EMS bulk archive directory is not accessible.

> Objects: | starEmsNotifRaisedTime

> Object: | starEmsBlkArchDirUsageOverLimit

> Object ID: | enterprises.8164.1.1000.2.36

> Description: | This notification is generated by EMS Process Monitoring when EMS bulk archive directory size usage threshold is exceeded. The starEmsThreshold varbind indicates current EMS bulk archive directory size value in percentage.

> Objects: | starEmsNotifRaisedTime starEmsProcMonThreshold

> Object: | starEmsBlkArchDirUsageNormal

> Object ID: | enterprises.8164.1.1000.2.37

> Description: | This notification is generated by EMS Process Monitoring when EMS bulk archive directory size usage threshold is comes to normal value. The starEmsThreshold varbind indicates current EMS bulk archive directory size usage value in percentage.

> Objects: | starEmsNotifRaisedTime starEmsProcMonThreshold

> Object: | starEmsInterfaceStateUp

> Object ID: | enterprises.8164.1.1000.2.38

> Description: | This notification is generated by EMS Process Monitoring when EMS interface state comes up. Varbinds indicate interface IP address and name.

> Objects: | starEmsNotifRaisedTime starEmsInterfaceAddr starEmsInterfaceName

> Object: | starEmsInterfaceStateDown

> Object ID: | enterprises.8164.1.1000.2.39

> Description: | This notification is generated by EMS Process Monitoring when EMS interface state goes down. Varbinds indicate interface address and name

> Objects: | starEmsNotifRaisedTime starEmsInterfaceAddr starEmsInterfaceName

> Object: | starEmsCPUUsageOverLimit

> Object ID: | enterprises.8164.1.1000.2.40

> Description: | This notification is generated by EMS Process Monitoring when EMS CPU usage threshold is exceeded. The starEmsThreshold varbind indicates current EMS CPU usage value in percentage.

> Objects: | starEmsNotifRaisedTime starEmsProcMonThreshold

> Object: | starEmsCPUUsageNormal

> Object ID: | enterprises.8164.1.1000.2.41

> Description: | This notification is generated by Process Monitoring when EMS CPU usage threshold comes to normal value. The starEmsThreshold varbind indicates current EMS CPU usage value in percentage.

> Objects: | starEmsNotifRaisedTime starEmsProcMonThreshold

> Object: | starEmsSwapUsageOverLimit

> Object ID: | enterprises.8164.1.1000.2.42

> Description: | This notification is generated by Process Monitoring when EMS swap usage threshold is exceeded. The starEmsThreshold varbind indicates current EMS swap usage value in percentage.

> Objects: | starEmsNotifRaisedTime starEmsProcMonThreshold

> Object: | starEmsSwapUsageNormal

> Object ID: | enterprises.8164.1.1000.2.43

> Description: | This notification is generated by Process Monitoring when EMS swap usage threshold comes to normal value. The starEmsThreshold varbind indicates current EMS swap usage value in percentage.

> Objects: | starEmsNotifRaisedTime starEmsProcMonThreshold

> Object: | starEmsPCFtpFailed

> Object ID: | enterprises.8164.1.1000.2.44

> Description: | This notification is generated by Periodic Configuration Saving module when FTP fails while fetching a config file from the IMG.

> Objects: | starEmsNotifRaisedTime starEmsImgAddr starEmsFtpFileName starEmsNotifInfo

> Object: | starEmsPCFileDeletionFailed

> Object ID: | enterprises.8164.1.1000.2.45

> Description: | This notification is generated by Periodic Configuration Saving module when deletion of file on the IMG fails.

> Objects: | starEmsNotifRaisedTime starEmsIMGAddr starEmsFtpFileName starEmsNotifInfo

> Object: | starEmsBulkStatFtpFailed

> Object ID: | enterprises.8164.1.1000.2.46

> Description: | This notification is generated by Bulkstat module when bulkstat file transfer operation from IMG fails or gets delayed than the expected time

> Objects: | starEmsNotifRaisedTime starEmsBulkStatFileXferTime starEmsIMGState starEmsIMGAddr

> Object: | starEmsBulkStatFtpClear

> Object ID: | enterprises.8164.1.1000.2.47

> Description: | This notification is generated by BulkStat module when bulkstat file transfer operation from IMG succeeds and starEmsBulkStatFtpFailed trap is already raised for the IMG.

> Objects: | starEmsNotifRaisedTime starEmsIMGAddr

> Object: | starEmsXMLFtpFailed

> Object ID: | enterprises.8164.1.1000.2.48

> Description: | This notification is generated by EMS when FTP of Bulkstat XML file on the NMS fails.

> Objects: | starEmsNotifRaisedTime starEmsXMLFtpDestAddr starEmsXMLFtpDestPath starEmsNotifInfo

> Object: | starEmsXMLFtpSuccess

> Object ID: | enterprises.8164.1.1000.2.49

> Description: | This notification is generated by EMS when FTP of Bulk stat XML file on the NMS succeed.

> Objects: | starEmsNotifRaisedTime starEmsXMLFtpDestAddr starEmsXMLFtpDestPath starEmsNotifInfo

> Object: | starEmsIMGUnmanageable

> Object ID: | enterprises.8164.1.1000.2.50

> Description: | This notification is generated by EMS when IMG becomes unmanageable.

> Objects: | starEmsNotifRaisedTime starEmsIMGName starEmsIMGAddr starEmsIMGPreviousState

> Object: | starEmsIMGManageable

> Object ID: | enterprises.8164.1.1000.2.51

> Description: | This notification is generated by EMS when IMG becomes manageable.

> Objects: | starEmsNotifRaisedTime starEmsIMGName starEmsIMGAddr starEmsIMGPreviousState

> Object: | starEmsPortMonThresholdBelowLimit

> Object ID: | enterprises.8164.1.1000.2.52

> Description: | This notification is generated by EMS Port Monitoring when delta value for a particular port has fallen below the configured threshold value.

> Objects: | starEmsNotifRaisedTime starEmsIMGName starEmsIMGAddr starSlotNum starPortNum starEmsPortMonThreshold starEmsPortMonCurrent

> Object: | starEmsPortMonThresholdNormal

> Object ID: | enterprises.8164.1.1000.2.53

> Description: | This notification is generated by EMS Port Monitoring when delta value for a particular port threshold comes to normal value.

> Objects: | starEmsNotifRaisedTime starEmsIMGName starEmsIMGAddr starSlotNum starPortNum starEmsPortMonThreshold starEmsPortMonCurrent

> Object: | starEmsPortMonError

> Object ID: | enterprises.8164.1.1000.2.54

> Description: | This notification is generated by EMS Port Monitoring when any error in fetching values from a particular IMG.

> Objects: | starEmsNotifRaisedTime starEmsIMGName starEmsIMGAddr starEmsNotifInfo

> Object: | starEmsWebServerProcDetectRestart

> Object ID: | enterprises.8164.1.1000.2.55

> Description: | This notification is generated by EMS Process Monitoring when EMS web server process restart is detected.

> Objects: | starEmsNotifRaisedTime

> Object: | starEmsDataBaseProcDetectRestart

> Object ID: | enterprises.8164.1.1000.2.56

> Description: | This notification is generated by EMS Process Monitoring when EMS Data Base process restart is detected.

> Objects: | starEmsNotifRaisedTime

> Object: | starEmsServerProcDetectRestart

> Object ID: | enterprises.8164.1.1000.2.57

> Description: | This notification is generated by EMS Process Monitoring when EMS server process restart is detected.

> Objects: | starEmsNotifRaisedTime

> Object: | starEmsScriptServerProcDetectRestart

> Object ID: | enterprises.8164.1.1000.2.58

> Description: | This notification is generated by EMS Process Monitoring when EMS Script server process restart is detected.

> Objects: | starEmsNotifRaisedTime

> Object: | starEmsBulkStatServerProcStart

> Object ID: | enterprises.8164.1.1000.2.59

> Description: | This notification is generated by EMS Process Monitoring when Ems Bulkstat server process comes up.

> Objects: | starEmsNotifRaisedTime

> Object: | starEmsBulkStatServerProcStop

> Object ID: | enterprises.8164.1.1000.2.60

> Description: | This notification is generated by EMS Process Monitoring when Ems Bulkstat server process goes down.

> Objects: | starEmsNotifRaisedTime

> Object: | starEmsBulkStatServerProcDetectRestart

> Object ID: | enterprises.8164.1.1000.2.61

> Description: | This notification is generated by EMS Process Monitoring when Ems Bulkstat server process restart is detected.

> Objects: | starEmsNotifRaisedTime

> Object: | starEmsBulkStatServerProcCPUUsageOverLimit

> Object ID: | enterprises.8164.1.1000.2.62

> Description: | This notification is generated by EMS Process Monitoring when EMS Bulkstat server process cpu usage threshold is exceeded. The starEmsThreshold varbind indicates current EMS Bulkstat server process cpu usage value in percentage.

> Objects: | starEmsNotifRaisedTime starEmsProcMonThreshold

> Object: | starEmsBulkStatServerProcCPUUsageNormal

> Object ID: | enterprises.8164.1.1000.2.63

> Description: | This notification is generated by EMS Process Monitoring when EMS Bulkstat server process cpu usage threshold comes to normal value. The starEmsThreshold varbind indicates current EMS Bulkstat server process cpu usage value in percentage.

> Objects: | starEmsNotifRaisedTime starEmsProcMonThreshold

> Object: | starEmsBulkStatParserProcStart

> Object ID: | enterprises.8164.1.1000.2.64

> Description: | his notification is generated by EMS Process Monitoring when Ems Bulkstat parser process comes up.

> Objects: | starEmsNotifRaisedTime

> Object: | starEmsBulkStatParserProcStop

> Object ID: | enterprises.8164.1.1000.2.65

> Description: | This notification is generated by EMS Process Monitoring when Ems Bulkstat parser process goes down.

> Objects: | starEmsNotifRaisedTime

> Object: | starEmsBulkStatParserProcDetectRestart

> Object ID: | enterprises.8164.1.1000.2.66

> Description: | This notification is generated by EMS Process Monitoring when Ems Bulkstat parser process restart is detected.

> Objects: | starEmsNotifRaisedTime

> Object: | starEmsBulkStatParserProcCPUUsageOverLimit

> Object ID: | enterprises.8164.1.1000.2.67

> Description: | This notification is generated by EMS Process Monitoring when EMS Bulkstat parser process cpu usage threshold is exceeded. The starEmsThreshold varbind indicates current EMS Bulkstat parser process cpu usage value in percentage.

> Objects: | starEmsNotifRaisedTime starEmsProcMonThreshold

> Object: | starEmsBulkStatParserProcCPUUsageNormal

> Object ID: | enterprises.8164.1.1000.2.68

> Description: | This notification is generated by EMS Process Monitoring when EMS Bulkstat parser process cpu usage threshold comes to normal value. The starEmsThreshold varbind indicates current EMS Bulkstat parser process cpu usage value in percentage.

> Objects: | starEmsNotifRaisedTime starEmsProcMonThreshold

> Object: | starEmsIMGRateControlStart

> Object ID: | enterprises.8164.1.1000.2.69

> Description: | This notification is generated by EMS when IMG Rate-Control is stated. IMG's CORBA server resource utilization is over limit.

> Objects: | starEmsNotifRaisedTime starEmsIMGName starEmsIMGAddr

> Object: | starEmsIMGRateControlStop

> Object ID: | enterprises.8164.1.1000.2.70

> Description: | This notification is generated by EMS when IMG Rate-Control is stopped. IMG's CORBA server resource utilization is over limit.

> Objects: | starEmsNotifRaisedTime starEmsIMGName starEmsIMGAddr

> Object: | starEmsMonitorQueueFull

> Object ID: | enterprises.8164.1.1000.2.71

> Description: | This notification is generated by EMS when monitor event queue is full.

> Objects: | starEmsNotifRaisedTime starEmsTotalPendingEvts starEmsMaxLimit starEmsClientAddr starEmsMonOldEvtTimeStamp starEmsMonitorType starEmsMonitorUserName

> Object: | starEmsMonitorQueueInLimit

> Object ID: | enterprises.8164.1.1000.2.72

> Description: | This notification is generated by EMS when the monitor event queue is partially full.

> Objects: | starEmsNotifRaisedTime starEmsTotalPendingEvts starEmsMaxLimit starEmsClientAddr starEmsMonitorType starEmsMonitorUserName

> Object: | starClusterFailoverHappened

> Object ID: | enterprises.8164.1.1000.2.73

> Description: | This notification is generated by EMS when cluster failover happens.

> Objects: | starEmsNotifRaisedTime starEmsPrevHostName starEmsCurrHostName

> Object: | starEmsDBBackupNoDiscSpace

> Object ID: | enterprises.8164.1.1000.2.74

> Description: | This notification is generated by EMS when disc space gets full. No disc space is available.

> Objects: | starEmsNotifRaisedTime starEmsDevicePath

> Object: | starEMSP2PProtocolUsageHigh

> Object ID: | enterprises.8164.1.1000.2.75

> Description: | This notification is generated by EMS when protocol values are beyond the threshold value.

> Objects: | starEmsNotifRaisedTime starEmsIMGName starEmsP2PProtocolType starEmsP2PProtocolVal

> Object: | starEmsP2PProtocolUsageLimit

> Object ID: | enterprises.8164.1.1000.2.76

> Description: | This notification is generated by EMS when protocol values are within limit.

> Objects: | starEmsNotifRaisedTime starEmsIMGName starEmsP2PProtocolType starEmsP2PProtocolVal

> Object: | starEmsKeywordDetectedInSyslog

> Object ID: | enterprises.8164.1.1000.2.77

> Description: | This notification is generated by EMS when a configured keyword is detected in the syslog message.

> Objects: | starEmsNotifRaisedTime starEmsSyslogLoggedTime starEmsSyslogFacility starEmsSyslogPriority starEmsSyslogHostname starEmsSyslogKeyword starEmsSyslogMessage starEmsSyslogFilePath

> Object: | starEmsDBMigration

> Object ID: | enterprises.8164.1.1000.2.78

> Description: | This notification is generated by EMS when the database migration is done for a particular database.

> Objects: | starEmsNotifRaisedTime starEmsDBName

> Object: | starEmsNBServerProcStart

> Object ID: | enterprises.8164.1.1000.2.79

> Description: | This notification is generated by EMS process monitoring when the EMS NB server process comes up.

> Objects: | starEmsNotifRaisedTime

> Object: | starEmsNBServerProcStop

> Object ID: | enterprises.8164.1.1000.2.80

> Description: | This notification is generated by EMS process monitoring when the EMS NB server process goes down.

> Objects: | starEmsNotifRaisedTime

> Object: | starEmsNBServerProcDetectRestart

> Object ID: | enterprises.8164.1.1000.2.81

> Description: | This notification is generated by EMS process monitoring when the EMS NB server process restart is detected.

> Objects: | starEmsNotifRaisedTime

> Object: | starEmsNBServerProcCPUUsageOverLimit

> Object ID: | enterprises.8164.1.1000.2.82

> Description: | This notification is generated by EMS process monitoring when the NB server process CPU usage threshold is exceeded. The starEmsThreshold varbind indicates current NB server process CPU value as a percentage.

> Objects: | starEmsNotifRaisedTime starEmsProcMonThreshold

> Object: | starEmsNBServerProcCPUUsageNormal

> Object ID: | enterprises.8164.1.1000.2.83

> Description: | This notification is generated by EMS process monitoring when the NB server process CPU usage threshold comes to a normal value. The starEmsThreshold varbind indicates current NB server process cpu value as a percentage.

> Objects: | starEmsNotifRaisedTime starEmsProcMonThreshold

> Object: | starEmsNotifyServiceProcStart

> Object ID: | enterprises.8164.1.1000.2.84

> Description: | This notification is generated by EMS process monitoring when the EMS notification service process comes up.

> Objects: | starEmsNotifRaisedTime

> Object: | starEmsNotifyServiceProcStop

> Object ID: | enterprises.8164.1.1000.2.85

> Description: | This notification is generated by EMS process monitoring when the EMS notification service process goes down.

> Objects: | starEmsNotifRaisedTime

> Object: | starEmsNotifyServiceProcDetectRestart

> Object ID: | enterprises.8164.1.1000.2.86

> Description: | This notification is generated by EMS process monitoring when the EMS notification service process restart is detected.

> Objects: | starEmsNotifRaisedTime

> Object: | starEmsNotifyServiceProcCPUUsageOverLimit

> Object ID: | enterprises.8164.1.1000.2.87

> Description: | This notification is generated by EMS process monitoring when the Ems Notification Service process CPU usage threshold is exceeded. The starEmsThreshold varbind indicates current Ems Notification Service process cpu usage value as a percentage.

> Objects: | starEmsNotifRaisedTime starEmsProcMonThreshold

> Object: | starEmsNotifyServiceProcCPUUsageNormal

> Object ID: | enterprises.8164.1.1000.2.88

> Description: | This notification is generated by EMS process monitoring when the Ems Notification Service process CPU usage threshold comes to normal. The starEmsThreshold varbind indicates current Ems Notification Service process cpu usage value as a percentage.

> Objects: | starEmsNotifRaisedTime starEmsProcMonThreshold

> Object: | starEmsBulkStatCounterThresholdAboveLimit

> Object ID: | enterprises.8164.1.1000.2.89

> Description: | This notification is generated by the EMS bulkstat parser when the delta value for a particular bulkstat counter has exceeded its configured threshold value.

> Objects: | starEmsNotifRaisedTime starEmsIMGName starEmsBulkstatCounter starEmsBulkStatRecordDetails starEmsBulkStatRecordTime starEmsBulkStatThreshold starEmsBulkStatCurrent

> Object: | starEmsBulkStatCounterThresholdNormal

> Object ID: | enterprises.8164.1.1000.2.90

> Description: | This notification is generated by the EMS bulkstat parser when the delta value for a particular bulkstat counter comes to the normal value.

> Objects: | starEmsNotifRaisedTime starEmsIMGName starEmsBulkstatCounter starEmsBulkStatRecordDetails starEmsBulkStatRecordTime starEmsBulkStatThreshold starEmsBulkStatCurrent

> Object: | starEmsCFDBDirAccessible

> Object ID: | enterprises.8164.1.1000.2.91

> Description: | This notification is generated by EMS Process Monitoring when EMS content filtering directory is accessible.

> Objects: | starEMSNotifRaisedTime

> Object: | starEmsCFDBDirNonAccessible

> Object ID: | enterprises.8164.1.1000.2.92

> Description: | This notification is generated by EMS Process Monitoring when EMS content filtering directory is not accessible. Possible Cause: None given. Action Clear: A starEmsCFDBDirAccessible message is generated when database comes back online.

> Objects: | starEMSNotifRaisedTime

> Object: | starEmsCFDBDirUsageOverLimit

> Object ID: | enterprises.8164.1.1000.2.93

> Description: | EMS content filtering directory usage threshold is exceeded. Possible Cause: This is a user-configurable parameter. Action Clear: A starEMSCFDBDirUsageNormal notification is issued when usage drops below the threshold.

> Objects: | starEMSNotifRaisedTime starEMSProcMonThreshold

> Object: | starEmsCFDBDirUsageNormal

> Object ID: | enterprises.8164.1.1000.2.94

> Description: | EMS content filtering directory usage has come to normal value.

> Objects: | starEMSNotifRaisedTime starEMSProcMonThreshold

> Object: | starEmsCFDbImportFailed

> Object ID: | enterprises.8164.1.1000.2.95

> Description: | This notification is generated by CFEMS when failed to Import database file. Possible Cause: None given Action Clear: A starEmsCFDbImportSucceeded message is generated when the database file is successfully imported.

> Objects: | starEmsNotifRaisedTime, starEmsCFMcrdbsHostAddress, starEmsCFDbType, starEmsCFSourceDbFileName

> Object: | starEmsCFDbImportSucceeded

> Object ID: | enterprises.8164.1.1000.2.96

> Description: | This notification is generated by CFEMS Database file is imported.

> Objects: | starEmsNotifRaisedTime, starEmsCFMcrdbsHostAddress, starEmsCFDbType, starEmsCFSourceDbFileName

> Object: | starEmsCFDbExportFailed

> Object ID: | enterprises.8164.1.1000.2.97

> Description: | This notification is generated by CFEMS when database has failed to export. Possible Cause: None given Action Clear: A starEmsCFDbExportSucceeded message is generated.

> Objects: | starEmsNotifRaisedTime, starEmsCFCdpHostAddress, starEmsCFDbType, starEmsCFSourceDbFileName

> Object: | starEmsCFDbExportSucceeded

> Object ID: | enterprises.8164.1.1000.2.98

> Description: | This notification is generated by CFEMS on successful export of a database file.

> Objects: | starEmsNotifRaisedTime, starEmsCFCdpHostAddress, starEmsCFDbType, starEmsCFSourceDbFileName

> Object: | starEmsCFDbConversionFailed

> Object ID: | enterprises.8164.1.1000.2.99

> Description: | CF database conversion/manipulation operation failed Possible Cause: None given Action Clear: a starEmsCFDbConversionSucceeded message is generated.

> Objects: | starEmsNotifRaisedTime, starEmsCFFromDbType, starEmsCFToDbType, starEmsCFSourceDbFileName, starEmsCFDestDbFileName

> Object: | starEmsCFDbConversionSucceeded

> Object ID: | enterprises.8164.1.1000.2.100

> Description: | This notification is generated by CFEMS when Database conversion done successfully.

> Objects: | starEmsNotifRaisedTime, starEmsCFFromDbType, starEmsCFToDbType, starEmsCFSourceDbFileName, starEmsCFDestDbFileName

> Object: | starEmsCFFtpConnetionFailed

> Object ID: | enterprises.8164.1.1000.2.101

> Description: | SFTP Connection failed. Possible Cause: None given Action Clear: None given

> Objects: | starEmsNotifRaisedTime, starEmsCFFtpHostInfo

> Object: | starEmsBulkStatCounterUsageOverLimit

> Object ID: | enterprises.8164.1.1000.2.102

> Description: | This notification is generated by EMS bulkstat parser when counter value for a particular bulkstat counter has reached or exceeded the configured threshold value. Possible Cause: This is a user-configurable parameter. Action Clear: A starEmsBulkStatCounterUsageNormal message is generated when usage drops below the threshold.

> Objects: | starEmsNotifRaisedTime, starEmsIMGName, starEmsBulkStatCounter, starEmsBulkStatRecordDetails, starEmsBulkStatRecordTime, starEmsBulkStatThreshold, starEmsBulkStatCounterValue

> Object: | starEmsBulkStatCounterUsageNormal

> Object ID: | enterprises.8164.1.1000.2.103

> Description: | This message is generated when usage drops below the threshold.

> Objects: | starEmsNotifRaisedTime, starEmsIMGName, starEmsBulkStatCounter, starEmsBulkStatRecordDetails, starEmsBulkStatRecordTime, starEmsBulkStatThreshold, starEmsBulkStatCounterValue

> Object: | starEmsConfigBackupFtpFailed

> Object ID: | enterprises.8164.1.1000.2.104

> Description: | This notification is generated by EMS when FTP of Config Backup file from STxx to EMS fails.

> Objects: | starEmsNotifRaisedTime starEmsIMGName starEmsNotifInfo

> Object: | starEmsConfigBackupFtpSuccess

> Object ID: | enterprises.8164.1.1000.2.105

> Description: | his notification is generated by EMS when FTP of Config Backup file from STxx to EMS succeed.

> Objects: | starEmsNotifRaisedTime starEmsIMGName starEmsNotifInfo

> starentMIB(8164).starentMIBObjects(1).starentEMSMIB(1000).
> starEmsMIBConformances(3)
> starentMIB(8164).starentMIBObjects(1).starentEMSMIB(1000).
> starEmsMIBConformances(3).starEmsMIBCompliances(1)

> Object: | starEmsMIBCompliance

> Object ID: | enterprises.8164.1.1000.3.1.1

> Description: | The compliance statements for entities which implement the STARENT EMS MIB.

> Required Groups: | starEmsNotifMgmtGroup starEmsNotifGroup

> starentMIB(8164).starentMIBObjects(1).starentEMSMIB(1000).
> starEmsMIBConformances(3).starEmsMIBGroups(2)

> Object Group: | starEmsNotifMgmtGroup

> Object ID: | enterprises.8164.1.1000.3.2.1

> Description: | This is a collection of objects related with notification management on EMS.

> Objects: | starEmsNotifInfo starEmsNotifRaisedTime starEmsProcMonThreshold starEmsInterfaceAddr starEmsInterfaceName starEmsIMGAddr starEmsFtpFileName starEmsIMGState starEmsBulkStatFileXferTime starEmsXMLFtpFileName starEmsXMLFtpDestAddr starEmsXMLFtpDestPath starEmsIMGPreviousState starEmsIMGName starEmsPortMonThreshold starEmsPortMonCurrent starEmsDevicePath starEmsPrevHostName starEmsCurrHostName starEmsP2PProtocolType starEmsP2PProtocolValue starEmsSyslogLoggedTime starEmsSyslogFacility starEmsSyslogPriority starEmsSyslogHostname starEmsSyslogKeyword starEmsSyslogMessage starEmsSyslogFilePath starEmsDBName starEmsBulkStatCounter starEmsBulkStatRecordDetails starEmsBulkStatRecordTime starEmsBulkStatThreshold starEmsBulkStatCurrent starEmsCFMcrdbsHostAddress, starEmsCFDbType, starEmsCFSourceDbFileName, starEmsCFCdpHostAddress, starEmsCFFromDbType, starEmsCFToDbType, starEmsCFDestDbFileName, starEmsBulkStatCounterValue

> Object Group: | starEmsNotifGroup

> Object ID: | enterprises.8164.1.1000.3.2.2

> Description: | A collection of EMS notifications.

> Object Group: | starEmsFmEmailFailed starEmsFmScriptFailed starEmsFmSyslogFailed starEmsWebServerProcStart starEmsWebServerProcStop starEmsWebServerProcCPUUsageOverLimit starEmsWebServerProcCPUUsageNormal starEmsDataBaseProcStart starEmsDataBaseProcStop starEmsDataBaseProcCPUUsageOverLimit starEmsDataBaseProcCPUUsageNormal starEmsServerProcStart starEmsServerProcStop starEmsServerProcCPUUsageOverLimit starEmsServerProcCPUUsageNormal starEmsScriptServerProcStart starEmsScriptServerProcStop starEmsScriptServerProcCPUUsageOverLimit starEmsScriptServerProcCPUUsageNormal starEmsServerDirAccessible starEmsServerDirNonAccessible starEmsServerDirUsageOverLimit starEmsServerDirUsageNormal starEmsDataBaseDirAccessible starEmsDataBaseDirNonAccessible starEmsDataBaseDirUsageOverLimit starEmsDataBaseDirUsageNormal starEmsFTPDirAccessible starEmsFTPDirNonAccessible starEmsFTPDirUsageOverLimit starEmsFTPDirUsageNormal starEmsBlkArchDirAccessible starEmsBlkArchDirNonAccessible starEmsBlkArchDirUsageOverLimit starEmsBlkArchDirUsageNormal starEmsInterfaceStateUp starEmsInterfaceStateDown starEmsCPUUsageOverLimit starEmsCPUUsageNormal starEmsSwapUsageOverLimit starEmsSwapUsageNormal starEmsPCFtpFailed starEmsPCFileDeletionFailed starEmsBulkStatFtpFailed starEmsBulkStatFtpClear starEmsXMLFtpFailed starEmsXMLFtpSuccess starEmsIMGUnmanageable starEmsIMGManageable starEmsPortMonThresholdBelowLimit starEmsPortMonThresholdNormal starEmsPortMonError starEmsWebServerProcDetectRestart starEmsDataBaseProcDetectRestart starEmsServerProcDetectRestart starEmsScriptServerProcDetectRestart starEmsBulkStatServerProcStart starEmsBulkStatServerProcStop starEmsBulkStatServerProcDetectRestart starEmsBulkStatServerProcCPUUsageOverLimit starEmsBulkStatServerProcCPUUsageNormal starEmsBulkStatParserProcStart starEmsBulkStatParserProcStop starEmsBulkStatParserProcDetectRestart starEmsBulkStatParserProcCPUUsageOverLimit starEmsBulkStatParserProcCPUUsageNormal starEmsIMGRateControlStart starEmsIMGRateControlStop starEmsMonitorQueueFull starEmsMonitorQueueInLimit starEmsNotifRaisedTime starClusterFailoverHappened starEmsDBBackupNoDiscSpace starEmsP2PProtocolUsageHigh starEmsP2PProtocolUsageLimit starEmsNBServerProcStart starEmsNBServerProcStop starEmsNBServerProcDetectRestart starEmsNBServerProcCPUUsageOverLimit starEmsNBServerProcCPUUsageNormal starEmsNotifyServiceProcStart starEmsNotifyServiceProcStop starEmsNotifyServiceProcDetectRestart starEmsNotifyServiceProcCPUUsageOverLimit starEmsNotifyServiceProcCPUUsageNormal starEmsKeywordDetectedInSyslog starEmsDBMigration starEmsBulkStatCounterThresholdAboveLimit starEmsBulkStatCounterThresholdNormal starEmsCFDBDirAccessible starEmsCFDBDirNonAccessible, starEmsCFDBDirUsageOverLimit, starEmsCFDBDirUsageNormal, starEmsCFDbImportFailed, starEmsCFDbImportSucceeded, starEmsCFDbExportFailed, starEmsCFDbExportSucceeded, starEmsCFDbConversionFailed, starEmsCFDbConversionSucceeded, starEmsCFFtpConnetionFailed, starEmsBulkStatCounterUsageOverLimit, starEmsBulkStatCounterUsageNormal starEmsConfigBackupFtpFailed starEmsConfigBackupFtpSuccess

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883