> ACS Packet Filter Configuration Mode Commands
> The Active Charging Service (ACS) Packet Filter Configuration Mode is used to create and configure ACS packet filters.
> Important: The commands or keywords/variables that are available are dependent on platform type, product version, and installed license(s).
> direction
> This command configures the direction in which the filter has to be applied.
> Product
> ACS
> Privilege
> Security Administrator, Administrator
> Syntax
> direction { bi-directional | downlink | uplink }
> default direction
> default
> Applies the default configuration.
> Default: bi-directional
> bi-directional
> Specifies that the filter is to be applied in both uplink and downlink directions.
> downlink
> Specifies that the filter is to be applied in only downlink direction.
> uplink
> Specifies that the filter is to be applied in only uplink direction.
> Usage
> Use this command to configure the direction in which the filter has to be applied.
> Example
> The following command configures the filter in the downlink direction:
> direction downlink
> end
> This command returns the CLI prompt to the Exec mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> end
> Usage
> Use this command to change to the Exec mode.
> exit
> This command exits the Packet Filter Configuration mode and returns to the Active Charging Service Configuration mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> exit
> Usage
> Use this command to return to the Active Charging Service Configuration mode.
> ip local-port
> This command configures the IP 5-tuple local port setting.
> Product
> ACS
> Privilege
> Security Administrator, Administrator
> Syntax
> ip local-port { = port_number | range start_port_number to end_port_number }
> no ip local-port
> no
> Removes the local-port configuration, if previously configured.
> = port_number
> Specifies the port number of the transport protocol.
> port_number must be the port number, and must be an integer from 1 through 65535.
> range start_port_number to end_port_number
> range specifies a range of port numbers.
> start_port_number and end_port_number must be integers from 1 through 65535. end_port_number must be greater than start_port_number.
> Usage
> Use this command to configure a specific or range of IP local port setting for a packet filter.
> Example
> The following command configures the IP local port as 456:
> ip local-port = 456
> ip protocol
> This command configures the IP protocol setting.
> Product
> ACS
> Privilege
> Security Administrator, Administrator
> Syntax
> ip protocol { = protocol_number | range start_protocol_number to end_protocol_number }
> no ip protocol
> no
> Removes the IP protocol configuration, if previously configured.
> = protocol_number
> Specifies the transport protocol field in the IP header.
> protocol_number must be the numerical value of the protocol, and must be an integer from 1 through 255.
> range start_protocol_number to end_protocol_number
> Important: In StarOS 9.0 and later releases this keyword is obsolete.
> range specifies a range of protocol assignment numbers.
> start_protocol_number and end_protocol_number must be integers from 1 through 255. end_protocol_number must be greater than start_protocol_number.
> Usage
> Use this command to configure the protocol setting for a packet filter.
> Example
> The following command configures the protocol assignment number 300:
> ip protocol = 300
> ip remote-address
> This command configures the IP remote address setting.
> Product
> ACS
> Privilege
> Security Administrator, Administrator
> Syntax
> ip remote-address { = { ip_address | ip_address/mask } | range { ip_address | ip_address/mask } to { ip_address | ip_address/mask } }
> no ip remote-address
> no
> Removes the remote address configuration, if previously configured.
> = { ip_address | ip_address/mask }
> ip_address specifies the IP address in IPv4 dotted decimal or IPv6 colon separated notation format.
> ip_address/mask specifies the IP address in IPv4 dotted decimal or IPv6 colon separated notation format, and the number of subnet bits representing the subnet mask in shorthand.
> range { start_ip_address | start_ip_address/mask } to { end_ip_address | end_ip_address/mask }
> Important: In StarOS 9.0 and later releases this keyword is obsoleted.
> range specifies a range of IP addresses.
> start_ip_address and end_ip_address specify, for the range, the starting and ending IP address in IPv4 dotted decimal or IPv6 colon separated notation format. end_ip_address must be greater than start_ip_address.
> start_ip_address/mask and end_ip_address/mask specify, for the range, the starting and ending IP address in IPv4 dotted decimal or IPv6 colon separated notation format, and the number of subnet bits representing the subnet mask in shorthand. end_ip_address/mask must be greater than start_ip_address/mask.
> Usage
> Use this command to configure the remote IP address setting for a packet filter.
> Example
> The following command configures the IP remote address as 1.2.3.4/24:
> ip remote-address = 1.2.3.4/24
> ip remote-port
> This command configures the IP remote port setting.
> Product
> ACS
> Privilege
> Security Administrator, Administrator
> Syntax
> ip remote-port { = port_number | range start_port_number to end_port_number }
> no ip remote-port
> no
> Removes the remote port configuration, if previously configured.
> = port_number
> Specifies port number of the transport protocol.
> port_number must be the port number, and must be an integer from 1 through 65535.
> range start_port_number to end_port_number
> Specifies a range of port numbers.
> start_port_number and end_port_number must be integers from 1 through 65535. end_port_number must be greater than start_port_number.
> Usage
> Use this command to configure a specific or range of IP remote port settings for a packet filter.
> Example
> The following command configures the IP remote port as 789:
> ip remote-port = 789
> priority
> This command configures the packet filter’s priority.
> Product
> ACS
> Privilege
> Security Administrator, Administrator
> Syntax
> priority priority
> no priority
> no
> Removes the priority configuration, if previously configured.
> priority
> Specifies this packet filter’s priority, and must be an integer from 0 through 255.
> Usage
> Use this command to configure the packet filter’s priority. Without this setting, this filter will not be used.
> Example
> The following command configures the packet filter’s priority as 3:
> priority 3

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883