> HLR Configuration Mode Commands
> The HLR Configuration Mode provides the commands and parameters to configure the home location register (HLR) node that is the database containing the subscriber profile and connection information for a specific GPRS/UMTS core network.
> The HLR Configuration Mode is a sub-mode derived from the MAP Configuration Mode which controls the MAP service configuration. It is the MAP service that provides the application-layer protocol support used to connect the HLR to other nodes in the network such as the SGSN.
> Important: The commands or keywords/variables that are available are dependent on platform type, product version, and installed license(s).
> end
> Exits the current configuration mode and returns to the Exec mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> end
> Usage
> Return to the Exec mode.
> exit
> Exits the current configuration mode and returns to the global configuration mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> exit
> Usage
> Return to the context configuration mode.
> imsi
> This command sets up IMSI (International Mobile Subscriber Identity) -based configuration. (IMSI) prefix which includes the Mobile Country Code (MCC), the Mobile Network Code (MNC).
> Product
> SGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> [ no ] imsi { any | starts-with prefix_number } { imsi [ sgsn-source-address-format point-code-ssn [ source-ssn ssn ] | isdn isdn_numbe r | mobile-global-title mgt_number | point-code pt-code } }
> no
> Removes the imsi-prefix definition from the configuration.
> any
> Configures acceptance of any IMSI prefix.
> start-with prefix_number
> Selects IMSI prefix-based routing.
> prefix_number is a string of up to 15 integers.
> imsi
> Enables configurable default behavior for routing.
> Entering imsi with the any keyword preserves the default behavior and the E.212 address is used as a destination address and the MAP request will be sent towards the HLR.
> If this keyword is not used with the any keyword, then the MAP request will be rejected.
> isdn isdn_number
> Defines the E.164 number of the HLR.
> isdn_number is a string of integers, up to 15.
> mobile-global-title mgt_number
> mgt_number is a string of integers, up to 15.
> point-code pt-code source-ssn ssn
> Defines the point code for the HLR.
> pt-code is a string of digits, up to 11; SS7 format preferred.
> sgsn-source-address-format point-code-ssn
> Selects HLR call process according to SCCP calling party address of the SGSN. This will be filled at MAP level, including the ITU point code address.
> source-ssn ssn
> Defines the SSN of the source that will be used for the call filtering.
> ssn: Must be an integer from 1 to 255.
> Usage
> Routing will be done according to IMSI parameters configured with this command.
> Example
> imsi starts-with 3 isdn 123456789 sgsn-source-address-form at point-code-ssn
> policy routing
> This command configures the policy for the routing of MAP messages. If this command is not configured or disabled (with the default keyword), then routing is done according to the configuration of the IMSI parameters.
> Product
> SGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> [ default | no ] policy routing { hlr-isdn | ms-isdn }
> default
> Resets the policy routing to the system default, disabled.
> no
> Removes the policy routing configuration from the system.
> hlr-isdn
> Selects HLR-ISDN based routing.
> ms-isdn
> Selects mobile station (MS)-ISDN based routing.
> Usage
> Use this command to set the policy for routing MAP messages.
> Example
> policy routing hlr-isdn

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883