> Performance Management
> This section contains additions and changes made to the performance commands available in this release. These additions and modifications are for Release 8.0 unless specifically noted for 8.1.
> New Commands
> Common Commands - New in Release 8.0
> The following common commands are new in Release 8.0.
> show diameter message-queue
> This command displays Diameter message queue statistics.
> CLI (Exec Mode)
> show diameter message-queue counters { inbound | outbound } [ endpoint endpoint_name [ peer-host peer_id [ peer-realm realm_id ] ] | session-id session_id ] [ | { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show multicast-sessions all
> New description table with counter description for output of this command added.
> CLI (Exec Mode)
> show show multicast-sessions [ command_keyword ] [ filter_keywords ] [| { grep grep_options | more }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> dns-client
> New command added to test and perform DNS query on the basis of specified DNS client name, DNS query domain name, and type of query.
> CLI (Exec Mode)
> dns-client dns_client_name [ query-type { A | AAAA | NAPTR | SRV }] query-name query_domain_nam e
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> Common Commands - New in Release 8.1
> show hd raid
> A new show command has been created to show the RAID created on the ST40 SMC hard disks.
> CLI (Exec Mode)
> show hd raid [ verbose ]
> Web Element Manager Path
> This functionality is not supported on the Web Element Manager at this time.
> show ipv6 interface summary
> Presents a summary of all configured ipv6 interfaces
> CLI (Exec Mode)
> show ipv6 interface summary
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show ipv6 neighbor
> A new command to show connected IPv6 neighbor addresses
> CLI (Exec Mode)
> show ipv6 neighbors [ ipv6 address ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show ipv6 route
> Shows ipv6 route to next gateway
> CLI (Exec Mode)
> show ipv6 route [ ipv6 prefix/prefix length ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show port info
> This command has been modified to include search capabilities for VLAN ID
> The output for this command has been modified to show LACP.
> CLI (Exec Mode)
> show port info slotnum/portnum
> Web Element Manager Path
> This functionality is not supported on the Web Element Manager at this time.
> show port table
> The output of this table is modified when ports are included in a Link Aggregation Group. The Redundant With column will show “LAG” for each aggregated port. If an aggregated port is collecting and distributing data, a “+” sign appears next to the LAG entry. If the port is collecting but not distributing data, a “-” appears instead.
> CLI (Exec Mode)
> show port table
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show subscribers
> The output of this command is modified to display following counters with various filter keywords:
> in packet dropped due to zero mbr
> out packet dropped due to zero mbr
> CLI (Exec Mode)
> show subscribers
> show subscribers full
> show subscribers full username
> show subscribers counters username
> show subscribers ggsn-only full
> show subscribers summary
> show subscribers ggsn-only summary
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show configuration errors
> New keyword IPMS is added with this command to display the errors in configuration for IPMS service on an AGW.
> CLI (Exec Mode)
> show configuration errors [ section { aaa-config | active-charging | asngw-service | asnpc-service | closed-rp-service | cscf-service | diameter | fa-service | ggsn-service | ha-service | imssh-service | ipms | ipsg-service | lac-service | lns-service | pdif-service | pdsn-service | policy-grp-config | subscriber-config } ] [ verbose ] [ | { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show ipms status
> New command added to display the IPMS support related statistics of IPMS client service on AGW and IPMs servers configured for this support on an AGW.
> CLI (Exec Mode)
> show ipms status [summary | all | server address ip_address]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> Common Commands - New in Release 8.3
> clear radius accounting archive
> This command clears archived RADIUS accounting messages associated with a AAA group, or all the archived RADIUS accounting messages in the context in which the command is executed depending on the option chosen. The scope of the command is limited to the context in which it is executed including for local context.
> CLI (Exec Mode)
> clear radius accounting archive { all | radius group group_name } [ -noconfirm ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> CF Commands - New in Release 8.0
> All of the following CF commands are new in Release 8.0.
> clear content-filtering category statistics
> This new command added to the Exec mode. This command clears all content filtering category statistics for database, SRDB manager instance, and database volume.
> CLI (Exec Mode)
> clear content-filtering category statistics [ all | facility srdbmgr [ all | instance instance_value ] | volume number volume_num]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> CF Commands - New in Release 8.1
> IMPORTANT: All of the following CF commands are only available in Release 8.1.
> clear active-charging url-blacklisting statistics
> This command clears URL Blacklisting feature related statistics.
> CLI (Exec Mode)
> clear active-charging url-blacklisting statistics [ rulebase name rulebase_name ] [ | { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show active-charging content-filtering category policy-id
> This command displays Content Filtering category policy definitions. This command replaces the show content-filtering category policy-id command available on StarOS 8.0 and earlier.
> CLI (Exec Mode)
> show active-charging content-filtering category policy-id { all | id policy_id } [ | { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show active-charging url-blacklisting statistics
> This command displays URL Blacklisting statistics.
> CLI (Exec Mode)
> show active-charging url-blacklisting statistics [ rulebase { all | name rulebase_name } ] [ verbose ] [ | { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show url-blacklisting database
> This command displays URL Blacklisting static database configurations.
> CLI (Exec Mode)
> show url-blacklisting database [ all | url url | facility acsmgr { all | instance instance } ] [ | { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show url-blacklisting url
> This command displays URL information of the URLs present in the Blacklisting database.
> CLI (Exec Mode)
> show url-blacklisting url url [ generic | exact-match ] [ | { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> ECS Commands - New in Release 8.0
> clear active-charging group-of-ruledefs statistics
> This command clears statistical information related to Active Charging Service group of ruledefs.
> CLI (Exec Mode)
> clear active-charging group-of-ruledefs statistics [ name group_of_ruledefs ] [ | { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show active-charging group-of-ruledefs
> This command displays information on group of ruledefs configured in a service.
> CLI (Exec Mode)
> show active-charging group-of-ruledefs { all | name group_of_ruledefs } [ service name service ] | statistics name group_of_ruledefs } [ | { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show active-charging packet-filter
> This command displays information on packet filters configured in a service.
> CLI (Exec Mode)
> show active-charging packet-filter { all | name packet_filter } [ service name service_name ] [ | { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> ECS Commands - New in Release 8.1
> The following ECS commands are new in Release 8.1.
> show active-charging timedef
> This command displays the details of timeslots configured in specified time definition(s).
> CLI (Exec Mode)
> show active-charging timedef { all | name timedef_name } [ service name service_name ] [ | { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> Firewall Commands - New in Release 8.0
> The following new Firewall commands are available in Release 8.0:
> clear active-charging firewall statistics
> This command clears Stateful Firewall statistics.
> CLI (Exec Mode)
> clear active-charging firewall statistics [ callid call_id | domain-name domain_name | protocol { icmp | ip | other | tcp | udp } | username user_name ] [ acsmgr instance instance_id ] [ | { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show active-charging firewall statistics
> This command displays Stateful Firewall statistics.
> CLI (Exec Mode)
> show active-charging firewall statistics [ callid call_id | domain-name domain_name | protocol { icmp | ip | other | tcp | udp } | username user_name ] [ acsmgr instance instance_id ] [ verbose ] [ | { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> threshold fw-deny-rule
> This command configures thresholds for Stateful Firewall Deny Rule.
> CLI (Global Configuration Mode)
> threshold fw-deny-rule high_thresh [ clear low_thresh ]
> default threshold fw-deny-rule
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> threshold fw-dos-attack
> This command configures thresholds for Stateful Firewall DoS attacks.
> CLI (Global Configuration Mode)
> threshold fw-dos-attack high_thresh [ clear low_thresh ]
> default threshold fw-dos-attack
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> threshold fw-drop-packet
> This command configures thresholds for Stateful Firewall drop packets.
> CLI (Global Configuration Mode)
> threshold fw-drop-packet high_thresh [ clear low_thresh ]
> default threshold fw-drop-packet
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> threshold fw-no-rule
> This command configures thresholds for Stateful Firewall no rules.
> CLI (Global Configuration Mode)
> threshold fw-no-rule high_thresh [ clear low_thresh ]
> default threshold fw-no-rule
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> Firewall Commands - New in Release 8.1
> The following new Firewall commands are available in Release 8.1:
> clear active-charging firewall track-list
> This command clears the list of servers being tracked for involvement in any Denial-of-Service (DOS) attacks.
> CLI (Exec Mode)
> clear active-charging firewall track-list attacking-servers
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show active-charging firewall track-list
> This command displays the list of servers being tracked for involvement in any Denial-of-Service (DOS) attacks.
> CLI (Exec Mode)
> show active-charging firewall track-list attacking-servers [ | { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> GGSN Commands - New in Release 8.0
> show gtpp group
> This new command added to the Exec mode. This command show all GTPP server group configuration information for a specific server group or all server groups configured in a context including default group.
> CLI (Exec Mode)
> show gtpp group [name gtpp_group_name | all] ] [ | { grep grep_options | more }]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> GGSN Commands - New in Release 8.1
> show mbms bearer-service
> New command added to display counters for MBMS related bearer service statistics:
> CLI (Exec Mode)
> show mbms bearer-service [ all | apn apn_name mcast-addr ip_address | service-type { broadcast | multicast } | full | instance instance_id | summary ] + [ | { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show gtpp storage-server
> New keyword streaming added to this command to show statistics/counters when CDRs stored on HDD for streaming mode.
> CLI (Exec Mode)
> show gtpp storage-server [ counters { all | group name name } | group name name | local file { counters { all | group name name } | statistics [ group name name ] } | status [ verbose ] ] | streaming { counters { all | group name name } | statistics [ group name name ] } [ | { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> HA Commands - New in Release 8.0
> Currently, there are no new HA commands in Release 8.0.
> HA Commands - New in Release 8.1
> Currently, there are no new HA commands in Release 8.1.
> NAT Commands - New in Release 8.3
> The following new NAT commands are available in Release 8.3:
> clear active-charging nat statistics
> This command clears NAT realm statistics.
> CLI (Exec Mode)
> clear active-charging nat statistics [ nat-realm nat_realm ] [ | { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> nat-realm schema
> This command creates and configures Network Address Translation (NAT) realm statistics schema.
> CLI (Bulk Statistics Configuration Mode)
> nat-realm schema schema_name format format_string
> no nat-realm schema schema_name
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show active-charging nat statistics
> This command displays NAT realm statistics.
> CLI (Exec Mode)
> show active-charging nat statistics [ nat-realm nat_realm ] [ | { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show bulkstats variables nat-realm
> This command displays available Network Address Translation (NAT) bulk statistics variables.
> CLI (Exec Mode)
> show bulkstats [ [ data ] | [ schemas ] | [ variables [ apn | asngw | asnpc | bcmcs | card | closedrp | common | context | cscf | ecs | fa | gtpc | gtpp | ha | ippool | ipsg | lac | nat-realm | pdif | port | ppp | radius | rp | sccp | sgsn | sgtp | ss7link | ss7rd | system | vpn ] [ obsolete ] ] [ | { grep grep_options | more } ] ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> threshold nat-port-chunks-usage
> This command configures the NAT port chunk utilization threshold settings.
> CLI (Global Configuration Mode)
> threshold nat-port-chunks-usage high_thresh [ clear low_thresh ]
> default threshold nat-port-chunks-usage
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> threshold poll nat-port-chunks-usage
> This command configures the polling interval over which to measure the NAT port chunks usage thresholding value.
> CLI (Global Configuration Mode)
> threshold poll nat-port-chunks-usage interval 30
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> snmp trap { enable | suppress } ThreshClearNATPortChunksUsage
> This command enables/suppresses generation of the ThreshClearNATPortChunksUsage trap.
> CLI (Global Configuration Mode)
> snmp trap enable ThreshClearNATPortChunksUsage
> snmp trap suppress ThreshClearNATPortChunksUsage
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> snmp trap { enable | suppress } ThreshNATPortChunksUsage
> This command enables/suppresses generation of the ThreshNATPortChunksUsage trap.
> CLI (Global Configuration Mode)
> snmp trap enable ThreshNATPortChunksUsage
> snmp trap suppress ThreshNATPortChunksUsage
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> PDIF Commands - New in Release 8.0
> PDIF is not supported in Release 8.0.
> PDIF Commands - New in Release 8.1
> The following new PDIF commands are available in Release 8.1.
> show certificate
> A new command to show the content of a configured X.509 trusted certificate
> CLI (Exec Mode)
> show certificate
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show crypto ikev2-ikesa security-associations summary table
> show crypto ikev2-ikesa security-associations summary table added to Exec Mode. Includes SA lifetime/lifetime remaining stats.
> CLI (Exec Mode)
> show crypto ikev2-ikesa security-associations summary
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show crypto managers instance
> This show command has been modified to show trusted certificate information. There is also a new variable do define the instance in question: instance_num
> CLI (Exec Mode)
> show crypto managers instance instance_num
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show crypto managers summary
> The show crypto managers summary command now show stats per service ip address for each manager.
> CLI (Exec Mode)
> show crypto managers summary
> Web Element Manager Path
> Performance | IPSecurity | crypto managers summary
> show crypto statistics ikev2
> A new command to show crypto statistics for IKEv2 for a particular pdif service
> Show crypto statistics has been changed to add the keywords s ervice-ip-address and service-name. ikev1 has been removed as an option.
> CLI (Exec Mode)
> show crypto statistics ikev2 [ service-ip-address <ip-address> | service-name <name> ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> PDSN Commands - New in Release 8.0
> show credit-control session
> This command shows the credit-control session information based on keywords.
> CLI (Exec Mode)
> show credit-control session [ all | callid | full | mdn | nai | summary ]
> [ | { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show credit-control statistics
> This command shows the credit-control statistics.
> CLI (Exec Mode)
> show credit-control statistics cc-service <name>
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> PDSN Commands - New in Release 8.1
> Currently, there are no new PDSN commands in Release 8.1.
> SGSN Commands - New in Release 8.0
> show network-service-entity
> Displays information regarding the network service entities (NSEs) in the network.
> CLI (Exec Mode)
> show network-service-entity { consolidated-status | fr-config | ip-config }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show sgsn-operator-policy full
> Displays the configuration information for one or all SGSN operator policies.
> CLI (Exec Mode)
> show sgsn-operator-policy full { all | name }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> SGSN Commands - New in Release 8.1
> clear super-charger
> Deletes the subscription data for one or all subscribers with valid super charger configurations.
> CLI (Exec Mode)
> clear super-charger { imsi <imsi> | all }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show freeze-ptmsi
> Command indicates whether an IMSI is associated with a frozen P-TMSI in the freeze-ptmsi list.
> CLI (Exec Mode)
> show freeze-ptmsi imsi <imsi>
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show super-charger
> Lists subscribers with valid super charger configuration.
> CLI (Exec Mode)
> show super-charger { imsi <imsi> | all }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> Modified Commands
> Common Commands - Modified in Release 8.0
> The following common commands have been modified in Release 8.0.
> clear cscf-service
> The li-packet-cable statistics option was added to the clear cscf-service command. This option clears Lawful Intercept statistics.
> CLI (Exec Mode)
> clear cscf-service [ li-packet-cable statistics | statistics [ name service_name | vpn-name name ] ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> clear subscribers
> The firewall { not-required | required } option has been added to this command. This option clears information for the specified subscribers. The firewall-policy fw_policy_name keyword is obsoleted.
> CLI (Exec Mode)
> clear subscribers firewall { not-required | required }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> clear subscribers gtp-version
> The gtp-version option has been added to this command. This option clears information for the specified subscribers.
> CLI (Exec Mode)
> clear subscribers gtp-version
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> monitor subscriber type
> The monitor subscriber functions have been enhanced to support the monitoring of the following new types:

> l | 1xrtt

> l | asngw

> l | closedrp

> l | evdorev0

> l | evdoreva

> l | ggsn

> l | ha

> l | ipsg

> l | lns

> l | pdif

> CLI (Exec Mode)
> monitor subscriber type [ 1xrtt | asngw | asnpc | closedrp | evdorev0 | evdoreva | ggsn | ha | ipsg | lns | pdif } next-call
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show aaa
> The group { all | name aaa_group } option was added to this command. This option displays AAA group configurations for a specified AAA group, or for all AAA groups.
> CLI (Exec Mode)
> show aaa { group { all | name aaa_group } | local counters } [ | { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show cscf-service
> The li-packet-cable statistics option was added to the show cscf-service command. This option displays Lawful Intercept statistics.
> CLI (Exec Mode)
> show cscf-service { all [ counters ] | diameter policy_control statistics | grey-list name name | li-packet-cable statistics | name service_name [ counters ] | statistics name service_name [ vpn-name name ] | subscription name service_name } [ | { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show radius counters all
> This command displays RADIUS accounting and/or authentication statistics information. The output of this command includes the following new fields:

> l | Access-Request Response Average Round Trip Time

> l | Accounting-Response Average Round Trip Time

> Also, in this command’s output, the “Authentication server address” and “Accounting server address” fields now include the following information:

> l | IP address

> l | Port number

> l | Server group name

> CLI (Exec Mode)
> show radius counters { all | radius group group_name all | server ip_address [ port number ] | summary [ all-contexts [ verbose ] ] } [ | { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show session subsystem facility aaamgr all
> The output of this command includes the following new fields:

> l | Total radius authorization responses dropped

> l | Total radius accounting responses dropped

> CLI (Exec Mode)
> show session subsystem facility aaamgr all
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show subscribers
> The firewall { not-required | required } option was added to this command. This option displays information for the specified subscribers. The firewall-policy fw_policy_name keyword is obsoleted.
> CLI (Exec Mode)
> show subscribers firewall { not-required | required }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show subscribers
> The following new keywords has been added to this command. This option displays information for the specified subscribers in SGSN service:

> l | sgsn-only [partial [qos [requested | negotiated]+]

> l | rnc id rnc_id

> l | ggsn ip_address

> CLI (Exec Mode)
> show subscribers [ command_keyword ] [ filter_keywords ] [ | { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show subscribers full
> The output of this command includes the following new fields:

> l | local ip addr

> l | ROHC cid-mode (local/remote)

> l | ROHC max-cid (local/remote)

> l | ROHC mrru (local/remote)

> l | ROHC max-hdr (local/remote)

> CLI (Exec Mode)
> show subscribers full
> Web Element Manager Path
> Click Performance | Subscriber Information | Subscriber Information tab.
> show subscribers gtp-version
> The gtp-version option has been added to this command. This option displays information for the specified subscribers.
> CLI (Exec Mode)
> show subscribers gtp-version
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> threshold monitoring
> The firewall keyword has been added to this command. This command enables thresholding for the specified option.
> CLI (Global Configuration Mode)
> [ no | default ] threshold monitoring { aaa-acct-archive-size | aaa-acct-failure | aaa-auth-failure | aaa-retry-rate | aaamgr-request-queue | asngw | call-setup | cpu-resource | cpu-session-throughput | content-filtering | cscf-service | ecs | fa-service | firewall | ha-service | ipsec | license | packets-filtered-dropped | packets-forwarded-to-cpu | pdsn-service | pdif | subscriber | system}
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> threshold poll
> This command configures the polling interval over which to count or measure the thresholding value. The following keywords have been added to this command:

> l | fw-deny-rule

> l | fw-dos-attack

> l | fw-drop-packet

> l | fw-no-rule

> CLI (Global Configuration Mode)
> [ default ] threshold poll { 10sec-cpu-utilization | a11-rrp-failure | a11-rrq-msg-discard | a11-rac-msg-discard | aaa-acct-archive-size | aaa-acct-failure | aaa-acct-failure-rate | aaa-auth-failure | aaa-auth-failure-rate | aaa-retry-rate | aaamgr-request-queue | active-subscriber | all-ppp-send-discard | available-ip-pool-group | call-reject-no-resource | call-setup | call-setup-failure | cpu-available-memory | cpu-load | cpu-orbs-crit | cpu-orbs-warn | cpu-session-throughput | cpu-utilization | cscf-service-route-failures | dereg-reply-error | fa-reg-reply-error | fw-deny-rule | fw-dos-attack | fw-drop-packet | fw-no-rule | ha-init-rrq-rcvd-rate | ha-svc-init-rrq-rcvd-rate| ip-pool-free | ip-pool-hold | ip-pool-release | ip-pool-used | ipsec-call-req-rej | ipsec-ike-failrate | ipsec-ike-failures | ipsec-ike-requests | ipsec-tunnels-established | ipsec-tunnels-setup | license-remaining-session | mgmt-cpu-memory-usage interval | mgmt-cpu-utilization | packets-filtered-dropped | packets-forwarded-to-cpu | pdif-current-sessions | pdif-current-active-sessions | pdsn-init-rrq-rcvd-rate | per-service-ggsn-sessions | per-service-ha-sessions | per-service-lns-sessions | per-service-pdsn-sessions | per-service-sgsn-sessions | per-service-sgsn-pdp-sessions | port-high-activity | port-rx-utilization | port-tx-utilization | ppp-setup-fail-rate | reg-reply-error | rereg-reply-error | rp-setup-fail-rate | storage-utilization | total-ggsn-sessions | total-ha-sessions | total-lns-sessions | total-pdsn-sessions | total-sgsn-sessions | total-sgsn-pdp sessions | total-subscriber } interval time
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show port table
> The introduction of the Quad Gig-E line Card on the ST40 means that additional information is available in the Redundant With... column whenever the port is used in a link aggregation. The following is added to the Show Port Table output in the Show Command Outputs chapter in the Counters and Statistics Reference:
> Extra information is shown in the “Redundant With” column when the port is in a Link Aggregation using the four-port Quad Gig-E line card (QGLC) in an ST40. It now shows LAG and the redundant card/port detail and a + character if the port is selected and a - character if it is not selected.
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> Common Commands - Modified in Release 8.1
> IMPORTANT: The following common commands have been modified in Release 8.1.
> clear subscribers
> This command clears information for specified subscriber sessions. The nat keyword was added to this command. This enables to clear information for subscribers with NAT required or not required, as specified.
> CLI (Exec Mode)
> clear subscribers [ keywords ] [ verbose ] [ -noconfirm ] [ | { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show dhcp-service name
> The output of this command now includes the “DHCP Client Identifier” field, which indicates the behavior relating to inclusion of client identifier DHCP option in DHCP messages.
> CLI (Exec Mode)
> show dhcp-service { all | name svc_name }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show diameter aaa-statistics
> This command displays Diameter AAA statistics. The output of this command includes the following new fields:

> l | Session Stats

> l | Total Sessions

> l | Freed Sessions

> l | Session Timeouts

> l | Active Sessions

> CLI (Exec Mode)
> show diameter aaa-statistics [ all | [ group group_name ] server server_name ] [ | { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show diameter authentication servers
> This command displays Diameter Authentication server information. The output of this command has been modified, and now displays the number of instances between the Diameter server and AAA Manager in up and down states.
> CLI (Exec Mode)
> show diameter authentication servers [ aaa-group group_name ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show diameter peers full all
> The output of this command includes the following new fields. These fields are displayed only when origin-host is configured as of “accept-inbound” connection type. If no inbound sockets are present these fields are not displayed.

> l | Inbound listening sockets

> l | Local Host

> l | Local Address

> l | Endpoint

> l | Task

> CLI (Exec Mode)
> show diameter peers [ full | summary ] [ all | [ endpoint endpoint_name ] [ peer-host peer_id ] [ peer-realm realm_id ]+ ] [ | { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show ims-authorization policy-control statistics
> The output of this command includes the following new fields:

> l | DPCA Session Stats:

> l | Total Secondary Create

> l | Total Secondary Terminate

> l | DPCA Experimental Result Code Stats:

> l | Error Initial Parameters

> l | Error Trigger Event

> l | Bearer Not Authorized

> l | Traffic Mapping Rejected

> l | PCC Rule Event

> l | Base Result Code

> CLI (Exec Mode)
> show ims-authorization policy-control statistics
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show ims-authorization sessions full
> The output of this command includes the following new fields:

> l | Primary PCRF: The primary Policy Control and Charging Rules Function (PCRF) server host name.

> l | Secondary PCRF: The secondary PCRF server host name.

> l | Guaranteed Uplink Bw (in bps): The guaranteed bandwidth for uplink direction, in bps.

> l | Guaranteed Downlink Bw (in bps): The guaranteed bandwidth for downlink direction, in bps.

> CLI (Exec Mode)
> show ims-authorization session [ full | summary ] | [ all | [ ims-auth-service ims_auth_svc_name | imsi imsi_value [ nsapi nsapi_value ] | apn apn_name | ip-address ip_address | callid call_id ] [ | { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show resources
> This command displays the resource information by CPU or session. In ACS Optimized mode, the output of this command displays the following ECS related fields:

> l | ECS Information:

> l | Capacity

> l | Enhanced Charging Service:

> l | In Use

> l | Max Used

> l | Limit

> l | License Status

> The output of this command for ACS Non-optimized mode remains unchanged.
> CLI (Exec Mode)
> show resources { cpu | session } [ | { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show session subsystem facility sessmgr all
> The output of this command includes the following new fields:

> l | aaa acct items (used/max)

> l | aaa buffer (used in MB/max in MB)

> l | Total aaa cancel auth

> l | Total aaa acct purged

> l | Total radius acct purged

> CLI (Exec Mode)
> show session subsystem facility sessmgr all
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show subscribers
> This command displays information for specified subscriber sessions. The nat keyword was added to this command. This enables viewing information for subscribers with NAT required or not required, as specified.
> CLI (Exec Mode)
> show subscribers [ command_keyword ] [ filter_keywords ] [ | { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show subscribers full
> This command displays information for specified subscriber sessions. The output of this command includes the following new fields:

> l | NAT Policy: Indicates whether Network Address Translation (NAT) is enabled for the subscriber.

> l | NAT Realm: The NAT realm associated with the subscriber.

> l | NAT IP address: The NAT IP address allocated from the NAT realm.

> CLI (Exec Mode)
> show subscribers full
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> Common Commands - Modified in Release 8.3
> IMPORTANT: The commands documented in this section are only available in Release 8.3.
> clear subscribers
> The nat-ip filter keyword was added to this command. This optional filter keyword enables clearing information for subscribers with NAT processing enabled and using a specific NAT IP address.
> CLI (Exec Mode)
> clear subscribers [ keywords ] [ verbose ] [ -noconfirm ] [ | { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show subscribers
> The nat-ip filter keyword was added to this command. This optional filter keyword enables displaying information for subscribers with NAT processing enabled and using a specific NAT IP address.
> CLI (Exec Mode)
> show subscribers [ command_keyword ] [ filter_keyword ] [ | { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show subscribers full
> The output of this command includes the following new fields:

> l | Nat port chunks allocated [start - end]: Indicates the NAT port range allocated to the subscriber.

> l | Client Type: Displays the total number of subscriber sessions that have been labeled as data (data-only) or regular (includes voice).

> CLI (Exec Mode)
> show subscribers full
> show subscribers full username
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> CF Commands - Modified in Release 8.0
> The following CF commands were modified for Release 8.0.
> show active-charging content-filtering category statistics
> The verbose and all keywords were added to this command. The all keyword enables viewing content filtering category statistics for each configured rulebase in the active charging service separately. The verbose keyword displays detailed information.
> CLI (Exec Mode)
> show active-charging content-filtering category statistics [ rulebase { name rulebase_name | all } ] [ verbose ] [ | { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show active-charging content-filtering server-group
> This command displays information for Content Filtering Server Groups configured in the service. The output of this command includes the following new field:

> l | URL-extraction: Indicates the ICAP URL extraction mode.

> CLI (Exec Mode)
> show active-charging content-filtering server-group [ statistics ] [ name cfsg_name ] [ | { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show content-filtering category database
> The optional keyword facility srdbmgr [ all | instance instance_value ] has been added to this command. This command displays the database statistics on the basis of running static rating database manager instances.
> CLI (Exec Mode)
> show content-filtering category database [ active | all | facility srdbmgr [ all | instance instance_value ] | url url_string ] [ verbose ] [ | { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show content-filtering category statistics
> The optional keyword facility srdbmgr [ all | instance instance_value ] has been added to this command. This command displays the content filtering category statistics on the basis of running static rating database manager instances.
> CLI (Exec Mode)
> show content-filtering category statistics [ facility srdbmgr [ all | instance instance_value ] ] [ | { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show content-filtering category statistics
> The optional keyword volume number volume_num has been added to this command. This command displays the content filtering category statistics on the basis of category database volume.
> CLI (Exec Mode)
> show content-filtering category statistics [ all | facility srdbmgr [ all | instance instance_value ] | volume number volume_num ] [ | { grep grep_options | more }]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> CF Commands - Modified in Release 8.1
> The following CF commands were modified for Release 8.1.
> show active-charging content-filtering category policy-id
> The output of this command includes the following new field:

> l | Reply Code: The reply code specified for www-reply-code-and-terminate-flow action.

> CLI (Exec Mode)
> show active-charging content-filtering category policy-id { all | id policy_id } [ | { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show active-charging content-filtering category statistics verbose
> The output of this command includes the following new fields:

> l | ALL (Default): Displays the number of URLs categorized by default action.

> l | Timeout: Displays the number of URLs categorized by time out action.

> l | x-category added during runtime, and the number of packets hit and blocked.

> CLI (Exec Mode)
> show active-charging content-filtering category statistics [ rulebase { all | name rulebase_name } ] [ verbose ] [ | { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show active-charging content-filtering server-group
> This command displays information for Content Filtering Server Groups configured in the service. The output of this command includes the following new field:

> l | URL-extraction: Indicates the ICAP URL extraction mode.

> CLI (Exec Mode)
> show active-charging content-filtering server-group [ statistics ] [ name cfsg_name ] [ | { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show active-charging service name
> This command displays service and configuration counters for the all/specified active charging service. The output of this command now displays a description of the Content Filtering Policy ID, if set in the ACS Configuration Mode.
> CLI (Exec Mode)
> show active-charging service { all | name svc_name } [ | { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show content-filtering category database
> The output of this command has been modified to display the “Last Upgrade Status” field only once at top level, and not per database. The database status is also modified to display the database status as OK, loading, merging for optcmd.bin, optcmd_f.bin, and optcmd_i.bin depending on what function is being done on which database.
> CLI (Exec Mode)
> show content-filtering category database [ active | all | facility srdbmgr [ all | instance instance_value ] | url url_string ] [ verbose ] [ | { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show content-filtering category policy-id
> This command displays information about the Category-based Content Filtering application on the basis of policy identifier. The output of this command now includes the following:

> l | Discarded-Flow-Content-ID: Displays the content ID for the discarded flows. If not configured, this field is not displayed.

> l | A description of the Content Filtering Policy ID, if set in the ACS Configuration Mode.

> CLI (Exec Mode)
> show content-filtering category policy-id cf_policy_id [ verbose ] [ | { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show content-filtering category statistics facility srdbmgr instance
> This command displays Category-based Content Filtering statistics. The output of this command now includes the following new field:

> l | x-category added during runtime, and the number of packets hit and blocked.

> CLI (Exec Mode)
> show content-filtering category statistics [ all | facility srdbmgr [ all | instance instance_value ] | volume number volume_num ] [ | { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> ECS Commands - Modified in Release 8.0
> The following ECS commands were modified in Release 8.0.
> show active-charging analyzer statistics name ip verbose
> The output of this command includes the following new fields:

> l | Uplink Bytes received after reassembly

> l | Uplink Pkts received after reassembly

> l | Downlink Bytes received after reassembly

> l | Downlink Pkts received after reassembly

> CLI (Exec Mode)
> show active-charging analyzer statistics name ip [ verbose ] [ | { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show active-charging charging-action name
> The output of this command now includes the following field:

> l | Service ID

> CLI (Exec Mode)
> show active-charging charging-action { { { all | name action_name } [ service name svc_name ] } | statistics [ name action_name ] } [ | { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show active-charging charging-action statistics
> The output of this command includes the following new fields:

> l | Upl Pkts Readdressed

> l | Dnl Pkts Readdressed

> l | Upl Bytes Readdressed

> l | Dnl Bytes Readdressed

> CLI (Exec Mode)
> show active-charging charging-action { { { all | name action_name } [ service name svc_name ] } | statistics [ name action_name ] } [ | { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show active-charging content-filtering server-group statistics
> The output of this command includes the following new fields:

> l | Failure Action (communication with server-group not attempted):

> l | Permit

> l | Content Insertion

> l | Discard

> l | Terminate Flow

> l | Redirect URL

> CLI (Exec Mode)
> show active-charging content-filtering server-group [ statistics ] [ name cfsg_name ] | [ | { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show active-charging edr-udr-file statistics
> The output of this command includes the following new fields:

> l | Overall Stats

> l | Files rotated due to records limit

> l | EDR Specific Stats

> l | EDR files rotated due to records limit

> l | UDR Specific Stats

> l | UDR files rotated due to records limit

> CLI (Exec Mode)
> show active-charging edr-udr-file statistics
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show active-charging ruledef
> This command displays information for rule definitions configured in a service. The following changes were made to this command:

> l | The firewall keyword was added to this command.

> l | The statistics keyword options have changed to: “statistics [ all { charging | firewall [ wide ] } | name ruledef_name [ wide ] ] }”.

> l | The “service svc_name” keyword is obsoleted.

> CLI (Exec Mode)
> show active-charging ruledef { all | charging | firewall | name ruledef_name | routing | statistics [ all { charging | firewall [ wide ] } | name ruledef_name [ wide ] ] } [ | { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> clear active-charging ruledef statistics
> This command clears Active Charging rule definition statistics. The charging and firewall keywords were added to this command.
> CLI (Exec Mode)
> clear active-charging ruledef statistics [ charging | firewall | name ruledef_name ] [ | { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show active-charging sessions
> The firewall { not-required | required } filter was added to this command. This option displays information on sessions with firewall processing required or not required as specified.
> CLI (Exec Mode)
> show active-charging sessions [ full | summary | display-dynamic-charging-rules | dynamic-charging ] { [ all ] | [ filters_keywords ] + } [ | { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show active-charging sessions full
> The output of this command includes the following new fields:

> l | NCQoS NRUPC Req Made

> l | NCQoS NRSPCA Req Made

> l | NCQoS NRUPC Req Failed

> l | NCQoS NRSPCA Req Failed

> l | NCQoS NRUPC Req Success

> l | NCQoS NRSPCA Req Success

> CLI (Exec Mode)
> show active-charging sessions [ full | summary | display-dynamic-charging-rules | dynamic-charging ] { [ all ] | [ filters_keywords ] + } [ | { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show active-charging sessions full all
> The output of this command includes the following new fields:

> l | Current Readdressed Sessions

> l | Total Readdressed Uplink Pkts

> l | Total Readdressed Uplink Bytes

> l | Total Readdressed Downlink Pkts

> l | Total Readdressed Downlink Bytes

> CLI (Exec Mode)
> show active-charging sessions [ full | summary | display-dynamic-charging-rules | dynamic-charging ] { [ all ] | [ filters_keywords ] + } [ | { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show active-charging subsystem
> The output of this command includes the following new fields:

> l | EDR/UDR statistics

> l | Records Generated

> l | Msgs sent to CDRMOD

> l | Records sent to CDRMOD

> l | Msgs bounced from CDRMOD

> l | Records bounced from CDRMOD

> l | Successful Msgs sent to CDRMOD

> l | Successful records sent to CDRMOD

> CLI (Exec Mode)
> show active-charging subsystem all
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show port info
> The output of this command is now enhanced for Frame Relay interface and LMI protocol related following counters:

> l | Path x e1 y

> l | Frame Relay Intf Type

> l | Frame Relay LMI Type

> l | Frame Relay LMI n391

> l | Frame Relay LMI n392

> l | Frame Relay LMI n393

> l | Frame Relay LMI t391

> l | Frame Relay LMI t392

> l | Number of DLCIs

> CLI (Exec Mode)
> show port { datalink counters [ slot/port ] | info [ slot/port ] | npu counters [ slot/port [ tagged | untagged | vlan tag_id ] ] | table | utilization table } [ | { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> ECS Commands - Modified in Release 8.1
> IMPORTANT: The following ECS commands were modified in Release 8.1.
> clear active-charging analyzer statistics
> This command is used to clear protocol analyzer statistics. The following P2P application protocol options were added to this command:

> l | ddlink

> l | halflife2

> l | hamachivpn

> l | irc

> l | oscar

> l | popo

> l | steam

> l | tvants

> l | tvuplayer

> l | uusee

> l | vpnx

> l | vtun

> l | winmx

> l | wofwarcraft

> l | xbox

> CLI (Exec Mode)
> clear active-charging analyzer statistics [ name protocol_name ] [ | { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> clear active-charging credit-control statistics
> This command clears prepaid credit control service statistics in an Active Charging Service. The group keyword was added to this command. This enables clearing statistics for a specific credit control group.
> CLI (Exec Mode)
> clear active-charging credit-control statistics [ group group_name ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show active-charging analyzer statistics name p2p
> The output of this command includes the following new fields:

> l | Ddlink

> l | Halflife2

> l | Hamachivpn

> l | Irc

> l | Oscar

> l | Popo

> l | Steam

> l | Tvants

> l | Tvuplayer

> l | Uusee

> l | Vpnx

> l | Vtun

> l | Winmx

> l | Wofwarcraft

> l | Xbox

> CLI (Exec Mode)
> show active-charging analyzer statistics name p2p
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show active-charging charging-action all
> The output of this command includes the following new fields:

> l | Billing Action:

> l | Event Data Record: Indicates whether EDRs are enabled/disabled.

> l | GGSN charging Data Record: Indicates whether GGSN CDRs are enabled/disabled.

> l | User Data Record: Indicates whether UDRs are enabled/disabled.

> l | Radius Accounting Record: Indicates whether RADIUS accounting records is enabled/disabled.

> CLI (Exec Mode)
> show active-charging charging-action { { { all | name action_name } [ service name svc_name ] } | statistics [ name action_name ] } [ | { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show active-charging credit-control statistics
> This command displays statistics for Diameter/RADIUS prepaid credit control service in an Active Charging Service. The group keyword was added to this command. This enables viewing statistics for a specific credit control group. If credit control group(s) are configured, the output of this command will display statistics per credit control group.
> CLI (Exec Mode)
> show active-charging credit-control { statistics [ all | group group_name ] | session-states [ rulebase rulebase_name ] [ content-id content_id ] } [ | { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show active-charging flows
> This command displays active charging flows in a system or service. The following P2P application protocol options were added to this command:

> l | ddlink

> l | halflife2

> l | hamachivpn

> l | irc

> l | oscar

> l | popo

> l | steam

> l | tvants

> l | tvuplayer

> l | uusee

> l | vpnx

> l | vtun

> l | winmx

> l | wofwarcraft

> l | xbox

> CLI (Exec Mode)
> show active-charging flows { all | [ connected-time [ < | > | greater-than | less-than ] seconds ] [ flow-id flow_id ] [ full ] [ idle-time [ < | > | greater-than | less-than ] seconds ] [ ip-address [ server | subscriber ] [ < | > | IPv4 | greater-than | less-than ] address ] [ port-number [ server | subscriber ] [ < | > | IPv4 | greater-than | less-than ] number ] [ rx-bytes [ < | > | greater-than | less-than ] number ] [ rx-packets [ < | > | greater-than | less-than ] number ] [ session-id session_id ] [ summary ] [ trans-proto { icmp | tcp | udp } ] [ tx-bytes [ < | > | greater-than | less-than ] number ] [ tx-packets [ < | > | greater-than | less-than ] number ] [ type flow_type ] } [ | { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show active-charging flows full
> This command displays active charging flows in a system or service. The output of this command includes the following new fields:

> l | MS NAT IP: The NAT IP address used by the subscriber flow.

> l | TCP MS NAT Port: The NAT port number used by the subscriber flow. This field is not displayed for one-to-one NAT.

> CLI (Exec Mode)
> show active-charging flows { all | [ connected-time [ < | > | greater-than | less-than ] seconds ] [ flow-id flow_id ] [ full ] [ idle-time [ < | > | greater-than | less-than ] seconds ] [ ip-address [ server | subscriber ] [ < | > | IPv4 | greater-than | less-than ] address ] [ port-number [ server | subscriber ] [ < | > | IPv4 | greater-than | less-than ] number ] [ rx-bytes [ < | > | greater-than | less-than ] number ] [ rx-packets [ < | > | greater-than | less-than ] number ] [ session-id session_id ] [ summary ] [ trans-proto { icmp | tcp | udp } ] [ tx-bytes [ < | > | greater-than | less-than ] number ] [ tx-packets [ < | > | greater-than | less-than ] number ] [ type flow_type ] } [ | { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show active-charging rulebase name
> The output of this command includes the following new fields:

> l | Flow Any Error Charging Action: Indicates the charging action configured for action on packets dropped by Firewall due to any error. If disabled, no accounting is performed on such packets.

> l | Type: Indicates the Firewall rule definition type.

> l | Firewall Configuration:

> l | Dos-Protection:

> l | Source-Route: Indicates status of protection against IP Source Route IP Option attacks.

> l | Win-Nuke: Indicates status of protection against Win Nuke attacks.

> l | Mime-Flood: Indicates status of protection against MIME Flood attacks.

> l | FTP-Bounce: Indicates status of protection against FTP Bounce attacks.

> l | IP-Unaligned-Timestamp: Indicates status of protection against IP Unaligned Timestamp attacks.

> l | Seq-Number-Prediction: Indicates status of protection against Sequence Number Prediction attacks.

> l | TCP-Window-Containment: Indicates status of protection against TCP Window Containment.

> l | Teardrop: Indicates status of protection against Teardrop attacks.

> l | UDP Flooding: Indicates status of protection against UDP Flooding attacks.

> l | ICMP Flooding: Indicates status of protection against ICMP Flooding attacks.

> l | SYN Flooding: Indicates status of protection against SYN Flooding attacks.

> l | Port Scan: Indicates status of protection against Port Scan attacks.

> l | Flooding:

> l | ICMP limit: The maximum number of ICMP packets allowed during a sampling interval.

> l | UDP limit: The maximum number of UDP packets allowed during a sampling interval.

> l | TCP-SYN limit: The maximum number of TCP-SYN packets allowed during a sampling interval.

> l | Sampling Interval: The flooding sampling interval, in seconds.

> l | TCP-SYN Flood Intercept:

> l | Mode: The TCP SYN flood intercept mode.

> l | Max-Attempts: The maximum number of attempts for sending proxy SYN to the target.

> l | Retrans-timeout: The SYN-Proxy retransmit timeout, in seconds.

> l | Watch-timeout: The TCP intercept watch timeout, in seconds.

> l | Mime-Flood Params:

> l | HTTP Header-Limit: The maximum number of headers allowed in an HTTP packet.

> l | HTTP Max-Header-Field-Size: The maximum header field size allowed in an HTTP header, in bytes.

> l | URL-Blacklisting Action: Indicates action to be taken on URL Blacklisting match.

> l | URL-Blacklisting EDR: Indicates whether EDRs will be generated on Blacklisting match.

> l | Content Filtering Flow Any Error: Indicates whether Content Filtering packets are allowed/discarded in case of ACS error scenarios.

> l | Content-Filtering: Indicates whether EDRs are generated for Content Filtering.

> l | Charging Action Priorities:

> l | Timedef: Indicates the time definition configured with the ruledef / group-of-ruledefs.

> CLI (Exec Mode)
> show active-charging rulebase { all [ service name svc_name ] | name rulebase_name [ service name svc_name ] | statistics [ name rulebase_name ] } [ | { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show active-charging rulebase statistics
> The output of this command includes the following new fields:

> l | R7Gx Rule-Matching Failure Stats:

> l | Total Dropped Packets

> l | Total Dropped Packet Bytes

> l | TCP MSS Inserted Pkts

> l | TCP MSS Limited Pkts

> l | EDRs:

> l | EDRs generated for any-error packets

> l | EDRs generated for flow-end content-filtering

> l | EDRs generated for firewall deny rule match

> l | EDRs generated for transaction completion

> CLI (Exec Mode)
> show active-charging rulebase { all [ service svc_name ] | name rulebase_name [ service svc_name ] | statistics [ name rulebase_name ] } | [ | { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show active-charging service
> The output of this command includes the following new fields:

> l | Content Filtering: Indicates whether active-charging category-based content-filtering is enabled.

> l | URL-Blacklisting: Indicates whether URL Blacklisting is enabled.

> l | URL-Blacklisting Match-method: Indicates the URL Blacklisting match method to look up URLs in the URL Blacklisting database.

> l | Content Filtering Match-method: Indicates the match method to look up URLs in the category-based content filtering database.

> The following fields were removed from the output of this command:

> l | Content Filtering Policy

> l | Content Filtering Categories

> l | Category

> l | Priority

> l | Action

> l | Content Insert

> l | Redirect

> l | EDR

> l | Timeout Action

> CLI (Exec Mode)
> show active-charging service { all | name service_name } [ | { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show active-charging sessions
> This command displays statistics for specific active charging service sessions. The following keywords were added to this command:

> l | The following P2P application protocol options were added to this command:

> l | ddlink

> l | halflife2

> l | hamachivpn

> l | irc

> l | oscar

> l | popo

> l | steam

> l | tvants

> l | tvuplayer

> l | uusee

> l | vpnx

> l | vtun

> l | winmx

> l | wofwarcraft

> l | xbox

> l | The nat keyword was added to this command. This enables viewing session information for sessions with Network Address Translation required or not required, as specified.

> CLI (Exec Mode)
> show active-charging sessions [ full | summary | display-dynamic-charging-rules | dynamic-charging ] { [ all ] | [ filters_keywords ] + } [ | { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show active-charging sessions
> This command displays statistics for specific active charging service sessions. The output of this command includes the following new fields:

> l | Current DDLINK Sessions

> l | Current HALFLIFE2 Sessions

> l | Current HAMACHIVPN Sessions

> l | Current IRC Sessions

> l | Current OSCAR Sessions

> l | Current POPO Sessions

> l | Current STEAM Sessions

> l | Current TVANTS Sessions

> l | Current TVUPLAYER Sessions

> l | Current UUSEE Sessions

> l | Current VPNX Sessions

> l | Current VTUN Sessions

> l | Current WINMX Sessions

> l | Current WOFWARCRAFT Sessions

> l | Current XBOX Sessions

> l | Predefined Firewall Rules Enabled List

> l | R7Gx Dropped Upl Pkts RuleMatch Fail

> l | R7Gx Dropped Upl Bytes RuleMatch Fail

> l | R7Gx Dropped Dnl Pkts RuleMatch Fail

> l | R7Gx Dropped Dnl Bytes RuleMatch Fail

> CLI (Exec Mode)
> show active-charging sessions [ full | summary | display-dynamic-charging-rules | dynamic-charging ] { [ all ] | [ filters_keywords ] + } [ | { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show active-charging subsystem
> The output of this command includes the following new fields:

> l | Session Creation Succ

> l | Session Creation Fail

> l | Total Flows Connected

> l | Total Flows Disconnected

> l | Total Uplink Pkts

> l | Total Uplink Bytes

> l | Total Downlink Pkts

> l | Total Downlink Bytes

> l | Total Rule-Hits

> l | Total Blacklisted URL hits

> l | Total Blacklisted URL misses

> l | Total P2P Voice flows

> l | Current P2P Voice flows

> CLI (Exec Mode)
> show active-charging subsystem all
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show active-charging subsystem facility acsmgr instance
> The output of this command includes the following new fields:

> l | Total Blacklisted URL hits

> l | Total Blacklisted URL misses

> CLI (Exec Mode)
> show active-charging subsystem facility acsmgr instance instance_value
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> ECS Commands - Modified in Release 8.3
> IMPORTANT: The following ECS commands were modified in Release 8.3.
> show active-charging edr-format statistics
> The output of this command includes the following new field:

> l | Total NAT bind records generated

> CLI (Exec Mode)
> show active-charging edr-format statistics
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show active-charging charging-action statistics name
> The output of this command includes the following new fields:

> l | PP Upl Pkts Readdressed

> l | PP Dnl Pkts Readdressed

> l | PP Upl Bytes Readdressed

> l | PP Dnl Bytes Readdressed

> l | pp-flow-action

> The following fields were modified:

> l | Statistic

> l | flow-action

> l | pp-flow-action

> l | flow-limit

> l | bandwidth-limit

> CLI (Exec Mode)
> show active-charging charging-action statistics name charging_action_name [ service-name service_name ] [ | { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show active-charging flows
> The nat filter keyword was added to this command. This optional keyword enables displaying information for flows with NAT processing disabled or enabled and optionally using a specific NAT IP address or a specific NAT IP address and NAT port number.
> CLI (Exec Mode)
> show active-charging flows { all | [ connected-time [ < | > | greater-than | less-than ] seconds ] [ flow-id flow_id ] [ full ] [ idle-time [ < | > | greater-than | less-than ] seconds ] [ ip-address [ server | subscriber ] [ < | > | IPv4 | greater-than | less-than ] address ] [ nat { not-required | required [ nat-ip nat_ip_address ] } ] [ port-number [ server | subscriber ] [ < | > | IPv4 | greater-than | less-than ] number ] [ rx-bytes [ < | > | greater-than | less-than ] number ] [ rx-packets [ < | > | greater-than | less-than ] number ] [ session-id session_id ] [ summary ] [ trans-proto { icmp | tcp | udp } ] [ tx-bytes [ < | > | greater-than | less-than ] number ] [ tx-packets [ < | > | greater-than | less-than ] number ] [ type flow_type ] } [ | { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show active-charging ruledef
> The following changes were made to this command:

> l | The post-processing keyword was added to this command. This enables to view post-processing ruledef related information.

> l | Output of the show active-charging ruledef statistics command includes the following new fields:

> l | Total Post-processing Ruledefs

> l | Uplink Packets

> l | Uplink Bytes

> l | Downlink Packets

> l | Downlink Bytes

> l | Hits

> CLI (Exec Mode)
> show active-charging ruledef { all | charging | firewall | name ruledef_name | post-processing | routing | statistics [ all { charging | firewall [ wide ] | post-processing } | name ruledef_name [ wide ] ] } [ | { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show active-charging rulebase name
> The output of this command includes the following new fields:

> l | Post-processing Action Priorities:

> l | Name

> l | Type

> l | Priority

> l | Charging-action

> l | Description

> CLI (Exec Mode)
> show active-charging rulebase name rulebase_name service name service_name [ | { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show active-charging rulebase statistics
> The output of this command includes the following new field:

> l | NBRs:

> l | Total NBRs generated

> l | NBRs generated for port chunk allocation

> l | NBRs generated for port chunk release

> CLI (Exec Mode)
> show active-charging rulebase statistics
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show active-charging rulebase statistics name
> The output of this command includes the following new fields:

> l | Total PP Dropped Packets

> l | Total PP Dropped Packet Bytes

> CLI (Exec Mode)
> show active-charging rulebase statistics name rulebase_name [ | { grep grep_options | more } ]
> show active-charging sessions full all
> The output of this command includes the following new field:

> l | PP Flow action Terminated Flows

> CLI (Exec Mode)
> show active-charging sessions full all [ | { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show active-charging subsystem all
> The output of this command includes the following new field:

> l | Total PP Rule-Hits

> CLI (Exec Mode)
> show active-charging subsystem all [ rulebase name rulebase_name ] [ | { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> Firewall Commands - Modified in Release 8.1
> The following Firewall commands were modified in Release 8.1.
> clear active-charging firewall statistics
> This command clears Active Charging Stateful Firewall statistics. The nat-realm keyword was added to this command. This enables clearing NAT realm statistics.
> CLI (Exec Mode)
> clear active-charging firewall statistics [ callid call_id | domain-name domain_name | nat-realm nat_realm | protocol { icmp | ip | other | tcp | udp } | username user_name ] [ acsmgr instance instance_id ] [ | { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show active-charging firewall statistics
> This command displays Active Charging Stateful Firewall statistics. The nat-realm keyword was added to this command. This enables viewing NAT realm statistics.
> CLI (Exec Mode)
> show active-charging firewall statistics [ callid call_id | domain-name domain_name | nat-realm nat_realm | protocol { icmp | ip | other | tcp | udp } | username user_name ] [ acsmgr instance instance_id ] [ verbose ] [ | { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> GGSN Commands - Modified in Release 8.0
> The following GGSN commands were modified in Release 8.0.
> show apn statistics name
> The output of this command enhanced and modified to include statistics for traffic policing and shaping:
> CLI (Exec Mode)
> show apn statistics [ all | name apn_name ] [| { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show gtpc full
> The output of this command now includes the following counters for direct tunnel support:

> l | GTP-U Tunnel Establishment

> CLI (Exec Mode)
> show gtpc [ full | counters | summary ] { all | apn apn_name | imsi imsi_value [ nsapi nsapi_value ] | callid callid | sgsn-address ip_address | ggsn-service ggsn_name | user-address ip_address | username username }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show gtpc statistics verbose
> The output of this command now includes the following counters for direct tunnel support:

> l | GTP-U Tunnel Establishment with RNC

> l | Direct Tunnels Established

> l | Direct Tunnels torn down by SGSNs

> l | Direct Tunnels that received Error Indication

> l | Direct Tunnel Flags update

> CLI (Exec Mode)
> show gtpc statistics [ sgsn-address ip_address | ggsn-service ggsn_name | apn-name apn_name ] [ verbose ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show gtpc statistics verbose
> The output of this command includes the following new fields:

> l | Update PDP Tx Reasons

> l | QoS Change

> l | Providing PDP address

> l | APN Restriction

> l | No APN Subscription

> l | Local IP Pool All Address Occupied

> CLI (Exec Mode)
> show gtpc statistics verbose
> Web Element Manager Path
> Click Performance | GGSN | GTPC Statistics.
> show gtpp counters all
> The output of this command now includes the following counters:

> l | Outstanding G-CDRs

> l | Possibly Duplicate Outstanding G-CDRs

> l | Archived G-CDRs

> l | G-CDRs buffered with AAAPROXY

> l | G-CDRs buffered with AAAMGR

> CLI (Exec Mode)
> show gtpp counter all
> Web Element Manager Path
> Click Performance | GGSN | GTPP Statistics.
> show gtpp statistics cgf-address
> The output of this command includes the following new fields:

> l | CDR Decode Error

> l | Seq No incorrect

> l | Unknown Cause

> CLI (Exec Mode)
> show gtpp statistics cgf-address
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> GGSN Commands - Modified in Release 8.1
> show gtpp storage-server
> A new keyword has been added to this command to display statistics and counter for files stored on the SMC hard disk.
> CLI (Exec Mode)
> show gtpp storage-server local file { counters | statistics }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show subscriber ggsn-only
> New counter has been added to display the applicable IP allocation method for MBMS session for GGSN subscribers. Added counter is:

> l | ip-type-unknown

> CLI (Exec Mode)
> show subscribers ggsn-only [ | { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show apn name
> Output of this command is modified for new counters for Bearer Control mode information and also irrelevant counters are removed from screen output of this command.
> Counters removed:

> l | ip vlan id

> l | eap msk lifetime

> l | rohc-profile-name

> l | compression mode

> l | data compression size

> l | min compression size

> l | dns-proxy-intercept-list

> Counter Added:

> l | Bearer Control Mode

> CLI (Exec Mode)
> show apn { all | name apn_name ] [ | { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show subscribers
> The output of this command is enhanced to display following counters with ggsn-only or other GGSN-specific filter keywords:

> l | in packet dropped due to zero mbr

> l | out packet dropped due to zero mbr

> CLI (Exec Mode)
> show subscribers
> show subscribers full
> show subscribers full username
> show subscribers counters username
> show subscribers ggsn-only full
> show subscribers summary
> show subscribers ggsn-only summary
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show gtpc statistics
> New keyword custom1 added to this command to display GTP-C statistics and counters for Preservation Mode and Free-of-Charge service. This is a customer-specific feature.
> CLI (Exec Mode)
> show gtpc statistics [ apn-name apn_name ] [ custom1 ] [sgsn-address address ] [ ggsn-service svc_name ] [ verbose ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> clear gtpc statistics
> New keyword custom1 added to this command to clear the GTP-C statistics and counters for Preservation Mode and Free-of-Charge service. This is a customer-specific feature.
> CLI (Exec Mode)
> clear gtpc statistics [ apn-name apn_name ] [ custom1 ] [sgsn-address address ] [ ggsn-service svc_name ] [ verbose ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show apn statistics
> Following counters has been added to the output of this command to indicate the auto readjusted dynamic burst size for guaranteed and peak burst size under traffic shaping feature:

> l | Burst Size

> l | Auto Readjust

> l | Auto Readjust Duration

> l | Peak Burst Size (bytes)

> l | Guaranteed Burst Size (bytes)

> CLI (Exec Mode)
> show apn statistics [ all | name apn_name ] [|{ grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show apn all
> Following counters has been added to the output of this command to indicate the auto readjusted dynamic burst size for guaranteed and peak burst size under traffic shaping feature:

> l | Burst Size

> l | Auto Readjust

> l | Auto Readjust Duration

> l | Peak Burst Size (bytes)

> l | Guaranteed Burst Size (bytes)

> CLI (Exec Mode)
> show apn { all | name apn_name ] [ | { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show subscribers ggsn-only
> Following counters has been added to the output of this command to indicate the auto readjusted dynamic burst size for guaranteed and peak burst size under traffic shaping feature:

> l | Downlink traffic-rate-limit

> l | Uplink traffic-rate-limit

> l | Downlink traffic-shaping

> l | Uplink traffic-shaping

> l | Burst Size

> l | Auto Readjust

> l | Auto Readjust Duration

> l | Peak Burst Size (bytes)

> l | Guaranteed Burst Size (bytes)

> l | Peak data rate (bps)

> l | Guaranteed data rate (bps)

> CLI (Exec Mode)
> show subscribers ggsn-only [ | { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> HA Commands - Modified in Release 8.0
> There were no HA commands modified in Release 8.0.
> HA Commands - Modified in Release 8.1
> There were no HA commands modified in Release 8.1.
> PDIF Commands - Modified in Release 8.0
> PDIF is not supported in Release 8.0.
> PDIF Commands - Modified in Release 8.1
> show crypto statistics ikev2
> This command has been modified to show the number of internal failure messages sent to the peer after an internal failure in ipsecmgr or dcardmgr.
> CLI (Exec Mode)
> show crypto statistics ikev2
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show crypto managers instance
> This command has been modified to show the number of internal failure messages sent to the peer after an internal failure in ipsecmgr or dcardmgr.
> CLI (Exec Mode)
> show crypto managers instance <instance number>
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show crypto map
> This command has been modified with the keyword ikev2-pdif. Now instead of seeing all created transform-sets without knowing which is in use, the new command returns only two: the one that created the IKE SA and the one that created the IPSec SA.
> CLI (Exec Mode)
> show crypto map map-type ikev2-pdif
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> This command has been modified with the keyword summary. This new option displays summary information for all crypto maps configured in the context.
> CLI (Exec Mode)
> show crypto map summary
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show session subsystem facility aaamgr all
> The output of this command includes the following new fields:

> l | aaa request (used/max)

> l | Total Diameter auth requests

> l | Current Diameter auth requests

> l | Total Diameter auth requests retried

> l | Total Diameter auth requests dropped

> l | Total radius auth responses dropped

> l | Total Diameter acct requests

> l | Current Diameter acct requests

> l | Total Diameter auth acct requests retried

> l | Total radius acct cancelled

> l | total radius acct purged

> l | total radius acct responses dropped

> l | Total aaamgr purged requests

> CLI (Exec Mode)
> show session subsystem facility aaamgr
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show crypto ipsec security-associations
> This command has been modified to indicate whether rekeying is enabled.
> CLI (Exec Mode)
> show crypto ipsec security associations
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> This command has been modified to display the SA State and Crypto Type.
> CLI (Exec Mode)
> show crypto ipsec security associations
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> PDIF Commands - Modified in Release 8.3
> show crypto transform-set
> This command has been modified in PDIF Release 8.3 to include the ipsec keyword for clarity. It does not change the command output.
> CLI (Exec Mode)
> Previous command syntax:
> show crypto transform-set
> Modified command syntax:
> show crypto ipsec transform-set
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show pdif-service statistics
> This command has been modified in PDIF Release 8.3 to include the Total Pkts Violations field in the command output. This field lists the total number of packets received from UEs and destined for the Internet that do not match any of the configured traffic selectors.
> CLI (Exec Mode)
> show pdif-service statistics
> show pdif-service statistics peer-address
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> PDSN Commands - Modified in Release 8.0
> There were no PDSN commands modified in Release 8.0.
> PDSN Commands - Modified in Release 8.1
> show hd raid verbose
> New fields have been added to the output for this command. When two SMCs contain different disk images, a user who wants to decide which disk to use needs the create/update time and event counts information.
> CLI (Exec Mode)
> show hd raid verbose
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> Session Control Manager Commands - Modified for Release 8.0
> Session Control Manager is not supported in Release 8.0.
> Session Control Manager Commands - Modified for Release 8.1
> The following commands have been modified in Release 8.1.
> clear cscf service
> This command was changed in synch with the associated show command.
> CLI (Exec Mode)
> clear cscf service { diameter policy_control statistics [ service-name service_name | vpn-name name ] | li-packet-cable statistics | statistics name service_name { all | calls | ip-security | message | package-name { message-summary | presence | reg | winfo } | registrations | sigcomp | tcp | vpn-name name } }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> clear cscf sessions
> This command was changed in synch with the associated show command.
> CLI (Exec Mode)
> clear cscf sessions { counters { calls | subscription } service service_name | service service_name { all | session-id id | aor aor }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> clear cscf sip
> This command was changed in synch with the associated show command.
> CLI (Exec Mode)
> clear cscf sip statistics [ name service_name [ interface { domain name domain_name | ip address ip_address } | vpn-name name ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show cscf service
> This command was expanded to allow more options.
> CLI (Exec Mode)
> show cscf service { all [ counters ] | diameter policy_control statistics service-name service_name [ vpn-name name ] | grey-list name name | li-packet-cable statistics | name service_name [ counters ] | statistics name service_name [ all | calls | ip-security | message | package-name { message-summary | presence | reg | winfo } | registrations | sigcomp | tcp | vpn-name name ] | subscription name service_name } [ | { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show cscf sessions
> This command was expanded to allow more options.
> CLI (Exec Mode)
> show cscf sessions { counters { calls { duration | first-response-time | invite-processing-time | post-answer-delay | post-dial-delay | service service_name | session-release-delay | session-setup-delay } service service_name | subscription { duration | service service_name | setup-time} service service_name } | duration | full [ callleg-id id | from-aor aor | service service_name | session-id id | to-aor aor ] [ media-type type ] | summary [ from-aor aor | service service_name | session-id id |
> to-aor aor ] } [ | { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show cscf sip
> This command has a new keyword - interface.
> CLI (Exec Mode)
> show cscf sip statistics name service_name [ interface { domain domain_name | ip address ip_address } | vpn-name name ] [ | { grep grep_options
> | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show cscf tcp connections
> This facility, remote-ip, and remote-port keywords have been added to specify SIP interfaces.
> CLI (Exec Mode)
> show cscf tcp connections service service_name [ facility { cscfmgr | sessmgr } | full | remote-ip ip_address | remote-port port_number ]
> [ | { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> SGSN Commands - Modified in Release 8.0
> The following SGSN commands were modified in Release 8.0.
> show dns-client
> The output of this command is now enhanced for SGSN specific counters to show DNS cache statistics with the following counters:

> l | DNS Cache Statistics

> l | Central Cache

> l | Local Cache

> l | Total Lookups

> l | Cache Hits (Positive Response)

> l | Cache Hits (Negative Response)

> l | Not Found in Cache

> l | Hit Ratio (Percentage)

> l | DNS Resolver Statistics

> l | Successful Queries

> l | Query Timeouts

> l | Domain Not Found

> l | Connection Refused

> l | Other Failures

> CLI (Exec Mode)
> show dns-client name { cache [ query-name name | query-type
> { A | SRV } ] | statistics }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show gmm-sm statistics
> This command has a new keyword - routing-area - which enables fine tuning the statistics display to a specified routing area.
> CLI (Exec Mode)
> show gmm-sm statistics [ gmm-only | sm-only ] [ gprs-service srvc_name [ nsei nse_id | routing-area mcc mc_code mnc mn_code lac loc_code rac ra_code ] ] | [ sgsn-service srvc_name [ rnc mcc mc_code mnc mn_code rnc-id rnc_id | routing area mcc mc_code mnc mn_code lac loc_code rac ra_code ] ] [ verbose ] [ | { grep grep_options | more } ]
> Web Element Manager Path
> Configuration of these features is not yet supported by the Web Element Manager.
> show gmm-sm statistics
> This command is enhanced with new keywords for RNC related statistics and output of this command is also enhanced for RNC related statistics.
> CLI (Exec Mode)
> show gmm-sm statistics { gmm-only [ gprs-service srvc_name ] | gprs-service srvc_name | sgsn-service srvc_name [ rnc mcc mc_code mnc mn_code rnc-id rnc_id | routing area mcc mc_code mnc mn_code lac loc_code rac ra_code ] | sm-only [ gprs-service srvc_name ] } [ verbose ] [ | { grep grep_options | more }]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show gmm-sm statistics
> Several new counters have been added under the heading of Network Overload Protection:

> l | Attach requests queued in the pacing queue:

> l | Inter SGSN RAU requests queued in the pacing queue:

> l | Number of Inter SGSN RAU and Attach requests in the pacing queue:

> l | Attach requests successfully dequeued from the pacing queue:

> l | Inter SGSN RAU requests successfully dequeued from the pacing queue:

> l | Attaches rejected:

> l | Inter SGSN RAUs rejected:

> l | Attaches dropped:

> l | Inter SGSN RAUs dropped:

> CLI (Exec Mode)
> show gmm-sm statistics [ verbose ]
> show gmm-sm statistics
> The SGSN GMM-SM statistics now supports counters for inter-rat / inter-service for RAU/Attaches. Previously, RAU (requests/accepts/rejects) statistics display counters were classified under 5 categories:
> 1.Intra-sgsn periodic rau
> 2.Intra-sgsn gprs-only rau
> 3.Intra-sgsn combined rau
> 4.Inter-sgsn periodic rau
> 5.Inter-sgsn combined rau
> The following categories have been added:
> 6.Intra-sgsn Inter-rat gprs-only rau
> 7.Intra-sgsn Inter-rat combined rau
> 8.Intra-sgsn Intra-rat Inter-service gprs-only rau
> 9.Intra-sgsn Intra-rat Inter-service combined rau
> The statistics for these categories, relate as follows:
> (4 & 5) -> RAU from completely different sgsn
> (6 & 7) -> RAU between sgsn-service <-> gprs-service
> (8 & 9) -> RAU between 2 sgsn-services or 2 gprs-services.
> A large range of counters have been added within the new categories:
> Routing Area Update Request:

> l | Total-Ps-Inter-Rat-RAU

> l | 3G-Ps-Inter-Rat-RAU

> l | 2G-Ps-Inter-Rat-RAU

> l | Total-Comb-Inter-Rat-RAU

> l | 3G-Comb-Inter-Rat-RAU

> l | 2G-Comb-Inter-Rat-RAU

> l | Total-Ps-Inter-Serv-RAU

> l | 3G-Ps-Inter-Serv-RAU

> l | 2G-Ps-Inter-Serv-RAU 0

> l | Total-Comb-Inter-Serv-RAU

> l | 3G-Comb-Inter-Serv-RAU

> l | 2G-Comb-Inter-Serv-RAU

> l | Ret-Total-Ps-Inter-Rat-RAU

> l | Ret-3G-Ps-Inter-Rat-RAU

> l | Ret-2G-Ps-Inter-Rat-RAU

> l | Ret-Total-Comb-Inter-Rat-RAU

> l | Ret-3G-Comb-Inter-Rat-RAU

> l | Ret-2G-Comb-Inter-Rat-RAU

> l | Ret-Total-Ps-Inter-Serv-RAU

> l | Ret-3G-Ps-Inter-Serv-RAU

> l | Ret-2G-Ps-Inter-Serv-RAU

> l | Ret-Total-Comb-Inter-Serv-RAU

> l | Ret-3G-Comb-Inter-Serv-RAU

> l | Ret-2G-Comb-Inter-Serv-RAU

> Routing Area Update Accept:

> l | Total-Ps-Inter-Rat-RAU-Acc

> l | 3G-Ps-Inter-Rat-RAU-Acc

> l | 2G-Ps-Inter-Rat-Acc

> l | Total-Comb-Inter-Rat-RAU-Acc

> l | 3G-Comb-Inter-Rat-RAU-Acc

> l | 2G-Comb-Inter-Rat-Acc

> l | Total-Ps-Inter-Serv-RAU-Acc

> l | 3G-Ps-Inter-Serv-RAU-Acc

> l | 2G-Ps-Inter-Serv-RAU-Acc

> l | Total-Comb-Inter-Serv-RAU-Acc

> l | 3G-Comb-Inter-Serv-RAU-Acc

> l | 2G-Comb-Inter-Serv-RAU-Acc

> l | Ret-Total-Ps-Inter-Rat-RAU-Acc

> l | Ret-3G-Ps-Inter-Rat-RAU-Acc

> l | Ret-2G-Ps-Inter-Rat-Acc

> l | Ret-Total-Comb-Inter-Rat-RAU-Acc

> l | Ret-3G-Comb-Inter-Rat-RAU-Acc

> l | Ret-2G-Comb-Inter-Rat-Acc

> l | Ret-Total-Ps-Inter-Serv-RAU-Acc

> l | Ret-3G-Ps-Inter-Serv-RAU-Acc

> l | Ret-2G-Ps-Inter-Serv-RAU-Acc

> l | Ret-Total-Comb-Inter-Serv-RAU-Acc

> l | Ret-3G-Comb-Inter-Serv-RAU-Acc

> l | Ret-2G-Comb-Inter-Serv-RAU-Acc

> Routing Area Update Reject:

> l | Inter RAT PS Only Routing Area Update Reject Causes:

> l | 3G-IMSI Unknown in HLR

> l | 2G-IMSI Unknown in HLR

> l | 3G-Illegal MS

> l | 2G-Illegal MS

> l | 3G-Illegal ME

> l | 2G-Illegal ME

> l | 3G-GPRS service not allowed

> l | 2G-GPRS service not allowed

> l | 3G-GPRS and Non-GPRS service not allowed

> l | 2G-GPRS and Non-GPRS service not allowed

> l | 3G-MsId not derived by Nw

> l | 2G-MsId not derived by Nw

> l | 3G-Implicitly Detached

> l | 2G-Implicitly Detached

> l | 3G-PLMN not allowed

> l | 2G-PLMN not allowed

> l | 3G-Location Area not allowed

> l | 2G-Location Area not allowed

> l | 3G-Roaming not allowed in this Location Area

> l | 2G-Roaming not allowed in this Location Area

> l | 3G-GPRS service not allowed in this PLMN

> l | 2G-GPRS service not allowed in this PLMN

> l | 3G-No suitable cells in this Location Area

> l | 2G-No suitable cells in this Location Area

> l | 3G-MSC not reachable

> l | 2G-MSC not reachable

> l | 3G-Network Failure

> l | 2G-Network Failure

> l | 3G-MAC Failure

> l | 2G-MAC Failure

> l | 3G-SYNC Failure

> l | 2G-SYNC Failure

> l | 3G-Congestion

> l | 2G-Congestion

> l | 3G-GSM Auth Unacceptable

> l | 2G-GSM Auth Unacceptable

> l | 3G-No PDP contexts activated

> l | 2G-No PDP contexts activated

> l | 3G-Retry from new cell

> l | 2G-Retry from new cell

> l | 3G-Semantically Wrong Msg

> l | 2G-Semantically Wrg Msg

> l | 3G-Invalid Mandatory Info

> l | 2G-Invalid Mandatory Info

> l | 3G-MSG type Non Existent

> l | 2G-MSG type Non Existent

> l | 3G-MSG type not compatible with protocol state

> l | 2G-MSG type not compatible with protocol state

> l | 3G-IE Non Existent

> l | 2G-IE Non Existent

> l | 3G-Conditional IE Error

> l | 2G-Conditional IE Error

> l | 3G-Message not compatible with protocol state

> l | 2G-Message not compatible with protocol state

> l | 3G-Protocol Error

> l | 2G-Protocol Error

> l | 3G-Unknown cause

> l | 2G-Unknown cause

> l | Inter RAT Comb. Routing Area Update Reject Causes:

> l | 3G-IMSI Unknown in HLR

> l | 2G-IMSI Unknown in HLR

> l | 3G-Illegal MS

> l | 2G-Illegal MS

> l | 3G-Illegal ME

> l | 2G-Illegal ME

> l | 3G-GPRS service not allowed

> l | 2G-GPRS service not allowed

> l | 3G-GPRS and Non-GPRS service not allowed

> l | 2G-GPRS and Non-GPRS service not allowed

> l | 3G-MsId not derived by Nw

> l | 2G-MsId not derived by Nw

> l | 3G-Implicitly Detached

> l | 2G-Implicitly Detached

> l | 3G-PLMN not allowed

> l | 2G-PLMN not allowed

> l | 3G-Location Area not allowed

> l | 2G-Location Area not allowed

> l | 3G-Roaming not allowed in this Location Area

> l | 2G-Roaming not allowed in this Location Area

> l | 3G-GPRS service not allowed in this PLMN

> l | 2G-GPRS service not allowed in this PLMN

> l | 3G-No suitable cells in this Location Area

> l | 2G-No suitable cells in this Location Area

> l | 3G-MSC not reachable

> l | 2G-MSC not reachable

> l | 3G-Network Failure

> l | 2G-Network Failure

> l | 3G-MAC Failure

> l | 2G-MAC Failure

> l | 3G-SYNC Failure

> l | 2G-SYNC Failure

> l | 3G-Congestion

> l | 2G-Congestion

> l | 3G-GSM Auth Unacceptable

> l | 2G-GSM Auth Unacceptable

> l | 3G-No PDP contexts activated

> l | 2G-No PDP contexts activated

> l | 3G-Retry from new cell

> l | 2G-Retry from new cell

> l | 3G-Semantically Wrong Msg

> l | 2G-Semantically Wrg Msg

> l | 3G-Invalid Mandatory Info

> l | 2G-Invalid Mandatory Info

> l | 3G-MSG type Non Existent

> l | 2G-MSG type Non Existent

> l | 3G-MSG type not compatible with protocol state

> l | 2G-MSG type not compatible with protocol state

> l | 3G-IE Non Existent

> l | 2G-IE Non Existent

> l | 3G-Conditional IE Error

> l | 2G-Conditional IE Error

> l | 3G-Message not compatible with protocol state

> l | 2G-Message not compatible with protocol state

> l | 3G-Protocol Error

> l | 2G-Protocol Error

> l | 3G-Unknown cause

> l | 2G-Unknown cause

> l | Inter Service PS Only Routing Area Update Reject Causes:

> l | 3G-IMSI Unknown in HLR

> l | 2G-IMSI Unknown in HLR

> l | 3G-Illegal MS

> l | 2G-Illegal MS

> l | 3G-Illegal ME

> l | 2G-Illegal ME

> l | 3G-GPRS service not allowed

> l | 2G-GPRS service not allowed

> l | 3G-GPRS and Non-GPRS service not allowed

> l | 2G-GPRS and Non-GPRS service not allowed

> l | 3G-MsId not derived by Nw

> l | 2G-MsId not derived by Nw

> l | 3G-Implicitly Detached

> l | 2G-Implicitly Detached

> l | 3G-PLMN not allowed

> l | 2G-PLMN not allowed

> l | 3G-Location Area not allowed

> l | 2G-Location Area not allowed

> l | 3G-Roaming not allowed in this Location Area

> l | 2G-Roaming not allowed in this Location Area

> l | 3G-GPRS service not allowed in this PLMN

> l | 2G-GPRS service not allowed in this PLMN

> l | 3G-No suitable cells in this Location Area

> l | 2G-No suitable cells in this Location Area

> l | 3G-MSC not reachable

> l | 2G-MSC not reachable

> l | 3G-Network Failure

> l | 2G-Network Failure

> l | 3G-MAC Failure

> l | 2G-MAC Failure

> l | 3G-SYNC Failure

> l | 2G-SYNC Failure

> l | 3G-Congestion

> l | 2G-Congestion

> l | 3G-GSM Auth Unacceptable

> l | 2G-GSM Auth Unacceptable

> l | 3G-No PDP contexts activated

> l | 2G-No PDP contexts activated

> l | 3G-Retry from new cell

> l | 2G-Retry from new cell

> l | 3G-Semantically Wrong Msg

> l | 2G-Semantically Wrg Msg

> l | 3G-Invalid Mandatory Info

> l | 2G-Invalid Mandatory Info

> l | 3G-MSG type Non Existent

> l | 2G-MSG type Non Existent

> l | 3G-MSG type not compatible with protocol state

> l | 2G-MSG type not compatible with protocol state

> l | 3G-IE Non Existent

> l | 2G-IE Non Existent

> l | 3G-Conditional IE Error

> l | 2G-Conditional IE Error

> l | 3G-Message not compatible with protocol state

> l | 2G-Message not compatible with protocol state

> l | 3G-Protocol Error

> l | 2G-Protocol Error

> l | 3G-Unknown cause

> l | 2G-Unknown cause

> l | Inter Service Comb. Routing Area Update Reject Causes:

> l | 3G-IMSI Unknown in HLR

> l | 2G-IMSI Unknown in HLR

> l | 3G-Illegal MS

> l | 2G-Illegal MS

> l | 3G-Illegal ME

> l | 2G-Illegal ME

> l | 3G-GPRS service not allowed

> l | 2G-GPRS service not allowed

> l | 3G-GPRS and Non-GPRS service not allowed

> l | 2G-GPRS and Non-GPRS service not allowed

> l | 3G-MsId not derived by Nw

> l | 2G-MsId not derived by Nw

> l | 3G-Implicitly Detached

> l | 2G-Implicitly Detached

> l | 3G-PLMN not allowed

> l | 2G-PLMN not allowed

> l | 3G-Location Area not allowed

> l | 2G-Location Area not allowed

> l | 3G-Roaming not allowed in this Location Area

> l | 2G-Roaming not allowed in this Location Area

> l | 3G-GPRS service not allowed in this PLMN

> l | 2G-GPRS service not allowed in this PLMN

> l | 3G-No suitable cells in this Location Area

> l | 2G-No suitable cells in this Location Area

> l | 3G-MSC not reachable

> l | 2G-MSC not reachable

> l | 3G-Network Failure

> l | 2G-Network Failure

> l | 3G-MAC Failure

> l | 2G-MAC Failure

> l | 3G-SYNC Failure

> l | 2G-SYNC Failure

> l | 3G-Congestion

> l | 2G-Congestion

> l | 3G-GSM Auth Unacceptable

> l | 2G-GSM Auth Unacceptable

> l | 3G-No PDP contexts activated

> l | 2G-No PDP contexts activated

> l | 3G-Retry from new cell

> l | 2G-Retry from new cell

> l | 3G-Semantically Wrong Msg

> l | 2G-Semantically Wrg Msg

> l | 3G-Invalid Mandatory Info

> l | 2G-Invalid Mandatory Info

> l | 3G-MSG type Non Existent

> l | 2G-MSG type Non Existent

> l | 3G-MSG type not compatible with protocol state

> l | 2G-MSG type not compatible with protocol state

> l | 3G-IE Non Existent

> l | 2G-IE Non Existent

> l | 3G-Conditional IE Error

> l | 2G-Conditional IE Error

> l | 3G-Message not compatible with protocol state

> l | 2G-Message not compatible with protocol state

> l | 3G-Protocol Error

> l | 2G-Protocol Error

> l | 3G-Unknown cause

> l | 2G-Unknown cause

> CLI (Exec Mode)
> show gmm-sm statistics [ verbose ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show gtpp counters all
> The output of this command is now enhanced for Ga interface support to SGSN with the following counters:

> l | Outstanding M-CDRs

> l | Possibly Duplicate Outstanding M-CDRs

> l | Archived M-CDRs

> l | M-CDRs buffered with AAAPROXY

> l | M-CDRs buffered with AAAMGR

> l | Outstanding S-CDRs

> l | Possibly Duplicate Outstanding S-CDRs

> l | Archived S-CDRs

> l | S-CDRs buffered with AAAPROXY

> l | S-CDRs buffered with AAAMGR

> l | Outstanding S-SMO-CDRs

> l | Possibly Duplicate Outstanding S-SMO-CDRs

> l | Archived S-SMO-CDRs

> l | S-SMO-CDRs buffered with AAAPROXY

> l | S-SMO-CDRs buffered with AAAMGR

> l | Outstanding S-SMT-CDRs

> l | Possibly Duplicate Outstanding S-SMT-CDRs

> l | Archived S-SMT-CDRs

> l | S-SMT-CDRs buffered with AAAPROXY

> l | S-SMT-CDRs buffered with AAAMGR

> l | Outstanding GMBH CDRs

> l | Possibly Duplicate Outstanding GMBH CDRs

> l | Archived GMBH CDRs

> l | GMBH CDRs buffered with AAAPROXY

> l | GMBH CDRs buffered with AAAMGR

> CLI (Exec Mode)
> show gtpp counter all
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show gtpp storage-server
> A new keyword has been added to this command to display statistics and counters for files stored on the SMC hard disk.
> CLI (Exec Mode)
> show gtpp storage-server local file { counters | statistics }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show gtpp storage-server statistics
> The output of this command is now enhanced for M-CDRs and S-CDRs for SGSN with the following counters:

> l | Store Requests (M-CDRs)

> l | Sent

> l | Retried

> l | Success

> l | Failed

> l | Store Requests (S-CDRs)

> l | Sent

> l | Retried

> l | Success

> l | Failed

> CLI (Exec Mode)
> show gtpp cstorage-server statistics
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show iups-service
> This command has been modified to limit the display of information to a specific RNC.
> CLI (Exec Mode)
> show iups-service { all | name srvc_name }[ rnc { all | mcc mcc_num mnc mnc_num } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show sccp-network
> There are new keywords (status all and status dpc) to fine tune the displayed information for the SCCP networks.
> CLI (Exec Mode)
> show sccp-network { ntwk_index | all } [ status [ all | dpc ] ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show session disconnect-reasons verbose
> The output of this command is now enhanced for SGSN related disconnect reason with the following counters:

> l | sgsn-attach-in-reg-state(291)

> l | sgsn-inbound-srns-in-reg-state(292)

> l | dt-ggsn-tun-reestablish-failed(293)

> CLI (Exec Mode)
> show session disconnect-reasons [ verbose ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show session subsystem
> The output of this command is now enhanced for S-CDRs, M-CDRs, S-SMO-CDRs, and S-SMT-CDRs with following counters:

> l | Total S-CDRs

> l | Current S-CDRs

> l | Total M-CDRs

> l | Current M-CDRs

> l | Total S-SMO-CDRs

> l | Current S-SMO-CDRs

> l | Total S-SMT-CDRs

> l | Current S-SMT-CDRs

> CLI (Exec Mode)
> show session subsystem [ full | facility facility [ all | instance id ] ] [ verbose ] [ | { grep grep_options | more }]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show sgtp-service
> The new keyword “sgsn-table” added to this command to show SGSN information.
> CLI (Exec Mode)
> show sgtp-service { all | ggsn-table | sgsn-table | name srvc_name }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show ss7-routing-domain
> This command is enhanced to display the SS7 domain related statistics for following protocols with different filter options:

> l | SSCF: Service Specific Coordination Function (q.2140)

> l | QSAAL: Signaling ATM Adaption Layer (SAAL)

> l | MTP3: SS7 Message Transfer Part-3

> l | M3UA: SS7 MTP3 User Adaptation Layer

> l | SCTP ASP: Stream Control Transmission Protocol (SCTP) application server process

> CLI (Exec Mode)
> show ss7-routing-domain domain_index { sscf | qsaal | mtp3 } { status | statistics } linkset [all | id linkset_id] link [all | id link_id ] {verbose}
> show ss7-routing-domain domain_index m3ua { status | statistics } { all | peer-server [all | id peer_id] {{verbose} | peer-server-process [all | instance instance_id]}} {verbose}
> show ss7-routing-domain domain_index sctp asp [all | instance instance_id ] statistics { gen | end-point }{verbose}
> show ss7-routing-domain domain_index mtp3 { status | statistics } { gen | destination-point-code [all | dest_point_code ] | linkset [all | id linkset_id ] {link [all | id link_id ]}} {verbose}
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show ss7-routing-domain
> This command has been enhanced in several ways - 1) with the ‘all’ keyword to display all SS7RD information with one command; 2) with the ‘mtp2’ keyword to access a display of statistics or status information for the MTP2 layer; and 3) to display routing tables.:

> l | MTP2: SS7 Message Transfer Part-2

> l | routes tables (with or without adjacent point codes)

> CLI (Exec Mode)
> show ss7-routing-domain { all | ss7rd_id { m3ua | mtp2 | mtp3 | qsaal | routes [ adjacent ] | sctp asp { all | instance asp_id } | sscf } }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show subscriber
> New filter keyword nsapi added to this existing command to show the subscriber information on the basis of network service access point identifier (NSAPI).
> CLI (Exec Mode)
> show subscribers [ command_keyword ] [ filter_keywords ] [ | { grep grep_options | more}]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show subscriber
> New filter keywords gprs-only and sgsn-only have been added to this existing command, used with valid filters, to focus the output to information for 2G or 3G SGSN connections/contexts.
> CLI (Exec Mode)
> show subscribers [ gprs-only | sgsn-only ] [ filter_keywords ] [ | { grep grep_options | more}]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show sgtpu statistics
> The output of this command is now enhanced with the following pairs of counters:

> l | Total Packets Rcvd

> l | Iu Release

> l | T3-tunnel Timer expiry

> l | Total Bytes Rcvd

> l | Iu Release

> l | T3-tunnel Timer expiry

> CLI (Exec Mode)
> show sgtpu statistics [ ggsn-address ipv4_address | iups-service iups_srvc_name | rnc-address ipv4_address | sgtp-service sgtp_srvc_name | gprs-service gprs_srvc_name nsei nse_id ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show llc statistics
> A new counter, Unit data requests Rx Drop is added to count the number of down link unit data packets (received from SNDCP) dropped by LLC.
> CLI (Exec Mode)
> show llc statistics [ verbose ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show sndcp statistics verbose
> The output of this command is now enhanced with the following PDU Drop Reason counters:

> l | SN-PDU Drop Reason

> l | Invalid SAPI State

> l | Invalid PDP Ctx

> l | Decode Failure

> l | Reassembly Drops

> l | Discard State

> l | Rx First Seg State

> l | Rx Subsequent Seg State

> l | New First Segment

> l | Reassembly Failure

> l | Reassembly Timeout

> l | DCOMP Error

> l | PCOMP Error

> l | PDP Ctx Modified

> l | PDP Ctx Deleted

> l | Other Reasons

> CLI (Exec Mode)
> show sndcp statistics [ verbose ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show sgtpu statistics
> The output of this command is now enhanced with the following pairs of counters:

> l | Total Packets Rcvd

> l | Pkts forward from queue

> l | BVC Reset/Block Rcvd

> l | Total Bytes Rcvd

> l | Bytes forward from queue

> l | BVC Reset/Block Rcvd

> CLI (Exec Mode)
> show sgtpu statistics [ ggsn-address ipv4_address | iups-service iups_srvc_name | rnc-address ipv4_address | sgtp-service sgtp_srvc_name | gprs-service gprs_srvc_name nsei nse_id ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show sgtpu statistics
> The output of this command is now enhanced with the following counters to count the packets and bytes that are dropped due to DP session in suspended state:

> l | Total Packets Rcvd

> l | Pkts when dp suspended

> l | Total Bytes Rcvd

> l | Pkts when dp suspended

> CLI (Exec Mode)
> show sgtpu statistics [ ggsn-address ipv4_address | iups-service iups_srvc_name | rnc-address ipv4_address | sgtp-service sgtp_srvc_name | gprs-service gprs_srvc_name nsei nse_id ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show gprs-service all
> The output of this command is now enhanced with the “SM-Ignore PCO IE Decode Error” parameter to ignore decoding error due to incorrect PCO IE length in SM messages.
> CLI (Exec Mode)
> show gprs-service all
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show gprs-service all
> The output of this command is now enhanced with the following counters:

> l | SM-Trim Trailing Spaces in APN

> l | SM-APN Partial match

> CLI (Exec Mode)
> show gprs-service all
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show gmm-sm statistics
> The output of this command is now enhanced with the following counters:

> l | Auth Triplets Reuse Counter

> l | 3G-Auth Triplets Reuse

> l | 2G-Auth Triplets Reuse

> CLI (Exec Mode)
> show gmm-sm statistics [ verbose ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show gprs-service all
> The output of this command is now enhanced with the “SM-APN(R) from First Sub Record” parameter to enable/disable APN from the first subscription record to be used in the requested APN.
> CLI (Exec Mode)
> show gprs-service all
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> SGSN Commands - Modified in Release 8.1
> clear sgtpu-statistics
> Adds a new keyword set gprs-service - nsei to clear statistics for a specific NSEI associated with the specified GPRS service in the current context.
> CLI (Exec Mode)
> clear sgtpu statistics [ ggsn-address ipv4_address | iups-service iups_srvc_name | rnc-address ipv4_address | sgtp-service sgtp_srvc_name | gprs-service gprs_srvc_name nsei nse_id ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show gmm-sm statistics
> The output of this command is now enhanced with the following two counters to count the current number of supporting and non-supporting Network Sharing Subscribers in the system:

> l | Network Sharing Subscribers

> l | 3G-Supporting-UE

> l | 3G-Non-Supporting-UE

> CLI (Exec Mode)
> show gmm-sm statistics [ gmm-only | sm-only ] [ gprs-service srvc_name [ nsei nse_id | routing-area mcc mc_code mnc mn_code lac loc_code rac ra_code ] ] | [ sgsn-service srvc_name [ rnc mcc mc_code mnc mn_code rnc-id rnc_id | routing area mcc mc_code mnc mn_code lac loc_code rac ra_code ] ] [ verbose ] [ | { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show gmm-sm statistics verbose
> The output of this command is now enhanced with the following two counters:

> l | 3G-Phase-2-Offload Failures

> l | 2G-Phase-2-Offload Failures

> CLI (Exec Mode)
> show gmm-sm statistics [ verbose ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show iups-service
> This command has been modified to limit the display of information to a specific RNC.
> CLI (Exec Mode)
> show iups-service { all | name srvc_name }[ rnc { all | rnc_id } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show sgtpu-statistics
> Adds a new keyword set gprs-service - nsei to display the statistics for a specific NSEI-based GTPU stats associated with the specified GPRS service in the current context.
> CLI (Exec Mode)
> show sgtpu statistics [ ggsn-address ipv4_address | iups-service iups_srvc_name | rnc-address ipv4_address | sgtp-service sgtp_srvc_name | gprs-service gprs_srvc_name nsei nse_id ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show gmm-sm statistics
> The output of this command is now enhanced with the following counters:

> l | Redirection Indication

> l | PLMN not allowed

> l | Location area not allowed

> l | Roaming not allowed in LA

> l | No GPRS services in PLMN

> l | CS/PS co-ord required

> l | Unknown Reasons

> CLI (Exec Mode)
> show gmm-sm statistics [ gmm-only | sm-only ] [ gprs-service srvc_name [ nsei nse_id | routing-area mcc mc_code mnc mn_code lac loc_code rac ra_code ] ] | [ sgsn-service srvc_name [ rnc mcc mc_code mnc mn_code rnc-id rnc_id | routing area mcc mc_code mnc mn_code lac loc_code rac ra_code ] ] [ verbose ] [ | { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show gmm-sm statistics
> The output of this command is now enhanced with the following counters:

> l | Detach Request

> l | 3G-Nw-Init-Reatch-Req

> l | 2G-Nw-Init-Reatch-Req

> l | 3G-Nw-Init-Reatch-Not-Req

> l | 2G-Nw-Init-Reatch-Not-Req

> l | 3G-Nw-Init-IMSI-Detach

> l | 2G-Nw-Init-IMSI-Detach

> l | Retransmission

> l | Ret-3G-Nw-Init-Reatch-Req

> l | Ret-2G-Nw-Init-Reatch-Req

> l | Ret-3G-Nw-Init-Reatch-Not

> l | Ret-2G-Nw-Init-Reatch-Not

> l | Ret-3G-Nw-Init-IMSI-Detach

> l | Ret-2G-Nw-Init-IMSI-Detach

> CLI (Exec Mode)
> show gmm-sm statistics [ gmm-only | sm-only ] [ gprs-service srvc_name [ nsei nse_id | routing-area mcc mc_code mnc mn_code lac loc_code rac ra_code ] ] | [ sgsn-service srvc_name [ rnc mcc mc_code mnc mn_code rnc-id rnc_id | routing area mcc mc_code mnc mn_code lac loc_code rac ra_code ] ] [ verbose ] [ | { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show gmm-sm statistics verbose
> The output of this command is now enhanced with the following counters:

> l | Retransmission

> l | Ret-3G-Nw-Init-Reatch-Req

> l | Ret-2G-Nw-Init-Reatch-Req

> l | Ret-3G-Nw-Init-Reatch-Not

> l | Ret-2G-Nw-Init-Reatch-Not

> l | Ret-3G-Nw-Init-IMSI-Detach

> l | Ret-2G-Nw-Init-IMSI-Detach

> CLI (Exec Mode)
> show gmm-sm statistics [ verbose ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show subscribers sgsn-only full
> The counter ‘Network Sharing Capability’ has been added to the output of this command to indicate if the MS supports network sharing or not.
> CLI (Exec Mode)
> show subscribers sgsn-only full [ | { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show sgtpu statistics
> The output of this command is now enhanced with the following counters:

> l | Total Error Ind Sent

> l | Sent to GGSN

> l | Sent to RNC

> l | Total Error Ind Rcvd

> l | Rcvd from GGSN

> l | Rcvd from RNC

> l | Rcvd from GGSN through RNC

> l | Rcvd from RNC through GGSN

> CLI (Exec Mode)
> show sgtpu statistics [ ggsn-address ipv4_address | iups-service iups_srvc_name | rnc-address ipv4_address | sgtp-service sgtp_srvc_name | gprs-service gprs_srvc_name nsei nse_id ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show gmm-sm statistics verbose
> The output of this command is now enhanced with the following counters:
> 2G APN Selection Failure Statistics:

> l | SDL-1:

> l | All Packet Services Barred

> l | PDP Type not Present, PDP Address Present

> l | PDP Type not Present, APN Present

> l | PDP Type, Address and APN not Present, No Single SubRec

> l | SDL-2:

> l | No SubRec matching PDP Type

> l | No SubRec matching PDP Type and APN, No Wildcard APN

> l | Multiple SubRecs matching PDP Type and APN, No Dynamic Address

> l | Multiple SubRecs matching PDP Type and APN, with Dynamic Address

> l | SDL-3:

> l | APN not Present

> l | No Wildcard APN, Multiple SubRecs matching PDP Type

> l | Multiple SubRecs with Wildcard APN and same PDP Type

> l | PDP Address Present

> l | No SubRec matching PDP Address

> l | Single SubRec matching PDP Address, No APN Match

> l | Multiple SubRecs matching PDP Address, APN not requested

> l | Multiple SubRecs matching PDP Address, No APN Match

> l | SDL-4:

> l | APN sent by MS

> l | VPLMN User, APN-OI not HPLMN, not VPLMN

> l | VPLMN User, APN-OI is VPLMN, VPLMN Addr not allowed

> l | VPLMN User, APN-OI is VPLMN, VPLMN AP Barred

> l | VPLMN User, APN-OI is HPLMN, HPLMN AP Barred

> l | VPLMN User, No APN-OI, VPLMN Addr not allowed, HPLMN AP Barred

> l | VPLMN User, No APN-OI, VPLMN AP Barred, HPLMN AP Barred

> l | HPLMN user, APN-OI not HPLMN

> l | APN from Single Context

> l | VPLMN Addr not allowed, HPLMN AP Barred

> l | VPLMN AP Barred, HPLMN AP Barred

> l | SDL-5:

> l | VPLMN User, VPLMN Addr not allowed

> l | VPLMN User, VPLMN AP Barred

> l | No Default APN for PDP Type

> l | Internal APN Selection Failures

> l | Wildcard APN with Static Address

> l | Unknown PDP Type in Subscribed Record

> CLI (Exec Mode)
> show gmm-sm statistics [ verbose ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> Obsoleted Commands
> The following commands were obsoleted from either Release 8.0 or 8.1.
> Common Commands - Obsoleted from Release 8.0
> No common commands were obsoleted from Release 8.0.
> Common Commands - Obsoleted from Release 8.1
> No common commands were obsoleted from Release 8.1.
> CF Commands - Obsoleted from Release 8.0
> No CF commands were obsoleted from Release 8.0.
> CF Commands - Obsoleted from Release 8.1
> show content-filtering category policy-id
> This command displays Content Filtering category policy definitions. This command is replaced by the show active-charging content-filtering category policy-id command.
> CLI (Exec Mode)
> show content-filtering category policy-id { all | id cf_policy_id } [ | { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> ECS Commands - Obsoleted from Release 8.0
> No ECS commands were obsoleted from Release 8.0.
> ECS Commands - Obsoleted from Release 8.1
> No ECS commands were obsoleted from Release 8.1.
> Firewall Commands - Obsoleted from Release 8.0
> clear firewall flows
> This command clears the active firewall flows based on different criteria and also clears the disconnect reason information of disconnected flows.
> CLI (Exec Mode)
> clear firewall flows {active { all | callid call_id | imsi num | msid num | username name } | disconnect-reasons } [ -noconfirm ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> clear firewall ruledef
> This command clears statistics of the firewall rule definitions (Ruledefs) based on Ruledef name.
> CLI (Exec Mode)
> clear firewall ruledef statistics [ name ruledef_name ] [ | { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> clear firewall statistics
> This command clears the statistics of firewall session based on different criteria.
> CLI (Exec Mode)
> clear firewall statistics [ callid call_id | destination ip_address [ port dest_port ] | domain-name domain_name | protocol { icmp | other | tcp | udp } | source ip_address [ port source_port ] [ destination ip_address [ port dest_port ] ] | username name ] [ acsmgr instance instance_id ] [ | { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show firewall flows
> This command displays the active firewall flows based on different criteria and also the reasons for disconnected flows.
> CLI (Exec Mode)
> show firewall flows { active { all | callid call_id | imsi num | msid num | username name } [ verbose ] | disconnect-reasons } [ | { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show firewall ruledef
> This command displays the firewall rule definitions (Ruledefs) based on different criteria with statistical information.
> CLI (Exec Mode)
> show firewall ruledef {all | name ruledef_name | statistics [ name ruledef_name ] } [ | { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show firewall statistics
> This command displays the statistics of firewall session based on different criteria.
> CLI (Exec Mode)
> show firewall statistics [ callid call_id | destination ip_address [ port dest_port ] | domain-name domain_name | protocol { icmp | other | tcp | udp } | source ip_address [ port source_port ] [ destination ip_address [ port dest_port ] ] | username name ] [ acsmgr instance instance_id ] [ verbose ] [ | { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> update firewall policy
> This command updates/changes the firewall access policy for the specified active subscriber session.
> CLI (Exec Mode)
> update firewall policy { all | callid call_id | context context_name | imsi imsi_num | ip-address ip_address | msid msid_num | username user_name } policy-name policy_name [ verbose ] [ -noconfirm ] [ | { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> Firewall Commands Obsoleted from Release 8.1
> No Firewall commands were obsoleted from Release 8.1.
> GGSN Commands - Obsoleted from Release 8.0
> No GGSN commands were obsoleted from Release 8.0.
> GGSN Commands - Obsoleted from Release 8.1
> No GGSN commands were obsoleted from Release 8.1.
> HA Commands - Obsoleted from Release 8.0
> No HA commands were obsoleted from Release 8.0.
> HA Commands - Obsoleted from Release 8.1
> No HA commands were obsoleted from Release 8.1.
> PDSN Commands - Obsoleted from Release 8.0
> No PDSN commands were obsoleted from Release 8.0.
> PDSN Commands - Obsoleted from Release 8.1
> No PDSN commands were obsoleted from Release 8.1.
> SGSN Commands - Obsoleted from Release 8.0
> No SGSN commands were obsoleted from Release 8.0.
> SGSN Commands - Obsoleted from Release 8.1
> No SGSN commands were obsoleted from Release 8.1.
> GTPP Storage Server Changes
> There were no GSS changes in Release 8.0 or 8.1.
> Web Element Manager Changes
> There were no Web Element manager changes in Release 8.0 or 8.1.

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883