> FA Schema Statistics
> This schema provides the following type of statistics:

> • | Counter: A counter records incremental data cumulatively and rolls over when the counter limit is reached. The limit depends upon the counter data type.

> • | Gauge: A gauge statistic indicates a single value representative of a single instance. This type is often used to track particular events in time.

> Important: The format string syntax is described by Schema Format String Syntax in the Bulk Statistics Overview chapter.
> Important: Unless otherwise indicated, all statistics are counters. For statistics with the Int32 data type, the roll-over to zero limit is 4,294,967,295. For statistics with the Int64 data type, the roll-over to zero limit is 18,446,744,073,709,551,615. All counter statistics are cumulative and reset only by one of the following methods: roll-over (as described above), after a system restart, or after a clear command is performed. All statistics are considered standards-based unless otherwise noted.
> The following variables are supported:
> FA Service Schema Statistics

> Statistic | Description | Data Type
> vpnname | The name of the context configured on the system that is currently facilitating the FA service. | String
> vpnid | The identification number of the context configured on the system that is currently facilitating the FA service. This is an internal reference number. | Int32
> servname | The name of the FA service for which the statistics are displayed. | String
> advert-send | The total number of agent advertisement messages sent to the subscriber’s mobile node. | Int32
> disc-expiry | The total number of sessions that were disconnected due to the expiration of their lifetime setting. | Int32
> disc-dereg | The total number of sessions that were disconnected due to de-registrations. | Int32
> disc-admin | The total number of sessions that were disconnected due to an administrative clearing of calls (i.e. executing the clear subscriber command). | Int32
> auth-attempt | The total number of AAA authentication attempts that were facilitated. | Int32
> auth-success | The total number of successful AAA authentication attempts that were facilitate. | Int32
> auth-failure | The total number of failed AAA authentication attempts that were facilitated. | Int32
> recv-total | The total number of registration requests received. | Int32
> recv-initial | The total number of initial registration requests received. | Int32
> recv-renewal | The total number of renewal registration requests received. | Int32
> recv-dereg | The total number of requests for de-registration received. | Int32
> accept-total | The total number of registration requests accepted. | Int32
> accept-initial | The total number of initial registration requests accepted. | Int32
> accept-renewal | The total number of renewal registration requests accepted. | Int32
> accept-dereg | The total number of requests for de-registration accepted. | Int32
> denied-total | The total number of registration requests denied. | Int32
> denied-initial | The total number of initial registration requests denied. | Int32
> denied-renewal | The total number of renewal registration requests denied. | Int32
> denied-dereg | The total number of requests for de-registration denied. | Int32
> discard-total | The total number of registration requests that were discarded. | Int32
> discard-initial | The total number of initial registration requests discarded. | Int32
> discard-renewal | The total number of renewal registration requests discarded. | Int32
> discard-dereg | The total number of requests for de-registration discarded. | Int32
> relayed-total | The total number of registration requests that have been relayed. | Int32
> relayed-initial | The total number of initial registration requests relayed. | Int32
> relayed-renewal | The total number of renewal registration requests relayed. | Int32
> relayed-dereg | The total number of requests for de-registration relayed. | Int32
> authfail-total | The total number of registration requests that failed authentication. | Int32
> authfail-initial | The total number of initial registration requests that failed authentication. | Int32
> authfail-renewal | The total number of renewal registration requests that failed authentication. | Int32
> authfail-dereg | The total number of requests for de-registration that failed authentication. | Int32
> denied-pdsn-total | The total number of registration requests that have been denied by the Packet Data Service Node/Foreign Agent (PDSNFA). Reasons for a PDSN/FA denial are described later in this table. | Int32
> denied-pdsn-initial | The total number of initial registration requests that were denied by the PDSN/FA. Reasons for a PDSN/FA denial are described later in this table. | Int32
> denied-pdsn-renewal | The total number of renewal registration requests denied by the PDSN/FA. Reasons for a PDSN/FA denial are described later in this table. | Int32
> denied-pdsn-dereg | The total number of requests for de-registration that were denied by the PDSN/FA. Reasons for a PDSN/FA denial are described later in this table. | Int32
> denied-ha-total | The total number of registration requests that have been denied by the Home Agent (HA). Reasons for a HA denial are described later in this table. | Int32
> denied-ha-initial | The total number of initial registration requests denied by the HA. Reasons for a HA denial are described later in this table. | Int32
> denied-ha-renewal | The total number of renewal registration requests denied by the HA. Reasons for a HA denial are described later in this table. | Int32
> denied-ha-dereg | The total number of requests for de-registration that were denied by the HA. Reasons for a HA denial are described later in this table. | Int32
> denied-pdsn-unspec | The total number of registration requests for which an FA reply code of 40H (Registration Denied - reason unspecified) was sent. | Int32
> denied-pdsn-timeout | The total number of registration requests for which a FA reply code of 4EH (Registration Denied - registration timeout) was sent. | Int32
> denied-pdsn-admin | The total number of registration requests for which a FA reply code of 41H (Registration Denied- administratively prohibited) was sent. | Int32
> denied-pdsn-resource | The total number of registration requests for which a FA reply code of 42H (Registration Denied - insufficient resources) was sent. | Int32
> denied-pdsn-mnauth | The total number of registration requests for which a FA reply code of 43H (Registration Denied - mobile node failed authentication) was sent. | Int32
> denied-pdsn-haauth | The total number of registration requests for which a FA reply code of 44H (Registration Denied - home agent authentication failure) was sent. | Int32
> denied-pdsn-lifetoolong | The total number of registration requests for which a FA reply code of 45H (Registration Denied - requested lifetime too long) was sent. | Int32
> denied-pdsn-badreq | The total number of registration requests for which a FA reply code of 46H (Registration Denied- administratively prohibited) was sent. | Int32
> denied-pdsn-badreply | The total number of registration requests for which a FA reply code of 47H (Registration Denied - poorly formed reply) was sent. | Int32
> denied-pdsn-missnai | The total number of registration requests for which a FA reply code of 61H (Registration Denied - missing NAI) was sent. | Int32
> denied-pdsn-misshomeagent | The total number of registration requests for which a FA reply code of 62H (Registration Denied - missing home agent) was sent. | Int32
> denide-pdsn-misshomeaddr | The total number of registration requests for which a FA reply code of 60H (Registration Denied - missing home address) was sent. | Int32
> denied-pdsn-unkchallenge | The total number of registration requests for which a FA reply code of 68H (Registration Denied - unknown challenge) was sent. | Int32
> denied-pdsn-misschallenge | The total number of registration requests for which a FA reply code of 69H (Registration Denied - missing challenge) was sent. | Int32
> denied-pdsn-stalechallenge | The total number of registration requests for which a FA reply code of 6AH (Registration Denied - stale challenge) was sent. | Int32
> denied-pdsn-mntoodistant | The total number of registration requests for which a FA reply code of 4CH (Registration Denied - reverse tunneling mobile node too distant) was sent. | Int32
> denied-pdsn-styleunavail | The total number of registration requests for which a FA reply code of 4FH (Registration Denied - reverse tunneling delivery style unavailable) was sent. | Int32
> denied-pdsn-hanetunreach | The total number of registration requests for which a FA reply code of 50H (Registration Denied - home network unreachable (ICMP error received) ) was sent. | Int32
> denied-pdsn-hahostunreach | The total number of registration requests for which a FA reply code of 51H (Registration Denied - home agent host unreachable (ICMP error received) ) was sent. | Int32
> denied-pdsn-haportunreach | The total number of registration requests for which a FA reply code of 52H (Registration Denied - home agent port unreachable (ICMP error received) ) was sent. | Int32
> denied-pdsn-haunreach | The total number of registration requests for which a FA reply code of 58H (Registration Denied - home agent unreachable (other ICMP error received) ) was sent. | Int32
> denied-pdsn-invcoa | The total number of registration requests for which a FA reply code of 4DH (Registration Denied - invalid care-of address) was sent. | Int32
> denied-pdsn-encapunavail | The total number of registration requests for which a FA reply code of 48H (Registration Denied - requested encapsulation unavailable) was sent. | Int32
> denied-pdsn-revtununavail | The total number of registration requests for which a FA reply code of 4AH (Registration Denied - requested reverse tunnel unavailable) was sent. | Int32
> denied-pdsn-revtunmand | The total number of registration requests for which a FA reply code of 4BH (Registration Denied - reverse tunnel is mandatory and ‘T’ bit not set) was sent. | Int32
> denied-pdsn-unknowncvse | The total number of registration requests for which a PDSN reply code of 8DH (Registration Denied - unsupported vendor ID or unable to interpret data in the CVSE) was received. | Int32
> denied-ha-faauth | The total number of registration requests for which a HA reply code of 84H (Registration Denied - foreign agent failed authentication) was received. | Int32
> denied-ha-badreq | The total number of registration requests for which a HA reply code of 86H (Registration Denied - poorly formed request) was received. | Int32
> denied-ha-mismatchid | The total number of registration requests for which a HA reply code of 85H (Registration Denied - registration Identification mismatch) was received. | Int32
> denied-ha-simulbind | The total number of registration requests for which a HA reply code of 87H (Registration Denied - too many simultaneous mobility bindings) was received. | Int32
> denied-ha-unknownha | The total number of registration requests for which a HA reply code of 88H (Registration Denied - unknown home agent address) was received. | Int32
> denied-ha-revtununavail | The total number of registration requests for which a HA reply code of 89H (Registration Denied - reverse tunneling unavailable) was received. | Int32
> replyrcv-total | The total number of registration replies received. This total includes initial, renewal and de-registration registration replies. | Int32
> replyrcv-totalrelayed | The total number of registration replies relayed. This total includes initial, renewal and de-registration registration replies. | Int32
> replyrcv-errors | The total number of registration replies that contained errors. | Int32
> replyrcv-initial | The total number of initial registration replies received. | Int32
> replyrcv-initialrelayed | The total number of initial registration replies relayed. | Int32
> replyrcv-renewal | The total number of renewal registration replies received. | Int32
> replyrcv-renewalrelayed | The total number of renewal registration replies relayed. | Int32
> replyrcv-dereg | The total number of replies for de-registration received. | Int32
> replyrcv-deregrelayed | The total number of replies for de-registration relayed. | Int32
> reqsent-initial | The total number of initial FA registration requests sent. | Int32
> reqsent-initial-resend | The total number of initial FA registration requests re-sent. | Int32
> reqsent-initial-noresend | The total number of initial FA registration requests that were not re-sent. | Int32
> reqsent-renew | The total number of FA registration renewal requests that were sent. | Int32
> reqsent-renew-resend | The total number of FA registration renewal requests that were re-sent. | Int32
> reqsent-renew-noresend | The total number of FA registration renewal requests that were not re-sent. | Int32
> reqsent-dereg | The total number of FA de-registration requests that were sent. | Int32
> reqsent-dereg-resend | The total number of FA de-registration requests that were re-sent. | Int32
> reqsent-dereg-noresend | The total number of FA de-registration requests that were not re-sent. | Int32
> replysent-total | The total number of registration replies sent. | Int32
> replysent-acceptreg | The total number of successful registration replies sent. | Int32
> replysent-acceptdereg | The total number of successful de-registration replies sent. | Int32
> replysent-badreq | The total number of registration replies that were sent with a reply code of 46H (Registration Denied - poorly formed reply). | Int32
> replysent-badreply | The total number of registration replies that were sent with a reply code of 47H (Registration Denied - poorly formed reply). | Int32
> replysent-unspecified | The total number of registration replies that were sent with a reply code of 40H (Registration Denied - reason unspecified). | Int32
> replysent-adminprohib | The total number of registration replies that were sent with a reply code of 41H (Registration Denied - administratively prohibited). | Int32
> replysent-noresources | The total number of registration replies that were sent with a reply code of 42H (Registration Denied - insufficient resources). | Int32
> replysent-mnauthfail | The total number of registration replies that were sent with a reply code of 43H (Registration Denied - mobile node failed authentication). | Int32
> replysent-haauthfail | The total number of registration replies that were sent with a reply code of 44H (Registration Denied - home agent failed authentication). | Int32
> replysent-lifetoolong | The total number of registration replies that were sent with a reply code of 45H (Registration Denied - requested lifetime too long). | Int32
> replysent-revtununavail | The total number of registration replies that were sent with a reply code of 4AH (Registration Denied - reverse tunneling unavailable). | Int32
> replysent-revtunmand | The total number of registration replies that were sent with a reply code of 4BH (Registration Denied - reverse tunneling mandatory). | Int32
> replysent-delstyleunavail | The total number of registration replies that were sent with a reply code of 4FH (Registration Denied - reverse tunneling delivery style unavailable). | Int32
> replysent-mntoodistant | The total number of registration replies sent with a reply code of 4CH (Registration Denied - reverse tunneling mobile node too distant). | Int32
> replysent-invcoa | The total number of registration replies sent with a reply code of 4DH (Registration Denied - invalid care-of address). | Int32
> replysent-regtimeout | The total number of registration replies sent with a reply code of 4EH (Registration Denied - registration timeout). | Int32
> replysent-hanetunreach | The total number of registration requests sent with an FA reply code of 50H (Registration Denied - home network unreachable (ICMP error received)). | init32
> replysent-hahostunreach | The total number of registration requests sent with an FA reply code of 51H (Registration Denied - home agent host unreachable (ICMP error received)). | init32
> replysent-haportunreach | The total number of registration requests sent with an FA reply code of 52H (Registration Denied - home agent port unreachable (ICMP error received)). | Int32
> replysent-haunreach | The total number of registration requests sent with an FA reply code of 58H (Registration Denied - home agent unreachable (other ICMP error received)). | init32
> replysent-missnai | The total number of registration replies sent with a reply code of 61H (Registration Denied - missing NAI). | Int32
> replysent-misshomeagent | The total number of registration replies sent with a reply code of 62H (Registration Denied - missing home agent). | Int32
> replysent-misshomeaddr | The total number of registration replies sent with a reply code of 60H (Registration Denied - missing home address). | Int32
> replysent-unkchallenge | The total number of registration replies sent with a reply code of 68H (Registration Denied - unknown challenge). | Int32
> replysent-misschallenge | The total number of registration replies sent with a reply code of 69H (Registration Denied - missing challenge). | Int32
> replysent-stalechallenge | The total number of registration replies sent with a reply code of 6AH (Registration Denied - challenge). | Int32
> replysent-senderrors | The total number of errors that occurred while sending replies. | Int32
> ttlprepaid | The total number of Prepaid calls facilitated by the service. | Int32
> curprepaid | The total number of Prepaid calls currently being facilitated by the service. | Int32
> ttlonlineauthsucc | The total number of successful Online Authentications for the service. | Int32
> ttlonlineauthfail | TThe total number of successful Online Authentications for the service. | Int32
> revoc-sent | The total number of FA registration revocations sent. | Int32
> revoc-retry-sent | The total number of FA registration revocation messages the system attempted to re-send. | Int32
> revoc-ack-recv | The total number of FA registration revocation acknowledgement messages received. | Int32
> revoc-timeout | The total number of timeouts that occurred during FA registration revocations. | Int32
> revoc-recv | The total number of FA registration revocations received | Int32
> revoc-ack-sent | The total number of The total number of FA registration revocation acknowledgement messages sent. | Int32
> Important: See Bulk Statistics Overview for statistics that are common to all schema.

> ‌

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883