> MAP Service Configuration Mode Commands
> The MAP Service Configuration Mode is used to configure properties for Mobile Application Part (MAP) service.
> Mobile Application Part (MAP) is a protocol which provides an application layer for the various nodes in the core mobile network and GPRS and UMTS core network to communicate with each other in order to provide services to mobile phone users. The MAP service provides the application-layer protocol support used to access the Home Location Register (HLR).
> Important: The commands or keywords/variables that are available are dependent on platform type, product version, and installed license(s).
> access-protocol
> Configures access protocol parameters for the MAP service as defined for a specific SCCP network instance.
> Product
> SGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> access-protocol sccp-network sccp_id
> no access-protocol
> sccp-network sccp_id
> Specifies the ID number of the SCCP network to use for the SGSN connection.
> sccp_id : Must be an integer from 1 to 16.
> no
> Removes the access protocol SCCP network instance ID from the configuration.
> Usage
> Use this command to associate access protocol parameters to a specific instance of the MAP service for an SCCP network.
> Example
> The following command associates the access protocols with the SCCP network ID #10:
> access-protocol sccp-network 10
> application-context-name
> Configure the operation timer(s) for one or more MAP application contexts.
> Product
> SGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> application-context-name application operation-timer value
> default application-context-name application operation-timer
> default
> Resets the operation timers for all applications to system defaults.
> application
> Select one of the following applications to enable the application:

> • | authentication-failure-report : Sets the reporting operation timer for authentication failure. The setting range for this timer is 15 to 30 seconds and the default setting is 15 seconds.

> • | cancel-location : Sets the cancel location operation timer. The setting range for this timer is 15 to 30 seconds and the default setting is 15 seconds.

> • | check-imei : Sets the check-IMEI operation timer. The setting range for this timer is 15 to 30 seconds for releases 8.0 and 8.1 and 1 to 30 seconds for releases 9.0 and higher. The default setting is 15 seconds.

> • | delete-subscriber-data : Sets the delete subscriber data operation timer. The setting range for this timer is 15 to 30 seconds and the default setting is 15 seconds.

> • | mo-fwd-sm : Sets the operation timer for fowarding mobile-originated SMS. The setting range for this timer is 1 to 10 minutes and the default setting is 1 minute (60 seconds).

> • | ms-purge : Sets the operation timer for MS-purge function. The setting range for this timer is 15 to 30 seconds and the default setting is 15 seconds.

> • | mt-fwd-sm : Sets the operation timer for fowarding mobile-terminated SMS. The setting range for this timer is 1 to 10 minutes and the default setting is 1 minute (60 seconds).

> • | ready-for-sm : Sets the operation timer for the ready for SMS operation. The setting range for this timer is 15 to 30 seconds and the default setting is 15 seconds.

> • | send-authentication-info : Sets the operation timer for the sending authentication information operation. The setting range for this timer is 15 to 30 seconds and the default setting is 15 seconds.

> • | stand-alone-insert-subscriber-data : Sets the operation timer for the standalone insert subscriber data operation. The setting range for this timer is 15 to 30 seconds and the default setting is 15 seconds.

> • | ugl-insert-subscriber-data : Sets the operation timer for the insert subscriber data portion of the update GPRS location operation. TThe setting range for this timer is 15 to 30 seconds and the default setting is 15 seconds.

> • | update-gprs-location : Sets the operation timer for the update GPRS location operation. The setting range for this timer is 15 to 30 seconds and the default setting is 15 seconds.

> operation-timer value
> Configures the operation timer for the selected application. Timer values are indicated above.
> Usage
> Repeat this command entering a different application each time to enable multiple applications.
> Example
> application-context-name stand-alone-insert-subscriber-data operation-timer operation-timer 20
> auth-vectors
> Configures the number of authorization vectors to be requested from the home location register (HLR) during call setup to provide subscriber authentication.
> Product
> SGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> auth-vectors number-to-request number
> default auth-vectors number-to-request
> default
> Resets the number of vectors requested from the HLR to the system default.
> number-to-request number
> number: Must be an integer from 1 to 5 to define the number of authorization vectors be requested from the HLR.
> Default is 5.
> Usage
> Set the number of requests to be received from the HLR.
> Example
> auth-vectors number-to-request 4
> end
> Exits the current configuration mode and returns to the Exec mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> end
> Usage
> Return to the Exec mode.
> equipment-identity-register
> Defines the address of the equipment-identity-register (EIR) used by the SGSN.
> Product
> SGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> equipment-identity-register { isdn E.164_num | point code pt_code } [ source-ssn ssn| check-imei-every-n-events times]
> no equipment-identity-register { isdn E.164_num | point code pt_code }
> no
> Deletes the EIR configuration.
> isdn number
> Enter the E.164 number of the EIR.
> number: must be a string of 1 to 15 digits.
> point code pt_code
> Enter SS7 point code address of the EIR in dotted-decimal format according to variant settings:

> • | ITU Range 0.0.1 to 7.255.7

> • | ANSI Range 0.0.1 to 255.255.255

> • | TTC Range 0.0.1 to 15.31.255

> • | or a string of 1 to 11 characters

> source-ssn ssn
> Identifies the subsystem number (SSN) to be used.
> ssn must be an integer from 1 to 255.
> check-imei-every-n-events times
> Configures the frequency with which a ‘check IMEI’ message is sent to the EIR. When set, the SGSN skips sending the ‘check IMEI’ message for the first N-1 received attach requests.
> times must be an integer from 1 to 15.
> Important: This feature must be enabled by enabling verify-equipment-identity in the gmm retrieve-equipment-identity imei command of the SGSN Operator Policy configuration mode.
> Usage
> Configure the identity of the EIR that the SGSN uses and the interaction parameters.
> Example
> equipment-identity-register point code 7.255.7
> exit
> Exits the current configuration mode and returns to the global configuration mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> exit
> Usage
> Return to the context configuration mode.
> hlr
> This command enters the configuration mode for the home location register (HLR). The HLR is a database containing the subscriber profile information for all mobile stations (MS) / user equipment (UE) connecting to a specific GPRS or UMTS core network.
> Important: The commands and options for this mode are documented in the HLR Configuration Mode chapter.
> Product
> SGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> hlr
> policy
> This command configures the Transaction Capabilities Application Part (TCAP) -specific MAP policy for either ANSI or ITU SS7 variants.
> Product
> SGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> [ default ] policy tcap { use-received-destination-address | use-received-source-address }
> use-received-destination-address
> Selecting this keyword overwrites stored CG and CD addresses with a new address received in first TC CNT msg
> use-received-source-address
> Selecting this keyword instructs the MAP service to use the received source address for the dialog.
> Usage
> Use this command to determine how TCAP will handle MAP messages.
> Example
> policy tcap use-received-destination-address
> short-message-service
> This command enables and disables the short message service (SMS service) and provides access to the SMS service configuration mode.
> Product
> SGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> [ no } short-message-service
> no
> Disables the SMS service.
> Usage
> Enter the command to access the SMS service configuration mode to fine tune the SMS functionality.
> Example
> short-message-service

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883