> Out-Address Configuration Mode Commands
> The Out-Address configuration mode provides the commands to configure the outgoing addresses for SCCP entities.
> Important: The commands or keywords/variables that are available are dependent on platform type, product version, and installed license(s).
> end
> Exits the configuration mode and returns to the Exec mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> end
> Usage
> Change the mode back to the Exec mode.
> exit
> Exits the configuration mode and returns to the Global configuration mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> exit
> Usage
> Return to the Global configuration mode.
> gt-address
> Configures the SCCP short address.
> Product
> SGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> gt-address gt_address
> gt_address
> A string of 1 to 15 digits to define the GT-address
> Usage
> Define the GT-address
> Example
> gt-address 010405525397
> gt-format
> The GT-format provides four formats that can be used during GTT.
> Product
> SGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> gt-format format_num
> format_num
> 1: Selects GT-format 1 options which include nature-of-address and odd/even. Once selected, the system enters GT-Format1 configuration mode.
> 2: Selects GT-format2 options which include translation-type. Once selected, the system enters GT-Format2 configuration mode.
> 3: Selects GT-format3 options which include encoding-scheme, numbering-plan3 and translation-type. Once selected, the system enters GT-Format1 configuration mode.
> 4: Selects GT-format4 options which include encoding-scheme, nature-of-address, numbering-plan, and translation-type. Once selected, the system enters GT-Format4 configuration mode.
> Usage
> Select the a GT-format that include encoding-scheme as part of the GTT process.
> Example
> gt-format 3
> ni-indicator
> Configures the National and International indicator to use during the GTT process.
> Product
> SGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> ni-indicator ni_ind
> ni_ind
> Select one of the following as the appropriate type of national indicator for the address structure:

> • | national

> • | international

> Usage
> Select the international indicator to be used for out-going addresses.
> Example
> ni-indicator international
> point-code
> Selects and configures the SS7-type point code for use with the out-going address.
> Product
> SGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> point-code pt_code
> pt_code
> Enter 1 to 11 digits in the point code format predefined during variant selection of GTT association.
> Usage
> Define an ITU point code to be used for out-going address processing.
> Example
> point-code 6.255.6
> routing-indicator
> Selects the type of routing and the indicator to be included in the out-going message.
> Product
> SGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> routing-indicator routing_ind
> routing_ind
> Select one of the following options:

> • | gt: Inserts an indicator that identifies routing based on global title.

> • | ssn: Inserts an indicator that identifies routing based on the subsystem number.

> Usage
> Select global title as the appropriate routing indicator.
> Example
> routing-indicator gt
> ssf
> Selects the subservice field as factor in the out-going address processing. ssf sets the network indicator in the subservice field for SS7 Message Signal Units (MSUs). The indicator carried in the message’s routing information typically identifies the structure of the point code as a message from within a nation or as a message coming from outside the national - international.
> Product
> SGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> ssf sub_svc_fld
> sub_svc_fld
> Select one of the following options:

> • | international: The network indicator identifies the message as international with a point code structure that does not match the national point code structure,

> • | national: The network indicator identifies the messages as having a national point code structure.

> • | reserved: Provides an alternate network indicator for national messages.

> • | spare: Provides an alternate network indicator for international messages.

> Usage
> Select the international NI for inclusion in out-going address subservice fields.
> Example
> ssf international
> ssn
> Selects the subsystem number to be included in the out-going message.
> Product
> SGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> ssn sub_sys_num
> sub_sys_num
> Enter an integer from 1 to 255.
> Usage
> Use subsystem number 44 in the out-going address.
> Example
> ssn 44

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883