> PDIF Schema Statistics
> The PDIF schema provides the following types of statistics:

> • | Counter: A counter records incremental data cumulatively and rolls over when the counter limit is reached. The limit depends upon the counter data type.

> • | Gauge: A gauge statistic indicates a single value representative of a single instance. This type is often used to track particular events in time.

> Important: The format string syntax is described by Schema Format String Syntax in the Bulk Statistics Overview chapter.
> Important: Unless otherwise indicated, all statistics are counters. For statistics with the Int32 data type, the roll-over to zero limit is 4,294,967,295. For statistics with the Int64 data type, the roll-over to zero limit is 18,446,744,073,709,551,615. All counter statistics are cumulative and reset only by one of the following methods: roll-over (as described above), after a system restart, or after a clear command is performed. All statistics are considered standards-based unless otherwise noted.
> The following variables are supported:
> PDIF Schema Statistics

> Statistic | Description | Data Type
> vpnname | The name of the context currently facilitating the service processing the subscriber session. | String
> vpnid | The identification number of the context currently facilitating the service processing the subscriber session. This is an internal reference number. | Int32
> svcname | The service name for which PDIF statistics are being displayed. | String
> svcid | The service ID for which PDIF statistics are being displayed. | Int32
> bindaddress | The bind IP address for this PDIF service. | String
> state | System-wide PDIF state identified by the following codes:
> • | unknown(0)
> • | noservice(1): Chassis is not configured/licensed for PDIF service.
> • | active(2): At least one PDIF service is available.
> • | temporary(3): PDIF service is running in a temporary capacity.
> • | outofservice(4): No PDIF service is currently active, but one or more PDIF services are configured.
> | Int32
> sess-curinprog | Number of PDIF service sessions in progress (including transient ones). | Int32
> sess-curact | Number of currently active PDIF sessions. | Int32
> sess-curdorm | Number of currently dormant PDIF sessions. | Int32
> sess-curactipv4 | Number of currently active IPV4 sessions. | Int32
> sess-cursip | Number of current simple IP sessions. | Int32
> sess-curmip | Number of current mobile IP sessions. | Int32
> sess-curpmip | Number of current proxy mobile IP sessions. | Int32
> sess-sipattempt | Number of attempted simple IP sessions. | Int32
> sess-sipsuccess | Number of successful simple IP sessions. | Int32
> sess-sipfail | Number of failed simple IP sessions. | Int32
> sess-mipattempt | Number of attempted mobile IP sessions. | Int32
> sess-mipsuccess | Number of successful mobile IP sessions. | Int32
> sess-mipfail | Number of failed mobile IP sessions. | Int32
> sess-pmipattempt | Number of attempted proxy mobile IP sessions. | Int32
> sess-pmipsuccess | Number of successful proxy mobile IP sessions completed. | Int32
> sess-pmipfail | Number of failed proxy mobile IP sessions. | Int32
> sess-sipfbacksucc | Number of successful sImple IP fallback sessions. | Int32
> sess-sipfbacknotdone | Number of sessions where simple IP fallback was not done. | Int32
> sess-sipfbacknorrq | Number of simple IP fallback sessions with no rrq request. | Int32
> sess-sipfbacknotallw | Number of simple IP fallback sessions that were not allowed. | Int32
> sess-sipfbacktagaddr | Number of simple IP fallback sessions that failed because of no tagged pool address. | Int32
> sess-sipfbackmisc | Number of simple IP fallback sessions that failed because of miscellaneous reasons. | Int32
> sess-ttlsetup | Total number of session setups. | Int32
> sess-ttlattempt | Total number of session attempts. | Int32
> sess-ttlattemptfail | Total number of session attempts that failed. | Int32
> sess-ttlrel | Total number of sessions released. | Int32
> sess-ttlrellocal | Total number of sessions released locally. | Int32
> sess-ttlrelremote | Total number of sessions released remotely. | Int32
> sess-ttlsip | Total Number of simple IP sessions. | Int32
> sess-ttlmip | Total number of mobile IP sessions. | Int32
> sess-ttl-pmip | Total number of proxy mobile IP sessions. | Int32
> sess-discbeforeconn | Number of sessions disconnected by remote node before being connected. | Int32
> sess-discipsec | Number of sessions terminated because of IPsec. | Int32
> discadmin | Number of sessions terminated because of admin release. | Int32
> sess-discidletimeout | Number of sessions terminated because of idle timer timeout. | Int32
> sess-discabstimeout | Number of sessions terminated because of absolute timeout. | Int32
> sess-disclongdur | Number of sessions terminated because of long duration timer timeout. | Int32
> sess-discmmdtimeout | Number of sessions terminated because of multimedia domain service timer expiry. | Int32
> sess-distysetuptimeout | Number of sessions terminated because of TY interface setup timeout. | Int32
> sess-discsesssetuptimeout | Number of sessions terminated because of Session Manager session setup timeout. | Int32
> sess-discnonexistpcrf | Number of sessions terminated because of non-existence of PCRF. | Int32
> sess-discnoresource | Number of sessions terminated because of no resources. | Int32
> sess-discauthfail | Number of sessions terminated because of AAA authentication failure. | Int32
> sess-discflowaddfail | Number of sessions terminated because of flow add failure. | Int32
> sess-discinvdestctx | Number of sessions terminated because of invalid destination context. | Int32
> sess-discsourceviol | Number of sessions terminated because of source IP address violation. | Int32
> sess-discmipremote | Number of sessions terminated because of remote mobile IP. | Int32
> sess-discmiplocal | Number od sessions terminated because of local mobile IP. | Int32
> sess-discdupreq | Number of sessions terminated because of a duplicated request. | Int32
> sess-discmacfail | Number of sessions terminated because of a MAC address failure. | Int32
> sess-discaddrfail | Number of sessions terminated because of an address failure. | Int32
> sess-discmisc | Number of sessions terminated for miscellaneous reasons. | Int32
> sess-remaining | Number of available sessions remaining. | Int32
> sess-limit | Session limit reached. | Int32
> mac-authreq | Number of MAC address authentication requests. | Int32
> mac-authreqvalid | Number of valid MAC address authentication requests. | Int32
> mac-authreqinv | Number of invalid MAC address authentication requests. | Int32
> mac-authsucc | Number of MAC address validation successes. | Int32
> mac-authsuccmatch | Number of successful MAC address matches. | Int32
> mac-authsucchssfail | Number of HSS server authentication failures. | Int32
> mac-authfail | Number of MAC address authentication failures because of an unauthorized MAC address. | Int32
> mac-authfaildiam | Number of MAC address authentication failures because of a Diameter error. | Int32
> mac-authfailuserunk | Number of MAC address authentication failures because of an unknown user. | Int32
> mac-authfailmacnotfound | Number of MAC address authentication failures because the MAC address was not found. | Int32
> mac-authfailmacmissing | Number of MAC address authentication failures because the MAC address was missing. | Int32
> mac-authfailmacmalformed | Number of MAC address authentication failures because the MAC address was malformed. | Int32
> mac-authfailnosh | Number of MAC address authentication failures because the Sh interface is down. | Int32
> mac-authfailother | Number of MAC address authentication failures because of another reason. | Int32
> eap-rxttlsrvrpassthru | Total number of EAP messages received from the EAP server in pass-through mode. | Int32
> eap-rxchalsrvrpassthru | Total number of EAP challenge messages sent to the EAP server in pass-through mode. | Int32
> eap-rxsuccsrvrpassthru | Total number of EAP-Success messages received from the EAP server in pass-through mode. | Int32
> eap-rxfailsrvrpassthru | Total number of EAP-Failure messages received from the EAP server in pass-through mode. | Int32
> eap-rxmobilepassthru | Total number of EAP messages received from mobile clients in pass-through mode. | Int32
> eap-txttlsrvrpassthru | Total number of EAP messages transmitted to the EAP server in pass-through mode. | Int32
> eap-txinitreqsrvrpassthru | Total number of EAP messages transmitted to the EAP server in pass-through mode for initial request. | Int32
> eap-txfwdreqsrvrpassthru | Total number of EAP messages transmitted to the EAP server in pass-through mode for forward request. | Int32
> ipsec-txpacket | Number of IPsec packets transmitted. | Int64
> ipsec-txoctet | Number of IPsec bytes transmitted. | Int64
> ipsec-rxpacket | Number of IPsec packets received. | Int64
> ipsec-rxoctet | Number of IPsec bytes received. | Int64
> ipsec-violpacket | Number of data packets that do not match any of the configured traffic selectors. | Counter32
> Important: See Bulk Statistics Overview for statistics that are common to all schema.�

> ‌

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883