--LINKSYS-MODEL-MIB { iso(1) org(3) dod(6) internet(1) private(4)
--      Enterprises(1) linksys(3955) }


LINKSYS-MODEL-MIB DEFINITIONS ::= BEGIN
-- Title: Linksys propritary MIB
-- Date: January 28, 2003    Version 1.01
--

    IMPORTS
		enterprises, IpAddress,             FROM RFC1155-SMI
		DisplayString, PhysAddress          FROM RFC1213-MIB
		OBJECT-TYPE                         FROM RFC-1212
		TRAP-TYPE                           FROM RFC-1215;


internet				OBJECT IDENTIFIER ::= { iso org(3) dod(6) 1 }
directory				OBJECT IDENTIFIER ::= { internet 1 }
mgmt					OBJECT IDENTIFIER ::= { internet 2 }
experimental			OBJECT IDENTIFIER ::= { internet 3 }
private					OBJECT IDENTIFIER ::= { internet 4 }
enterprises				OBJECT IDENTIFIER ::= { private 1 }
linksys                 OBJECT IDENTIFIER ::= { enterprises 3955 }
common                  OBJECT IDENTIFIER ::= { linksys 1 }
management              OBJECT IDENTIFIER ::= { linksys 2 }
control                 OBJECT IDENTIFIER ::= { linksys 3 }
information             OBJECT IDENTIFIER ::= { linksys 4 }
products                OBJECT IDENTIFIER ::= { linksys 5 }
basicMgt                OBJECT IDENTIFIER ::= { management 1 }
advanceMgt              OBJECT IDENTIFIER ::= { management 2 }
wanMgt                  OBJECT IDENTIFIER ::= { management 3 }
vpnMgt                  OBJECT IDENTIFIER ::= { management 4 }
firewallMgt             OBJECT IDENTIFIER ::= { management 5 }
wirelessMgt             OBJECT IDENTIFIER ::= { management 6 }
adslRemoteNode          OBJECT IDENTIFIER ::= { management 7 }
wirelessCommon          OBJECT IDENTIFIER ::= { wirelessMgt 1 }
ieee80211b              OBJECT IDENTIFIER ::= { wirelessMgt 2 }
ieee80211a              OBJECT IDENTIFIER ::= { wirelessMgt 3 }
statusInfo              OBJECT IDENTIFIER ::= { information 1 }
statisticsInfo          OBJECT IDENTIFIER ::= { information 2 }
printServer             OBJECT IDENTIFIER ::= { products 1 }
networkStorageServer    OBJECT IDENTIFIER ::= { products 2 }


-- the Common Group

	commonFirmwareVer OBJECT-TYPE
		SYNTAX	DisplayString
		ACCESS	read-only
		STATUS	mandatory
		DESCRIPTION
				" The firmware version of this managed node. "
		::= { common 1 }
	
	commonMIBfileVer OBJECT-TYPE
		SYNTAX	DisplayString
		ACCESS	read-only
		STATUS	mandatory
		DESCRIPTION
				" Defines the current version of Linksys MIB definition.
				Initially the version number is 1.00.00. "
		::= { common 2 }
	
	commonDevType OBJECT-TYPE
		SYNTAX	INTEGER {
		      		others(1),
		      		adsl-gateway(2),
		      		cable-gateway(3),
		      		router(4),
		      		accessPoint(5),
		      		wirelessNIC(6),
		      		wirelessAdapter(7),
		      		managementNIC(8)
		      	}
		ACCESS	read-only
		STATUS	mandatory
		DESCRIPTION
				"The hardware type of this managed node."
		::= { common 3 }
	
	commonModelId OBJECT-TYPE
		SYNTAX	DisplayString
		ACCESS	read-only
		STATUS	mandatory
		DESCRIPTION
				" The hardware model ID of this managed node. "
		::= { common 4 }
	
	commonTable OBJECT-TYPE
		SYNTAX	SEQUENCE OF CommonEntry
		ACCESS	not-accessible
		STATUS	mandatory
		DESCRIPTION
				" Table of basic information that can be used to identify this
			managed node."
		::= { common 5 }
	
	commonEntry OBJECT-TYPE
		SYNTAX	CommonEntry
		ACCESS	not-accessible
		STATUS	mandatory
		DESCRIPTION
				" An entry in the table, containing read only identification
				information."
		INDEX	{ commonIfIndex, commonFunIndex }
		::= { commonTable 1 }
	
	CommonEntry ::=
		SEQUENCE {
			commonIfIndex 			INTEGER,
			commonFunIndex			INTEGER,
			commonNote    			DisplayString
		}
	
	commonIfIndex OBJECT-TYPE
		SYNTAX	INTEGER
		ACCESS	read-only
		STATUS	mandatory
		DESCRIPTION
				"The interface on which this entry's equivalence is effective.
				The interface identified by a particular value of this index is
				the same interface as identified by the same value of ifIndex."
		::= { commonEntry 1 }
	
	commonFunIndex OBJECT-TYPE
		SYNTAX	INTEGER {
		      		wan-connection(1),
		      		dhcp(2),
		      		access-log(3),
		      		ip-range-filter(4),
		      		port-range-filter(5),
		      		mac-filter(6),
		      		app-forwarding(7),
		      		upnp-forwarding(8),
		      		dynamic-route(9),
		      		static-route(10),
		      		dmz(11),
		      		mac-clone(12),
		      		ieee802dot11(13),
		      		firewall(14),
		      		vpn(15)
		      	}
		ACCESS	read-only
		STATUS	mandatory
		DESCRIPTION
				"The type of function, distinguished according to hardware
				model of this managed node."
		::= { commonEntry 2 }
	
	commonNote OBJECT-TYPE
		SYNTAX	DisplayString
		ACCESS	read-only
		STATUS	mandatory
		DESCRIPTION
				"Notification for the specified function."
		::= { commonEntry 3 }


-- the Management Group

	mgtSystemReset OBJECT-TYPE
		SYNTAX	INTEGER {
		      		warm-start(1),
		      		cold-start(2)
		      	}
		ACCESS	read-write
		STATUS	mandatory
		DESCRIPTION
				"Indicates whether to set the managed node to do warm start or
				cold start. Definition refers to RFC1215."
		::= { basicMgt 1 }
	
	mgtFactoryReset OBJECT-TYPE
		SYNTAX	INTEGER {
		      		disable(0),
		      		enable(1)
		      	}
		ACCESS	read-write
		STATUS	mandatory
		DESCRIPTION
				"Indicates whether to set the managed node to restore factory
				default settings or not."
		::= { basicMgt 2 }
	
	mgtAdministrator OBJECT-TYPE
		SYNTAX	DisplayString (SIZE(0..64))
		ACCESS	read-write
		STATUS	mandatory
		DESCRIPTION
				"The authorized password used to access the system."
		::= { basicMgt 3 }
	
	mgtAdminUsername OBJECT-TYPE
		SYNTAX	DisplayString (SIZE(0..64))
		ACCESS	read-write
		STATUS	mandatory
		DESCRIPTION
				"The user name used to access the system."
		::= { basicMgt 4 }
	
	mgtSaveConfiguration OBJECT-TYPE
		SYNTAX	INTEGER {
		      		none(0),
		      		apply(1)
		      	}
		ACCESS	read-write
		STATUS	mandatory
		DESCRIPTION
				"Indicates whether to store Enterprise MIB objects value in
				non-volatile RAM and reinitializing the managed node."
		::= { basicMgt 5 }
	
	mgtHostName OBJECT-TYPE
		SYNTAX	DisplayString (SIZE(0..32))
		ACCESS	read-write
		STATUS	mandatory
		DESCRIPTION
				"Supply a host name for the router. Some ISPs require this name as
				identification. Leaving this field will work."
		::= { basicMgt 6 }
	
	mgtDomainName OBJECT-TYPE
		SYNTAX	DisplayString (SIZE(0..64))
		ACCESS	read-write
		STATUS	mandatory
		DESCRIPTION
				"Supply a domain name for the router. Some ISPs require this name as
				identification. Leaving this field will work."
		::= { basicMgt 7 }
	
	mgtNodeNetAddress OBJECT-TYPE
		SYNTAX	IpAddress
		ACCESS	read-write
		STATUS	mandatory
		DESCRIPTION
				"The IP address to which identifies this managed node from
				internal networking."
		::= { basicMgt 8 }
	
	mgtNodeSubnetMask OBJECT-TYPE
		SYNTAX	IpAddress
		ACCESS	read-write
		STATUS	mandatory
		DESCRIPTION
				"The subnet mask associated with the IP address of this system. The
				value of the mask is an IP address with all the network bits set to
				1 and all the hosts bits set to 0."
		::= { basicMgt 9 }
	
	mgtDhcpStatus OBJECT-TYPE
		SYNTAX	INTEGER {
		      		disable(0),
		      		enable(1)
		      	}
		ACCESS	read-write
		STATUS	mandatory
		DESCRIPTION
				"Indicates whether to configure the managed node to automatically
				assign IP address to each of LAN clients."
		::= { basicMgt 10 }
	
	mgtDhcpStartNetAddr OBJECT-TYPE
		SYNTAX	IpAddress
		ACCESS	read-write
		STATUS	mandatory
		DESCRIPTION
				"Specifies a start IP address to which DHCP will issue to "
		::= { basicMgt 11 }
	
	mgtDhcpNumberUsers OBJECT-TYPE
		SYNTAX	INTEGER
		ACCESS	read-write
		STATUS	mandatory
		DESCRIPTION
				"The number of clients to which plan on networking to this
				managed node."
		::= { basicMgt 12 }

-- the Community Table

	mgtCommunityTable OBJECT-TYPE
		SYNTAX	SEQUENCE OF MgtCommunityEntry
		ACCESS	not-accessible
		STATUS	mandatory
		DESCRIPTION
			" Table of access community. "
		::= { basicMgt 13 }
	
	mgtCommunityEntry OBJECT-TYPE
		SYNTAX	MgtCommunityEntry
		ACCESS	not-accessible
		STATUS	mandatory
		DESCRIPTION
			 	" An entry in the table, containing read/write
			 	community names. "
		INDEX	{ mgtCommunityIndex }
		::= { mgtCommunityTable 1 }
	
	MgtCommunityEntry ::=
		SEQUENCE {
			mgtCommunityIndex		INTEGER,
			mgtCommunityName 		DisplayString,
			mgtCommunityType 		INTEGER
		}
	
	mgtCommunityIndex OBJECT-TYPE
		SYNTAX	INTEGER
		ACCESS	read-only
		STATUS	mandatory
		DESCRIPTION
				"An unique value for each community."
		::= { mgtCommunityEntry 1 }
	
	mgtCommunityName OBJECT-TYPE
		SYNTAX	DisplayString (SIZE(0..32))
		ACCESS	read-write
		STATUS	mandatory
		DESCRIPTION
			"The name used to manage the SNMP protocol entity."
		::= { mgtCommunityEntry 2 }
	
	mgtCommunityType OBJECT-TYPE
		SYNTAX	INTEGER {
		      		read-only(1),
		      		read-write(2)
		      	}
		ACCESS	read-write
		STATUS	mandatory
		DESCRIPTION
			"Specifies the privilege for this community name."
		::= { mgtCommunityEntry 3 }


-- The Advance Management Group --

	advMgtRefreshMIB OBJECT-TYPE
		SYNTAX	INTEGER {
		      		none(0),
		      		apply(1)
		      	}
		ACCESS	read-write
		STATUS	mandatory
		DESCRIPTION
				"Refresh Enterprise MIB object data from RAM NV."
		::= { advanceMgt 1 }
	
	advMgtWanReqBlockStatus OBJECT-TYPE
		SYNTAX	INTEGER {
		      		disable(0),
		      		enable(1)
		      	}
		ACCESS	read-write
		STATUS	mandatory
		DESCRIPTION
				"Set to enable(1) will prevent local network from
				being 'pinged' or detected and also can reinforce
				local network security by hiding the network port."
		::= { advanceMgt 2 }
	
	advMgtIpSecPassThroughStatus OBJECT-TYPE
		SYNTAX	INTEGER {
		      		disable(0),
		      		enable(1)
		      	}
		ACCESS	read-write
		STATUS	mandatory
		DESCRIPTION
				"Specifies to enable(1) or disable(0) IPSec Pass
				Through ability."
		::= { advanceMgt 3 }
	
	advMgtPptpPassThroughStatus OBJECT-TYPE
		SYNTAX	INTEGER {
		      		disable(0),
		      		enable(1)
		      	}
		ACCESS	read-write
		STATUS	mandatory
		DESCRIPTION
				"Point-to-Point Tunneling Protocol is the method
				used to enable VPN tunnels. This object can be
				used to specify the PPTP pass through ability."
		::= { advanceMgt 4 }
	
	advMgtL2TPPassThroughStatus OBJECT-TYPE
		SYNTAX	INTEGER {
		      		disable(0),
		      		enable(1)
		      	}
		ACCESS	read-write
		STATUS	mandatory
		DESCRIPTION
				"Specifies to enable(1) or disable(0) Layer Two
				Tunneling Protocol Pass Through ability."
		::= { advanceMgt 5 }
	
	advMgtRemoteMgtStatus OBJECT-TYPE
		SYNTAX	INTEGER {
		      		disable(0),
		      		enable(1)
		      	}
		ACCESS	read-write
		STATUS	mandatory
		DESCRIPTION
				"Specifies whether allow this managed node to be
				managed from a remote location."
		::= { advanceMgt 6 }
	
	advMgtRemoteUpgradeStatus OBJECT-TYPE
		SYNTAX	INTEGER {
		      		disable(0),
		      		enable(1)
		      	}
		ACCESS	read-write
		STATUS	mandatory
		DESCRIPTION
				"Specifies whether allow the managed node's firmware
				to be upgraded from a remote location."
		::= { advanceMgt 7 }
	
	advMgtAccessLogStatus OBJECT-TYPE
		SYNTAX	INTEGER {
		      		disable(0),
		      		enable(1)
		      	}
		ACCESS	read-write
		STATUS	mandatory
		DESCRIPTION
				"Specifies whether to send access log messages to
				specific management entities."
		::= { advanceMgt 8 }
	
	advMgtMulticastPassStatus OBJECT-TYPE
		SYNTAX	INTEGER {
		      		disable(0),
		      		enable(1)
		      	}
		ACCESS	read-write
		STATUS	mandatory
		DESCRIPTION
				"Specifies whether allow for multiple transmissions
				to specific receptions at the same time."
		::= { advanceMgt 9 }
	
	advMgtMtuStatus OBJECT-TYPE
		SYNTAX	INTEGER {
		      		disable(0),
		      		enable(1)
		      	}
		ACCESS	read-write
		STATUS	mandatory
		DESCRIPTION
				"Indicates whether to use specific MTU size, refer
				to advMgtMtuSize object, as the largest packet size."
		::= { advanceMgt 10 }
	
	advMgtMtuSize OBJECT-TYPE
		SYNTAX	INTEGER
		ACCESS	read-write
		STATUS	mandatory
		DESCRIPTION
				"Specifies the largest packet size permitted for
				network transmission."
		::= { advanceMgt 11 }
	
	advMgtLocalTimeZone OBJECT-TYPE
		SYNTAX	INTEGER
		ACCESS	read-write
		STATUS	mandatory
		DESCRIPTION
				"Indicates local time zone for this managed node."
		::= { advanceMgt 12 }


-- The Routing group for both LAN and WAN. --

	routingMethodTable OBJECT-TYPE
		SYNTAX	SEQUENCE OF RoutingMethodEntry
		ACCESS	not-accessible
		STATUS	mandatory
		DESCRIPTION
				"The table of dynamic routing settings which can
				automatically adjust to physical changes in the
				network's layout."
		::= { advanceMgt 13 }
	
	routingMethodEntry OBJECT-TYPE
		SYNTAX	RoutingMethodEntry
		ACCESS	not-accessible
		STATUS	mandatory
		DESCRIPTION
				"The protocol information for one of this entity's
				routing method."
		INDEX	{ routingMethodIndex }
		::= { routingMethodTable 1 }
	
	RoutingMethodEntry ::=
		SEQUENCE {
			routingMethodIndex			INTEGER,
			dynamicRoutingTX  			INTEGER,
			dynamicRoutingRX  			INTEGER
		}
	
	routingMethodIndex OBJECT-TYPE
		SYNTAX	INTEGER
		ACCESS	read-only
		STATUS	mandatory
		DESCRIPTION
				"An unique value for each routing method."
		::= { routingMethodEntry 1 }
	
	dynamicRoutingTX OBJECT-TYPE
		SYNTAX	INTEGER {
		      		disable(0),
		      		rip1(1),
		      		rip1-compatible(2),
		      		rip2(3)
		      	}
		ACCESS	read-write
		STATUS	mandatory
		DESCRIPTION
				"Indicates the protocol to which transmit data on the
				network."
		::= { routingMethodEntry 2 }
	
	dynamicRoutingRX OBJECT-TYPE
		SYNTAX	INTEGER {
		      		disable(0),
		      		rip1(1),
		      		rip2(2)
		      	}
		ACCESS	read-write
		STATUS	mandatory
		DESCRIPTION
		 		"Indicates the protocol to which receive data on the
		 		network."
		::= { routingMethodEntry 3 }


-- The DMZ group which can support multiple DMZ. --

	dmzTable OBJECT-TYPE
		SYNTAX	SEQUENCE OF DmzEntry
		ACCESS	not-accessible
		STATUS	mandatory
		DESCRIPTION
				"The table of DMZ settings which allow one local
				user to be exposed to the Internet to use a
				special-purpose service."
		::= { advanceMgt 14 }
	
	dmzEntry OBJECT-TYPE
		SYNTAX	DmzEntry
		ACCESS	not-accessible
		STATUS	mandatory
		DESCRIPTION
				"The IP addresses information for one of DMZ."
		INDEX	{ dmzIndex }
		::= { dmzTable 1 }
	
	DmzEntry ::=
		SEQUENCE {
			dmzIndex					INTEGER,
			dmzRemoteIPAddress			IpAddress,
			dmzHostIPAddress			IpAddress
		}
	
	dmzIndex OBJECT-TYPE
		SYNTAX	INTEGER
		ACCESS	read-only
		STATUS	mandatory
		DESCRIPTION
			"An unique value for each DMZ setting."
		::= { dmzEntry 1 }
	
	dmzRemoteIPAddress OBJECT-TYPE
		SYNTAX	IpAddress
		ACCESS	read-write
		STATUS	mandatory
		DESCRIPTION
				"Specifies the remote host IP address to which maps
				to the local host specified by dmzHostIPAddress
				object."
		::= { dmzEntry 2 }

	dmzHostIPAddress OBJECT-TYPE
		SYNTAX	IpAddress
		ACCESS	read-write
		STATUS	mandatory
		DESCRIPTION
		        "Specifies the local host IP address which will be
		        exposed to the Internet."
		::= { dmzEntry 3 }


-- the StaticRoutingTable Group

	staticRoutingTable OBJECT-TYPE
		SYNTAX	SEQUENCE OF StaticRoutingEntry
		ACCESS	not-accessible
		STATUS	mandatory
		DESCRIPTION
				"The table of static routing methods which
				specifies pre-determined pathway that network
				information must travel to reach a specific
				host or network."
		::= { advanceMgt 15 }

	staticRoutingEntry OBJECT-TYPE
		SYNTAX	StaticRoutingEntry
		ACCESS	not-accessible
		STATUS	mandatory
		DESCRIPTION
				"The configuration information for one of static
				routing."
		INDEX	{ staticRoutingIndex }
		::= { staticRoutingTable 1 }

	StaticRoutingEntry ::=
		SEQUENCE {
			staticRoutingIndex				INTEGER,
			destinationNetAddress			IpAddress,
			routingSubnetMask				IpAddress,
			routingDefaultGateway			IpAddress,
			routingHopCount					INTEGER,
			routingInterface				INTEGER,
			nFlagStatus						INTEGER
		}

	staticRoutingIndex OBJECT-TYPE
		SYNTAX	INTEGER
		ACCESS	read-only
		STATUS	mandatory
		DESCRIPTION
			"An unique value for each static routing method."
		::= { staticRoutingEntry 1 }

	destinationNetAddress OBJECT-TYPE
		SYNTAX	IpAddress
		ACCESS	read-write
		STATUS	mandatory
		DESCRIPTION
				"The IP address of the remote network or host to
				which will be assigned a static route."
		::= { staticRoutingEntry 2 }

	routingSubnetMask OBJECT-TYPE
        SYNTAX	IpAddress
        ACCESS	read-write
        STATUS	mandatory
        DESCRIPTION
                "Determines which portion of an IP address is the
                network portion, and which portion is the host
                portion."
        ::= { staticRoutingEntry 3 }

	routingDefaultGateway OBJECT-TYPE
        SYNTAX	IpAddress
        ACCESS	read-write
        STATUS	mandatory
        DESCRIPTION
                "Specifies the IP address of the gateway device
                that allows for contact between the managed node
                and the remote network or host."
        ::= { staticRoutingEntry 4 }

	routingHopCount OBJECT-TYPE
        SYNTAX	INTEGER
        ACCESS	read-write
        STATUS	mandatory
        DESCRIPTION
                "Specifies the maximun number of hops that packets to
                the destination specified by this route entry should
                be forwarded."
        ::= { staticRoutingEntry 5 }

	routingInterface OBJECT-TYPE
        SYNTAX	INTEGER {
              		lan(1),
              		wan(2)
              	}
        ACCESS	read-write
        STATUS	mandatory
        DESCRIPTION
                "Specifies the physical interface to which will apply
                this routing configuration."
        ::= { staticRoutingEntry 6 }

	nFlagStatus OBJECT-TYPE
        SYNTAX	INTEGER {
              		free(0),
              		ready(1),
              		active(2)
              	}
        ACCESS	read-write
        STATUS	mandatory
        DESCRIPTION
                "Indicates the operation status for this routing
                entry."
        ::= { staticRoutingEntry 7 }


-- the TrapManagerTable Group

	trapManagerTable OBJECT-TYPE
        SYNTAX	SEQUENCE OF TrapManagerEntry
        ACCESS	not-accessible
        STATUS	mandatory
        DESCRIPTION
                "Table of SNMP Trap message receivers."
        ::= { advanceMgt 16 }

	trapManagerEntry OBJECT-TYPE
        SYNTAX	TrapManagerEntry
        ACCESS	not-accessible
        STATUS	mandatory
        DESCRIPTION
                "An entry in the table contains the host IP
                address which will receive trap messages."
        INDEX	{ trapManagerIndex }
        ::= { trapManagerTable 1 }

	TrapManagerEntry ::=
        SEQUENCE {
        	trapManagerIndex                INTEGER,
        	trapMgrNetAddress               IpAddress
        }

	trapManagerIndex OBJECT-TYPE
        SYNTAX	INTEGER
        ACCESS	read-only
        STATUS	mandatory
        DESCRIPTION
                "An unique value for each trap receiver."
        ::= { trapManagerEntry 1 }

	trapMgrNetAddress OBJECT-TYPE
        SYNTAX	IpAddress
        ACCESS	read-write
        STATUS	mandatory
        DESCRIPTION
                "The IP address to which will receive the Log
                message sent via trap protocol."
        ::= { trapManagerEntry 2 }

	advMgtUPnPStatus OBJECT-TYPE
        SYNTAX	INTEGER {
					disable(0),
					enable(1)
				}
        ACCESS	read-write
        STATUS	mandatory
        DESCRIPTION
                "Specifies whether allow Windows XP to automatically
                confiure the managed node for various Internet
                applications."
        ::= { advanceMgt 17 }

	advMgtUPnPControl OBJECT-TYPE
        SYNTAX	INTEGER {
					disable(0),
					enable(1)
				}
        ACCESS	read-write
        STATUS	mandatory
        DESCRIPTION
                "Specifies whether allow Windows XP to read and write
                the UPnP Forwarding of managed node using UPnP."
        ::= { advanceMgt 18 }
        
	advMgtUPnPConnectControl OBJECT-TYPE
        SYNTAX	INTEGER {
					disable(0),
					enable(1)
				}
        ACCESS	read-write
        STATUS	mandatory
        DESCRIPTION
                "Specifies whether allow Windows XP to read and write
                the UPnP WAN Connection of managed node using UPnP."
        ::= { advanceMgt 19 }        


-- The WAN Management Group --

	wanConnectionTable OBJECT-TYPE
        SYNTAX	SEQUENCE OF WanConnectionEntry
        ACCESS	not-accessible
        STATUS	mandatory
        DESCRIPTION
                " Table of WAN connection management. "
        ::= { wanMgt 1 }

	wanConnectionEntry OBJECT-TYPE
        SYNTAX	WanConnectionEntry
        ACCESS	not-accessible
        STATUS	mandatory
        DESCRIPTION
                " An entry in the table specifies the connection
                configuration for WAN interface."
        INDEX	{ wanIndex }
        ::= { wanConnectionTable 1 }

	WanConnectionEntry ::=
        SEQUENCE {
			wanIndex						INTEGER,
			wanIfIndex						INTEGER,
			wanConnectionType				INTEGER,
			wanNetAddress					IpAddress,
			wanPhysicalAddr					PhysAddress,
			wanSubnetMask					IpAddress,
			wanDefaultGateway				IpAddress,
			wanDHCPStatus					INTEGER,
			wanLoginStatus					INTEGER,
			wanLoginUserName				DisplayString,
			wanLoginPassword				DisplayString,
			wanRasPlan						INTEGER,
			wanWorkingMode					INTEGER,
			wanConnectedState				INTEGER,
			wanConnectedIdleTime			INTEGER,
			wanConnectedRedialPeriod		INTEGER
        }

	wanIndex OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  deprecated
        DESCRIPTION
                "An unique value for each WAN connection configuration."
        ::= { wanConnectionEntry 1 }

	wanIfIndex OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  deprecated
        DESCRIPTION
                "The interface on which this entry's equivalence is effective.
                The interface identified by a particular value of this index is
                the same interface as identified by the same value of ifIndex."
        ::= { wanConnectionEntry 2 }

	wanConnectionType OBJECT-TYPE
        SYNTAX	INTEGER {
              		dynamic(1),
              		static(2),
              		pppoe(3),
              		ras(4),
              		pptp(5),
              		hbs(6)                  -- heart-beat-signal
				}
        ACCESS	read-write
        STATUS	mandatory
        DESCRIPTION
                "Indicates the protocol to which adopted by this
                WAN connection."
        ::= { wanConnectionEntry 3 }

	wanNetAddress OBJECT-TYPE
        SYNTAX	IpAddress
        ACCESS	read-write
        STATUS	mandatory
        DESCRIPTION
                "The IP address that this managed node has, when
                seen from the external WAN, or the Internet."
        ::= { wanConnectionEntry 4 }

	wanPhysicalAddr OBJECT-TYPE
        SYNTAX	PhysAddress
        ACCESS	read-write
        STATUS	mandatory
        DESCRIPTION
                "The physical address that this managed node has,
                when seen from the external WAN, or the Internet."
        ::= { wanConnectionEntry 5 }

	wanSubnetMask OBJECT-TYPE
        SYNTAX	IpAddress
        ACCESS	read-write
        STATUS	mandatory
        DESCRIPTION
                "The subnet mask seen by external users on the
                Internet."
        ::= { wanConnectionEntry 6 }

	wanDefaultGateway OBJECT-TYPE
        SYNTAX	IpAddress
        ACCESS	read-write
        STATUS	mandatory
        DESCRIPTION
                "The IP address of remote host to which in respect
                to the forwarding of datagrams received by, but not
                addressed to, this managed node."
        ::= { wanConnectionEntry 7 }

	wanDHCPStatus OBJECT-TYPE
        SYNTAX	INTEGER {
              		release(0),
              		renew(1)
				}
        ACCESS	read-write
        STATUS	mandatory
        DESCRIPTION
                "Indicates to release or renew the IP address of
                this managed node which seen from the external
                WAN, or the Internet."
        ::= { wanConnectionEntry 8 }

	wanLoginStatus OBJECT-TYPE
        SYNTAX	INTEGER {
              		disable(0),
              		pppoe(1),
              		ras(2)
				}
        ACCESS	read-write
        STATUS	mandatory
        DESCRIPTION
                "Specifies to cut the connection to ISP, set to
                disable(0), or to build up a PPPoE or RAS
                connection."
        ::= { wanConnectionEntry 9 }

	wanLoginUserName OBJECT-TYPE
        SYNTAX	DisplayString (SIZE(0..64))
        ACCESS	read-write
        STATUS	mandatory
        DESCRIPTION
                "The authorized user name used to access the ISP."
        ::= { wanConnectionEntry 10 }

	wanLoginPassword OBJECT-TYPE
        SYNTAX	DisplayString (SIZE(0..64))
        ACCESS	read-write
        STATUS	mandatory
        DESCRIPTION
                "The authorized password used to access the ISP."
        ::= { wanConnectionEntry 11 }

	wanRasPlan OBJECT-TYPE
        SYNTAX	INTEGER {
              		ethernet-512k(0),
              		ethernet-256k(1)
              	}
        ACCESS	read-write
        STATUS	mandatory
        DESCRIPTION
                "Specifies the type of Remote Access Service plan
                used to connect with the ISP."
        ::= { wanConnectionEntry 12 }

	wanWorkingMode OBJECT-TYPE
        SYNTAX	INTEGER {
              		gateway(1),             -- enable NAT
              		router(2)               -- disable NAT
              	}
        ACCESS	read-write
        STATUS	mandatory
        DESCRIPTION
                "Specifies the working mode for this managed node.
                Gateway mode should be used if this node is hosting
                local network's connection to the Internet. Router
                mode should be used if this node exists on a
                network with other routers."
        ::= { wanConnectionEntry 13 }

	wanConnectedState OBJECT-TYPE
        SYNTAX	INTEGER {
              		keepAlive(0),
              		onDemand(1)
              	}
        ACCESS	read-write
        STATUS	mandatory
        DESCRIPTION
                "Specifies the state to keepAlive(0) will keep the
                PPPoE-enabled Internet access connected indefinitely,
                even when it sits idle. Otherwise the connection
                to the ISP will be cutted after a preiod of time
                specified in wanConnectedIdleTime object."
        ::= { wanConnectionEntry 14 }

	wanConnectedIdleTime OBJECT-TYPE
        SYNTAX	INTEGER
        ACCESS	read-write
        STATUS	mandatory
        DESCRIPTION
                "Specifies the number of minutes that want to have
                elapsed before Internet access disconnects. A zero
                value indicates to remain the Internet connection
                on at all times."
        ::= { wanConnectionEntry 15 }

	wanConnectedRedialPeriod OBJECT-TYPE
        SYNTAX	INTEGER
        ACCESS	read-write
        STATUS	mandatory
        DESCRIPTION
                "PPPoE retry to dial to ISP, due to ISP equipment bug in HK"
        ::= { wanConnectionEntry 16 }


-- the WAN Dns Network Address Table Group

	wanDnsNetAddressTable OBJECT-TYPE
        SYNTAX	SEQUENCE OF WanDnsNetAddressEntry
        ACCESS	not-accessible
        STATUS	mandatory
        DESCRIPTION
                "Table of DNS Server IP addresses."
        ::= { wanMgt 2 }


	wanDnsNetAddressEntry OBJECT-TYPE
        SYNTAX	WanDnsNetAddressEntry
        ACCESS	not-accessible
        STATUS	mandatory
        DESCRIPTION
                "An entry in the table contains one DNS server IP
                address."
        INDEX	{ wanDnsNetAddressIndex }
        ::= { wanDnsNetAddressTable 1 }

	WanDnsNetAddressEntry ::=
        SEQUENCE {
			wanDnsNetAddressIndex 			INTEGER,
			wanDnsIfIndex					INTEGER,
			wanDnsNetAddress				IpAddress
        }

	wanDnsNetAddressIndex OBJECT-TYPE
        SYNTAX	INTEGER
        ACCESS	read-only
        STATUS	mandatory
        DESCRIPTION
                "An unique value for each DNS server."
        ::= { wanDnsNetAddressEntry 1 }

	wanDnsIfIndex OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  deprecated
        DESCRIPTION
                "The interface on which this entry's equivalence is
                effective. The interface identified by a particular
                value of this index isthe same interface as identified
                by the same value of ifIndex."
        ::= { wanDnsNetAddressEntry 2 }

	wanDnsNetAddress OBJECT-TYPE
        SYNTAX	IpAddress
        ACCESS	read-write
        STATUS	mandatory
        DESCRIPTION
                "Specifies the IP address of DNS server to which
                will translate domain or website names into
                Internet addresses or URLs."
        ::= { wanDnsNetAddressEntry 3 }


-- the VPN Management Group

	vpnIpsecTable OBJECT-TYPE
        SYNTAX	SEQUENCE OF VpnIpsecEntry
        ACCESS	not-accessible
        STATUS	mandatory
        DESCRIPTION
                "Table of VPN Tunnel configuration."
        ::= { vpnMgt 1 }

	vpnIpsecEntry OBJECT-TYPE
        SYNTAX	VpnIpsecEntry
        ACCESS	not-accessible
        STATUS	mandatory
        DESCRIPTION
                "An entry in the table contains configuration
                for each tunnel."
        INDEX	{ vpnTunnelIndex }
        ::= { vpnIpsecTable 1 }

	VpnIpsecEntry ::=
        SEQUENCE {
			vpnTunnelIndex					INTEGER,
			vpnTunnelState					INTEGER,
			vpnTunnelName					DisplayString,
			vpnLocalIdType					INTEGER,
			vpnLocalIp						IpAddress,
			vpnLocalSubnet					IpAddress,
			vpnLocalSubnetMask				IpAddress,
			vpnLocalRangeBeg				IpAddress,
			vpnLocalRangeEnd				IpAddress,
			vpnRemoteIdType					INTEGER,
			vpnRemoteIp						IpAddress,
			vpnRemoteSubnet					IpAddress,
			vpnRemoteSubnetMask				IpAddress,
			vpnRemoteRangeBeg				IpAddress,
			vpnRemoteRangeEnd				IpAddress,
			vpnRemoteSecurityGateway		IpAddress,
			vpnEspEncrypt					INTEGER,
			vpnEspAuth						INTEGER,
			vpnKeyMethod					INTEGER,
			vpnIsakmpPfs					INTEGER,
			vpnIsakmpPreSharedKey			DisplayString,
			vpnManualEncryptKey				DisplayString,
			vpnManualAuthKey				DisplayString,
			vpnManualInboundSpi				DisplayString,
			vpnManualOutboundSpi			DisplayString,
			vpnTunnelStatus					INTEGER
        }

	vpnTunnelIndex OBJECT-TYPE
        SYNTAX	INTEGER
        ACCESS	read-only
        STATUS	mandatory
        DESCRIPTION
                "An unique value for each independent tunnel."
        ::= { vpnIpsecEntry 1 }

	vpnTunnelState OBJECT-TYPE
        SYNTAX	INTEGER { disable(0), enable(1) }
        ACCESS	read-write
        STATUS	mandatory
        DESCRIPTION
                "Status of selected tunnel, disable or enable."
        ::= { vpnIpsecEntry 2 }

	vpnTunnelName OBJECT-TYPE
        SYNTAX	DisplayString (SIZE(0..15))
        ACCESS	read-write
        STATUS	mandatory
        DESCRIPTION
                "Name of selected tunnel."
        ::= { vpnIpsecEntry 3 }

	vpnLocalIdType OBJECT-TYPE
        SYNTAX	INTEGER { ip(0), subnet(1), range(2) }
        ACCESS	read-write
        STATUS	mandatory
        DESCRIPTION
                "Select the local LAN user(s) behind the router
                that can use this VPN tunnel. This may be a single
                IP address, a Sub-network or a range of addresses.
                Notice that the Local Secure Group must match the
                other router's Remote Secure Group."
        ::= { vpnIpsecEntry 4 }

	vpnLocalIp OBJECT-TYPE
        SYNTAX	IpAddress
        ACCESS	read-write
        STATUS	mandatory
        DESCRIPTION
                "The IP address if vpnLocalIdType is ip(0)."
        ::= { vpnIpsecEntry 5 }

	vpnLocalSubnet OBJECT-TYPE
        SYNTAX	IpAddress
        ACCESS	read-write
        STATUS	mandatory
        DESCRIPTION
                "The Sub-network IP if vpnLocalIdType is subnet(1)."
        ::= { vpnIpsecEntry 6 }

	vpnLocalSubnetMask OBJECT-TYPE
        SYNTAX	IpAddress
        ACCESS	read-write
        STATUS	mandatory
        DESCRIPTION
                "The Sub-network mask if vpnLocalIdType is subnet(1)."
        ::= { vpnIpsecEntry 7 }

	vpnLocalRangeBeg OBJECT-TYPE
        SYNTAX	IpAddress
        ACCESS	read-write
        STATUS	mandatory
        DESCRIPTION
                "The start address of IP range if vpnLocalIdType
                is range(2)."
        ::= { vpnIpsecEntry 8 }

	vpnLocalRangeEnd OBJECT-TYPE
        SYNTAX	IpAddress
        ACCESS	read-write
        STATUS	mandatory
        DESCRIPTION
                "The end address of IP range if vpnLocalIdType is
                range(2)."
        ::= { vpnIpsecEntry 9 }

	vpnRemoteIdType OBJECT-TYPE
        SYNTAX	INTEGER { ip(0), subnet(1), range(2) }
        ACCESS	read-write
        STATUS	mandatory
        DESCRIPTION
                "Select the remote LAN user(s) behind the remote
                gateway can use this VPN tunnel. This may be a
                single IP address, a Sub-network, range of addresses
                or any addresses. If [Any] is set, the router acts
                as responder and accepts request from any remote user.
                In this case, the pre-shared key of this tunnel should
                be set as a different string from other tunnels'.
                Notice that Remote Secure Group must match the
                other router's Local Secure Group."
        ::= { vpnIpsecEntry 10 }

	vpnRemoteIp OBJECT-TYPE
        SYNTAX	IpAddress
        ACCESS	read-write
        STATUS	mandatory
        DESCRIPTION
                "The IP address if vpnRemoteIdType is ip(0)."
        ::= { vpnIpsecEntry 11 }

	vpnRemoteSubnet OBJECT-TYPE
        SYNTAX	IpAddress
        ACCESS	read-write
        STATUS	mandatory
        DESCRIPTION
                "The Sub-network IP if vpnRemoteIdType is subnet(1)."
        ::= { vpnIpsecEntry 12 }

	vpnRemoteSubnetMask OBJECT-TYPE
        SYNTAX	IpAddress
        ACCESS	read-write
        STATUS	mandatory
        DESCRIPTION
                "The Sub-network mask if vpnRemoteIdType is subnet(1)."
        ::= { vpnIpsecEntry 13 }

	vpnRemoteRangeBeg OBJECT-TYPE
        SYNTAX	IpAddress
        ACCESS	read-write
        STATUS	mandatory
        DESCRIPTION
                "The start address of IP range if vpnRemoteIdType
                is range(2)."
        ::= { vpnIpsecEntry 14 }

	vpnRemoteRangeEnd OBJECT-TYPE
        SYNTAX	IpAddress
        ACCESS	read-write
        STATUS	mandatory
        DESCRIPTION
                "The end address of IP range if vpnRemoteIdType is
                range(2)."
        ::= { vpnIpsecEntry 15 }

	vpnRemoteSecurityGateway OBJECT-TYPE
        SYNTAX	IpAddress
        ACCESS	read-write
        STATUS	mandatory
        DESCRIPTION
                "The IP address in this field must match the public
                IP address (i.e. WAN IP Address) of the remote gateway
                at the other end of this tunnel. If the remote gateway
                has a dynamic IP address, select [Any] in this field.
                In this case, the pre-shared key of this tunnel should
                be set as a different string from other tunnels'.
                Another type is [FQDN]. It allows you to enter a
                fully-qualified domain name of the remote gateway."
        ::= { vpnIpsecEntry 16 }

	vpnEspEncrypt OBJECT-TYPE
        SYNTAX	INTEGER { disable(0), des(1), des3(2) }
        ACCESS	read-write
        STATUS	mandatory
        DESCRIPTION
                "The Encryption method determines the length of the
                key used to encrypt/decrypt ESP packets. Either DES
                or 3DES may be selected. Notice that both sides must
                use the same Encryption method."
        ::= { vpnIpsecEntry 17 }

	vpnEspAuth OBJECT-TYPE
        SYNTAX	INTEGER { disable(0), md5(1), sha(2) }
        ACCESS	read-write
        STATUS	mandatory
        DESCRIPTION
                "Authentication, determines a method to authenticate
                the ESP packets. Either MD5 or SHA may be selected.
                Notice that both sides must use the same Authentication
                method."
        ::= { vpnIpsecEntry 18 }

	vpnKeyMethod OBJECT-TYPE
        SYNTAX	INTEGER { isakmp(0), manual(1) }
        ACCESS	read-write
        STATUS	mandatory
        DESCRIPTION
                "The router supports both automatic and manual key
                management. When choosing automatic key management,
                IKE(Internet Key Exchange) protocols are used to
                negotiate key material for SA. If manual key management
                is selected, no key negotiation is needed. Basically,
                manual key management is used in small static
                environments or for troubleshooting purpose. Notice
                that both sides must use the same Key Management method."
        ::= { vpnIpsecEntry 19 }

	vpnIsakmpPfs OBJECT-TYPE
        SYNTAX	INTEGER { disable(0), enable(1) }
        ACCESS	read-write
        STATUS	mandatory
        DESCRIPTION
                "If PFS is enabled, IKE Phase 2 negotiation will
                generate a new key material for IP traffic encryption
                and authentication. Note: that both sides must have
                this selected."
        ::= { vpnIpsecEntry 20 }

	vpnIsakmpPreSharedKey OBJECT-TYPE
        SYNTAX	DisplayString (SIZE(0..23))
        ACCESS	read-only
        STATUS	mandatory
        DESCRIPTION
                "IKE uses the Pre-shared Key field to authenticate the
                remote IKE peer. Both character and hexadecimal value
                are acceptable in this field. e.g. [My-@123] or
                [0x4d795f40313233] Note: that both sides must use the
                same Pre-shared Key."
        ::= { vpnIpsecEntry 21 }

	vpnManualEncryptKey OBJECT-TYPE
        SYNTAX	DisplayString (SIZE(0..23))
        ACCESS	read-only
        STATUS	mandatory
        DESCRIPTION
                "This field specifies a key used to encrypt and decrypt
                IP traffic. Both character and hexadecimal value are
                acceptable in this field. Note: that both sides must use
                the same Encryption Key."
        ::= { vpnIpsecEntry 22 }

	vpnManualAuthKey OBJECT-TYPE
        SYNTAX	DisplayString (SIZE(0..19))
        ACCESS	read-only
        STATUS	mandatory
        DESCRIPTION
                "This field specifies a key used to authenticate IP
                traffic.Both character and hexadecimal value are
                acceptable in this field. Note: that both sides must
                use the same Authentication Key."
        ::= { vpnIpsecEntry 23 }

	vpnManualInboundSpi OBJECT-TYPE
        SYNTAX	DisplayString (SIZE(0..9))
        ACCESS	read-write
        STATUS	mandatory
        DESCRIPTION
                "The SPI(Security Parameter Index) is carried in the ESP
                header. This enables the receiver to select the SA, under
                which a packet should be processed. The SPI is a 32-bit
                value. Both decimal and hexadecimal values are acceptable.
                e.g. [987654321] or [0x3ade68b1]. Each tunnel must have
                unique an Inbound SPI and Outbound SPI. No two tunnels
                share the same SPI. Notice that Inbound SPI must match
                the other router's Outbound SPI, and vice versa."
        ::= { vpnIpsecEntry 24 }

	vpnManualOutboundSpi OBJECT-TYPE
        SYNTAX	DisplayString (SIZE(0..9))
        ACCESS	read-write
        STATUS	mandatory
        DESCRIPTION
                "The SPI(Security Parameter Index) is carried in the ESP
                header. This enables the receiver to select the SA, under
                which a packet should be processed. The SPI is a 32-bit
                value. Both decimal and hexadecimal values are acceptable.
                e.g. [987654321] or [0x3ade68b1]. Each tunnel must have
                unique an Inbound SPI and Outbound SPI. No two tunnels
                share the same SPI. Notice that Inbound SPI must match
                the other router's Outbound SPI, and vice versa."
        ::= { vpnIpsecEntry 25 }


	vpnTunnelStatus OBJECT-TYPE
        SYNTAX	INTEGER { connected(0), disconnected(1) }
        ACCESS	read-write
        STATUS	mandatory
        DESCRIPTION
                "Indicates the connection status of the selected tunnel.
                The state is either connected(0) or disconnected(1)."
        ::= { vpnIpsecEntry 26 }


-- the Firewall Management Group

	fwProtection OBJECT-TYPE
        SYNTAX	INTEGER {
              		disable(0),
              		enable(1)
              	}
        ACCESS	read-write
        STATUS	mandatory
        DESCRIPTION
                "Set to disable or enable the firewall function
                utilized on this managed node."
        ::= { firewallMgt 1 }


-- the Wireless Common Group

	stationMacFilter OBJECT-TYPE
		SYNTAX	INTEGER {
					disable(0),
					enable(1)
				}
		ACCESS	read-write
		STATUS	mandatory
		DESCRIPTION
				"Set to disable(0) or enable(1) the wireless
				station physical address filter."
		::= { wirelessCommon 1 }
	
	apClientModeEnable OBJECT-TYPE
		SYNTAX	INTEGER {			   
					disable (0),
					enable (1)
				} 
		ACCESS	read-write
		STATUS	mandatory
		DESCRIPTION
				"set/get enable or disable AP client mode"
		::= { wirelessCommon 2 }
	    
	apClientMacNum OBJECT-TYPE
		SYNTAX	INTEGER (1..20)
		ACCESS	read-write
		STATUS	mandatory
		DESCRIPTION
				"set/get the numbers of AP Client MAC address list"
		::= { wirelessCommon 3 }
	    
	apClientMacTable OBJECT-TYPE
		SYNTAX	SEQUENCE OF ApClientMacEntry
		ACCESS	not-accessible
		STATUS	mandatory
		DESCRIPTION
				"set/get the MAC address list of AP Client"
		::= { wirelessCommon 4 }

	apClientMacEntry OBJECT-TYPE
		SYNTAX  ApClientMacEntry
		ACCESS  not-accessible
		STATUS  mandatory
		DESCRIPTION
				"A MAC address table for AP client mode."
		INDEX  { apClientMacIndex }
		::= { apClientMacTable 1 }
	
	ApClientMacEntry ::=
		SEQUENCE {
			apClientMacIndex      INTEGER,
			apClientMacAddress    PhysAddress,
		}                               
	                                    
	apClientMacIndex OBJECT-TYPE        
		SYNTAX	INTEGER                 
		ACCESS	read-only               
		STATUS	mandatory               
		DESCRIPTION                     
				"A index value for each MAC address. "
		::= { apClientMacEntry 1 }
	
	apClientMacAddress OBJECT-TYPE
		SYNTAX	PhysAddress
		ACCESS	read-write
		STATUS	mandatory
		DESCRIPTION
				"The MAC address."
		::= { apClientMacEntry 2 }    

	apBridgeModeEnable OBJECT-TYPE
		SYNTAX	INTEGER {			   
					disable (0),
					enable (1)
				} 
		ACCESS	read-write
		STATUS	mandatory
		DESCRIPTION
				"set/get enable or disable  Bridge mode"
		::= { wirelessCommon 5 }
	    
	apBridgeMacNum OBJECT-TYPE
		SYNTAX	INTEGER (1..20)
		ACCESS	read-write
		STATUS	mandatory
		DESCRIPTION
				"set/get the numbers of Bridge MAC address list"
		::= { wirelessCommon 6 }
	    
	apBridgeMacTable OBJECT-TYPE
		SYNTAX	SEQUENCE OF ApBridgeMacEntry
		ACCESS	not-accessible
		STATUS	mandatory
		DESCRIPTION
				"set/get the MAC address list of  Bridge"
		::= { wirelessCommon 7 }

	apBridgeMacEntry OBJECT-TYPE
		SYNTAX	ApBridgeMacEntry
		ACCESS	not-accessible
		STATUS	mandatory
		DESCRIPTION
				"A MAC address table for AP Bridge mode."
		INDEX  { apBridgeMacIndex }
		::= { apBridgeMacTable 1 }
	
	ApBridgeMacEntry ::=
		SEQUENCE {
			apBridgeMacIndex      INTEGER,
			apBridgeMacAddress    PhysAddress,
		}
	
	apBridgeMacIndex OBJECT-TYPE
		SYNTAX	INTEGER
		ACCESS	read-only
		STATUS	mandatory
		DESCRIPTION
				"A index value for each MAC address. "
		::= { apBridgeMacEntry 1 }
	
	apBridgeMacAddress OBJECT-TYPE
		SYNTAX	PhysAddress
		ACCESS	read-write
		STATUS	mandatory
		DESCRIPTION
				"The MAC address."
		::= { apBridgeMacEntry 2 }    

	apRepeatorModeEnable OBJECT-TYPE
		SYNTAX	INTEGER {			   
					disable (0),
					enable (1)
				} 
		ACCESS	read-write
		STATUS	mandatory
		DESCRIPTION
				"set/get enable or disable repeater mode"
		::= { wirelessCommon 8 }
	    
	apRepeatorMacNum OBJECT-TYPE
		SYNTAX	INTEGER (1..20)
		ACCESS	read-write
		STATUS	mandatory
		DESCRIPTION
				"set/get the numbers of repeater MAC address list"
		::= { wirelessCommon 9 }
	    
	apRepeatorMacTable OBJECT-TYPE
		SYNTAX	SEQUENCE OF ApRepeatorMacEntry
		ACCESS	not-accessible
		STATUS	mandatory
		DESCRIPTION
				"set/get the MAC address list of repeater"
		::= { wirelessCommon 10 }

	apRepeatorMacEntry OBJECT-TYPE
		SYNTAX	ApRepeatorMacEntry
		ACCESS	not-accessible
		STATUS	mandatory
		DESCRIPTION
				"A MAC address table for AP Repeator mode."
		INDEX  { apRepeatorMacIndex }
		::= { apRepeatorMacTable 1 }
	
	ApRepeatorMacEntry ::=
		SEQUENCE {
			apRepeatorMacIndex      INTEGER,
			apRepeatorMacAddress    PhysAddress,
		}
	
	apRepeatorMacIndex OBJECT-TYPE
		SYNTAX	INTEGER
		ACCESS	read-only
		STATUS	mandatory
		DESCRIPTION
				"A index value for each MAC address. "
		::= { apRepeatorMacEntry 1 }
	
	apRepeatorMacAddress OBJECT-TYPE
		SYNTAX	PhysAddress
		ACCESS	read-write
		STATUS	mandatory
		DESCRIPTION
				"The MAC address."
		::= { apRepeatorMacEntry 2 }    


-- the Wireless 802.11b Group
	ieee80211bBroadcastSSID OBJECT-TYPE
        SYNTAX	INTEGER {
              		disable(0),
              		enable(1)
              	}
        ACCESS	read-write
        STATUS	mandatory
        DESCRIPTION
				"The attribute is only valid for Access Point and the 
				master of IBSS.	When the attribute is enable, the SSID 
				field in beacon frames is blank, also the device will 
				not response the Probe Request with unspecified SSID."
        ::= { ieee80211b 1 }

	ieee80211bSSIDString OBJECT-TYPE
        SYNTAX	DisplayString (SIZE(0..32))
        ACCESS	read-write
        STATUS	mandatory
        DESCRIPTION
				"When in read access, this attribute reflects the Service 
				Set ID of the current wireless connection. When in write 
				access, it is the desired Service Set ID."
        ::= { ieee80211b 2 }

	ieee80211bChannel OBJECT-TYPE
        SYNTAX	INTEGER (1..14)
        ACCESS	read-write
        STATUS	mandatory
        DESCRIPTION
				"When in read access, this attribute reflects the channel 
				number of the current wireless connection. When in write 
				access, it is the desired channel to connect."
        ::= { ieee80211b 3 }

	ieee80211bWep OBJECT-TYPE
        SYNTAX	INTEGER {
              		disable(0),
              		enable(1)
              	}
        ACCESS	read-write
        STATUS	mandatory
        DESCRIPTION
				"Specify the WEP status of device. If the attribute is 
				set as enable, the WEP mechanism is used for transmitting 
				data frames."
        ::= { ieee80211b 4 }

	ieee80211bWepAuthMethod  OBJECT-TYPE
        SYNTAX	INTEGER {
              		both(0),
              		open-key(1),
              		share-key(2)
              		}
        ACCESS	read-write
        STATUS	mandatory
        DESCRIPTION
                "Specify the authentication algorithms supported by the 
                station or AP."
        ::= { ieee80211b 5 }

	ieee80211bWepBits OBJECT-TYPE
        SYNTAX	INTEGER {
              		wep64bits(0),
              		wep128bits(1)
              	}
        ACCESS	read-write
        STATUS	mandatory
        DESCRIPTION
				"When WEP is enabled, this attribute specifies whether 
				64-bit or 128-bit encryption/decryption algorithm is used."
        ::= { ieee80211b 6 }

	ieee80211bDefaultKey  OBJECT-TYPE
        SYNTAX	INTEGER (1..4)
        ACCESS	read-write
        STATUS	mandatory
        DESCRIPTION
                "The index of default WEP encryption key for transmission. 
                It can be 1 to 4."
        ::= { ieee80211b 7 }

	ieee80211bWep64bitkey1 OBJECT-TYPE
        SYNTAX	OCTET STRING (SIZE(0..10))
        ACCESS	read-write
        STATUS	mandatory
        DESCRIPTION
				"The WEP key #1 value for 64-bit WEP encryption. It's HEX 
				value in ASCII format. For example: WEP key: 0x12 0x34 
				0x56 0x78 0x90 is specified as '1234567890'."
        ::= { ieee80211b 8 }

	ieee80211bWep64bitkey2 OBJECT-TYPE
        SYNTAX	OCTET STRING (SIZE(0..10))
        ACCESS	read-write
        STATUS	mandatory
        DESCRIPTION
				"The WEP key #2 value for 64-bit WEP encryption. It's HEX 
				value in ASCII format. For example: WEP key: 0x12 0x34 
				0x56 0x78 0x90 is specified as '1234567890'."
        ::= { ieee80211b 9 }

	ieee80211bWep64bitkey3 OBJECT-TYPE
        SYNTAX	OCTET STRING (SIZE(0..10))
        ACCESS	read-write
        STATUS	mandatory
        DESCRIPTION
				"The WEP key #3 value for 64-bit WEP encryption. It's HEX 
				value in ASCII format. For example: WEP key: 0x12 0x34 
				0x56 0x78 0x90 is specified as '1234567890'."
        ::= { ieee80211b 10 }

	ieee80211bWep64bitkey4 OBJECT-TYPE
        SYNTAX	OCTET STRING (SIZE(0..10))
        ACCESS	read-write
        STATUS	mandatory
        DESCRIPTION
				"The WEP key #4 value for 64-bit WEP encryption. It's HEX 
				value in ASCII format. For example: WEP key: 0x12 0x34 
				0x56 0x78 0x90 is specified as '1234567890'."
        ::= { ieee80211b 11 }

	ieee80211bWep128bitkey1 OBJECT-TYPE
        SYNTAX	OCTET STRING (SIZE(0..26))
        ACCESS	read-write
        STATUS	mandatory
        DESCRIPTION
				"The WEP key #1 value for 128-bit WEP encryption. It's HEX 
				value in ASCII format. For example: WEP key: 0x12 0x34 
				0x56 0x78 0x90 is specified as '1234567890'."
        ::= { ieee80211b 12 }

	ieee80211bWep128bitkey2 OBJECT-TYPE
        SYNTAX	OCTET STRING (SIZE(0..26))
        ACCESS	read-write
        STATUS	mandatory
        DESCRIPTION
				"The WEP key #2 value for 128-bit WEP encryption. It's HEX 
				value in ASCII format. For example: WEP key: 0x12 0x34 
				0x56 0x78 0x90 is specified as '1234567890'."
        ::= { ieee80211b 13 }

	ieee80211bWep128bitkey3 OBJECT-TYPE
        SYNTAX	OCTET STRING (SIZE(0..26))
        ACCESS	read-write
        STATUS	mandatory
        DESCRIPTION
				"The WEP key #3 value for 128-bit WEP encryption. It's HEX 
				value in ASCII format. For example: WEP key: 0x12 0x34 
				0x56 0x78 0x90 is specified as '1234567890'."
        ::= { ieee80211b 14 }

	ieee80211bWep128bitkey4 OBJECT-TYPE
        SYNTAX	OCTET STRING (SIZE(0..26))
        ACCESS	read-write
        STATUS	mandatory
        DESCRIPTION
                "The WEP key #4 value for 128-bit WEP encryption. It's HEX 
                value in ASCII format. For example: WEP key: 0x12 0x34 
                0x56 0x78 0x90 is specified as '1234567890'."
        ::= { ieee80211b 15 }


	ieee80211bBeaconInterval OBJECT-TYPE
        SYNTAX	INTEGER (0..65535)
        ACCESS	read-write
        STATUS	mandatory
        DESCRIPTION
                "This value specifies the beacon interval duration in 
                miliseconds."
        ::= { ieee80211b 16 }

	ieee80211bRTSThreshold OBJECT-TYPE
        SYNTAX	INTEGER (0..2347)
        ACCESS	read-write
        STATUS	mandatory
        DESCRIPTION
                "This attribute shall indicate the number of octets in an 
                MPDU, below which an RTS/CTS handshake shall not be 
                performed at the beginning of any frame exchange sequence 
                where the MPDU is of type Data or Management, the MPDU has 
                an individual address in the address1 field, and the length 
                of the MPDU is greater than this threshold. Setting this 
                attribute to be larger than the maximum MSDU size shall 
                have the effect of turnning off the RTS/CTS	handshake for 
                frames of Data and Management type transmitted by this 
                device.	Setting this attribute to zero shall have the 
                effect of turnning on the RTS/CTS handshake for all frames 
                of Data and Management type transmitted by the device."
        ::= { ieee80211b 17 }

	ieee80211bFragmentThreshold OBJECT-TYPE
        SYNTAX	INTEGER (256..2346)
        ACCESS	read-write
        STATUS	mandatory
        DESCRIPTION
				"This attribute shall specify the current maximum size, in 
				octets, of the MPDU that may be delivered to PHY. An MSDU 
				shall be broken into fragments if its size exceeds the value 
				of this attribute after adding MAC headers and trailers. An 
				MSDU or MMPDU shall be fragmented when the resulting frame
				has an individual address in Address1 field, and the length 
				of frame is larger than this threshold."
        ::= { ieee80211b 18 }

	ieee80211bDTIMInterval OBJECT-TYPE
        SYNTAX	INTEGER (0..255)
        ACCESS	read-write
        STATUS	mandatory
        DESCRIPTION
				"Specify the number of beacon intervals that shall elapse 
				between transmission of Beacon frames containing a TIM 
				element whose DTIM Count field is 0. This value is 
				transmitted in the DTIM Period field of Beacon frames."
        ::= { ieee80211b 19 }

	ieee80211bBasicRate    OBJECT-TYPE
        SYNTAX	INTEGER (1..15)
        ACCESS	read-write
        STATUS	mandatory
        DESCRIPTION
				"The value is a bit-map of basic data rates. It specifies 
				the basic rates used and reported for this BSS by the AP. 
				The highest rate specified is the rate that the AP uses 
				when transmitting broadcast/multicast and management 
				frames. Bit0 = 1Mbps, Bit1 = 2Mbps, Bit2 = 5.5Mbps, and
				Bit3 = 11Mbps. The basic data rates also specifies the 
				rates that must be supported by all stations to join this 
				BSS."
        ::= { ieee80211b 20 }

	ieee80211bTXRate OBJECT-TYPE
        SYNTAX	INTEGER {
					rate-1Mbps(1),
					rate-2Mbps(2),
					rate-5dot5Mbps(3),
					rate-11Mbps(4),
					auto-fallback(5)
				}
        ACCESS	read-write
        STATUS	mandatory
        DESCRIPTION
				"The default transmission rate of the staion or access 
				point. When set as auto-fallback, the tx rate auto-fallback 
				between 11, 5.5, 2, and 1Mbps."
        ::= { ieee80211b 21 }

	ieee80211bPreambleType OBJECT-TYPE
        SYNTAX	INTEGER {
              		longPreamble(0),
              		shortPreamble(1)
              	}
        ACCESS	read-write
        STATUS	mandatory
        DESCRIPTION
				"For wireless stations, this attribute specifies whether 
				frames are transmitted with the short or long preamble. 
				For access points, when set to shortPreamble, it force 
				the AP to disallow associations from stations that do not 
				support short preamble. In longPreamble mode, it allow 
				all stations to associate, which carries the risk that 
				legacy systems may associate with the BSS and then 
				proceed to interfere with the short preamble packets."
        ::= { ieee80211b 22 }

	ieee80211bRadioFunction OBJECT-TYPE
        SYNTAX	INTEGER {
              		disable(0),
              		enable(1)
              	}
        ACCESS	read-write
        STATUS	mandatory
        DESCRIPTION
				"Enable/Disable the RF radio function. When disable, no RF 
				signal will be generated on the air, also no RF signal 
				will be received. But the MAC function of the wireless 
				interface is still working. When enable, the interface is 
				working normally."
        ::= { ieee80211b 23 }

	ieee80211bDeviceFunction OBJECT-TYPE
        SYNTAX	INTEGER {
              		disable(0),
              		enable(1)
              	}
        ACCESS	read-write
        STATUS	mandatory
        DESCRIPTION
				"Enable/Disable the function of the device. When disable, 
				not only the RF radio is turned off, but also the MAC 
				function of wireless interface is also turned off. When 
				enable, the interface is working normally."
        ::= { ieee80211b 24 }

	ieee80211bDomain OBJECT-TYPE
        SYNTAX	INTEGER {
              		usa-canada(1),
              		most-of-europe(2),
              		spain(3),
              		france(4),
              		japan(5),
              		worldwide(6)
              	}
        ACCESS	read-only
        STATUS	mandatory
        DESCRIPTION
				"The attribute describe the regulatory domain the PLCP 
				and PMD support in this wireless interface."
        ::= { ieee80211b 25 }

	ieee80211bSignalStrength OBJECT-TYPE
        SYNTAX	INTEGER (0..100)
        ACCESS	read-only
        STATUS	mandatory
        DESCRIPTION
				"The signal strength of the current wireless connection. 
				The unit is percentage. It's only valid for wireless 
				station in infrastructure mode. When the link is 
				disconnected, the value should be 0."
        ::= { ieee80211b 26 }

	ieee80211bOperationMode OBJECT-TYPE
        SYNTAX	INTEGER {
              		adhoc(0),
              		infrastructure(1)
              	}
        ACCESS	read-write
        STATUS	mandatory
        DESCRIPTION
				"Specify the type of BSS the station shall use when 
				scanning for a BSS with which to connect. When set to 
				infrastructure, the station shall only connect to an 
				Access Point. When set to adhoc, the station shall only
		 connect to an IBSS network."
        ::= { ieee80211b 27 }

	ieee80211bPassPhrase OBJECT-TYPE
        SYNTAX          DisplayString (SIZE(0..30))
        ACCESS          read-write
        STATUS          mandatory
        DESCRIPTION
				"The ASCII string used to generate the actual 4 WEP 
				keys. The length of the attribute can be 0 to 30. 
				The algorithm of the WEP key generation is based on 
				the algorithm proposed by Intersil. The algorithm
				to generate 64-bit WEP key and 128-bit WEP key are 
				different. When in 64-bit mode, it uses Intersil's 
				proprietary algorithm to generate 4 different WEP
				keys. When in 128-bit mode, it uses MD5 to generate 
				4 WEP keys with identical key value."
        ::= { ieee80211b 28 }

	ieee80211bLinkQuality OBJECT-TYPE
        SYNTAX	INTEGER (0..100)
        ACCESS	read-only
        STATUS	mandatory
        DESCRIPTION
				"The link quality of the current wireless connection. 
				The unit is percentage. If the link is disconnected, 
				the value should be 0."
        ::= { ieee80211b 29 }


-- the Wireless 802.11a Group
	ieee80211aBroadcastSSID OBJECT-TYPE
        SYNTAX	INTEGER {
              		disable(0),
              		enable(1)
              	}
        ACCESS	read-write
        STATUS	mandatory
        DESCRIPTION
                "set/get enable or disable broadcast SSID"
        ::= { ieee80211a 1 }

	ieee80211aSSIDString OBJECT-TYPE
        SYNTAX	DisplayString (SIZE(0..32))
        ACCESS	read-write
        STATUS	mandatory
        DESCRIPTION
                "set/get SSID String"
        ::= { ieee80211a 2 }

	ieee80211aChannel OBJECT-TYPE
        SYNTAX	INTEGER {
              		channel36(1),
              		channel40(2),
              		channel44(3),
              		channel48(4),
              		channel52(5),
              		channel56(6),
              		channel60(7),
              		channel64(8),
              		channel42(9),
              		channel50(10),
              		channel58(11)
              	}
        ACCESS	read-write
        STATUS	mandatory
        DESCRIPTION
                "set/get Current Channel, 42/50/58 channel is for turbo mode"
        ::= { ieee80211a 3 }

	ieee80211aWep OBJECT-TYPE
        SYNTAX	INTEGER {
              		disable(0),
              		enable(1)
              	}
        ACCESS	read-write
        STATUS	mandatory
        DESCRIPTION
                "set/get enable or disable WEP encryption"
        ::= { ieee80211a 4 }

	ieee80211aWepauthmethod  OBJECT-TYPE
        SYNTAX	INTEGER {
              		both(0),
              		open-key(1),
              		share-key(2)
              	}
        ACCESS	read-write
        STATUS	mandatory
        DESCRIPTION
                "set/get Authentication method"
        ::= { ieee80211a 5 }

	ieee80211aDefaultKey  OBJECT-TYPE
        SYNTAX	INTEGER (1..4)
        ACCESS	read-write
        STATUS	mandatory
        DESCRIPTION
                "set/get the default WEP KEY ID"
        ::= { ieee80211a 6 }

	ieee80211aWepbits OBJECT-TYPE
        SYNTAX	INTEGER {
              		wep64bits(0),
              		wep128bits(1),
              		wep152bits(2)
              	}
        ACCESS	read-write
        STATUS	mandatory
        DESCRIPTION
                "set/get WEP encryption bit length"
        ::= { ieee80211a 7 }

	ieee80211aWep64bitkey1 OBJECT-TYPE
        SYNTAX	DisplayString (SIZE(0..10))
        ACCESS	read-write
        STATUS	mandatory
        DESCRIPTION
                "set/get 64bit key 1"
        ::= { ieee80211a 8 }

	ieee80211aWep64bitkey2 OBJECT-TYPE
        SYNTAX	DisplayString (SIZE(0..10))
        ACCESS	read-write
        STATUS	mandatory
        DESCRIPTION
                "set/get 64bit key 2"
        ::= { ieee80211a 9 }

	ieee80211aWep64bitkey3 OBJECT-TYPE
        SYNTAX	DisplayString (SIZE(0..10))
        ACCESS	read-write
        STATUS	mandatory
        DESCRIPTION
                "set/get 64bit key 3"
        ::= { ieee80211a 10 }

	ieee80211aWep64bitkey4 OBJECT-TYPE
        SYNTAX	DisplayString (SIZE(0..10))
        ACCESS	read-write
        STATUS	mandatory
        DESCRIPTION
                "set/get 64bit key 4"
        ::= { ieee80211a 11 }

	ieee80211aWep128bitkey1 OBJECT-TYPE
        SYNTAX	DisplayString (SIZE(0..26))
        ACCESS	read-write
        STATUS	mandatory
        DESCRIPTION
                "set/get 128 bit key 1"
        ::= { ieee80211a 12 }

	ieee80211aWep128bitkey2 OBJECT-TYPE
        SYNTAX	DisplayString (SIZE(0..26))
        ACCESS	read-write
        STATUS	mandatory
        DESCRIPTION
                "set/get 128 bit key 2"
        ::= { ieee80211a 13 }

	ieee80211aWep128bitkey3 OBJECT-TYPE
        SYNTAX	DisplayString (SIZE(0..26))
        ACCESS	read-write
        STATUS	mandatory
        DESCRIPTION
                "set/get 128 bit key 3"
        ::= { ieee80211a 14 }

	ieee80211aWep128bitkey4 OBJECT-TYPE
        SYNTAX	DisplayString (SIZE(0..26))
        ACCESS	read-write
        STATUS	mandatory
        DESCRIPTION
                "set/get 128 bit key 4"
        ::= { ieee80211a 15 }

	ieee80211aWep152bitkey1 OBJECT-TYPE
        SYNTAX	DisplayString (SIZE(0..32))
        ACCESS	read-write
        STATUS	mandatory
        DESCRIPTION
                "set/get 152 bit key 1"
        ::= { ieee80211a 16 }

	ieee80211aWep152bitkey2 OBJECT-TYPE
        SYNTAX	DisplayString (SIZE(0..32))
        ACCESS	read-write
        STATUS	mandatory
        DESCRIPTION
                "set/get 152 bit key 2"
        ::= { ieee80211a 17 }

	ieee80211aWep152bitkey3 OBJECT-TYPE
        SYNTAX	DisplayString (SIZE(0..32))
        ACCESS	read-write
        STATUS	mandatory
        DESCRIPTION
                "set/get 152 bit key 3"
        ::= { ieee80211a 18 }

	ieee80211aWep152bitkey4 OBJECT-TYPE
        SYNTAX	DisplayString (SIZE(0..32))
        ACCESS	read-write
        STATUS	mandatory
        DESCRIPTION
                "set/get 152 bit key 4"
        ::= { ieee80211a 19 }

	ieee80211aBeaconInterval OBJECT-TYPE
        SYNTAX	INTEGER (0..65535)
        ACCESS	read-write
        STATUS	mandatory
        DESCRIPTION
                "set/get Beacon Interval"
        ::= { ieee80211a 20 }

	ieee80211aRTSThreshold OBJECT-TYPE
        SYNTAX	INTEGER (0..2432)
        ACCESS	read-write
        STATUS	mandatory
        DESCRIPTION
                "set/get RTS Threshold"
        ::= { ieee80211a 21 }

	ieee80211aFragmentThreshold OBJECT-TYPE
        SYNTAX	INTEGER (0..2346)
        ACCESS	read-write
        STATUS	mandatory
        DESCRIPTION
                "set/get Fragmentation Threshold"
        ::= { ieee80211a 22 }

	ieee80211aDTIMInterval OBJECT-TYPE
        SYNTAX	INTEGER (0..255)
        ACCESS	read-write
        STATUS	mandatory
        DESCRIPTION
                "set/get DTIM Interval"
        ::= { ieee80211a 23 }

	ieee80211aBasicRate OBJECT-TYPE
        SYNTAX	INTEGER {
              		rate6mbps(0)
              	}
        ACCESS	read-write
        STATUS	mandatory
        DESCRIPTION
                "set/get Basic rate"
        ::= { ieee80211a 24 }

	ieee80211aTXRate OBJECT-TYPE
        SYNTAX	INTEGER {
              		rate6Mbps(0),
              		rate9Mbps(1),
              		rate12Mbps(2),
              		rate18Mbps(3),
              		rate24Mbps(4),
              		rate36Mbps(5),
              		rate48Mbps(6),
              		rate54Mbps(7),
              		bestRate(8)
              	}
        ACCESS	read-write
        STATUS	mandatory
        DESCRIPTION
                "set/get Transmit rate"
        ::= { ieee80211a 25 }

	ieee80211aTurboMode OBJECT-TYPE
        SYNTAX	INTEGER {
					disable(0),
					enable(1)
				}
        MAX-ACCESS read-write
        STATUS	current
        DESCRIPTION
				"set/get enable or disable turbo mode"
		::= { ieee80211a 26 }

	ieee80211aPhyOFDMEnable OBJECT-TYPE
        SYNTAX	INTEGER {
					disable(0),
					enable(1)
				}
        MAX-ACCESS read-write
        STATUS	current
        DESCRIPTION
				"set/get enable or disable OFDM modulation"
		::= { ieee80211a 27 }

	ieee80211aPhyOFDMAutoChannelSelect OBJECT-TYPE
        SYNTAX	INTEGER {
					disable(0),
					enable(1)
				}
        MAX-ACCESS read-write
        STATUS	current
        DESCRIPTION
			"set/get enable or disable auto find the channel with less 
			interference "
		::= { ieee80211a 28 }

	ieee80211aRadioFunction OBJECT-TYPE
        SYNTAX	INTEGER {
              		disable(0),
              		enable(1)
              	}
        ACCESS	read-write
        STATUS	mandatory
        DESCRIPTION
                "set/get enable or disable radio function"
        ::= { ieee80211a 29 }

	ieee80211aDeviceFunction OBJECT-TYPE
        SYNTAX	INTEGER {
              		disable(0),
              		enable(1)
              	}
        ACCESS	read-write
        STATUS	mandatory
        DESCRIPTION
                "set/get enable or disable device"
        ::= { ieee80211a 30 }

	ieee80211aDomain OBJECT-TYPE
        SYNTAX	INTEGER {
              		usa-canada(1),
              		most-of-europe(2),
              		spain(3),
              		france(4),
              		japan(5),
              		worldwide(6)
              	}
        ACCESS	read-only
        STATUS	mandatory
        DESCRIPTION
                "Get regular domain"
        ::= { ieee80211a 31 }

	ieee80211aSignalStrength OBJECT-TYPE
        SYNTAX	INTEGER
        ACCESS	read-only
        STATUS	mandatory
        DESCRIPTION
                "Get signal strength (for NIC)"
        ::= { ieee80211a 32 }

	ieee80211aOperationMode OBJECT-TYPE
        SYNTAX	INTEGER {
              		adhoc(0),
              		infrastructure(1)
              	}
        ACCESS	read-write
        STATUS	mandatory
        DESCRIPTION
                "set/get The operation mode of this NIC."
        ::= { ieee80211a 33 }

	ieee80211aLinkQuality OBJECT-TYPE
        SYNTAX	INTEGER
        ACCESS	read-only
        STATUS	mandatory
        DESCRIPTION
                "Get the link quality of this NIC."
        ::= { ieee80211a 34 }


-- the DSL group

        -- the remote Node group
        -- When user want to creat one remote entry who should create the
        -- entry from remoteNodeTable first and then setting the relative
        -- information at remoteNodeIPBridgeTable, remoteNodeATMTable and
        -- remoteNodeFilterSetTable.  After that the user can then set up
        -- this object by setting it to active. At the mean time the snmp
        -- agent will do the relationship check, the status will be active
        -- if sucdessful, otherwise the status will be deactive and the
        -- error status will shows at remoteNodeErrString.

        -- adslRemoteNode OBJECT-TYPE
        remoteNodeNumber OBJECT-TYPE
                SYNTAX  INTEGER
                ACCESS  read-only
                STATUS  mandatory
                DESCRIPTION
                        "The number of network interfaces (regardless of
                        their current state) present on this system."
                ::= { adslRemoteNode 1 }

        remoteNodeErrString OBJECT-TYPE
                SYNTAX  DisplayString
                ACCESS  read-only
                STATUS  mandatory
                DESCRIPTION
                        "The error status of saving one remote node settings.
                        The string will clear once it is accessed from the
                        SNMP server."
                ::= { adslRemoteNode 2 }

        remoteNodeStatusTable OBJECT-TYPE
                SYNTAX  SEQUENCE OF RemoteNodeStatusEntry
                ACCESS  not-accessible
                STATUS  mandatory
                DESCRIPTION
                        "A list of remote node status entries."
                ::= { adslRemoteNode 3 }

        remoteNodeStatusEntry OBJECT-TYPE
                SYNTAX  RemoteNodeStatusEntry
                ACCESS  not-accessible
                STATUS  mandatory
                DESCRIPTION
                "An remote node status entry containing comment object
                 for a remote node status."
                INDEX   { remoteNodeStatusIndex }
                ::= { remoteNodeStatusTable 1 }

        RemoteNodeStatusEntry ::=
                SEQUENCE {
                        remoteNodeStatusIndex
                                INTEGER,
                                remoteNodeStatusIfIndex
                                                INTEGER,
                        remoteNodeStatus
                                INTEGER,
                        remoteNodeISPnode
                                INTEGER
                }

        remoteNodeStatusIndex OBJECT-TYPE
                SYNTAX  INTEGER
                ACCESS  read-only
                STATUS  mandatory
                DESCRIPTION
                        "The index of remote node status entry."
                ::= { remoteNodeStatusEntry 1 }

		remoteNodeStatusIfIndex OBJECT-TYPE
		        SYNTAX  INTEGER
		        ACCESS  read-only
		        STATUS  deprecated
		        DESCRIPTION
		        		"The interface on which this entry's equivalence is effective.
						The interface identified by a particular value of this index is
						the same interface as identified by the same value of ifIndex."
		        ::= { remoteNodeStatusEntry 2 }

        remoteNodeStatus OBJECT-TYPE
                SYNTAX  INTEGER {
                        other(1),          -- none of the following
                        active(2),          -- active one remote node entry.
                        deactive(3),        -- deactive one remote node entry.
                        delete(4)            -- delete one remote node entry.
                }
                ACCESS  read-write
                STATUS  mandatory
                DESCRIPTION
                "This object allows you to activate/deactivate/delete this remote node."
                ::= { remoteNodeStatusEntry 3 }

        remoteNodeISPnode OBJECT-TYPE
                SYNTAX  INTEGER {
                        no(0),
                        yes(1)
                }
                ACCESS  read-write
                STATUS  mandatory
                DESCRIPTION
                        "The object allows you to set the remote node to ISP node."
                ::= { remoteNodeStatusEntry 4 }

        remoteNodeGeneralTable OBJECT-TYPE
                SYNTAX  SEQUENCE OF RemoteNodeGeneralEntry
                ACCESS  not-accessible
                STATUS  mandatory
                DESCRIPTION
                        "A list of remote node general entries."
                ::= { adslRemoteNode 4 }

        remoteNodeGeneralEntry OBJECT-TYPE
                SYNTAX  RemoteNodeGeneralEntry
                ACCESS  not-accessible
                STATUS  mandatory
                DESCRIPTION
                "An remote node general entry containing comment object for a
                remote node general information."
                INDEX   { remoteNodeGeneralIndex }
                ::= { remoteNodeGeneralTable 1 }

        RemoteNodeGeneralEntry ::=
                SEQUENCE {
                        remoteNodeGeneralIndex
                                INTEGER,
                                remoteNodeGeneralIfIndex
                                                INTEGER,
                        remoteNodeName
                                DisplayString,
                        remoteNodeEncap
                                INTEGER,
                        remoteNodeMultiplex
                                INTEGER,
                        remoteNodeServiceName
                                DisplayString,
                        remoteNodeAuthen
                                INTEGER,
                        remoteNodeRoute
                                INTEGER,
                        remoteNodeBridge
                                INTEGER
                }

        remoteNodeGeneralIndex OBJECT-TYPE
                SYNTAX  INTEGER
                ACCESS  read-only
                STATUS  mandatory
                DESCRIPTION
                        "The index of remote node general entry."
                ::= { remoteNodeGeneralEntry 1 }

		remoteNodeGeneralIfIndex OBJECT-TYPE
		        SYNTAX  INTEGER
		        ACCESS  read-only
		        STATUS  deprecated
		        DESCRIPTION
		        		"The interface on which this entry's equivalence is effective.
						The interface identified by a particular value of this index is
						the same interface as identified by the same value of ifIndex."
		        ::= { remoteNodeGeneralEntry 2 }

        remoteNodeName OBJECT-TYPE
                SYNTAX  DisplayString (SIZE (0..10))
                ACCESS  read-write
                STATUS  mandatory
                DESCRIPTION
                        "The name of the Internet service provider.  This
                        information is for identification purpose only."
                ::= { remoteNodeGeneralEntry 3 }

        remoteNodeEncap OBJECT-TYPE
                SYNTAX  INTEGER {
                        other(1),          -- none of the following
                        ppp(2),
                        pppoe(3),
                        mpoa(4),
                        enet-encap(5)
                }
                ACCESS  read-write
                STATUS  mandatory
                DESCRIPTION
                        "This if the method of encapsulation used by the ISP."
                ::= { remoteNodeGeneralEntry 4 }

        remoteNodeMultiplex OBJECT-TYPE
                SYNTAX  INTEGER {
                        other(1),          -- none of the following
                        llc-based(2),
                        vc-based(3)
                }
                ACCESS  read-write
                STATUS  mandatory
                DESCRIPTION
                        "This if the methos of multiplexing used by the ISP.
                        Choices are vc-based or llc-based"
                ::= { remoteNodeGeneralEntry 5 }

        remoteNodeServiceName OBJECT-TYPE
                SYNTAX  DisplayString (SIZE (0..32))
                ACCESS  read-write
                STATUS  mandatory
                DESCRIPTION
                        "The PPPoE service name.  This is valid only when PPPoE
                        encapsulation is chosen."
                ::= { remoteNodeGeneralEntry 6 }


        remoteNodeAuthen OBJECT-TYPE
                SYNTAX  INTEGER {
                        other(1),          -- none of the following
                        chap-pap(2),
                        chap(3),
                        pap(4)
                }
                ACCESS  read-write
                STATUS  mandatory
                DESCRIPTION
                        "This object sets the authentication protocol used
                        for outgoing calls.  Options for this object are :
                        chap/pap - Your Device will accept CHAP or PAP.
                        chap - Your Device will accept CHAP.
                        PAP - Your Device will accept PAP."
                ::= { remoteNodeGeneralEntry 7 }

        remoteNodeRoute OBJECT-TYPE
                SYNTAX  INTEGER {
                        other(1),          -- none of the following
                        ip(2),
                        none(3)
                }
                ACCESS  read-write
                STATUS  mandatory
                DESCRIPTION
                        "This object determines the protocol that your Device
                        will route.  Choices are IP or none."
                ::= { remoteNodeGeneralEntry 8 }

        remoteNodeBridge OBJECT-TYPE
                SYNTAX  INTEGER {
                        no(0),
                        yes(1)
                }
                ACCESS  read-write
                STATUS  mandatory
                DESCRIPTION
                        "Bridging is used for protocols that the Device
                        does not route, e.g. SNA, or not truned on in the
                        previous Route object.  When bridging is enabled,
                        your Device will forward any packet that it does
                        not route to this remote node; otherwise, the
                        packets are discarded.  Choose Yes to enable or No
                        to disable the Bridge field."
                ::= { remoteNodeGeneralEntry 9 }





        -- remoteNodeATMTable OBJECT-TYPE

        remoteNodeATMTable OBJECT-TYPE
                SYNTAX  SEQUENCE OF RemoteNodeATMEntry
                ACCESS  not-accessible
                STATUS  mandatory
                DESCRIPTION
                        "A list of remote node ATM entries."
                ::= { adslRemoteNode 5 }

        remoteNodeATMEntry OBJECT-TYPE
                SYNTAX  RemoteNodeATMEntry
                ACCESS  not-accessible
                STATUS  mandatory
                DESCRIPTION
                		"An remote node ATM entry containing comment object for a
                		remote node ATM information."
                INDEX   	{ remoteNodeATMIndex }
                ::= { remoteNodeATMTable 1 }

        RemoteNodeATMEntry ::=
                SEQUENCE {
                        remoteNodeATMIndex
                                INTEGER,
                                remoteNodeATMIfIndex
                                                INTEGER,
                        remoteNodeVPI
                                INTEGER,
                        remoteNodeVCI
                                INTEGER,
                        remoteNodeQosType
                                INTEGER,
                        remoteNodePCR
                                INTEGER,
                        remoteNodeSCR
                                INTEGER,
                        remoteNodeMBS
                                INTEGER
                }

        remoteNodeATMIndex OBJECT-TYPE
                SYNTAX  INTEGER
                ACCESS  read-write
                STATUS  mandatory
                DESCRIPTION
                        "The index of remote node ATM entry."
                ::= { remoteNodeATMEntry 1 }

		remoteNodeATMIfIndex OBJECT-TYPE
		        SYNTAX  INTEGER
		        ACCESS  read-only
		        STATUS  deprecated
		        DESCRIPTION
		        		"The interface on which this entry's equivalence is effective.
						The interface identified by a particular value of this index is
						the same interface as identified by the same value of ifIndex."
		        ::= { remoteNodeATMEntry 2 }

        remoteNodeVPI OBJECT-TYPE
                SYNTAX  INTEGER (0..255)
                ACCESS  read-write
                STATUS  mandatory
                DESCRIPTION
                        "The Virtual Path Identifier(VPI) is supplied by your
                        telephone company.  The valid range for the VPI is 0 to 255."
                ::= { remoteNodeATMEntry 3 }

        remoteNodeVCI OBJECT-TYPE
                SYNTAX  INTEGER (32..65535)
                ACCESS  read-write
                STATUS  mandatory
                DESCRIPTION
                        "The Virtual Channel Identifier(VCI) number is supplied by
                        your telephone company.  The valid range is 32 to 65535."
                ::= { remoteNodeATMEntry 4 }

        remoteNodeQosType OBJECT-TYPE
                SYNTAX  INTEGER {
                        other(1),          -- none of the following
                        cbr(2),
                        ubr(3)
                }
                ACCESS  read-write
                STATUS  mandatory
                DESCRIPTION
                        "This is the ATM Qos Type.  There are 2 options: cbr and ubr.
                        cbr (Continuous Bit Rate) specifys fixed (always-on) bandwidth.
                        UBR (Unspecified Bit Rage) is for applications that are non-time
                        senstive, such as e-mail."
                ::= { remoteNodeATMEntry 5 }

        remoteNodePCR OBJECT-TYPE
                SYNTAX  INTEGER
                ACCESS  read-write
                STATUS  mandatory
                DESCRIPTION
                        "This is the maximum rate at shich the sender can send cells."
                ::= { remoteNodeATMEntry 6 }

        remoteNodeSCR OBJECT-TYPE
                SYNTAX  INTEGER
                ACCESS  read-write
                STATUS  mandatory
                DESCRIPTION
                        "Sustained Cell Rate (SCR) is the mean cell rate of
                        a bursty, on-off traffic source that can be sent at
                        the peak rate, and a parameter for burst-type traffic.
                        The SCR must be less than the PCR."
                ::= { remoteNodeATMEntry 7 }

        remoteNodeMBS OBJECT-TYPE
                SYNTAX  INTEGER (0..65535)
                ACCESS  read-write
                STATUS  mandatory
                DESCRIPTION
                        "MBS is the Maximum Burst Size  of cells that can be sent
                         at the peak rate.  The MBS must be less than 65535"
                ::= { remoteNodeATMEntry 8 }


-- the Control Group

-- the FilterIPRangeTable Group

	filterIPRangeTable OBJECT-TYPE
        SYNTAX	SEQUENCE OF FilterIPRangeEntry
        ACCESS	not-accessible
        STATUS	mandatory
        DESCRIPTION
                "A list of filter IP range entry."
        ::= { control 1 }

	filterIPRangeEntry OBJECT-TYPE
        SYNTAX	FilterIPRangeEntry
        ACCESS	not-accessible
        STATUS	mandatory
        DESCRIPTION
                "Filter IP range entry can be used to block specific internal users from
                 accessing the Internet.  Each entry has start IP and end IP settings,
                 if user's IP is in this range, he will be blocked."
        INDEX	{ filterIPRangeIndex }
        ::= { filterIPRangeTable 1 }

	FilterIPRangeEntry ::=
        SEQUENCE {
			filterIPRangeIndex				INTEGER,
			filterIPStart					IpAddress,
			filterIPEnd						IpAddress
        }

	filterIPRangeIndex OBJECT-TYPE
        SYNTAX	INTEGER
        ACCESS	read-only
        STATUS	mandatory
        DESCRIPTION
                "Index of filter IP range table."
        ::= { filterIPRangeEntry 1 }

	filterIPStart OBJECT-TYPE
        SYNTAX	IpAddress
        ACCESS	read-write
        STATUS	mandatory
        DESCRIPTION
                "Start IP address of filter IP range entry."
        ::= { filterIPRangeEntry 2 }

	filterIPEnd OBJECT-TYPE
        SYNTAX	IpAddress
        ACCESS	read-write
        STATUS	mandatory
        DESCRIPTION
                "End IP address of filter IP range entry."
        ::= { filterIPRangeEntry 3 }


-- the FilterPortRangeTable Group

	filterPortRangeTable OBJECT-TYPE
        SYNTAX	SEQUENCE OF FilterPortRangeEntry
        ACCESS	not-accessible
        STATUS	mandatory
        DESCRIPTION
                "A list of filter port range entry."
        ::= { control 2 }

	filterPortRangeEntry OBJECT-TYPE
        SYNTAX	FilterPortRangeEntry
        ACCESS	not-accessible
        STATUS	mandatory
        DESCRIPTION
				"Filter port range entry can be used to block specific 
				packets from  going out to Internet.  Each entry has 
				protocol and port range settings, if out-going packet's 
				destination port is in this port range and protocol is 
				identical, then it will be blocked."
        INDEX	{ filterPortRangeIndex }
        ::= { filterPortRangeTable 1 }

	FilterPortRangeEntry ::=
        SEQUENCE {
			filterPortRangeIndex				INTEGER,
			filterPortProto						INTEGER,
			filterPortStart						INTEGER,
			filterPortEnd						INTEGER
        }

	filterPortRangeIndex OBJECT-TYPE
        SYNTAX	INTEGER
        ACCESS	read-only
        STATUS	mandatory
        DESCRIPTION
                "Index of filter port range table."
        ::= { filterPortRangeEntry 1 }

	filterPortProto OBJECT-TYPE
        SYNTAX	INTEGER {
              		both(0),
              		udp(1),
              		tcp(2)
              	}
        ACCESS	read-write
        STATUS	mandatory
        DESCRIPTION
                "Protocol setting of FilterPortRangeEntry, it can be TCP, 
                UDP or both (TCP and UDP)."
        ::= { filterPortRangeEntry 2 }

	filterPortStart OBJECT-TYPE
        SYNTAX	INTEGER
        ACCESS	read-write
        STATUS	mandatory
        DESCRIPTION
                "Start port setting of FilterPortRangeEntry"
        ::= { filterPortRangeEntry 3 }

	filterPortEnd OBJECT-TYPE
        SYNTAX	INTEGER
        ACCESS	read-write
        STATUS	mandatory
        DESCRIPTION
                "End port setting of FilterPortRangeEntry"
        ::= { filterPortRangeEntry 4 }


-- the FilterMACTable Group

	filterMACTable OBJECT-TYPE
        SYNTAX	SEQUENCE OF FilterMACEntry
        ACCESS	not-accessible
        STATUS	mandatory
        DESCRIPTION
                "A list of filter Mac entry."
        ::= { control 3 }

	filterMACEntry OBJECT-TYPE
        SYNTAX	FilterMACEntry
        ACCESS	not-accessible
        STATUS	mandatory
        DESCRIPTION
				"Filter MAC range entry can be used to block specific 
				internal users from accessing the Internet. Each entry 
				has a MAC setting, if user's MAC is identical with this 
				setting, he will be blocked."
        INDEX	{ filterMACIndex }
        ::= { filterMACTable 1 }

	FilterMACEntry ::=
        SEQUENCE {
			filterMACIndex					INTEGER,
			filterMAC						PhysAddress
        }

	filterMACIndex OBJECT-TYPE
        SYNTAX	INTEGER
        ACCESS	read-only
        STATUS	mandatory
        DESCRIPTION
                "Index of filterMACTable."
        ::= { filterMACEntry 1 }

	filterMAC OBJECT-TYPE
        SYNTAX	PhysAddress
        ACCESS	read-write
        STATUS	mandatory
        DESCRIPTION
                "The MAC setting of filterMACEntry."
        ::= { filterMACEntry 2 }


-- the ForwardTable Group

	forwardTable OBJECT-TYPE
        SYNTAX	SEQUENCE OF ForwardEntry
        ACCESS	not-accessible
        STATUS	mandatory
        DESCRIPTION
                "A list of forwardEntry."
        ::= { control 4 }

	forwardEntry OBJECT-TYPE
        SYNTAX	ForwardEntry
        ACCESS	not-accessible
        STATUS	mandatory
        DESCRIPTION
				"You can use Forwarding to set up public services on your 
				network.  When user send this type of request to your 
				network via the Internet, the router will forward those 
				requests to the appropriate PC."
        INDEX	{ forwardIndex }
        ::= { forwardTable 1 }

	ForwardEntry ::=
        SEQUENCE {
			forwardIndex					INTEGER,
			servicePortStart				INTEGER,
			servicePortEnd					INTEGER,
			servicePortProto				INTEGER,
			forwardIPAddress				IpAddress
        }

	forwardIndex OBJECT-TYPE
        SYNTAX	INTEGER
        ACCESS	read-only
        STATUS	mandatory
        DESCRIPTION
                "Index of forwardTable"
        ::= { forwardEntry 1 }

	servicePortStart OBJECT-TYPE
        SYNTAX	INTEGER
        ACCESS	read-write
        STATUS	mandatory
        DESCRIPTION
                "The start port setting of forward public service port range."
        ::= { forwardEntry 2 }

	servicePortEnd OBJECT-TYPE
        SYNTAX	INTEGER
        ACCESS	read-write
        STATUS	mandatory
        DESCRIPTION
                "The end port setting of forward public service port range."
        ::= { forwardEntry 3 }

	servicePortProto OBJECT-TYPE
        SYNTAX	INTEGER {
              		both(0),
              		udp(1),
              		tcp(2)
              	}
        ACCESS	read-write
        STATUS	mandatory
        DESCRIPTION
                "The protocol setting of forward public service port range."
        ::= { forwardEntry 4 }

	forwardIPAddress OBJECT-TYPE
        SYNTAX	IpAddress
        ACCESS	read-write
        STATUS	mandatory
        DESCRIPTION
                "The LAN side forward server IP address."
        ::= { forwardEntry 5 }


-- the Port Triggering Group

	portTriggeringTable OBJECT-TYPE
        SYNTAX	SEQUENCE OF PortTriggeringEntry
        ACCESS	not-accessible
        STATUS	mandatory
        DESCRIPTION
                "A list of portTriggeringEntry"
        ::= { control 5 }

	portTriggeringEntry OBJECT-TYPE
        SYNTAX	PortTriggeringEntry
        ACCESS	not-accessible
        STATUS	mandatory
        DESCRIPTION
                "Port triggering allows the Router to watch outgoing data for specific port numbers.
                 The IP address of the computer that sends the matching data is remembered by the
                 Router, so that when the requested data returns through the firewall, the data is
                 pulled back to the proper computer by way of IP address and port mapping rules."
        INDEX	{ portTriggeringIndex }
        ::= { portTriggeringTable 1 }

	PortTriggeringEntry ::=
        SEQUENCE {
			portTriggeringIndex				INTEGER,
			appName							DisplayString,
			triggerPortStart				INTEGER,
			triggerPortEnd					INTEGER,
			incomingPortStart				INTEGER,
			incomingPortEnd					INTEGER
        }

	portTriggeringIndex OBJECT-TYPE
        SYNTAX	INTEGER
        ACCESS	read-only
        STATUS	mandatory
        DESCRIPTION
                "Index of portTriggeringTable."
        ::= { portTriggeringEntry 1 }

	appName OBJECT-TYPE
        SYNTAX	DisplayString (SIZE(0..12))
        ACCESS	read-write
        STATUS	mandatory
        DESCRIPTION
                "Name description of this portTriggeringEntry."
        ::= { portTriggeringEntry 2 }

	triggerPortStart OBJECT-TYPE
        SYNTAX	INTEGER
        ACCESS	read-write
        STATUS	mandatory
        DESCRIPTION
                "The start port of triggering port range."
        ::= { portTriggeringEntry 3 }

	triggerPortEnd OBJECT-TYPE
        SYNTAX	INTEGER
        ACCESS	read-write
        STATUS	mandatory
        DESCRIPTION
                "The end port of triggering port range."
        ::= { portTriggeringEntry 4 }

	incomingPortStart OBJECT-TYPE
        SYNTAX	INTEGER
        ACCESS	read-write
        STATUS	mandatory
        DESCRIPTION
                "The start port of incoming port range."
        ::= { portTriggeringEntry 5 }

	incomingPortEnd OBJECT-TYPE
        SYNTAX	INTEGER
        ACCESS	read-write
        STATUS	mandatory
        DESCRIPTION
                "The end port of incoming port range."
        ::= { portTriggeringEntry 6 }


-- the Wireless MAC Access Group

	wlanAccessMACTable OBJECT-TYPE
        SYNTAX	SEQUENCE OF WlanAccessMACEntry
        ACCESS	not-accessible
        STATUS	mandatory
        DESCRIPTION
                "Table of wireless station physical addresses that
                will put under control."
        ::= { control 6 }

	wlanAccessMACEntry OBJECT-TYPE
        SYNTAX	WlanAccessMACEntry
        ACCESS	not-accessible
        STATUS	mandatory
        DESCRIPTION
                "An entry in the table controls the assocaition
                with access point for each wireless station."
        INDEX	{ wlanAccessMACIndex }
        ::= { wlanAccessMACTable 1 }

	WlanAccessMACEntry ::=
        SEQUENCE {
			wlanAccessMACIndex				INTEGER,
			wlanAccessMAC					PhysAddress,
			wlanAccessStatus				INTEGER
        }

	wlanAccessMACIndex OBJECT-TYPE
        SYNTAX	INTEGER
        ACCESS	read-only
        STATUS	mandatory
        DESCRIPTION  
                "An unique value for each wireless station."
        ::= { wlanAccessMACEntry 1 }

	wlanAccessMAC OBJECT-TYPE
        SYNTAX	PhysAddress
        ACCESS	read-write
        STATUS	mandatory
        DESCRIPTION
                "Specifies the physical address to which will be
                controlled the association state with the access
                point."
        ::= { wlanAccessMACEntry 2 }

	wlanAccessStatus OBJECT-TYPE
        SYNTAX	INTEGER {
              		block(0),
              		allow(1)
              	}
        ACCESS	read-write
        STATUS	mandatory
        DESCRIPTION
                "Indicates the association state with the access
                point for the specified wireless client."
        ::= { wlanAccessMACEntry 3 }


-- the UPnP ForwardTable Group

	uPnPforwardTable OBJECT-TYPE
		SYNTAX	SEQUENCE OF UPnPforwardEntry
		ACCESS	not-accessible
		STATUS	mandatory
		DESCRIPTION
				"A list of UPnP forwarding application setting entry."
		::= { control 7 }

	uPnPforwardEntry OBJECT-TYPE
		SYNTAX	UPnPforwardEntry
		ACCESS	not-accessible
		STATUS	mandatory
		DESCRIPTION
				"UPnP forwarding entry can be used to preset
				application	setting as well as options for
				customization of port services for other
				applications."
		INDEX	{ uPnPforwardIndex }
		::= { uPnPforwardTable 1 }

	UPnPforwardEntry ::=
		SEQUENCE {
			uPnPforwardIndex				INTEGER,
			uPnPserviceName					DisplayString,
			uPnPExtPort						INTEGER,
			uPnPservicePortProto			INTEGER,
			uPnPIntPort						INTEGER,
			uPnPforwardIPAddress			IpAddress,
			uPnPforwardStatus				INTEGER
		}

	uPnPforwardIndex OBJECT-TYPE
		SYNTAX	INTEGER
		ACCESS	read-only
		STATUS	mandatory
		DESCRIPTION
				"An unique value for each UPnP forwarding setting."
		::= { uPnPforwardEntry 1 }

	uPnPserviceName OBJECT-TYPE
		SYNTAX	DisplayString (SIZE(0..11))
		ACCESS	read-write
		STATUS	mandatory
		DESCRIPTION
				"Indicates the most widely used Internet applicaiton 
				name. Such as FTP, Telnet, SMTP and DNS."
		::= { uPnPforwardEntry 2 }

	uPnPExtPort OBJECT-TYPE
		SYNTAX	INTEGER
		ACCESS	read-write
		STATUS	mandatory
		DESCRIPTION
				"Specifies the external port number used by Internet
				application server. Check with the Internet application
				software documentation for more information."
		::= { uPnPforwardEntry 3 }
	
	uPnPservicePortProto OBJECT-TYPE
		SYNTAX	INTEGER {
					udp(1),
					tcp(2)
				}
		ACCESS	read-write
		STATUS	mandatory
		DESCRIPTION
				"Specifies the Transport layer protocol to which
				this Internet application will use."
		::= { uPnPforwardEntry 4 }
	
	uPnPIntPort OBJECT-TYPE
		SYNTAX	INTEGER
		ACCESS	read-write
		STATUS	mandatory
		DESCRIPTION
				"Specifies the internal port number used by Internet
				application server. Check with the Internet application
				software documentation for more information."
		::= { uPnPforwardEntry 5 }
	
	uPnPforwardIPAddress OBJECT-TYPE
		SYNTAX	IpAddress
		ACCESS	read-write
		STATUS	mandatory
		DESCRIPTION
				"Specifies the IP address of Internet application server
				to which the Internet users can access."
		::= { uPnPforwardEntry 6 }

	uPnPforwardStatus OBJECT-TYPE
		SYNTAX	INTEGER { 
					disable(0), 
					enable(1)
				}
		ACCESS	read-write
		STATUS	mandatory
		DESCRIPTION
				"Indicates whether to enable the defined service."
		::= { uPnPforwardEntry 7 }


-- the Status Information Group

-- the DHCPActiveTable Group

	dhcpActiveTable OBJECT-TYPE
        SYNTAX	SEQUENCE OF DHCPActiveEntry
        ACCESS	not-accessible
        STATUS	mandatory
        DESCRIPTION
                "A list of dhcpActiveEntry."
        ::= { statusInfo 1 }

	dhcpActiveEntry OBJECT-TYPE
        SYNTAX	DHCPActiveEntry
        ACCESS	not-accessible
        STATUS	mandatory
        DESCRIPTION
                "The dhcpActiveEntry shows out the information of DHCP client PCs."
        INDEX	{ dhcpActiveIndex }
        ::= { dhcpActiveTable 1 }

	DHCPActiveEntry ::=
        SEQUENCE {
			dhcpActiveIndex                 INTEGER,
			dhcpClientHostName              DisplayString,
			dhcpNetAddress                  IpAddress,
			dhcpPhysicalAddress             PhysAddress
        }

	dhcpActiveIndex OBJECT-TYPE
        SYNTAX	INTEGER
        ACCESS	read-only
        STATUS	mandatory
        DESCRIPTION
                "The index of dhcpActiveTable."
        ::= { dhcpActiveEntry 1 }

	dhcpClientHostName OBJECT-TYPE
        SYNTAX	DisplayString (SIZE(0..32))
        ACCESS	read-only
        STATUS	mandatory
        DESCRIPTION
                "The host name of DHCP client PC."
        ::= { dhcpActiveEntry 2 }

	dhcpNetAddress OBJECT-TYPE
        SYNTAX	IpAddress
        ACCESS	read-only
        STATUS	mandatory
        DESCRIPTION
                "The IP address of DHCP client PC."
        ::= { dhcpActiveEntry 3 }

	dhcpPhysicalAddress OBJECT-TYPE
        SYNTAX	PhysAddress
        ACCESS	read-only
        STATUS	mandatory
        DESCRIPTION
                "The MAC address of DHCP client PC."
        ::= { dhcpActiveEntry 4 }


-- the OutingLogTable Group

	outgoingLogTable OBJECT-TYPE
        SYNTAX	SEQUENCE OF OutgoingLogEntry
        ACCESS	not-accessible
        STATUS	mandatory
        DESCRIPTION
                "A list of outgoingLogEntry."
        ::= { statusInfo 2 }

	outgoingLogEntry OBJECT-TYPE
        SYNTAX	OutgoingLogEntry
        ACCESS	not-accessible
        STATUS	mandatory
        DESCRIPTION
				"The outgoing log entry lists the IP address of Internet 
				site that users on your network have accessed."
        INDEX	{ outgoingLogIndex }
        ::= { outgoingLogTable 1 }

	OutgoingLogEntry ::=
        SEQUENCE {
			outgoingLogIndex				INTEGER,
			sourceIPLAN						IpAddress,
			destinationIP					IpAddress,
			servicePortNumber				INTEGER
        }

	outgoingLogIndex OBJECT-TYPE
        SYNTAX	INTEGER
        ACCESS	read-only
        STATUS	mandatory
        DESCRIPTION
                "The index of outgoingLogTable"
        ::= { outgoingLogEntry 1 }

	sourceIPLAN OBJECT-TYPE
        SYNTAX	IpAddress
        ACCESS	read-only
        STATUS	mandatory
        DESCRIPTION
                "The source IP address of the outgoing log entry."
        ::= { outgoingLogEntry 2 }

	destinationIP OBJECT-TYPE
        SYNTAX	IpAddress
        ACCESS	read-only
        STATUS	mandatory
        DESCRIPTION
                "The destination IP address of the outgoing log entry."
        ::= { outgoingLogEntry 3 }


	servicePortNumber OBJECT-TYPE
        SYNTAX	INTEGER
        ACCESS	read-only
        STATUS	mandatory
        DESCRIPTION
                "The destination port number of the outgoing log entry."
        ::= { outgoingLogEntry 4 }


-- the IncomingLogTable Group

	incomingLogTable OBJECT-TYPE
        SYNTAX	SEQUENCE OF IncomingLogEntry
        ACCESS	not-accessible
        STATUS	mandatory
        DESCRIPTION
                "A list of incomingLogEntry."
        ::= { statusInfo 3 }

	incomingLogEntry OBJECT-TYPE
        SYNTAX	IncomingLogEntry
        ACCESS	not-accessible
        STATUS	mandatory
        DESCRIPTION
                "The incoming log entry shows out the log of incoming 
                Internet traffic."
        INDEX	{ incomingLogIndex }
        ::= { incomingLogTable 1 }

	IncomingLogEntry ::=
        SEQUENCE {
			incomingLogIndex					INTEGER,
			sourceIP							IpAddress,
			destinationPortNumber				INTEGER
        }

	incomingLogIndex OBJECT-TYPE
        SYNTAX	INTEGER
        ACCESS	read-only
        STATUS	mandatory
        DESCRIPTION
                "Index of incomingLogTable."
        ::= { incomingLogEntry 1 }

	sourceIP OBJECT-TYPE
        SYNTAX	IpAddress
        ACCESS	read-only
        STATUS	mandatory
        DESCRIPTION
                "The source IP address of incoming log entry."
        ::= { incomingLogEntry 2 }

	destinationPortNumber OBJECT-TYPE
        SYNTAX	INTEGER
        ACCESS	read-only
        STATUS	mandatory
        DESCRIPTION
                "The destination port number of incoming log entry."
        ::= { incomingLogEntry 3 }


-- the WAN Connection Status Information Group --

	infWANStatusTable OBJECT-TYPE
        SYNTAX	SEQUENCE OF InfWANStatusEntry
        ACCESS	not-accessible
        STATUS	mandatory
        DESCRIPTION
                " Table of WAN connection status. "
        ::= { statusInfo 4 }

	infWANStatusEntry OBJECT-TYPE
        SYNTAX	InfWANStatusEntry
        ACCESS	not-accessible
        STATUS	mandatory
        DESCRIPTION
                " An entry in the table, containing connection status of
                one WAN interface. "
        INDEX	{ infWANStatusIndex }
        ::= { infWANStatusTable 1 }

	InfWANStatusEntry ::=
        SEQUENCE {
			infWANStatusIndex						INTEGER,
			infWANPortStatus						INTEGER,
			infWANPPPoEFailureCode					INTEGER,
			infWANPPPoEDetailErrorCode				DisplayString,
			infWANDHCPStatus						INTEGER,
			infWANDHCPDetailErrorCode				DisplayString,
			infWANDNSStatus							INTEGER,
			infWANPPTPFailureCode					INTEGER,
			infWANPPTPDetailErrorCode				DisplayString
        }

	infWANStatusIndex OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  deprecated
        DESCRIPTION
                "Index of infWANStatusTable."
        ::= { infWANStatusEntry 1 }

	infWANPortStatus OBJECT-TYPE
        SYNTAX	INTEGER {
              		link(0),
              		no-link(1)
              	}
        ACCESS	read-only
        STATUS	mandatory
        DESCRIPTION
                "Show the WAN Port physical link status"
        ::= { infWANStatusEntry 2 }

	infWANPPPoEFailureCode OBJECT-TYPE
        SYNTAX	INTEGER {
              		connected(0),
              		other-error(1),
              		no-pppoe-server(2),
              		username-password-error(3),
              		lcp-nego-fail(4),
              		disconnected-by-ISP(5)
              	}
        ACCESS	read-only
        STATUS	mandatory
        DESCRIPTION
                "Show out the WAN PPPoE connection status."
        ::= { infWANStatusEntry 3 }

	infWANPPPoEDetailErrorCode OBJECT-TYPE
        SYNTAX	DisplayString (SIZE(0..4))
        ACCESS	read-only
        STATUS	mandatory
        DESCRIPTION
                " Detail error code of the current PPPoE connection."
        ::= { infWANStatusEntry 4 }

	infWANDHCPStatus OBJECT-TYPE
        SYNTAX	INTEGER {
              		ok(0),
              		other-error(1),
              		no-DHCP-server(2)
              	}
        ACCESS	read-only
        STATUS	mandatory
        DESCRIPTION
                "Show out the status of WAN DHCP."
        ::= { infWANStatusEntry 5 }

	infWANDHCPDetailErrorCode OBJECT-TYPE
        SYNTAX	DisplayString (SIZE(0..4))
        ACCESS	read-only
        STATUS	mandatory
        DESCRIPTION
                "Detail error code of the current DHCP connection."
        ::= { infWANStatusEntry 6 }

	infWANDNSStatus OBJECT-TYPE
        SYNTAX	INTEGER {
              		ok(0),
              		no-DNS-server-assigned(1),
              		no-DNS-server-working(2)
              	}
        ACCESS	read-only
        STATUS	mandatory
        DESCRIPTION
                "Show the WAN DNS status."
        ::= { infWANStatusEntry 7 }

	infWANPPTPFailureCode OBJECT-TYPE
        SYNTAX	INTEGER {
              		connected(0),
              		other-error(1),
              		no-PPTP-server(2),
              		username-password-error(3),
              		disconnected-by-ISP(4)
              	}
        ACCESS	read-only
        STATUS	mandatory
        DESCRIPTION
                "Show the WAN PPTP connection status."
        ::= { infWANStatusEntry 8 }

	infWANPPTPDetailErrorCode OBJECT-TYPE
        SYNTAX	DisplayString (SIZE(0..4))
        ACCESS	read-only
        STATUS	mandatory
        DESCRIPTION
                " Detail error code of the current PPTP connection."
        ::= { infWANStatusEntry 9 }


	infNodeWLANStatus OBJECT-TYPE
        SYNTAX	INTEGER {
              		wlan-OK(0),
              		initialization-failed(1)
              	}
        ACCESS	read-only
        STATUS	mandatory
        DESCRIPTION
                "Show the WLAN status."
        ::= { statusInfo 5 }

	nicDevicePresent OBJECT-TYPE
        SYNTAX	INTEGER {
              		absent(0),
              		present(1)
              	}
        ACCESS	read-only
        STATUS	mandatory
        DESCRIPTION
                "The target device is present on the system or not."
        ::= { statusInfo 6 }

	nicDriverInstallation OBJECT-TYPE
        SYNTAX	INTEGER {
              		not-installed(0),
              		installed(1)
              	}
        ACCESS	read-only
        STATUS	mandatory
        DESCRIPTION
                "The driver was installed or not."
        ::= { statusInfo 7 }

	nicDriverStatus OBJECT-TYPE
        SYNTAX	INTEGER {
              		disabled(1),
              		working(2),
              		not-working(3)
              	}
        ACCESS	read-only
        STATUS	mandatory
        DESCRIPTION
                "The working status of the driver."
        ::= { statusInfo 8 }


	nicConnectionStatus OBJECT-TYPE
        SYNTAX	INTEGER {
              		connected(0),
              		disconnected(1)
              	}
        ACCESS	read-only
        STATUS	mandatory
        DESCRIPTION
                "The connection status of the device."
        ::= { statusInfo 9 }

	nicOSVersion OBJECT-TYPE
        SYNTAX	DisplayString
        ACCESS	read-only
        STATUS	mandatory
        DESCRIPTION
                "The version number of the Windows OS."
        ::= { statusInfo 10 }

	nicDriverVersion OBJECT-TYPE
        SYNTAX	DisplayString
        ACCESS	read-only
        STATUS	mandatory
        DESCRIPTION
                "The version number of the device driver"
        ::= { statusInfo 11 }

	nicFirmwareVersion OBJECT-TYPE
        SYNTAX	DisplayString
        ACCESS	read-only
        STATUS	mandatory
        DESCRIPTION
                "The version number of the device firmware"
        ::= { statusInfo 12 }

	nicUtilityVersion OBJECT-TYPE
        SYNTAX	DisplayString
        ACCESS	read-only
        STATUS	mandatory
        DESCRIPTION
                "The version number of the configure Utility"
        ::= { statusInfo 13 }


-- the Statistics Information Group

END

