
Cisco Evolved Programmable Network Manager API
Evolved Programmable Network Manager API Documentation

# Server-Sent Events API Resources

## CLI Template Server-Sent Events

The service provides notifications about CLI templates

Resource | Description | API Version
--- | --- | ---
GET CliTemplate Stream GET sse/CliTemplate | Notifications about CLI templates |

## Clients Server-Sent Events

Provides notifications about wired and wireless clients.

Resource | Description | API Version
--- | --- | ---
GET Client Sessions Stream GET sse/ClientSessions | Represents detail view of client sessions. It provides device and session related attributes including security, connected device, session time, traffic, etc. |
GET Client Stream GET sse/Clients | Represents client view with information about the end points. It provides end point information such as MAC address, IP address, username, and status. |

## Device Details Server-Sent Events

The service provides notifications about managed devices

Resource | Description | API Version
--- | --- | ---
GET Alarms Stream GET sse/Alarms | Provides notifications about alarms. Alarm is a representation of the fault or change of state that occurred in the managed system. Limitations: SSE notifications do not include annotations added to the alarm, hence "annotations" block will not be returned in response |
GET Devices Stream GET sse/Devices | Notifications about devices |
GET Modules Stream GET sse/Modules | Notifications about device modules |
GET Rogue AP Alarms Stream GET sse/RogueApAlarms | Provides notifications about rogue AP alarms. Rogue AP alarm is a representation basic alarm attributes and some additional details. Limitations: There is no notifications about alarms annotations being changed. |

## Wireless Device Details Server-Sent Events

The service provides notifications about wireless devices

Resource | Description | API Version
--- | --- | ---
GET Wireless Access Point Stream GET sse/AccessPoints | Wireless Access Point Notifications |