
Cisco Evolved Programmable Network Manager API
Evolved Programmable Network Manager API Documentation

# GET AutoApRadioDetails

Represents a radio interface of an autonomous access point.

Since Product Version: 1.2

- Jump To

- v1
- v2
- v3
- v4

### Resource Information

Rate Limiting? | Yes
Sorting? | Yes
Paging? | Yes
Filtering? | Yes
Group Filtering? | No
Aggregation? | No
Response Formats | xml json
User Group | NBI Read
HTTP Methods | GET

API version v1 is deprecated

This API version has been deprecated. It will be removed in a future release of the product. Please develop new clients using the latest API version. Please modify your existing clients to use a later API version.

## Resource URL

/webacs/api/v1/data/AutoApRadioDetails

Deprecated

This version has been deprecated. Please use v4.

## Response Parameters

Attribute | Description
--- | ---
adminStatus RadioAdminStatusEnum | Administrative status of the radio interface Allowed values UNKNOWN ENABLE DISABLE
antennaAzimAngle Float | Displays the horizontal angle of the antenna
antennaDiversity String | Displays if antenna diversity is enabled or disabled. Antenna diversity refers to the access point sampling the radio signal from two integrated antenna ports to choose the preferred antenna. Allowed values: 'Connector A', 'Connector B', 'Enabled', 'NA'
antennaElevAngle Float | Displays the elevation angle of the antenna.
antennaGain Integer | The external antenna gain, measured in 0.5 dBi units. This is the raw value from device. It is different from displayed in the UI. An integer value 7 means 7 x 0.5 = 3.5 dBm of gain.
antennaMode String | Displays the antenna mode. Allowed values: Sector A, Sector B, Omni, NA (non-applicable).
antennaName String | Antenna name
antennaType String | Antenna type. Allowed values: Internal, External, NA
apIpAddress String | IP address of the access point
apName String | Name of the access point
baseRadioMac String | Base radio MAC address
channelControl String | Radio channel control. Allowed values: Automatic, Custom, NA
channelNumber ChannelNumberEnum | Current operational channel number Allowed values UNKNOWN _1 _2 _3 _4 _5 _6 _7 _8 _9 _10 _11 _12 _13 _14 _20 _21 _22 _23 _24 _25 _26 _34 _36 _38 _40 _42 _44 _46 _48 _52 _56 _60 _64 _100 _104 _108 _112 _116 _120 _124 _128 _132 _136 _140 _144 _149 _153 _157 _161 _165 _169 _173
clientCount String | Client count connected to the radio interface
ethernetMac String | MAC address of the ethernet interface on the AP
ifDescr String | SNMP ifDescr
nativePowerUseStandard boolean | Native power use standard
operBand Cd11HtPhyOperBandEnum | 802.11 operational band Allowed values UNKNOWN BAND24GHZ BAND5GHZ
operStatus RadioOperStatusEnum | Operational status of the radio interface Allowed values DOWN UP NOTASSOCIATED UNKNOWN
phyType Dot11PhyTypeEnum | 802.11 phy type Allowed values UNKNOWN FHSS DSSS IRBASEBAND OFDM HRDSSS ERP HT
powerLevel Integer | Power level of the radio
radioMac String | Radio MAC address
radioRole AutoApRadioRoleEnum | Radio role Allowed values UNKNOWN WGB BRIDGE CLIENT ROOT REPEATER APBRIDGE APREPEATER IBSS NRBRIDGE APBRBRIDGE SCANNER
radioType String | Radio type. Allowed values: 802.11a, 802.11b/g, 802.11b/g/n, 802.11a/n

## Sample Payloads

Sample payloads are for information only. They are automatically generated and the values included may not be representative of actual valid data values.

### Sample XML Payload

https://10.64.88.203/webacs/api/v1/data/AutoApRadioDetails/15

    <?xml version="1.0" ?>
    <queryResponse type="AutoApRadioDetails" responseType="getEntity" requestUrl="https://10.64.88.203/webacs/api/v1/data/AutoApRadioDetails/15" rootUrl="https://10.64.88.203/webacs/api/v1/data">
      <entity dtoType="autoApRadioDetailsDTO" type="AutoApRadioDetails" url="https://10.64.88.203/webacs/api/v1/data/AutoApRadioDetails/15">
        <autoApRadioDetailsDTO displayName="String value" id="15" uuid="String value">
          <adminStatus>UNKNOWN</adminStatus>
          <antennaAzimAngle>15.0</antennaAzimAngle>
          <antennaElevAngle>15.0</antennaElevAngle>
          <antennaGain>15</antennaGain>
          <antennaName>String value</antennaName>
          <apName>String value</apName>
          <channelNumber>UNKNOWN</channelNumber>
          <ifDescr>String value</ifDescr>
          <nativePowerUseStandard>true</nativePowerUseStandard>
          <operBand>UNKNOWN</operBand>
          <operStatus>DOWN</operStatus>
          <phyType>UNKNOWN</phyType>
          <powerLevel>15</powerLevel>
          <radioRole>UNKNOWN</radioRole>
          <antennaDiversity>String value</antennaDiversity>
          <antennaMode>String value</antennaMode>
          <antennaType>String value</antennaType>
          <apIpAddress>String value</apIpAddress>
          <baseRadioMac>String value</baseRadioMac>
          <channelControl>String value</channelControl>
          <clientCount>String value</clientCount>
          <ethernetMac>String value</ethernetMac>
          <radioMac>String value</radioMac>
          <radioType>String value</radioType>
        </autoApRadioDetailsDTO>
      </entity>
    </queryResponse>

### Sample JSON Payload

https://10.64.88.203/webacs/api/v1/data/AutoApRadioDetails/15.json

    {
      "queryResponse" : {
        "@type" : "AutoApRadioDetails",
        "@responseType" : "getEntity",
        "@requestUrl" : "https : //10.64.88.203/webacs/api/v1/data/AutoApRadioDetails/15",
        "@rootUrl" : "https : //10.64.88.203/webacs/api/v1/data",
        "entity" : {
          "@dtoType" : "autoApRadioDetailsDTO",
          "@type" : "AutoApRadioDetails",
          "@url" : "https : //10.64.88.203/webacs/api/v1/data/AutoApRadioDetails/15",
          "autoApRadioDetailsDTO" : {
            "@displayName" : "String value",
            "@id" : 15,
            "@uuid" : "String value",
            "adminStatus" : "UNKNOWN",
            "antennaAzimAngle" : 15,
            "antennaElevAngle" : 15,
            "antennaGain" : 15,
            "antennaName" : "String value",
            "apName" : "String value",
            "channelNumber" : "UNKNOWN",
            "ifDescr" : "String value",
            "nativePowerUseStandard" : true,
            "operBand" : "UNKNOWN",
            "operStatus" : "DOWN",
            "phyType" : "UNKNOWN",
            "powerLevel" : 15,
            "radioRole" : "UNKNOWN",
            "antennaDiversity" : "String value",
            "antennaMode" : "String value",
            "antennaType" : "String value",
            "apIpAddress" : "String value",
            "baseRadioMac" : "String value",
            "channelControl" : "String value",
            "clientCount" : "String value",
            "ethernetMac" : "String value",
            "radioMac" : "String value",
            "radioType" : "String value"
          }
        }
      }
    }

### Resource Information

Rate Limiting? | Yes
Sorting? | Yes
Paging? | Yes
Filtering? | Yes
Group Filtering? | No
Aggregation? | No
Response Formats | xml json
User Group | NBI Read
HTTP Methods | GET

## Resource URL

/webacs/api/v2/data/AutoApRadioDetails

Unmodified

This resource has not been modified since the previous API version.

Deprecated

This version has been deprecated. Please use v4.

## Response Parameters

Attribute | Description
--- | ---
adminStatus RadioAdminStatusEnum | Administrative status of the radio interface Allowed values UNKNOWN ENABLE DISABLE
antennaAzimAngle Float | Displays the horizontal angle of the antenna
antennaDiversity String | Displays if antenna diversity is enabled or disabled. Antenna diversity refers to the access point sampling the radio signal from two integrated antenna ports to choose the preferred antenna. Allowed values: 'Connector A', 'Connector B', 'Enabled', 'NA'
antennaElevAngle Float | Displays the elevation angle of the antenna.
antennaGain Integer | The external antenna gain, measured in 0.5 dBi units. This is the raw value from device. It is different from displayed in the UI. An integer value 7 means 7 x 0.5 = 3.5 dBm of gain.
antennaMode String | Displays the antenna mode. Allowed values: Sector A, Sector B, Omni, NA (non-applicable).
antennaName String | Antenna name
antennaType String | Antenna type. Allowed values: Internal, External, NA
apIpAddress String | IP address of the access point
apName String | Name of the access point
baseRadioMac String | Base radio MAC address
channelControl String | Radio channel control. Allowed values: Automatic, Custom, NA
channelNumber ChannelNumberEnum | Current operational channel number Allowed values UNKNOWN _1 _2 _3 _4 _5 _6 _7 _8 _9 _10 _11 _12 _13 _14 _20 _21 _22 _23 _24 _25 _26 _34 _36 _38 _40 _42 _44 _46 _48 _52 _56 _60 _64 _100 _104 _108 _112 _116 _120 _124 _128 _132 _136 _140 _144 _149 _153 _157 _161 _165 _169 _173
clientCount String | Client count connected to the radio interface
ethernetMac String | MAC address of the ethernet interface on the AP
ifDescr String | SNMP ifDescr
nativePowerUseStandard boolean | Native power use standard
operBand Cd11HtPhyOperBandEnum | 802.11 operational band Allowed values UNKNOWN BAND24GHZ BAND5GHZ
operStatus RadioOperStatusEnum | Operational status of the radio interface Allowed values DOWN UP NOTASSOCIATED UNKNOWN
phyType Dot11PhyTypeEnum | 802.11 phy type Allowed values UNKNOWN FHSS DSSS IRBASEBAND OFDM HRDSSS ERP HT
powerLevel Integer | Power level of the radio
radioMac String | Radio MAC address
radioRole AutoApRadioRoleEnum | Radio role Allowed values UNKNOWN WGB BRIDGE CLIENT ROOT REPEATER APBRIDGE APREPEATER IBSS NRBRIDGE APBRBRIDGE SCANNER
radioType String | Radio type. Allowed values: 802.11a, 802.11b/g, 802.11b/g/n, 802.11a/n

## Sample Payloads

Sample payloads are for information only. They are automatically generated and the values included may not be representative of actual valid data values.

### Sample XML Payload

https://10.64.88.203/webacs/api/v2/data/AutoApRadioDetails/15

    <?xml version="1.0" ?>
    <queryResponse type="AutoApRadioDetails" responseType="getEntity" requestUrl="https://10.64.88.203/webacs/api/v2/data/AutoApRadioDetails/15" rootUrl="https://10.64.88.203/webacs/api/v2/data">
      <entity dtoType="autoApRadioDetailsDTO" type="AutoApRadioDetails" url="https://10.64.88.203/webacs/api/v2/data/AutoApRadioDetails/15">
        <autoApRadioDetailsDTO displayName="String value" id="15" uuid="String value">
          <adminStatus>UNKNOWN</adminStatus>
          <antennaAzimAngle>15.0</antennaAzimAngle>
          <antennaElevAngle>15.0</antennaElevAngle>
          <antennaGain>15</antennaGain>
          <antennaName>String value</antennaName>
          <apName>String value</apName>
          <channelNumber>UNKNOWN</channelNumber>
          <ifDescr>String value</ifDescr>
          <nativePowerUseStandard>true</nativePowerUseStandard>
          <operBand>UNKNOWN</operBand>
          <operStatus>DOWN</operStatus>
          <phyType>UNKNOWN</phyType>
          <powerLevel>15</powerLevel>
          <radioRole>UNKNOWN</radioRole>
          <antennaDiversity>String value</antennaDiversity>
          <antennaMode>String value</antennaMode>
          <antennaType>String value</antennaType>
          <apIpAddress>String value</apIpAddress>
          <baseRadioMac>String value</baseRadioMac>
          <channelControl>String value</channelControl>
          <clientCount>String value</clientCount>
          <ethernetMac>String value</ethernetMac>
          <radioMac>String value</radioMac>
          <radioType>String value</radioType>
        </autoApRadioDetailsDTO>
      </entity>
    </queryResponse>

### Sample JSON Payload

https://10.64.88.203/webacs/api/v2/data/AutoApRadioDetails/15.json

    {
      "queryResponse" : {
        "@type" : "AutoApRadioDetails",
        "@requestUrl" : "https://10.64.88.203/webacs/api/v2/data/AutoApRadioDetails/15",
        "@responseType" : "getEntity",
        "@rootUrl" : "https://10.64.88.203/webacs/api/v2/data",
        "entity" : [ {
          "@dtoType" : "autoApRadioDetailsDTO",
          "@type" : "AutoApRadioDetails",
          "@url" : "https://10.64.88.203/webacs/api/v2/data/AutoApRadioDetails/15",
          "autoApRadioDetailsDTO" : {
            "@displayName" : "String value",
            "@id" : 15,
            "@uuid" : "String value",
            "adminStatus" : "UNKNOWN",
            "antennaAzimAngle" : 15.0,
            "antennaDiversity" : "String value",
            "antennaElevAngle" : 15.0,
            "antennaGain" : 15,
            "antennaMode" : "String value",
            "antennaName" : "String value",
            "antennaType" : "String value",
            "apIpAddress" : "String value",
            "apName" : "String value",
            "baseRadioMac" : "String value",
            "channelControl" : "String value",
            "channelNumber" : "UNKNOWN",
            "clientCount" : "String value",
            "ethernetMac" : "String value",
            "ifDescr" : "String value",
            "nativePowerUseStandard" : true,
            "operBand" : "UNKNOWN",
            "operStatus" : "DOWN",
            "phyType" : "UNKNOWN",
            "powerLevel" : 15,
            "radioMac" : "String value",
            "radioRole" : "UNKNOWN",
            "radioType" : "String value"
          }
        } ]
      }
    }

### Resource Information

Rate Limiting? | Yes
Sorting? | Yes
Paging? | Yes
Filtering? | Yes
Group Filtering? | No
Aggregation? | No
Response Formats | xml json
User Group | NBI Read
HTTP Methods | GET

## Resource URL

/webacs/api/v3/data/AutoApRadioDetails

Unmodified

This resource has not been modified since the previous API version.

Deprecated

This version has been deprecated. Please use v4.

## Response Parameters

Attribute | Description
--- | ---
adminStatus RadioAdminStatusEnum | Administrative status of the radio interface Allowed values UNKNOWN ENABLE DISABLE
antennaAzimAngle Float | Displays the horizontal angle of the antenna
antennaDiversity String | Displays if antenna diversity is enabled or disabled. Antenna diversity refers to the access point sampling the radio signal from two integrated antenna ports to choose the preferred antenna. Allowed values: 'Connector A', 'Connector B', 'Enabled', 'NA'
antennaElevAngle Float | Displays the elevation angle of the antenna.
antennaGain Integer | The external antenna gain, measured in 0.5 dBi units. This is the raw value from device. It is different from displayed in the UI. An integer value 7 means 7 x 0.5 = 3.5 dBm of gain.
antennaMode String | Displays the antenna mode. Allowed values: Sector A, Sector B, Omni, NA (non-applicable).
antennaName String | Antenna name
antennaType String | Antenna type. Allowed values: Internal, External, NA
apIpAddress String | IP address of the access point
apName String | Name of the access point
baseRadioMac String | Base radio MAC address
channelControl String | Radio channel control. Allowed values: Automatic, Custom, NA
channelNumber ChannelNumberEnum | Current operational channel number Allowed values UNKNOWN _1 _2 _3 _4 _5 _6 _7 _8 _9 _10 _11 _12 _13 _14 _20 _21 _22 _23 _24 _25 _26 _34 _36 _38 _40 _42 _44 _46 _48 _52 _56 _60 _64 _100 _104 _108 _112 _116 _120 _124 _128 _132 _136 _140 _144 _149 _153 _157 _161 _165 _169 _173
clientCount String | Client count connected to the radio interface
ethernetMac String | MAC address of the ethernet interface on the AP
ifDescr String | SNMP ifDescr
nativePowerUseStandard boolean | Native power use standard
operBand Cd11HtPhyOperBandEnum | 802.11 operational band Allowed values UNKNOWN BAND24GHZ BAND5GHZ
operStatus RadioOperStatusEnum | Operational status of the radio interface Allowed values DOWN UP NOTASSOCIATED UNKNOWN
phyType Dot11PhyTypeEnum | 802.11 phy type Allowed values UNKNOWN FHSS DSSS IRBASEBAND OFDM HRDSSS ERP HT
powerLevel Integer | Power level of the radio
radioMac String | Radio MAC address
radioRole AutoApRadioRoleEnum | Radio role Allowed values UNKNOWN WGB BRIDGE CLIENT ROOT REPEATER APBRIDGE APREPEATER IBSS NRBRIDGE APBRBRIDGE SCANNER
radioType String | Radio type. Allowed values: 802.11a, 802.11b/g, 802.11b/g/n, 802.11a/n

## Sample Payloads

Sample payloads are for information only. They are automatically generated and the values included may not be representative of actual valid data values.

### Sample XML Payload

https://10.64.88.203/webacs/api/v3/data/AutoApRadioDetails/15

    <?xml version="1.0" ?>
    <queryResponse type="AutoApRadioDetails" responseType="getEntity" requestUrl="https://10.64.88.203/webacs/api/v3/data/AutoApRadioDetails/15" rootUrl="https://10.64.88.203/webacs/api/v3/data">
      <entity dtoType="autoApRadioDetailsDTO" type="AutoApRadioDetails" url="https://10.64.88.203/webacs/api/v3/data/AutoApRadioDetails/15">
        <autoApRadioDetailsDTO displayName="String value" id="15" uuid="String value">
          <adminStatus>UNKNOWN</adminStatus>
          <antennaAzimAngle>15.0</antennaAzimAngle>
          <antennaElevAngle>15.0</antennaElevAngle>
          <antennaGain>15</antennaGain>
          <antennaName>String value</antennaName>
          <apName>String value</apName>
          <channelNumber>UNKNOWN</channelNumber>
          <ifDescr>String value</ifDescr>
          <nativePowerUseStandard>true</nativePowerUseStandard>
          <operBand>UNKNOWN</operBand>
          <operStatus>DOWN</operStatus>
          <phyType>UNKNOWN</phyType>
          <powerLevel>15</powerLevel>
          <radioRole>UNKNOWN</radioRole>
          <antennaDiversity>String value</antennaDiversity>
          <antennaMode>String value</antennaMode>
          <antennaType>String value</antennaType>
          <apIpAddress>String value</apIpAddress>
          <baseRadioMac>String value</baseRadioMac>
          <channelControl>String value</channelControl>
          <clientCount>String value</clientCount>
          <ethernetMac>String value</ethernetMac>
          <radioMac>String value</radioMac>
          <radioType>String value</radioType>
        </autoApRadioDetailsDTO>
      </entity>
    </queryResponse>

### Sample JSON Payload

https://10.64.88.203/webacs/api/v3/data/AutoApRadioDetails/15.json

    {
      "queryResponse" : {
        "@type" : "AutoApRadioDetails",
        "@requestUrl" : "https://10.64.88.203/webacs/api/v3/data/AutoApRadioDetails/15",
        "@responseType" : "getEntity",
        "@rootUrl" : "https://10.64.88.203/webacs/api/v3/data",
        "entity" : [ {
          "@dtoType" : "autoApRadioDetailsDTO",
          "@type" : "AutoApRadioDetails",
          "@url" : "https://10.64.88.203/webacs/api/v3/data/AutoApRadioDetails/15",
          "autoApRadioDetailsDTO" : {
            "@displayName" : "String value",
            "@id" : 15,
            "@uuid" : "String value",
            "adminStatus" : "UNKNOWN",
            "antennaAzimAngle" : 15.0,
            "antennaDiversity" : "String value",
            "antennaElevAngle" : 15.0,
            "antennaGain" : 15,
            "antennaMode" : "String value",
            "antennaName" : "String value",
            "antennaType" : "String value",
            "apIpAddress" : "String value",
            "apName" : "String value",
            "baseRadioMac" : "String value",
            "channelControl" : "String value",
            "channelNumber" : "UNKNOWN",
            "clientCount" : "String value",
            "ethernetMac" : "String value",
            "ifDescr" : "String value",
            "nativePowerUseStandard" : true,
            "operBand" : "UNKNOWN",
            "operStatus" : "DOWN",
            "phyType" : "UNKNOWN",
            "powerLevel" : 15,
            "radioMac" : "String value",
            "radioRole" : "UNKNOWN",
            "radioType" : "String value"
          }
        } ]
      }
    }

### Resource Information

Rate Limiting? | Yes
Sorting? | Yes
Paging? | Yes
Filtering? | Yes
Group Filtering? | No
Aggregation? | No
Response Formats | xml json
User Group | NBI Read
HTTP Methods | GET

## Resource URL

/webacs/api/v4/data/AutoApRadioDetails

Updated

Since version 4 types of attributes apIpAddress, clientCount have been changed. Attributes antennaDiversity, antennaMode, antennaType, and channelControl have been removed because these attributes are not collected for Autonomous AP radios.

## Response Parameters

Attribute | Description
--- | ---
adminStatus RadioAdminStatusEnum | Administrative status of the radio interface Allowed values UNKNOWN ENABLE DISABLE
antennaAzimAngle Float | Displays the horizontal angle of the antenna
antennaElevAngle Float | Displays the elevation angle of the antenna.
antennaGain Integer | The external antenna gain, measured in 0.5 dBi units. This is the raw value from device. It is different from displayed in the UI. An integer value 7 means 7 x 0.5 = 3.5 dBm of gain.
antennaName String | Antenna name
apIpAddress InetAddress | IP address of the access point
apName String | Name of the access point
baseRadioMac MacAddress | Base radio MAC address
channelNumber ChannelNumberEnum | Current operational channel number Allowed values UNKNOWN _1 _2 _3 _4 _5 _6 _7 _8 _9 _10 _11 _12 _13 _14 _20 _21 _22 _23 _24 _25 _26 _34 _36 _38 _40 _42 _44 _46 _48 _52 _56 _60 _64 _100 _104 _108 _112 _116 _120 _124 _128 _132 _136 _140 _144 _149 _153 _157 _161 _165 _169 _173
clientCount int | Client count connected to the radio interface
ethernetMac MacAddress | MAC address of the ethernet interface on the AP
ifDescr String | SNMP ifDescr
nativePowerUseStandard boolean | Native power use standard
operBand Cd11HtPhyOperBandEnum | 802.11 operational band Allowed values UNKNOWN BAND24GHZ BAND5GHZ
operStatus RadioOperStatusEnum | Operational status of the radio interface Allowed values DOWN UP NOTASSOCIATED UNKNOWN
phyType Dot11PhyTypeEnum | 802.11 phy type Allowed values UNKNOWN FHSS DSSS IRBASEBAND OFDM HRDSSS ERP HT
powerLevel Integer | Power level of the radio
radioMac MacAddress | Radio MAC address
radioRole AutoApRadioRoleEnum | Radio role Allowed values UNKNOWN WGB BRIDGE CLIENT ROOT REPEATER APBRIDGE APREPEATER IBSS NRBRIDGE APBRBRIDGE SCANNER
radioType AutoApRadioTypeEnum | Radio type Allowed values 802.11a 802.11b/g 802.11b/g/n 802.11a/n Unknown

## Sample Payloads

Sample payloads are for information only. They are automatically generated and the values included may not be representative of actual valid data values.

### Sample XML Payload

https://10.64.88.203/webacs/api/v4/data/AutoApRadioDetails/15

    <?xml version="1.0" ?>
    <queryResponse type="AutoApRadioDetails" responseType="getEntity" requestUrl="https://10.64.88.203/webacs/api/v4/data/AutoApRadioDetails/15" rootUrl="https://10.64.88.203/webacs/api/v4/data">
      <entity dtoType="autoApRadioDetailsDTO" type="AutoApRadioDetails" url="https://10.64.88.203/webacs/api/v4/data/AutoApRadioDetails/15">
        <autoApRadioDetailsDTO displayName="String value" id="15" uuid="String value">
          <adminStatus>UNKNOWN</adminStatus>
          <antennaAzimAngle>15.0</antennaAzimAngle>
          <antennaElevAngle>15.0</antennaElevAngle>
          <antennaGain>15</antennaGain>
          <antennaName>String value</antennaName>
          <apName>String value</apName>
          <channelNumber>UNKNOWN</channelNumber>
          <ifDescr>String value</ifDescr>
          <nativePowerUseStandard>true</nativePowerUseStandard>
          <operBand>UNKNOWN</operBand>
          <operStatus>DOWN</operStatus>
          <phyType>UNKNOWN</phyType>
          <powerLevel>15</powerLevel>
          <radioRole>UNKNOWN</radioRole>
          <apIpAddress>
            <address>192.168.115.243</address>
          </apIpAddress>
          <baseRadioMac>
            <octets>000a959d6816</octets>
          </baseRadioMac>
          <clientCount>1</clientCount>
          <ethernetMac>
            <octets>000a959d6816</octets>
          </ethernetMac>
          <radioMac>
            <octets>000a959d6816</octets>
          </radioMac>
          <radioType>802.11a</radioType>
        </autoApRadioDetailsDTO>
      </entity>
    </queryResponse>

### Sample JSON Payload

https://10.64.88.203/webacs/api/v4/data/AutoApRadioDetails/15.json

    {
      "queryResponse" : {
        "@type" : "AutoApRadioDetails",
        "@requestUrl" : "https://10.64.88.203/webacs/api/v4/data/AutoApRadioDetails/15",
        "@responseType" : "getEntity",
        "@rootUrl" : "https://10.64.88.203/webacs/api/v4/data",
        "entity" : [ {
          "@dtoType" : "autoApRadioDetailsDTO",
          "@type" : "AutoApRadioDetails",
          "@url" : "https://10.64.88.203/webacs/api/v4/data/AutoApRadioDetails/15",
          "autoApRadioDetailsDTO" : {
            "@displayName" : "String value",
            "@id" : 15,
            "@uuid" : "String value",
            "adminStatus" : "UNKNOWN",
            "antennaAzimAngle" : 15.0,
            "antennaElevAngle" : 15.0,
            "antennaGain" : 15,
            "antennaName" : "String value",
            "apIpAddress" : {
              "address" : "192.168.115.243"
            },
            "apName" : "String value",
            "baseRadioMac" : {
              "octets" : "000a959d6816"
            },
            "channelNumber" : "UNKNOWN",
            "clientCount" : 1,
            "ethernetMac" : {
              "octets" : "000a959d6816"
            },
            "ifDescr" : "String value",
            "nativePowerUseStandard" : true,
            "operBand" : "UNKNOWN",
            "operStatus" : "DOWN",
            "phyType" : "UNKNOWN",
            "powerLevel" : 15,
            "radioMac" : {
              "octets" : "000a959d6816"
            },
            "radioRole" : "UNKNOWN",
            "radioType" : "802.11a"
          }
        } ]
      }
    }