
Cisco Evolved Programmable Network Manager API
Evolved Programmable Network Manager API Documentation

# GET WlanTemplates

Provides information about WLAN templates stored on this system.

Since Product Version: 2.2

- Jump To

- v1
- v2
- v3
- v4

### Resource Information

Rate Limiting? | Yes
Sorting? | Yes
Paging? | Yes
Filtering? | Yes
Group Filtering? | No
Aggregation? | No
Response Formats | xml json
User Group | NBI Read
HTTP Methods | GET

API version v1 is deprecated

This API version has been deprecated. It will be removed in a future release of the product. Please develop new clients using the latest API version. Please modify your existing clients to use a later API version.

## Resource URL

/webacs/api/v1/data/WlanTemplates

## Response Parameters

Attribute | Description
--- | ---
aaaAllowOverride boolean | Is allow AAA override enabled?
aaaLdapPrimaryServer String | Primary LDAP server.
aaaLdapSecondaryServer String | Secondary LDAP server.
aaaLdapTertiaryServer String | Tertiary LDAP server.
aaaLocalEapAuthenticationEnabled boolean | Is local EAP authentication enabled?
aaaLocalEapAuthenticationProfileName String | When aaaLocalEapAuthenticationEnabled is true, this defines the EAP profile that will be used.
aaaRadiusAccountingPrimaryServer String | When aaaRadiusAccountingServersEnabled is true, this is the primary RADIUS accounting server.
aaaRadiusAccountingSecondaryServer String | When aaaRadiusAccountingServersEnabled is true, this is the secondary RADIUS accounting server.
aaaRadiusAccountingServersEnabled boolean | Is RADIUS accounting enabled?
aaaRadiusAccountingTertiaryServer String | When aaaRadiusAccountingServersEnabled is true, this is the tertiary RADIUS accounting server.
aaaRadiusAccountingWlcSpecificEnabled boolean | Is controller specific RADIUS accounting servers enabled?
aaaRadiusAuthenticationPrimaryServer String | When aaaRadiusAuthenticationServersEnabled is true, this is the primary RADIUS authentication server.
aaaRadiusAuthenticationSecondaryServer String | When aaaRadiusAuthenticationServersEnabled is true, this is the secondary RADIUS authentication server.
aaaRadiusAuthenticationServersEnabled boolean | Is RADIUS authentication enabled?
aaaRadiusAuthenticationTertiaryServer String | When aaaRadiusAuthenticationServersEnabled is true, this is the tertiary RADIUS authentication server.
aaaRadiusAuthenticationWlcSpecificEnabled boolean | Is controller specific RADIUS authentication servers enabled?
aaaRadiusInterimUpdateEnabled boolean | Is RADIUS server accounting interim update enabled?
aaaRadiusInterimUpdateInterval int | When aaaRadiusInterimUpdateEnabled is true, this determines the update interval. Measured in seconds.
adminStatus boolean | Is the WLAN administratively enabled?
advancedAironetIeEnabled boolean | Is Aironet Information Elements (IEs) enabled for this WLAN?
advancedClientExclusionEnabled boolean | Is automatic client exclusion enabled for this WLAN?
advancedClientExclusionTimeout int | When advancedClientExclusionEnabled is true, this denotes the length of the timeout. A value of zero represents an infinite timeout. Measured in seconds.
advancedCoverageHoleDetectionEnabled boolean | Is Coverage Hole Detection enabled for this WLAN?
advancedDhcpAddressAssignmentRequired boolean | Are all clients required to obtain an IP address from the DHCP server for this WLAN?
advancedDhcpProfilingEnabled boolean | Should the wireless controller collect the DHCP attributes of clients on this WLAN?
advancedDhcpServerIpAddress InetAddress | If this contains a valid address, an IPv4 DHCP server has been specified for this WLAN.
advancedDiagnosticChannelEnabled boolean | Is the diagnostic channel available for this WLAN?
advancedDot11anDtimPeriod int | Denotes the Delivery Traffic Indication Map (DTIM) interval for 802.11a/n radios, during which broadcast and multicast frames will be transmitted. A value of one results in a broadcast after every beacon, two for every other beacon, and so on.
advancedDot11bgnDtimPeriod int | Denotes the Delivery Traffic Indication Map (DTIM) interval for 802.11b/g/n radios, during which broadcast and multicast frames will be transmitted. A value of one results in a broadcast after every beacon, two for every other beacon, and so on.
advancedFlexConnectCentralDhcpProcessingEnabled boolean | Are DHCP packets received by the access point sent to the controller then forwarded to the WLAN's corresponding VLAN?
advancedFlexConnectLearnClientIpEnabled boolean | Is client IP address learning enabled?
advancedFlexConnectLocalAuthEnabled boolean | Is local authentication enabled?
advancedFlexConnectLocalSwitchingEnabled boolean | When true, access points will locally switch traffic, rather than forwarding to the wireless controller.
advancedFlexConnectNatPatEnabled boolean | Is Network Address Translation (NAT) and Port Address Translation (PAT) enabled?
advancedFlexConnectOverrideDnsEnabled boolean | When true, clients are given the DNS server of the access point rather than of the WLAN's configured interface.
advancedFlexConnectReapCentralAssociation boolean | Is Reap Central Association enabled?
advancedFlexConnectVlanCentralSwitchingEnabled boolean | Is VLAN based central switching enabled?
advancedHttpProfilingEnabled boolean | Should the wireless controller collect the HTTP attributes of clients on this WLAN?
advancedIpv6Enabled boolean | Is IPv6 enabled?
advancedKtsCacEnabled boolean | Is CAC based on the Key Telephone System (KTS) enabled on this WLAN?
advancedLoadBalancingBandSelectEnabled boolean | Is client band select enabled?
advancedLoadBalancingEnabled boolean | Is client load balancing enabled?
advancedMaximumClients int | Denotes the maximum number of clients. A value of zero means unlimited.
advancedMdnsProfileName String | When advancedMdnsSnoopingEnabled is true, this denotes the mDNS profile. Clients receive service advertisements only for the services associated with the profile.
advancedMdnsSnoopingEnabled boolean | Is mDNS snooping enabled?
advancedMediaSessionSnoopingEnabled boolean | Should the access point snoop on Session Initiation Protocol (SIP) traffic, and report back to the controller the establishment termination and failure of voice calls?
advancedMfpClientProtection DisabledEnabledRequiredEnum | Denotes whether client management frame protection (MFP) is enabled (optional), required, or disabled for this WLAN. Allowed values DISABLED ENABLED REQUIRED
advancedMfpSignatureGenerationEnabled boolean | Do 802.11 management frames transmitted by the access point have a signature to verify authenticity?
advancedMfpVersion int | Denotes the version of management frame protection (MFP).
advancedOverrideInterfaceAclName String | Denotes an IPv4 ACL that overrides the ACL configured for the WLAN's interface.
advancedOverrideInterfaceIpv6AclName String | Denotes an IPv6 ACL that overrides the ACL configured for the WLAN's interface.
advancedPassiveClientEnabled boolean | Should the controller forward ARP requests out to the WLAN for passive clients?
advancedPeerToPeerBlocking Peer2PeerBlockingEnum | Denotes whether peer-to-peer blocking is disabled, enabled, or if the packets are forwarded to the next device. Allowed values DISABLE DROP FORWARDUP ALLOWPRIVATEGROUP
advancedPmipMobilityType PmipMobilityTypeEnum | Denotes the Proxy Mobile IP (PMIP) type for this WLAN. Allowed values NONE PMIP
advancedPmipProfile String | Denotes the Proxy Mobile IP (PMIP) profile for this WLAN.
advancedPmipRealm String | Denotes the default realm of the Proxy Mobile IPv6 (PMIPv6) WLAN.
advancedScanDeferPriority0 boolean | Is priority 0 for the channel scan enabled?
advancedScanDeferPriority1 boolean | Is priority 1 for the channel scan enabled?
advancedScanDeferPriority2 boolean | Is priority 2 for the channel scan enabled?
advancedScanDeferPriority3 boolean | Is priority 3 for the channel scan enabled?
advancedScanDeferPriority4 boolean | Is priority 4 for the channel scan enabled?
advancedScanDeferPriority5 boolean | Is priority 5 for the channel scan enabled?
advancedScanDeferPriority6 boolean | Is priority 6 for the channel scan enabled?
advancedScanDeferPriority7 boolean | Is priority 7 for the channel scan enabled?
advancedScanDeferTime int | Denotes the channel scan defer time. Measured in milliseconds.
advancedSessionTimeout int | Denotes the maximum time for a client session before requiring reauthentication. Zero means no timeout. Measured in seconds.
advancedSessionTimeoutEnabled boolean | Is advancedSessionTimeout enabled?
advancedWifiDirectClientsPolicy DisabledAllowedNotAllowedEnum | Denotes the Wi-Fi Direct Clients Policy for this WLAN. Allowed values DISABLED ALLOWED NOTALLOWED XCONNECTNOTALLOW
broadcastSsidEnabled boolean | Is SSID broadcasting enabled?
ckipKeyIndex int | When ckipSecurityEnabled is true, this denotes the key index.
ckipKeyPermutationEnabled boolean | When ckipSecurityEnabled is true, this denotes whether key permutation is enabled.
ckipKeySize CkipEncryptionTypeEnum | When ckipSecurityEnabled is true, this denotes the key size. Allowed values NONE LEN40 LEN104
ckipMmhModeEnabled boolean | When ckipSecurityEnabled is true, this denotes whether multimodular mode hashing is enabled.
ckipSecurityEnabled boolean | Is CKIP layer 2 security enabled?
hotspot2Enable WlanMcHotSpotEnableTemplate | This attribute represents enablement of HotSpot 2.0.
Attribute | Description
--- | ---
hotSpot2Enabled boolean | Is HotSpot 2.0 enabled?
hotspot2Operators WlanMcHotSpotOperatorConfigTemplate[] | These attributes represent HotSpot 2.0 operators.
Attribute | Description
--- | ---
operatorId int | Operator index of the hotspot provider.
operatorLang String | Language code.
operatorName String | Operator name of the hotspot provider.
hotspot2Ports WlanMcHotSpotPortConfigTemplate[] | These attributes represent HotSpot 2.0 port configurations.
Attribute | Description
--- | ---
portConfigId int | Port configuration index.
portNo PortNoEnum | Port number used for the IP. Allowed values ICMPESP FTP SSH HTTP TTLSVPN PPTPVPN VOIP IKEV2 IPSECNAT
portStatus PortStatusEnum | Status of the IP port. Allowed values CLOSED OPEN UNKNOWN
protocolName ProtocolNameEnum | Internet protocol name. This parameter provides information on the connection status of the most commonly used communication protocols and ports. Allowed values ICMP FTP IKEV2 ESP
hotspot2Wan WlanMcHotSpotWanTemplate | These attributes represent HotSpot 2.0 WAN metrics configuration.
Attribute | Description
--- | ---
downLinkSpeed int | Downlink speed of the WAN backhaul link. Measured in Kbps.
upLinkSpeed int | Uplink speed of the WAN backhaul. Measured in Kbps.
wanLinkStatus WanLinkStatusEnum | WAN link status. Allowed values LINKUP LINKDOWN LINKINTESTSTATE NOTCONFIGURED
wanSymLinkStatus WanSymLinkStatusEnum | WAN symmetric link status. Allowed values SAME DIFFERENT
hotspotCellularNetworks WlanMc3GppConfigTemplate[] | These attributes represent 802.11u cellular network parameters.
Attribute | Description
--- | ---
countryCode String | Mobile country code in Binary Coded Decimal (BCD) format.
gppIndex int | Cellular index.
networkCode String | Mobile network code in Binary Coded Decimal (BCD) format.
hotspotDomains WlanMcDomainConfigTemplate[] | These attributes represent 802.11u domains.
Attribute | Description
--- | ---
domainId int | Domain index.
domainName String | Domain name operating in the WLAN network.
hotspotGeneral WlanMcGeneralConfigTemplate | These attributes represent 802.11u general parameters.
Attribute | Description
--- | ---
heSsid MacAddress | The Homogenous Extended Service Set Identifier (HESSID).
internetAccess boolean | Is Internet Access enabled?
ipv4AddressAvailType IPv4AddressAvailTypeEnum | IPv4 type address. Allowed values NOTAVAILABLE PUBLIC PORTRESTRICTED SINGLENATPRIVATE DOUBLENATPRIVATE PORTRESTRICTEDSINGLENATPRIVATE PORTRESTRICTEDDOUBLENATPRIVATE UNKNOWN
ipv6AddressAvailType IPv6AddressAvailTypeEnum | IPv6 type address. Allowed values NOTAVAILABLE AVAILABLE UNKNOWN
networkAuthType NetworkAuthTypeEnum | Network authentication type for 802.11u on this WLAN. Allowed values ACCEPTANCE ENROLLMENT REDIRECTION DNSREDIRECTION NOTCONFIGURED
networkType NetworkTypeEnum | Network type of this WLAN. Allowed values PRIVATE PRIVATEWITHGUESTACCESS PUBLICPAID PUBLICFREE PERSONALDEVICE EMERGENCYSERVICEONLY TESTEQUIPMENT WILDCARD UNKNOWN
status boolean | Is 802.11u enabled?
hotspotOuiTemplate WlanMcOuiConfigTemplate[] | These attributes represent 802.11u OUIs.
Attribute | Description
--- | ---
oui String | Organization Unique Identifier (OUI).
ouiId int | OUI index.
ouiInBeacon boolean | Are Organization Unique Identifier (OUI) beacon responses enabled?
hotspotRealms WlanMcRealmConfigTemplate[] | These attributes represent 802.11u realms.
Attribute | Description
--- | ---
realmEapMethods WlanMcRealmEapConfigTemplate[] | Extensible Authentication Protocol (EAP) list.
Attribute | Description
--- | ---
innerAuthMethods WlanMcRealmEapAuthConfigTemplate[] | Auth method list.
Attribute | Description
--- | ---
realmEapAuthId int | Auth method index.
realmEapAuthMethod RealmEapAuthMethodEnum | Inner auth method. Allowed values NONEAPINNERAUTH INNERAUTHEAP CREDENTIAL TUNNELEDEAPCREDENTIAL
realmEapAuthParam RealmEapAuthParamEnum | Auth param. Allowed values NONE PAP CHAP MSCHAP MSCHAPV2 LEAP PEAP EAPTLS EAPFAST EAPSIM EAPTTLS EAPAKA SIM USIM NFCSECURE HARDWARETOKEN SOFTTOKEN CERTIFICATE USERNAMEPASSWORD RESERVED ANONYMOUS VENDORSPECIFIC
realmEapId int | EAP index.
realmEapMethod RealmEapMethodEnum | EAP method for the realm in the WLAN. Allowed values NONE LEAP EAPPEAP EAPTLS EAPFAST EAPSIM EAPTTLS EAPAKA
realmId int | Realm index.
realmName String | Realm name.
hotspotServiceAdvertisement WlanMcServiceAdConfigTemplate | These attributes represent MSAP (Mobility Service Advertisement Protocol) parameters.
Attribute | Description
--- | ---
msapEnable boolean | Is Mobility Service Advertisement Protocol (MSAP) enabled?
serverIndex int | Server index.
interfaceName String | Denotes the interface, or interface group, for this WLAN. See interfaceType to determine if this is an interface or interface group.
interfaceType InterfaceMappingTypeEnum | Denotes whether an interface or interface group is used for this interface. See interfaceName for the name of the interface or interface group. Allowed values INTERFACE INTERFACEGROUP
isWiredLan boolean | Is this a wired LAN?
lanType LanTypeEnum | Denotes the LAN type. Allowed values WIRELESS GUEST REMOTE
lastModified long | The time the template was last modified. Measured in milliseconds since the Unix epoch.
layer2FastTransitionEnabled boolean | Is fast transition (FT) between access points enabled?
layer2FastTransitionOverDsEnabled boolean | When layer2FastTransitionEnabled is true, the denotes whether fast transition over a distributed system is enabled.
layer2FastTransitionReassociationTimeout int | When layer2FastTransitionEnabled is true, this denotes the transition timeout. Measured in seconds.
layer2MacFilteringEnabled boolean | Is MAC filtering enabled?
layer3GlobalWebAuthEnabled boolean | When a layer 3 web policy is true, this denotes whether the template uses global or template-defined Web Auth configuration.
layer3PreauthenticationAcl String | When a layer 3 web policy is true, this denotes the IPv4 ACL for traffic between the client and the wireless controller.
layer3PreauthenticationIpv6Acl String | When a layer 3 web policy is true, this denotes the IPv6 ACL for traffic between the client and the wireless controller.
layer3VpnPassthroughEnabled boolean | Is VPN passthrough enabled?
layer3WebAuthFlexAcl String | When a layer 3 web policy is true, this denotes the the FlexConnect ACL for external web authentication in locally switched WLANs.
layer3WebAuthType WlanWebAuthTypeEnum | When a layer 3 web policy is true and layer3GlobalWebAuth is false, this denotes the type of web authentication to be used. Allowed values DEFAULT CUSTOMIZED EXTERNAL
layer3WebPolicyAuthenticationEnabled boolean | Is the authentication web policy enabled?
layer3WebPolicyConditionalRedirectEnabled boolean | Is the conditional redirect web policy enabled?
layer3WebPolicyOnMacFailureEnabled boolean | Is the WebAuth on MAC failure web policy enabled?
layer3WebPolicyPassthroughEnabled boolean | Is the passthrough web policy enabled?
multicastVlanEnabled boolean | Is a multicast VLAN enabled?
multicastVlanInterface String | When multicastVlanInterface is true, this denotes the multicast VLAN.
profileName String | Profile name of the WLAN.
qos7920Cac PhoneSupport7920Enum | Denotes the Call Admission Control (CAC) configuration for Cisco 7920 phones. Allowed values DISABLED CLIENTCAC APCAC CLIENTANDAPCAC
qosAvcProfileName String | Denotes the Application Visibility and Control (AVC) profile for this WLAN.
qosNbarVisibilityEnabled boolean | Is Network Based Application Recognition (NBAR) deep packet inspection enabled on this WLAN?
qosNetflowMonitor String | Denotes the Netflow monitor configured for this WLAN.
qosPerSSidBurstRealTimeUpstreamRate int | Denotes the peak data rate limit for upstream UDP traffic for the WLAN. Zero means no restriction. Measured in Kbps.
qosPerSsidAverageDownstreamRate int | Denotes the average data rate limit for downstream TCP traffic for the WLAN. Zero means no restriction. Measured in Kbps.
qosPerSsidAverageRealTimeDownstreamRate int | Denotes the average data rate limit for downstream UDP traffic for the WLAN. Zero means no restriction. Measured in Kbps.
qosPerSsidAverageRealTimeUpstreamRate int | Denotes the average data rate limit for upstream UDP traffic for the WLAN. Zero means no restriction. Measured in Kbps.
qosPerSsidAverageUpstreamRate int | Denotes the average data rate limit for upstream TCP traffic for the WLAN. Zero means no restriction. Measured in Kbps.
qosPerSsidBurstDownstreamRate int | Denotes the peak data rate limit for downstream TCP traffic for the WLAN. Zero means no restriction. Measured in Kbps.
qosPerSsidBurstRealTimeDownstreamRate int | Denotes the peak data rate limit for downstream UDP traffic for the WLAN. Zero means no restriction. Measured in Kbps.
qosPerSsidBurstUpstreamRate int | Denotes the peak data rate limit for upstream TCP traffic for the WLAN. Zero means no restriction. Measured in Kbps.
qosPerUserAverageDownstreamRate int | Denotes the average data rate limit for downstream TCP traffic for a client. Zero means no restriction. Measured in Kbps.
qosPerUserAverageRealTimeDownstreamRate int | Denotes the average data rate limit for downstream UDP traffic for a client. Zero means no restriction. Measured in Kbps.
qosPerUserAverageRealTimeUpstreamRate int | Denotes the average data rate limit for upstream UDP traffic for a client. Zero means no restriction. Measured in Kbps.
qosPerUserAverageUpstreamRate int | Denotes the average data rate limit for upstream TCP traffic for a client. Zero means no restriction. Measured in Kbps.
qosPerUserBurstDownstreamRate int | Denotes the peak data rate limit for downstream TCP traffic for a client. Zero means no restriction. Measured in Kbps.
qosPerUserBurstRealTimeDownstreamRate int | Denotes the peak data rate limit for downstream UDP traffic for a client. Zero means no restriction. Measured in Kbps.
qosPerUserBurstRealTimeUpstreamRate int | Denotes the peak data rate limit for upstream UDP traffic for a client. Zero means no restriction. Measured in Kbps.
qosPerUserBurstUpstreamRate int | Denotes the peak data rate limit for upstream TCP traffic for a client. Zero means no restriction. Measured in Kbps.
qosProfile QosEnum | Denotes the QoS level for the WLAN. Allowed values BRONZE SILVER GOLD PLATINUM
qosWmmPolicy DisabledAllowedRequiredEnum | Denotes the state of the Wi-fi Multimedia (WMM) policy for this WLAN. Allowed values DISABLED ALLOWED REQUIRED
radioPolicy RadioPolicyEnum | Denotes the WLAN radio policy. Allowed values ALL ONLY80211A ONLY80211B ONLY80211G ONLY80211BG ONLY80211AG ONLY80211AB NONE REMOTELAN
ssid String | SSID of the WLAN.
templateName String | The name of the WLAN template.
vpnPassThroughGatewayAddress InetAddress | When layer3VpnPassthroughEnabled is true, this denotes the IP address of the VPN gateway.
webAuthExternalUrl String | When a layer 3 web policy is enabled, layer3GlobalWebAuthEnabled is false, and layer3WebAuthType is set to "External", this denotes the URL of the authentication server.
webAuthLoginFailurePage String | When a layer 3 web policy is enabled, layer3GlobalWebAuthEnabled is false, and layer3WebAuthType is set to "Customized", this denotes the page for authentication failures.
webAuthLoginPage String | When a layer 3 web policy is enabled, layer3GlobalWebAuthEnabled is false, and layer3WebAuthType is set to "Customized", this denotes the page for authentication.
webAuthLogoutPage String | When a layer 3 web policy is enabled, layer3GlobalWebAuthEnabled is false, and layer3WebAuthType is set to "Customized", this denotes the page for logout.
webPassthruEmailInputEnabled boolean | When layer3WebPolicyPassthroughEnabled is true, this denotes whether the client is prompted to enter an email address when connecting.
wepAllowSharedKeyAuthentication boolean | When wepSecurityEnabled is true, this denotes whether shared key authentication is enabled.
wepKeyIndex int | When wepSecurityEnabled is true, this denotes the key index.
wepKeySize WepEncryptionTypeEnum | When wepSecurityEnabled is true, this denotes whether shared key authentication is enabled. Allowed values WEP104 NONE WEP40 WEP128 AESOCB128 WEP_40 WEP_104
wepSecurityEnabled boolean | Is WEP layer 2 security enabled?
wpa2Enabled boolean | When wpaSecurityEnabled is true, this denotes whether the WPA2 policy is enabled.
wpa2EncryptionProtocolAes boolean | When wpaSecurityEnabled and wpa2Enabled are true, this denotes whether AES encryption is supported for the WPA2 policy.
wpa2EncryptionProtocolTkip boolean | When wpaSecurityEnabled and wpa2Enabled are true, this denotes whether TKIP encryption is supported for the WPA2 policy.
wpaAuthenticationKeyManagement8021x boolean | When wpaSecurityEnabled is true, this denotes whether 802.1X key management is enabled.
wpaAuthenticationKeyManagementCckm boolean | When wpaSecurityEnabled is true, this denotes whether Cisco Centralized Key Management (CCKM) is enabled.
wpaAuthenticationKeyManagementFt8021x boolean | When wpaSecurityEnabled is true, this denotes whether Fast Transition (FT) 802.1X key management is enabled.
wpaAuthenticationKeyManagementFtPsk boolean | When wpaSecurityEnabled is true, this denotes whether Fast Transition (FT) preshared key management is enabled.
wpaAuthenticationKeyManagementPmf8021x boolean | When wpaSecurityEnabled is true, this denotes whether Protected Management Frame (PMF) 802.1X key management is enabled.
wpaAuthenticationKeyManagementPmfPsk boolean | When wpaSecurityEnabled is true, this denotes whether Protected Management Frame (PMF) preshared key management is enabled.
wpaAuthenticationKeyManagementPsk boolean | When wpaSecurityEnabled is true, this denotes whether preshared key management is enabled.
wpaControllerSpecificPresharedKeyEnabled boolean | Is controller specific preshared key enabled?
wpaEnabled boolean | When wpaSecurityEnabled is true, this denotes whether the WPA1 policy is enabled.
wpaEncryptionProtocolAes boolean | When wpaSecurityEnabled and wpaEnabled are both true, this denotes whether AES encryption is supported for the WPA1 policy.
wpaEncryptionProtocolTkip boolean | When wpaSecurityEnabled and wpaEnabled are both true, this denotes whether TKIP encryption is supported for the WPA1 policy.
wpaPresharedKey String | When wpaSecurityEnabled is true, this contains preshared key in HEX or ASCII format.
wpaPresharedKeyFormat PskFormatEnum | When wpaSecurityEnabled is true, this denotes preshared key format. Allowed values DEFAULT HEX ASCII
wpaSecurityEnabled boolean | Is WPA layer 2 security enabled?
x8021KeySize x8021EncryptionTypeEnum | When x8021SecurityEnabled is true, this denotes the 802.1X key size. Allowed values WEP104 WEP40 WEP128 NONE WEP_40 WEP_104
x8021SecurityEnabled boolean | Is 802.1X layer 2 security enabled?

## Sample Payloads

Sample payloads are for information only. They are automatically generated and the values included may not be representative of actual valid data values.

### Sample XML Payload

https://10.64.88.203/webacs/api/v1/data/WlanTemplates/15

    <?xml version="1.0" ?>
    <queryResponse type="WlanTemplates" responseType="getEntity" requestUrl="https://10.64.88.203/webacs/api/v1/data/WlanTemplates/15" rootUrl="https://10.64.88.203/webacs/api/v1/data">
      <entity dtoType="wlanTemplatesDTO" type="WlanTemplates" url="https://10.64.88.203/webacs/api/v1/data/WlanTemplates/15">
        <wlanTemplatesDTO displayName="String value" id="15" uuid="String value">
          <aaaAllowOverride>true</aaaAllowOverride>
          <aaaLdapPrimaryServer>String value</aaaLdapPrimaryServer>
          <aaaLdapSecondaryServer>String value</aaaLdapSecondaryServer>
          <aaaLdapTertiaryServer>String value</aaaLdapTertiaryServer>
          <aaaLocalEapAuthenticationEnabled>true</aaaLocalEapAuthenticationEnabled>
          <aaaLocalEapAuthenticationProfileName>String value</aaaLocalEapAuthenticationProfileName>
          <aaaRadiusAccountingPrimaryServer>String value</aaaRadiusAccountingPrimaryServer>
          <aaaRadiusAccountingSecondaryServer>String value</aaaRadiusAccountingSecondaryServer>
          <aaaRadiusAccountingServersEnabled>true</aaaRadiusAccountingServersEnabled>
          <aaaRadiusAccountingTertiaryServer>String value</aaaRadiusAccountingTertiaryServer>
          <aaaRadiusAuthenticationPrimaryServer>String value</aaaRadiusAuthenticationPrimaryServer>
          <aaaRadiusAuthenticationSecondaryServer>String value</aaaRadiusAuthenticationSecondaryServer>
          <aaaRadiusAuthenticationServersEnabled>true</aaaRadiusAuthenticationServersEnabled>
          <aaaRadiusAuthenticationTertiaryServer>String value</aaaRadiusAuthenticationTertiaryServer>
          <aaaRadiusInterimUpdateEnabled>true</aaaRadiusInterimUpdateEnabled>
          <aaaRadiusInterimUpdateInterval>1</aaaRadiusInterimUpdateInterval>
          <adminStatus>true</adminStatus>
          <advancedAironetIeEnabled>true</advancedAironetIeEnabled>
          <advancedClientExclusionEnabled>true</advancedClientExclusionEnabled>
          <advancedClientExclusionTimeout>1</advancedClientExclusionTimeout>
          <advancedCoverageHoleDetectionEnabled>true</advancedCoverageHoleDetectionEnabled>
          <advancedDhcpAddressAssignmentRequired>true</advancedDhcpAddressAssignmentRequired>
          <advancedDhcpProfilingEnabled>true</advancedDhcpProfilingEnabled>
          <advancedDhcpServerIpAddress>
            <address>192.168.115.243</address>
          </advancedDhcpServerIpAddress>
          <advancedDiagnosticChannelEnabled>true</advancedDiagnosticChannelEnabled>
          <advancedDot11anDtimPeriod>1</advancedDot11anDtimPeriod>
          <advancedDot11bgnDtimPeriod>1</advancedDot11bgnDtimPeriod>
          <advancedFlexConnectCentralDhcpProcessingEnabled>true</advancedFlexConnectCentralDhcpProcessingEnabled>
          <advancedFlexConnectLearnClientIpEnabled>true</advancedFlexConnectLearnClientIpEnabled>
          <advancedFlexConnectLocalAuthEnabled>true</advancedFlexConnectLocalAuthEnabled>
          <advancedFlexConnectLocalSwitchingEnabled>true</advancedFlexConnectLocalSwitchingEnabled>
          <advancedFlexConnectNatPatEnabled>true</advancedFlexConnectNatPatEnabled>
          <advancedFlexConnectOverrideDnsEnabled>true</advancedFlexConnectOverrideDnsEnabled>
          <advancedFlexConnectReapCentralAssociation>true</advancedFlexConnectReapCentralAssociation>
          <advancedFlexConnectVlanCentralSwitchingEnabled>true</advancedFlexConnectVlanCentralSwitchingEnabled>
          <advancedHttpProfilingEnabled>true</advancedHttpProfilingEnabled>
          <advancedIpv6Enabled>true</advancedIpv6Enabled>
          <advancedKtsCacEnabled>true</advancedKtsCacEnabled>
          <advancedLoadBalancingBandSelectEnabled>true</advancedLoadBalancingBandSelectEnabled>
          <advancedLoadBalancingEnabled>true</advancedLoadBalancingEnabled>
          <advancedMaximumClients>1</advancedMaximumClients>
          <advancedMdnsProfileName>String value</advancedMdnsProfileName>
          <advancedMdnsSnoopingEnabled>true</advancedMdnsSnoopingEnabled>
          <advancedMediaSessionSnoopingEnabled>true</advancedMediaSessionSnoopingEnabled>
          <advancedMfpClientProtection>DISABLED</advancedMfpClientProtection>
          <advancedMfpSignatureGenerationEnabled>true</advancedMfpSignatureGenerationEnabled>
          <advancedMfpVersion>1</advancedMfpVersion>
          <advancedOverrideInterfaceAclName>String value</advancedOverrideInterfaceAclName>
          <advancedOverrideInterfaceIpv6AclName>String value</advancedOverrideInterfaceIpv6AclName>
          <advancedPassiveClientEnabled>true</advancedPassiveClientEnabled>
          <advancedPeerToPeerBlocking>DISABLE</advancedPeerToPeerBlocking>
          <advancedPmipMobilityType>NONE</advancedPmipMobilityType>
          <advancedPmipProfile>String value</advancedPmipProfile>
          <advancedPmipRealm>String value</advancedPmipRealm>
          <advancedScanDeferPriority0>true</advancedScanDeferPriority0>
          <advancedScanDeferPriority1>true</advancedScanDeferPriority1>
          <advancedScanDeferPriority2>true</advancedScanDeferPriority2>
          <advancedScanDeferPriority3>true</advancedScanDeferPriority3>
          <advancedScanDeferPriority4>true</advancedScanDeferPriority4>
          <advancedScanDeferPriority5>true</advancedScanDeferPriority5>
          <advancedScanDeferPriority6>true</advancedScanDeferPriority6>
          <advancedScanDeferPriority7>true</advancedScanDeferPriority7>
          <advancedScanDeferTime>1</advancedScanDeferTime>
          <advancedSessionTimeout>1</advancedSessionTimeout>
          <advancedWifiDirectClientsPolicy>DISABLED</advancedWifiDirectClientsPolicy>
          <broadcastSsidEnabled>true</broadcastSsidEnabled>
          <ckipKeyIndex>1</ckipKeyIndex>
          <ckipKeyPermutationEnabled>true</ckipKeyPermutationEnabled>
          <ckipKeySize>NONE</ckipKeySize>
          <ckipMmhModeEnabled>true</ckipMmhModeEnabled>
          <ckipSecurityEnabled>true</ckipSecurityEnabled>
          <interfaceName>String value</interfaceName>
          <interfaceType>INTERFACE</interfaceType>
          <isWiredLan>true</isWiredLan>
          <lanType>WIRELESS</lanType>
          <layer2FastTransitionEnabled>true</layer2FastTransitionEnabled>
          <layer2FastTransitionOverDsEnabled>true</layer2FastTransitionOverDsEnabled>
          <layer2FastTransitionReassociationTimeout>1</layer2FastTransitionReassociationTimeout>
          <layer2MacFilteringEnabled>true</layer2MacFilteringEnabled>
          <layer3GlobalWebAuthEnabled>true</layer3GlobalWebAuthEnabled>
          <layer3PreauthenticationAcl>String value</layer3PreauthenticationAcl>
          <layer3PreauthenticationIpv6Acl>String value</layer3PreauthenticationIpv6Acl>
          <layer3VpnPassthroughEnabled>true</layer3VpnPassthroughEnabled>
          <layer3WebAuthFlexAcl>String value</layer3WebAuthFlexAcl>
          <layer3WebAuthType>DEFAULT</layer3WebAuthType>
          <layer3WebPolicyAuthenticationEnabled>true</layer3WebPolicyAuthenticationEnabled>
          <layer3WebPolicyConditionalRedirectEnabled>true</layer3WebPolicyConditionalRedirectEnabled>
          <layer3WebPolicyOnMacFailureEnabled>true</layer3WebPolicyOnMacFailureEnabled>
          <layer3WebPolicyPassthroughEnabled>true</layer3WebPolicyPassthroughEnabled>
          <multicastVlanEnabled>true</multicastVlanEnabled>
          <multicastVlanInterface>String value</multicastVlanInterface>
          <profileName>String value</profileName>
          <qos7920Cac>DISABLED</qos7920Cac>
          <qosAvcProfileName>String value</qosAvcProfileName>
          <qosNbarVisibilityEnabled>true</qosNbarVisibilityEnabled>
          <qosNetflowMonitor>String value</qosNetflowMonitor>
          <qosPerSSidBurstRealTimeUpstreamRate>1</qosPerSSidBurstRealTimeUpstreamRate>
          <qosPerSsidAverageDownstreamRate>1</qosPerSsidAverageDownstreamRate>
          <qosPerSsidAverageRealTimeDownstreamRate>1</qosPerSsidAverageRealTimeDownstreamRate>
          <qosPerSsidAverageRealTimeUpstreamRate>1</qosPerSsidAverageRealTimeUpstreamRate>
          <qosPerSsidAverageUpstreamRate>1</qosPerSsidAverageUpstreamRate>
          <qosPerSsidBurstDownstreamRate>1</qosPerSsidBurstDownstreamRate>
          <qosPerSsidBurstRealTimeDownstreamRate>1</qosPerSsidBurstRealTimeDownstreamRate>
          <qosPerSsidBurstUpstreamRate>1</qosPerSsidBurstUpstreamRate>
          <qosPerUserAverageDownstreamRate>1</qosPerUserAverageDownstreamRate>
          <qosPerUserAverageRealTimeDownstreamRate>1</qosPerUserAverageRealTimeDownstreamRate>
          <qosPerUserAverageRealTimeUpstreamRate>1</qosPerUserAverageRealTimeUpstreamRate>
          <qosPerUserAverageUpstreamRate>1</qosPerUserAverageUpstreamRate>
          <qosPerUserBurstDownstreamRate>1</qosPerUserBurstDownstreamRate>
          <qosPerUserBurstRealTimeDownstreamRate>1</qosPerUserBurstRealTimeDownstreamRate>
          <qosPerUserBurstRealTimeUpstreamRate>1</qosPerUserBurstRealTimeUpstreamRate>
          <qosPerUserBurstUpstreamRate>1</qosPerUserBurstUpstreamRate>
          <qosProfile>BRONZE</qosProfile>
          <qosWmmPolicy>DISABLED</qosWmmPolicy>
          <radioPolicy>ALL</radioPolicy>
          <ssid>String value</ssid>
          <vpnPassThroughGatewayAddress>
            <address>192.168.115.243</address>
          </vpnPassThroughGatewayAddress>
          <webAuthExternalUrl>String value</webAuthExternalUrl>
          <webAuthLoginFailurePage>String value</webAuthLoginFailurePage>
          <webAuthLoginPage>String value</webAuthLoginPage>
          <webAuthLogoutPage>String value</webAuthLogoutPage>
          <webPassthruEmailInputEnabled>true</webPassthruEmailInputEnabled>
          <wepAllowSharedKeyAuthentication>true</wepAllowSharedKeyAuthentication>
          <wepKeyIndex>1</wepKeyIndex>
          <wepKeySize>WEP104</wepKeySize>
          <wepSecurityEnabled>true</wepSecurityEnabled>
          <wpa2Enabled>true</wpa2Enabled>
          <wpa2EncryptionProtocolAes>true</wpa2EncryptionProtocolAes>
          <wpa2EncryptionProtocolTkip>true</wpa2EncryptionProtocolTkip>
          <wpaAuthenticationKeyManagement8021x>true</wpaAuthenticationKeyManagement8021x>
          <wpaAuthenticationKeyManagementCckm>true</wpaAuthenticationKeyManagementCckm>
          <wpaAuthenticationKeyManagementFt8021x>true</wpaAuthenticationKeyManagementFt8021x>
          <wpaAuthenticationKeyManagementFtPsk>true</wpaAuthenticationKeyManagementFtPsk>
          <wpaAuthenticationKeyManagementPmf8021x>true</wpaAuthenticationKeyManagementPmf8021x>
          <wpaAuthenticationKeyManagementPmfPsk>true</wpaAuthenticationKeyManagementPmfPsk>
          <wpaAuthenticationKeyManagementPsk>true</wpaAuthenticationKeyManagementPsk>
          <wpaEnabled>true</wpaEnabled>
          <wpaEncryptionProtocolAes>true</wpaEncryptionProtocolAes>
          <wpaEncryptionProtocolTkip>true</wpaEncryptionProtocolTkip>
          <wpaPresharedKey>String value</wpaPresharedKey>
          <wpaPresharedKeyFormat>DEFAULT</wpaPresharedKeyFormat>
          <wpaSecurityEnabled>true</wpaSecurityEnabled>
          <x8021KeySize>WEP104</x8021KeySize>
          <x8021SecurityEnabled>true</x8021SecurityEnabled>
          <aaaRadiusAccountingWlcSpecificEnabled>true</aaaRadiusAccountingWlcSpecificEnabled>
          <aaaRadiusAuthenticationWlcSpecificEnabled>true</aaaRadiusAuthenticationWlcSpecificEnabled>
          <advancedSessionTimeoutEnabled>true</advancedSessionTimeoutEnabled>
          <hotspot2Enable>
            <hotSpot2Enabled>true</hotSpot2Enabled>
          </hotspot2Enable>
          <hotspot2Operators>
            <hotspot2Operator>
              <operatorId>1</operatorId>
              <operatorLang>String value</operatorLang>
              <operatorName>String value</operatorName>
            </hotspot2Operator>
            <hotspot2Operator>
              <operatorId>11</operatorId>
              <operatorLang>Another string value</operatorLang>
              <operatorName>Another string value</operatorName>
            </hotspot2Operator>
          </hotspot2Operators>
          <hotspot2Ports>
            <hotspot2Port>
              <portConfigId>1</portConfigId>
              <portNo>ICMPESP</portNo>
              <portStatus>CLOSED</portStatus>
              <protocolName>ICMP</protocolName>
            </hotspot2Port>
            <hotspot2Port>
              <portConfigId>11</portConfigId>
              <portNo>FTP</portNo>
              <portStatus>OPEN</portStatus>
              <protocolName>FTP</protocolName>
            </hotspot2Port>
          </hotspot2Ports>
          <hotspot2Wan>
            <downLinkSpeed>1</downLinkSpeed>
            <upLinkSpeed>1</upLinkSpeed>
            <wanLinkStatus>LINKUP</wanLinkStatus>
            <wanSymLinkStatus>SAME</wanSymLinkStatus>
          </hotspot2Wan>
          <hotspotCellularNetworks>
            <hotspotCellularNetwork>
              <countryCode>String value</countryCode>
              <gppIndex>1</gppIndex>
              <networkCode>String value</networkCode>
            </hotspotCellularNetwork>
            <hotspotCellularNetwork>
              <countryCode>Another string value</countryCode>
              <gppIndex>11</gppIndex>
              <networkCode>Another string value</networkCode>
            </hotspotCellularNetwork>
          </hotspotCellularNetworks>
          <hotspotDomains>
            <hotspotDomain>
              <domainId>1</domainId>
              <domainName>String value</domainName>
            </hotspotDomain>
            <hotspotDomain>
              <domainId>11</domainId>
              <domainName>Another string value</domainName>
            </hotspotDomain>
          </hotspotDomains>
          <hotspotGeneral>
            <heSsid>
              <octets>000a959d6816</octets>
            </heSsid>
            <internetAccess>true</internetAccess>
            <ipv4AddressAvailType>NOTAVAILABLE</ipv4AddressAvailType>
            <ipv6AddressAvailType>NOTAVAILABLE</ipv6AddressAvailType>
            <networkAuthType>ACCEPTANCE</networkAuthType>
            <networkType>PRIVATE</networkType>
            <status>true</status>
          </hotspotGeneral>
          <hotspotOuiTemplates>
            <hotspotOuiTemplate>
              <oui>String value</oui>
              <ouiId>1</ouiId>
              <ouiInBeacon>true</ouiInBeacon>
            </hotspotOuiTemplate>
            <hotspotOuiTemplate>
              <oui>Another string value</oui>
              <ouiId>11</ouiId>
              <ouiInBeacon>false</ouiInBeacon>
            </hotspotOuiTemplate>
          </hotspotOuiTemplates>
          <hotspotRealms>
            <hotspotRealm>
              <realmEapMethods>
                <realmEapMethod>
                  <innerAuthMethods>
                    <innerAuthMethod>
                      <realmEapAuthId>1</realmEapAuthId>
                      <realmEapAuthMethod>NONEAPINNERAUTH</realmEapAuthMethod>
                      <realmEapAuthParam>NONE</realmEapAuthParam>
                    </innerAuthMethod>
                    <innerAuthMethod>
                      <realmEapAuthId>11</realmEapAuthId>
                      <realmEapAuthMethod>INNERAUTHEAP</realmEapAuthMethod>
                      <realmEapAuthParam>PAP</realmEapAuthParam>
                    </innerAuthMethod>
                  </innerAuthMethods>
                  <realmEapId>1</realmEapId>
                  <realmEapMethod>NONE</realmEapMethod>
                </realmEapMethod>
                <realmEapMethod>
                  <innerAuthMethods>
                    <innerAuthMethod>
                      <realmEapAuthId>1</realmEapAuthId>
                      <realmEapAuthMethod>NONEAPINNERAUTH</realmEapAuthMethod>
                      <realmEapAuthParam>NONE</realmEapAuthParam>
                    </innerAuthMethod>
                    <innerAuthMethod>
                      <realmEapAuthId>11</realmEapAuthId>
                      <realmEapAuthMethod>INNERAUTHEAP</realmEapAuthMethod>
                      <realmEapAuthParam>PAP</realmEapAuthParam>
                    </innerAuthMethod>
                  </innerAuthMethods>
                  <realmEapId>11</realmEapId>
                  <realmEapMethod>LEAP</realmEapMethod>
                </realmEapMethod>
              </realmEapMethods>
              <realmId>1</realmId>
              <realmName>String value</realmName>
            </hotspotRealm>
            <hotspotRealm>
              <realmEapMethods>
                <realmEapMethod>
                  <innerAuthMethods>
                    <innerAuthMethod>
                      <realmEapAuthId>1</realmEapAuthId>
                      <realmEapAuthMethod>NONEAPINNERAUTH</realmEapAuthMethod>
                      <realmEapAuthParam>NONE</realmEapAuthParam>
                    </innerAuthMethod>
                    <innerAuthMethod>
                      <realmEapAuthId>11</realmEapAuthId>
                      <realmEapAuthMethod>INNERAUTHEAP</realmEapAuthMethod>
                      <realmEapAuthParam>PAP</realmEapAuthParam>
                    </innerAuthMethod>
                  </innerAuthMethods>
                  <realmEapId>1</realmEapId>
                  <realmEapMethod>NONE</realmEapMethod>
                </realmEapMethod>
                <realmEapMethod>
                  <innerAuthMethods>
                    <innerAuthMethod>
                      <realmEapAuthId>1</realmEapAuthId>
                      <realmEapAuthMethod>NONEAPINNERAUTH</realmEapAuthMethod>
                      <realmEapAuthParam>NONE</realmEapAuthParam>
                    </innerAuthMethod>
                    <innerAuthMethod>
                      <realmEapAuthId>11</realmEapAuthId>
                      <realmEapAuthMethod>INNERAUTHEAP</realmEapAuthMethod>
                      <realmEapAuthParam>PAP</realmEapAuthParam>
                    </innerAuthMethod>
                  </innerAuthMethods>
                  <realmEapId>11</realmEapId>
                  <realmEapMethod>LEAP</realmEapMethod>
                </realmEapMethod>
              </realmEapMethods>
              <realmId>11</realmId>
              <realmName>Another string value</realmName>
            </hotspotRealm>
          </hotspotRealms>
          <hotspotServiceAdvertisement>
            <msapEnable>true</msapEnable>
            <serverIndex>1</serverIndex>
          </hotspotServiceAdvertisement>
          <lastModified>2</lastModified>
          <templateName>String value</templateName>
          <wpaControllerSpecificPresharedKeyEnabled>true</wpaControllerSpecificPresharedKeyEnabled>
        </wlanTemplatesDTO>
      </entity>
    </queryResponse>

### Sample JSON Payload

https://10.64.88.203/webacs/api/v1/data/WlanTemplates/15.json

    {
      "queryResponse" : {
        "@type" : "WlanTemplates",
        "@responseType" : "getEntity",
        "@requestUrl" : "https : //10.64.88.203/webacs/api/v1/data/WlanTemplates/15",
        "@rootUrl" : "https : //10.64.88.203/webacs/api/v1/data",
        "entity" : {
          "@dtoType" : "wlanTemplatesDTO",
          "@type" : "WlanTemplates",
          "@url" : "https : //10.64.88.203/webacs/api/v1/data/WlanTemplates/15",
          "wlanTemplatesDTO" : {
            "@displayName" : "String value",
            "@id" : 15,
            "@uuid" : "String value",
            "aaaAllowOverride" : true,
            "aaaLdapPrimaryServer" : "String value",
            "aaaLdapSecondaryServer" : "String value",
            "aaaLdapTertiaryServer" : "String value",
            "aaaLocalEapAuthenticationEnabled" : true,
            "aaaLocalEapAuthenticationProfileName" : "String value",
            "aaaRadiusAccountingPrimaryServer" : "String value",
            "aaaRadiusAccountingSecondaryServer" : "String value",
            "aaaRadiusAccountingServersEnabled" : true,
            "aaaRadiusAccountingTertiaryServer" : "String value",
            "aaaRadiusAuthenticationPrimaryServer" : "String value",
            "aaaRadiusAuthenticationSecondaryServer" : "String value",
            "aaaRadiusAuthenticationServersEnabled" : true,
            "aaaRadiusAuthenticationTertiaryServer" : "String value",
            "aaaRadiusInterimUpdateEnabled" : true,
            "aaaRadiusInterimUpdateInterval" : 1,
            "adminStatus" : true,
            "advancedAironetIeEnabled" : true,
            "advancedClientExclusionEnabled" : true,
            "advancedClientExclusionTimeout" : 1,
            "advancedCoverageHoleDetectionEnabled" : true,
            "advancedDhcpAddressAssignmentRequired" : true,
            "advancedDhcpProfilingEnabled" : true,
            "advancedDhcpServerIpAddress" : {
              "address" : "192.168.115.243"
            },
            "advancedDiagnosticChannelEnabled" : true,
            "advancedDot11anDtimPeriod" : 1,
            "advancedDot11bgnDtimPeriod" : 1,
            "advancedFlexConnectCentralDhcpProcessingEnabled" : true,
            "advancedFlexConnectLearnClientIpEnabled" : true,
            "advancedFlexConnectLocalAuthEnabled" : true,
            "advancedFlexConnectLocalSwitchingEnabled" : true,
            "advancedFlexConnectNatPatEnabled" : true,
            "advancedFlexConnectOverrideDnsEnabled" : true,
            "advancedFlexConnectReapCentralAssociation" : true,
            "advancedFlexConnectVlanCentralSwitchingEnabled" : true,
            "advancedHttpProfilingEnabled" : true,
            "advancedIpv6Enabled" : true,
            "advancedKtsCacEnabled" : true,
            "advancedLoadBalancingBandSelectEnabled" : true,
            "advancedLoadBalancingEnabled" : true,
            "advancedMaximumClients" : 1,
            "advancedMdnsProfileName" : "String value",
            "advancedMdnsSnoopingEnabled" : true,
            "advancedMediaSessionSnoopingEnabled" : true,
            "advancedMfpClientProtection" : "DISABLED",
            "advancedMfpSignatureGenerationEnabled" : true,
            "advancedMfpVersion" : 1,
            "advancedOverrideInterfaceAclName" : "String value",
            "advancedOverrideInterfaceIpv6AclName" : "String value",
            "advancedPassiveClientEnabled" : true,
            "advancedPeerToPeerBlocking" : "DISABLE",
            "advancedPmipMobilityType" : "NONE",
            "advancedPmipProfile" : "String value",
            "advancedPmipRealm" : "String value",
            "advancedScanDeferPriority0" : true,
            "advancedScanDeferPriority1" : true,
            "advancedScanDeferPriority2" : true,
            "advancedScanDeferPriority3" : true,
            "advancedScanDeferPriority4" : true,
            "advancedScanDeferPriority5" : true,
            "advancedScanDeferPriority6" : true,
            "advancedScanDeferPriority7" : true,
            "advancedScanDeferTime" : 1,
            "advancedSessionTimeout" : 1,
            "advancedWifiDirectClientsPolicy" : "DISABLED",
            "broadcastSsidEnabled" : true,
            "ckipKeyIndex" : 1,
            "ckipKeyPermutationEnabled" : true,
            "ckipKeySize" : "NONE",
            "ckipMmhModeEnabled" : true,
            "ckipSecurityEnabled" : true,
            "interfaceName" : "String value",
            "interfaceType" : "INTERFACE",
            "isWiredLan" : true,
            "lanType" : "WIRELESS",
            "layer2FastTransitionEnabled" : true,
            "layer2FastTransitionOverDsEnabled" : true,
            "layer2FastTransitionReassociationTimeout" : 1,
            "layer2MacFilteringEnabled" : true,
            "layer3GlobalWebAuthEnabled" : true,
            "layer3PreauthenticationAcl" : "String value",
            "layer3PreauthenticationIpv6Acl" : "String value",
            "layer3VpnPassthroughEnabled" : true,
            "layer3WebAuthFlexAcl" : "String value",
            "layer3WebAuthType" : "DEFAULT",
            "layer3WebPolicyAuthenticationEnabled" : true,
            "layer3WebPolicyConditionalRedirectEnabled" : true,
            "layer3WebPolicyOnMacFailureEnabled" : true,
            "layer3WebPolicyPassthroughEnabled" : true,
            "multicastVlanEnabled" : true,
            "multicastVlanInterface" : "String value",
            "profileName" : "String value",
            "qos7920Cac" : "DISABLED",
            "qosAvcProfileName" : "String value",
            "qosNbarVisibilityEnabled" : true,
            "qosNetflowMonitor" : "String value",
            "qosPerSSidBurstRealTimeUpstreamRate" : 1,
            "qosPerSsidAverageDownstreamRate" : 1,
            "qosPerSsidAverageRealTimeDownstreamRate" : 1,
            "qosPerSsidAverageRealTimeUpstreamRate" : 1,
            "qosPerSsidAverageUpstreamRate" : 1,
            "qosPerSsidBurstDownstreamRate" : 1,
            "qosPerSsidBurstRealTimeDownstreamRate" : 1,
            "qosPerSsidBurstUpstreamRate" : 1,
            "qosPerUserAverageDownstreamRate" : 1,
            "qosPerUserAverageRealTimeDownstreamRate" : 1,
            "qosPerUserAverageRealTimeUpstreamRate" : 1,
            "qosPerUserAverageUpstreamRate" : 1,
            "qosPerUserBurstDownstreamRate" : 1,
            "qosPerUserBurstRealTimeDownstreamRate" : 1,
            "qosPerUserBurstRealTimeUpstreamRate" : 1,
            "qosPerUserBurstUpstreamRate" : 1,
            "qosProfile" : "BRONZE",
            "qosWmmPolicy" : "DISABLED",
            "radioPolicy" : "ALL",
            "ssid" : "String value",
            "vpnPassThroughGatewayAddress" : {
              "address" : "192.168.115.243"
            },
            "webAuthExternalUrl" : "String value",
            "webAuthLoginFailurePage" : "String value",
            "webAuthLoginPage" : "String value",
            "webAuthLogoutPage" : "String value",
            "webPassthruEmailInputEnabled" : true,
            "wepAllowSharedKeyAuthentication" : true,
            "wepKeyIndex" : 1,
            "wepKeySize" : "WEP104",
            "wepSecurityEnabled" : true,
            "wpa2Enabled" : true,
            "wpa2EncryptionProtocolAes" : true,
            "wpa2EncryptionProtocolTkip" : true,
            "wpaAuthenticationKeyManagement8021x" : true,
            "wpaAuthenticationKeyManagementCckm" : true,
            "wpaAuthenticationKeyManagementFt8021x" : true,
            "wpaAuthenticationKeyManagementFtPsk" : true,
            "wpaAuthenticationKeyManagementPmf8021x" : true,
            "wpaAuthenticationKeyManagementPmfPsk" : true,
            "wpaAuthenticationKeyManagementPsk" : true,
            "wpaEnabled" : true,
            "wpaEncryptionProtocolAes" : true,
            "wpaEncryptionProtocolTkip" : true,
            "wpaPresharedKey" : "String value",
            "wpaPresharedKeyFormat" : "DEFAULT",
            "wpaSecurityEnabled" : true,
            "x8021KeySize" : "WEP104",
            "x8021SecurityEnabled" : true,
            "aaaRadiusAccountingWlcSpecificEnabled" : true,
            "aaaRadiusAuthenticationWlcSpecificEnabled" : true,
            "advancedSessionTimeoutEnabled" : true,
            "hotspot2Enable" : {
              "hotSpot2Enabled" : true
            },
            "hotspot2Operators" : {
              "hotspot2Operator" : [{
                "operatorId" : 1,
                "operatorLang" : "String value",
                "operatorName" : "String value"
              },
              {
                "operatorId" : 11,
                "operatorLang" : "Another string value",
                "operatorName" : "Another string value"
              }]
            },
            "hotspot2Ports" : {
              "hotspot2Port" : [{
                "portConfigId" : 1,
                "portNo" : "ICMPESP",
                "portStatus" : "CLOSED",
                "protocolName" : "ICMP"
              },
              {
                "portConfigId" : 11,
                "portNo" : "FTP",
                "portStatus" : "OPEN",
                "protocolName" : "FTP"
              }]
            },
            "hotspot2Wan" : {
              "downLinkSpeed" : 1,
              "upLinkSpeed" : 1,
              "wanLinkStatus" : "LINKUP",
              "wanSymLinkStatus" : "SAME"
            },
            "hotspotCellularNetworks" : {
              "hotspotCellularNetwork" : [{
                "countryCode" : "String value",
                "gppIndex" : 1,
                "networkCode" : "String value"
              },
              {
                "countryCode" : "Another string value",
                "gppIndex" : 11,
                "networkCode" : "Another string value"
              }]
            },
            "hotspotDomains" : {
              "hotspotDomain" : [{
                "domainId" : 1,
                "domainName" : "String value"
              },
              {
                "domainId" : 11,
                "domainName" : "Another string value"
              }]
            },
            "hotspotGeneral" : {
              "heSsid" : {
                "octets" : "000a959d6816"
              },
              "internetAccess" : true,
              "ipv4AddressAvailType" : "NOTAVAILABLE",
              "ipv6AddressAvailType" : "NOTAVAILABLE",
              "networkAuthType" : "ACCEPTANCE",
              "networkType" : "PRIVATE",
              "status" : true
            },
            "hotspotOuiTemplates" : {
              "hotspotOuiTemplate" : [{
                "oui" : "String value",
                "ouiId" : 1,
                "ouiInBeacon" : true
              },
              {
                "oui" : "Another string value",
                "ouiId" : 11,
                "ouiInBeacon" : false
              }]
            },
            "hotspotRealms" : {
              "hotspotRealm" : [{
                "realmEapMethods" : {
                  "realmEapMethod" : [{
                    "innerAuthMethods" : {
                      "innerAuthMethod" : [{
                        "realmEapAuthId" : 1,
                        "realmEapAuthMethod" : "NONEAPINNERAUTH",
                        "realmEapAuthParam" : "NONE"
                      },
                      {
                        "realmEapAuthId" : 11,
                        "realmEapAuthMethod" : "INNERAUTHEAP",
                        "realmEapAuthParam" : "PAP"
                      }]
                    },
                    "realmEapId" : 1,
                    "realmEapMethod" : "NONE"
                  },
                  {
                    "innerAuthMethods" : {
                      "innerAuthMethod" : [{
                        "realmEapAuthId" : 1,
                        "realmEapAuthMethod" : "NONEAPINNERAUTH",
                        "realmEapAuthParam" : "NONE"
                      },
                      {
                        "realmEapAuthId" : 11,
                        "realmEapAuthMethod" : "INNERAUTHEAP",
                        "realmEapAuthParam" : "PAP"
                      }]
                    },
                    "realmEapId" : 11,
                    "realmEapMethod" : "LEAP"
                  }]
                },
                "realmId" : 1,
                "realmName" : "String value"
              },
              {
                "realmEapMethods" : {
                  "realmEapMethod" : [{
                    "innerAuthMethods" : {
                      "innerAuthMethod" : [{
                        "realmEapAuthId" : 1,
                        "realmEapAuthMethod" : "NONEAPINNERAUTH",
                        "realmEapAuthParam" : "NONE"
                      },
                      {
                        "realmEapAuthId" : 11,
                        "realmEapAuthMethod" : "INNERAUTHEAP",
                        "realmEapAuthParam" : "PAP"
                      }]
                    },
                    "realmEapId" : 1,
                    "realmEapMethod" : "NONE"
                  },
                  {
                    "innerAuthMethods" : {
                      "innerAuthMethod" : [{
                        "realmEapAuthId" : 1,
                        "realmEapAuthMethod" : "NONEAPINNERAUTH",
                        "realmEapAuthParam" : "NONE"
                      },
                      {
                        "realmEapAuthId" : 11,
                        "realmEapAuthMethod" : "INNERAUTHEAP",
                        "realmEapAuthParam" : "PAP"
                      }]
                    },
                    "realmEapId" : 11,
                    "realmEapMethod" : "LEAP"
                  }]
                },
                "realmId" : 11,
                "realmName" : "Another string value"
              }]
            },
            "hotspotServiceAdvertisement" : {
              "msapEnable" : true,
              "serverIndex" : 1
            },
            "lastModified" : 2,
            "templateName" : "String value",
            "wpaControllerSpecificPresharedKeyEnabled" : true
          }
        }
      }
    }

### Resource Information

Rate Limiting? | Yes
Sorting? | Yes
Paging? | Yes
Filtering? | Yes
Group Filtering? | No
Aggregation? | No
Response Formats | xml json
User Group | NBI Read
HTTP Methods | GET

## Resource URL

/webacs/api/v2/data/WlanTemplates

Unmodified

This resource has not been modified since the previous API version.

## Response Parameters

Attribute | Description
--- | ---
aaaAllowOverride boolean | Is allow AAA override enabled?
aaaLdapPrimaryServer String | Primary LDAP server.
aaaLdapSecondaryServer String | Secondary LDAP server.
aaaLdapTertiaryServer String | Tertiary LDAP server.
aaaLocalEapAuthenticationEnabled boolean | Is local EAP authentication enabled?
aaaLocalEapAuthenticationProfileName String | When aaaLocalEapAuthenticationEnabled is true, this defines the EAP profile that will be used.
aaaRadiusAccountingPrimaryServer String | When aaaRadiusAccountingServersEnabled is true, this is the primary RADIUS accounting server.
aaaRadiusAccountingSecondaryServer String | When aaaRadiusAccountingServersEnabled is true, this is the secondary RADIUS accounting server.
aaaRadiusAccountingServersEnabled boolean | Is RADIUS accounting enabled?
aaaRadiusAccountingTertiaryServer String | When aaaRadiusAccountingServersEnabled is true, this is the tertiary RADIUS accounting server.
aaaRadiusAccountingWlcSpecificEnabled boolean | Is controller specific RADIUS accounting servers enabled?
aaaRadiusAuthenticationPrimaryServer String | When aaaRadiusAuthenticationServersEnabled is true, this is the primary RADIUS authentication server.
aaaRadiusAuthenticationSecondaryServer String | When aaaRadiusAuthenticationServersEnabled is true, this is the secondary RADIUS authentication server.
aaaRadiusAuthenticationServersEnabled boolean | Is RADIUS authentication enabled?
aaaRadiusAuthenticationTertiaryServer String | When aaaRadiusAuthenticationServersEnabled is true, this is the tertiary RADIUS authentication server.
aaaRadiusAuthenticationWlcSpecificEnabled boolean | Is controller specific RADIUS authentication servers enabled?
aaaRadiusInterimUpdateEnabled boolean | Is RADIUS server accounting interim update enabled?
aaaRadiusInterimUpdateInterval int | When aaaRadiusInterimUpdateEnabled is true, this determines the update interval. Measured in seconds.
adminStatus boolean | Is the WLAN administratively enabled?
advancedAironetIeEnabled boolean | Is Aironet Information Elements (IEs) enabled for this WLAN?
advancedClientExclusionEnabled boolean | Is automatic client exclusion enabled for this WLAN?
advancedClientExclusionTimeout int | When advancedClientExclusionEnabled is true, this denotes the length of the timeout. A value of zero represents an infinite timeout. Measured in seconds.
advancedCoverageHoleDetectionEnabled boolean | Is Coverage Hole Detection enabled for this WLAN?
advancedDhcpAddressAssignmentRequired boolean | Are all clients required to obtain an IP address from the DHCP server for this WLAN?
advancedDhcpProfilingEnabled boolean | Should the wireless controller collect the DHCP attributes of clients on this WLAN?
advancedDhcpServerIpAddress InetAddress | If this contains a valid address, an IPv4 DHCP server has been specified for this WLAN.
advancedDiagnosticChannelEnabled boolean | Is the diagnostic channel available for this WLAN?
advancedDot11anDtimPeriod int | Denotes the Delivery Traffic Indication Map (DTIM) interval for 802.11a/n radios, during which broadcast and multicast frames will be transmitted. A value of one results in a broadcast after every beacon, two for every other beacon, and so on.
advancedDot11bgnDtimPeriod int | Denotes the Delivery Traffic Indication Map (DTIM) interval for 802.11b/g/n radios, during which broadcast and multicast frames will be transmitted. A value of one results in a broadcast after every beacon, two for every other beacon, and so on.
advancedFlexConnectCentralDhcpProcessingEnabled boolean | Are DHCP packets received by the access point sent to the controller then forwarded to the WLAN's corresponding VLAN?
advancedFlexConnectLearnClientIpEnabled boolean | Is client IP address learning enabled?
advancedFlexConnectLocalAuthEnabled boolean | Is local authentication enabled?
advancedFlexConnectLocalSwitchingEnabled boolean | When true, access points will locally switch traffic, rather than forwarding to the wireless controller.
advancedFlexConnectNatPatEnabled boolean | Is Network Address Translation (NAT) and Port Address Translation (PAT) enabled?
advancedFlexConnectOverrideDnsEnabled boolean | When true, clients are given the DNS server of the access point rather than of the WLAN's configured interface.
advancedFlexConnectReapCentralAssociation boolean | Is Reap Central Association enabled?
advancedFlexConnectVlanCentralSwitchingEnabled boolean | Is VLAN based central switching enabled?
advancedHttpProfilingEnabled boolean | Should the wireless controller collect the HTTP attributes of clients on this WLAN?
advancedIpv6Enabled boolean | Is IPv6 enabled?
advancedKtsCacEnabled boolean | Is CAC based on the Key Telephone System (KTS) enabled on this WLAN?
advancedLoadBalancingBandSelectEnabled boolean | Is client band select enabled?
advancedLoadBalancingEnabled boolean | Is client load balancing enabled?
advancedMaximumClients int | Denotes the maximum number of clients. A value of zero means unlimited.
advancedMdnsProfileName String | When advancedMdnsSnoopingEnabled is true, this denotes the mDNS profile. Clients receive service advertisements only for the services associated with the profile.
advancedMdnsSnoopingEnabled boolean | Is mDNS snooping enabled?
advancedMediaSessionSnoopingEnabled boolean | Should the access point snoop on Session Initiation Protocol (SIP) traffic, and report back to the controller the establishment termination and failure of voice calls?
advancedMfpClientProtection DisabledEnabledRequiredEnum | Denotes whether client management frame protection (MFP) is enabled (optional), required, or disabled for this WLAN. Allowed values DISABLED ENABLED REQUIRED
advancedMfpSignatureGenerationEnabled boolean | Do 802.11 management frames transmitted by the access point have a signature to verify authenticity?
advancedMfpVersion int | Denotes the version of management frame protection (MFP).
advancedOverrideInterfaceAclName String | Denotes an IPv4 ACL that overrides the ACL configured for the WLAN's interface.
advancedOverrideInterfaceIpv6AclName String | Denotes an IPv6 ACL that overrides the ACL configured for the WLAN's interface.
advancedPassiveClientEnabled boolean | Should the controller forward ARP requests out to the WLAN for passive clients?
advancedPeerToPeerBlocking Peer2PeerBlockingEnum | Denotes whether peer-to-peer blocking is disabled, enabled, or if the packets are forwarded to the next device. Allowed values DISABLE DROP FORWARDUP ALLOWPRIVATEGROUP
advancedPmipMobilityType PmipMobilityTypeEnum | Denotes the Proxy Mobile IP (PMIP) type for this WLAN. Allowed values NONE PMIP
advancedPmipProfile String | Denotes the Proxy Mobile IP (PMIP) profile for this WLAN.
advancedPmipRealm String | Denotes the default realm of the Proxy Mobile IPv6 (PMIPv6) WLAN.
advancedScanDeferPriority0 boolean | Is priority 0 for the channel scan enabled?
advancedScanDeferPriority1 boolean | Is priority 1 for the channel scan enabled?
advancedScanDeferPriority2 boolean | Is priority 2 for the channel scan enabled?
advancedScanDeferPriority3 boolean | Is priority 3 for the channel scan enabled?
advancedScanDeferPriority4 boolean | Is priority 4 for the channel scan enabled?
advancedScanDeferPriority5 boolean | Is priority 5 for the channel scan enabled?
advancedScanDeferPriority6 boolean | Is priority 6 for the channel scan enabled?
advancedScanDeferPriority7 boolean | Is priority 7 for the channel scan enabled?
advancedScanDeferTime int | Denotes the channel scan defer time. Measured in milliseconds.
advancedSessionTimeout int | Denotes the maximum time for a client session before requiring reauthentication. Zero means no timeout. Measured in seconds.
advancedSessionTimeoutEnabled boolean | Is advancedSessionTimeout enabled?
advancedWifiDirectClientsPolicy DisabledAllowedNotAllowedEnum | Denotes the Wi-Fi Direct Clients Policy for this WLAN. Allowed values DISABLED ALLOWED NOTALLOWED XCONNECTNOTALLOW
broadcastSsidEnabled boolean | Is SSID broadcasting enabled?
ckipKeyIndex int | When ckipSecurityEnabled is true, this denotes the key index.
ckipKeyPermutationEnabled boolean | When ckipSecurityEnabled is true, this denotes whether key permutation is enabled.
ckipKeySize CkipEncryptionTypeEnum | When ckipSecurityEnabled is true, this denotes the key size. Allowed values NONE LEN40 LEN104
ckipMmhModeEnabled boolean | When ckipSecurityEnabled is true, this denotes whether multimodular mode hashing is enabled.
ckipSecurityEnabled boolean | Is CKIP layer 2 security enabled?
hotspot2Enable WlanMcHotSpotEnableTemplate | This attribute represents enablement of HotSpot 2.0.
Attribute | Description
--- | ---
hotSpot2Enabled boolean | Is HotSpot 2.0 enabled?
hotspot2Operators WlanMcHotSpotOperatorConfigTemplate[] | These attributes represent HotSpot 2.0 operators.
Attribute | Description
--- | ---
operatorId int | Operator index of the hotspot provider.
operatorLang String | Language code.
operatorName String | Operator name of the hotspot provider.
hotspot2Ports WlanMcHotSpotPortConfigTemplate[] | These attributes represent HotSpot 2.0 port configurations.
Attribute | Description
--- | ---
portConfigId int | Port configuration index.
portNo PortNoEnum | Port number used for the IP. Allowed values ICMPESP FTP SSH HTTP TTLSVPN PPTPVPN VOIP IKEV2 IPSECNAT
portStatus PortStatusEnum | Status of the IP port. Allowed values CLOSED OPEN UNKNOWN
protocolName ProtocolNameEnum | Internet protocol name. This parameter provides information on the connection status of the most commonly used communication protocols and ports. Allowed values ICMP FTP IKEV2 ESP
hotspot2Wan WlanMcHotSpotWanTemplate | These attributes represent HotSpot 2.0 WAN metrics configuration.
Attribute | Description
--- | ---
downLinkSpeed int | Downlink speed of the WAN backhaul link. Measured in Kbps.
upLinkSpeed int | Uplink speed of the WAN backhaul. Measured in Kbps.
wanLinkStatus WanLinkStatusEnum | WAN link status. Allowed values LINKUP LINKDOWN LINKINTESTSTATE NOTCONFIGURED
wanSymLinkStatus WanSymLinkStatusEnum | WAN symmetric link status. Allowed values SAME DIFFERENT
hotspotCellularNetworks WlanMc3GppConfigTemplate[] | These attributes represent 802.11u cellular network parameters.
Attribute | Description
--- | ---
countryCode String | Mobile country code in Binary Coded Decimal (BCD) format.
gppIndex int | Cellular index.
networkCode String | Mobile network code in Binary Coded Decimal (BCD) format.
hotspotDomains WlanMcDomainConfigTemplate[] | These attributes represent 802.11u domains.
Attribute | Description
--- | ---
domainId int | Domain index.
domainName String | Domain name operating in the WLAN network.
hotspotGeneral WlanMcGeneralConfigTemplate | These attributes represent 802.11u general parameters.
Attribute | Description
--- | ---
heSsid MacAddress | The Homogenous Extended Service Set Identifier (HESSID).
internetAccess boolean | Is Internet Access enabled?
ipv4AddressAvailType IPv4AddressAvailTypeEnum | IPv4 type address. Allowed values NOTAVAILABLE PUBLIC PORTRESTRICTED SINGLENATPRIVATE DOUBLENATPRIVATE PORTRESTRICTEDSINGLENATPRIVATE PORTRESTRICTEDDOUBLENATPRIVATE UNKNOWN
ipv6AddressAvailType IPv6AddressAvailTypeEnum | IPv6 type address. Allowed values NOTAVAILABLE AVAILABLE UNKNOWN
networkAuthType NetworkAuthTypeEnum | Network authentication type for 802.11u on this WLAN. Allowed values ACCEPTANCE ENROLLMENT REDIRECTION DNSREDIRECTION NOTCONFIGURED
networkType NetworkTypeEnum | Network type of this WLAN. Allowed values PRIVATE PRIVATEWITHGUESTACCESS PUBLICPAID PUBLICFREE PERSONALDEVICE EMERGENCYSERVICEONLY TESTEQUIPMENT WILDCARD UNKNOWN
status boolean | Is 802.11u enabled?
hotspotOuiTemplate WlanMcOuiConfigTemplate[] | These attributes represent 802.11u OUIs.
Attribute | Description
--- | ---
oui String | Organization Unique Identifier (OUI).
ouiId int | OUI index.
ouiInBeacon boolean | Are Organization Unique Identifier (OUI) beacon responses enabled?
hotspotRealms WlanMcRealmConfigTemplate[] | These attributes represent 802.11u realms.
Attribute | Description
--- | ---
realmEapMethods WlanMcRealmEapConfigTemplate[] | Extensible Authentication Protocol (EAP) list.
Attribute | Description
--- | ---
innerAuthMethods WlanMcRealmEapAuthConfigTemplate[] | Auth method list.
Attribute | Description
--- | ---
realmEapAuthId int | Auth method index.
realmEapAuthMethod RealmEapAuthMethodEnum | Inner auth method. Allowed values NONEAPINNERAUTH INNERAUTHEAP CREDENTIAL TUNNELEDEAPCREDENTIAL
realmEapAuthParam RealmEapAuthParamEnum | Auth param. Allowed values NONE PAP CHAP MSCHAP MSCHAPV2 LEAP PEAP EAPTLS EAPFAST EAPSIM EAPTTLS EAPAKA SIM USIM NFCSECURE HARDWARETOKEN SOFTTOKEN CERTIFICATE USERNAMEPASSWORD RESERVED ANONYMOUS VENDORSPECIFIC
realmEapId int | EAP index.
realmEapMethod RealmEapMethodEnum | EAP method for the realm in the WLAN. Allowed values NONE LEAP EAPPEAP EAPTLS EAPFAST EAPSIM EAPTTLS EAPAKA
realmId int | Realm index.
realmName String | Realm name.
hotspotServiceAdvertisement WlanMcServiceAdConfigTemplate | These attributes represent MSAP (Mobility Service Advertisement Protocol) parameters.
Attribute | Description
--- | ---
msapEnable boolean | Is Mobility Service Advertisement Protocol (MSAP) enabled?
serverIndex int | Server index.
interfaceName String | Denotes the interface, or interface group, for this WLAN. See interfaceType to determine if this is an interface or interface group.
interfaceType InterfaceMappingTypeEnum | Denotes whether an interface or interface group is used for this interface. See interfaceName for the name of the interface or interface group. Allowed values INTERFACE INTERFACEGROUP
isWiredLan boolean | Is this a wired LAN?
lanType LanTypeEnum | Denotes the LAN type. Allowed values WIRELESS GUEST REMOTE
lastModified long | The time the template was last modified. Measured in milliseconds since the Unix epoch.
layer2FastTransitionEnabled boolean | Is fast transition (FT) between access points enabled?
layer2FastTransitionOverDsEnabled boolean | When layer2FastTransitionEnabled is true, the denotes whether fast transition over a distributed system is enabled.
layer2FastTransitionReassociationTimeout int | When layer2FastTransitionEnabled is true, this denotes the transition timeout. Measured in seconds.
layer2MacFilteringEnabled boolean | Is MAC filtering enabled?
layer3GlobalWebAuthEnabled boolean | When a layer 3 web policy is true, this denotes whether the template uses global or template-defined Web Auth configuration.
layer3PreauthenticationAcl String | When a layer 3 web policy is true, this denotes the IPv4 ACL for traffic between the client and the wireless controller.
layer3PreauthenticationIpv6Acl String | When a layer 3 web policy is true, this denotes the IPv6 ACL for traffic between the client and the wireless controller.
layer3VpnPassthroughEnabled boolean | Is VPN passthrough enabled?
layer3WebAuthFlexAcl String | When a layer 3 web policy is true, this denotes the the FlexConnect ACL for external web authentication in locally switched WLANs.
layer3WebAuthType WlanWebAuthTypeEnum | When a layer 3 web policy is true and layer3GlobalWebAuth is false, this denotes the type of web authentication to be used. Allowed values DEFAULT CUSTOMIZED EXTERNAL
layer3WebPolicyAuthenticationEnabled boolean | Is the authentication web policy enabled?
layer3WebPolicyConditionalRedirectEnabled boolean | Is the conditional redirect web policy enabled?
layer3WebPolicyOnMacFailureEnabled boolean | Is the WebAuth on MAC failure web policy enabled?
layer3WebPolicyPassthroughEnabled boolean | Is the passthrough web policy enabled?
multicastVlanEnabled boolean | Is a multicast VLAN enabled?
multicastVlanInterface String | When multicastVlanInterface is true, this denotes the multicast VLAN.
profileName String | Profile name of the WLAN.
qos7920Cac PhoneSupport7920Enum | Denotes the Call Admission Control (CAC) configuration for Cisco 7920 phones. Allowed values DISABLED CLIENTCAC APCAC CLIENTANDAPCAC
qosAvcProfileName String | Denotes the Application Visibility and Control (AVC) profile for this WLAN.
qosNbarVisibilityEnabled boolean | Is Network Based Application Recognition (NBAR) deep packet inspection enabled on this WLAN?
qosNetflowMonitor String | Denotes the Netflow monitor configured for this WLAN.
qosPerSSidBurstRealTimeUpstreamRate int | Denotes the peak data rate limit for upstream UDP traffic for the WLAN. Zero means no restriction. Measured in Kbps.
qosPerSsidAverageDownstreamRate int | Denotes the average data rate limit for downstream TCP traffic for the WLAN. Zero means no restriction. Measured in Kbps.
qosPerSsidAverageRealTimeDownstreamRate int | Denotes the average data rate limit for downstream UDP traffic for the WLAN. Zero means no restriction. Measured in Kbps.
qosPerSsidAverageRealTimeUpstreamRate int | Denotes the average data rate limit for upstream UDP traffic for the WLAN. Zero means no restriction. Measured in Kbps.
qosPerSsidAverageUpstreamRate int | Denotes the average data rate limit for upstream TCP traffic for the WLAN. Zero means no restriction. Measured in Kbps.
qosPerSsidBurstDownstreamRate int | Denotes the peak data rate limit for downstream TCP traffic for the WLAN. Zero means no restriction. Measured in Kbps.
qosPerSsidBurstRealTimeDownstreamRate int | Denotes the peak data rate limit for downstream UDP traffic for the WLAN. Zero means no restriction. Measured in Kbps.
qosPerSsidBurstUpstreamRate int | Denotes the peak data rate limit for upstream TCP traffic for the WLAN. Zero means no restriction. Measured in Kbps.
qosPerUserAverageDownstreamRate int | Denotes the average data rate limit for downstream TCP traffic for a client. Zero means no restriction. Measured in Kbps.
qosPerUserAverageRealTimeDownstreamRate int | Denotes the average data rate limit for downstream UDP traffic for a client. Zero means no restriction. Measured in Kbps.
qosPerUserAverageRealTimeUpstreamRate int | Denotes the average data rate limit for upstream UDP traffic for a client. Zero means no restriction. Measured in Kbps.
qosPerUserAverageUpstreamRate int | Denotes the average data rate limit for upstream TCP traffic for a client. Zero means no restriction. Measured in Kbps.
qosPerUserBurstDownstreamRate int | Denotes the peak data rate limit for downstream TCP traffic for a client. Zero means no restriction. Measured in Kbps.
qosPerUserBurstRealTimeDownstreamRate int | Denotes the peak data rate limit for downstream UDP traffic for a client. Zero means no restriction. Measured in Kbps.
qosPerUserBurstRealTimeUpstreamRate int | Denotes the peak data rate limit for upstream UDP traffic for a client. Zero means no restriction. Measured in Kbps.
qosPerUserBurstUpstreamRate int | Denotes the peak data rate limit for upstream TCP traffic for a client. Zero means no restriction. Measured in Kbps.
qosProfile QosEnum | Denotes the QoS level for the WLAN. Allowed values BRONZE SILVER GOLD PLATINUM
qosWmmPolicy DisabledAllowedRequiredEnum | Denotes the state of the Wi-fi Multimedia (WMM) policy for this WLAN. Allowed values DISABLED ALLOWED REQUIRED
radioPolicy RadioPolicyEnum | Denotes the WLAN radio policy. Allowed values ALL ONLY80211A ONLY80211B ONLY80211G ONLY80211BG ONLY80211AG ONLY80211AB NONE REMOTELAN
ssid String | SSID of the WLAN.
templateName String | The name of the WLAN template.
vpnPassThroughGatewayAddress InetAddress | When layer3VpnPassthroughEnabled is true, this denotes the IP address of the VPN gateway.
webAuthExternalUrl String | When a layer 3 web policy is enabled, layer3GlobalWebAuthEnabled is false, and layer3WebAuthType is set to "External", this denotes the URL of the authentication server.
webAuthLoginFailurePage String | When a layer 3 web policy is enabled, layer3GlobalWebAuthEnabled is false, and layer3WebAuthType is set to "Customized", this denotes the page for authentication failures.
webAuthLoginPage String | When a layer 3 web policy is enabled, layer3GlobalWebAuthEnabled is false, and layer3WebAuthType is set to "Customized", this denotes the page for authentication.
webAuthLogoutPage String | When a layer 3 web policy is enabled, layer3GlobalWebAuthEnabled is false, and layer3WebAuthType is set to "Customized", this denotes the page for logout.
webPassthruEmailInputEnabled boolean | When layer3WebPolicyPassthroughEnabled is true, this denotes whether the client is prompted to enter an email address when connecting.
wepAllowSharedKeyAuthentication boolean | When wepSecurityEnabled is true, this denotes whether shared key authentication is enabled.
wepKeyIndex int | When wepSecurityEnabled is true, this denotes the key index.
wepKeySize WepEncryptionTypeEnum | When wepSecurityEnabled is true, this denotes whether shared key authentication is enabled. Allowed values WEP104 NONE WEP40 WEP128 AESOCB128 WEP_40 WEP_104
wepSecurityEnabled boolean | Is WEP layer 2 security enabled?
wpa2Enabled boolean | When wpaSecurityEnabled is true, this denotes whether the WPA2 policy is enabled.
wpa2EncryptionProtocolAes boolean | When wpaSecurityEnabled and wpa2Enabled are true, this denotes whether AES encryption is supported for the WPA2 policy.
wpa2EncryptionProtocolTkip boolean | When wpaSecurityEnabled and wpa2Enabled are true, this denotes whether TKIP encryption is supported for the WPA2 policy.
wpaAuthenticationKeyManagement8021x boolean | When wpaSecurityEnabled is true, this denotes whether 802.1X key management is enabled.
wpaAuthenticationKeyManagementCckm boolean | When wpaSecurityEnabled is true, this denotes whether Cisco Centralized Key Management (CCKM) is enabled.
wpaAuthenticationKeyManagementFt8021x boolean | When wpaSecurityEnabled is true, this denotes whether Fast Transition (FT) 802.1X key management is enabled.
wpaAuthenticationKeyManagementFtPsk boolean | When wpaSecurityEnabled is true, this denotes whether Fast Transition (FT) preshared key management is enabled.
wpaAuthenticationKeyManagementPmf8021x boolean | When wpaSecurityEnabled is true, this denotes whether Protected Management Frame (PMF) 802.1X key management is enabled.
wpaAuthenticationKeyManagementPmfPsk boolean | When wpaSecurityEnabled is true, this denotes whether Protected Management Frame (PMF) preshared key management is enabled.
wpaAuthenticationKeyManagementPsk boolean | When wpaSecurityEnabled is true, this denotes whether preshared key management is enabled.
wpaControllerSpecificPresharedKeyEnabled boolean | Is controller specific preshared key enabled?
wpaEnabled boolean | When wpaSecurityEnabled is true, this denotes whether the WPA1 policy is enabled.
wpaEncryptionProtocolAes boolean | When wpaSecurityEnabled and wpaEnabled are both true, this denotes whether AES encryption is supported for the WPA1 policy.
wpaEncryptionProtocolTkip boolean | When wpaSecurityEnabled and wpaEnabled are both true, this denotes whether TKIP encryption is supported for the WPA1 policy.
wpaPresharedKey String | When wpaSecurityEnabled is true, this contains preshared key in HEX or ASCII format.
wpaPresharedKeyFormat PskFormatEnum | When wpaSecurityEnabled is true, this denotes preshared key format. Allowed values DEFAULT HEX ASCII
wpaSecurityEnabled boolean | Is WPA layer 2 security enabled?
x8021KeySize x8021EncryptionTypeEnum | When x8021SecurityEnabled is true, this denotes the 802.1X key size. Allowed values WEP104 WEP40 WEP128 NONE WEP_40 WEP_104
x8021SecurityEnabled boolean | Is 802.1X layer 2 security enabled?

## Sample Payloads

Sample payloads are for information only. They are automatically generated and the values included may not be representative of actual valid data values.

### Sample XML Payload

https://10.64.88.203/webacs/api/v2/data/WlanTemplates/15

    <?xml version="1.0" ?>
    <queryResponse type="WlanTemplates" responseType="getEntity" requestUrl="https://10.64.88.203/webacs/api/v2/data/WlanTemplates/15" rootUrl="https://10.64.88.203/webacs/api/v2/data">
      <entity dtoType="wlanTemplatesDTO" type="WlanTemplates" url="https://10.64.88.203/webacs/api/v2/data/WlanTemplates/15">
        <wlanTemplatesDTO displayName="String value" id="15" uuid="String value">
          <aaaAllowOverride>true</aaaAllowOverride>
          <aaaLdapPrimaryServer>String value</aaaLdapPrimaryServer>
          <aaaLdapSecondaryServer>String value</aaaLdapSecondaryServer>
          <aaaLdapTertiaryServer>String value</aaaLdapTertiaryServer>
          <aaaLocalEapAuthenticationEnabled>true</aaaLocalEapAuthenticationEnabled>
          <aaaLocalEapAuthenticationProfileName>String value</aaaLocalEapAuthenticationProfileName>
          <aaaRadiusAccountingPrimaryServer>String value</aaaRadiusAccountingPrimaryServer>
          <aaaRadiusAccountingSecondaryServer>String value</aaaRadiusAccountingSecondaryServer>
          <aaaRadiusAccountingServersEnabled>true</aaaRadiusAccountingServersEnabled>
          <aaaRadiusAccountingTertiaryServer>String value</aaaRadiusAccountingTertiaryServer>
          <aaaRadiusAuthenticationPrimaryServer>String value</aaaRadiusAuthenticationPrimaryServer>
          <aaaRadiusAuthenticationSecondaryServer>String value</aaaRadiusAuthenticationSecondaryServer>
          <aaaRadiusAuthenticationServersEnabled>true</aaaRadiusAuthenticationServersEnabled>
          <aaaRadiusAuthenticationTertiaryServer>String value</aaaRadiusAuthenticationTertiaryServer>
          <aaaRadiusInterimUpdateEnabled>true</aaaRadiusInterimUpdateEnabled>
          <aaaRadiusInterimUpdateInterval>1</aaaRadiusInterimUpdateInterval>
          <adminStatus>true</adminStatus>
          <advancedAironetIeEnabled>true</advancedAironetIeEnabled>
          <advancedClientExclusionEnabled>true</advancedClientExclusionEnabled>
          <advancedClientExclusionTimeout>1</advancedClientExclusionTimeout>
          <advancedCoverageHoleDetectionEnabled>true</advancedCoverageHoleDetectionEnabled>
          <advancedDhcpAddressAssignmentRequired>true</advancedDhcpAddressAssignmentRequired>
          <advancedDhcpProfilingEnabled>true</advancedDhcpProfilingEnabled>
          <advancedDhcpServerIpAddress>
            <address>192.168.115.243</address>
          </advancedDhcpServerIpAddress>
          <advancedDiagnosticChannelEnabled>true</advancedDiagnosticChannelEnabled>
          <advancedDot11anDtimPeriod>1</advancedDot11anDtimPeriod>
          <advancedDot11bgnDtimPeriod>1</advancedDot11bgnDtimPeriod>
          <advancedFlexConnectCentralDhcpProcessingEnabled>true</advancedFlexConnectCentralDhcpProcessingEnabled>
          <advancedFlexConnectLearnClientIpEnabled>true</advancedFlexConnectLearnClientIpEnabled>
          <advancedFlexConnectLocalAuthEnabled>true</advancedFlexConnectLocalAuthEnabled>
          <advancedFlexConnectLocalSwitchingEnabled>true</advancedFlexConnectLocalSwitchingEnabled>
          <advancedFlexConnectNatPatEnabled>true</advancedFlexConnectNatPatEnabled>
          <advancedFlexConnectOverrideDnsEnabled>true</advancedFlexConnectOverrideDnsEnabled>
          <advancedFlexConnectReapCentralAssociation>true</advancedFlexConnectReapCentralAssociation>
          <advancedFlexConnectVlanCentralSwitchingEnabled>true</advancedFlexConnectVlanCentralSwitchingEnabled>
          <advancedHttpProfilingEnabled>true</advancedHttpProfilingEnabled>
          <advancedIpv6Enabled>true</advancedIpv6Enabled>
          <advancedKtsCacEnabled>true</advancedKtsCacEnabled>
          <advancedLoadBalancingBandSelectEnabled>true</advancedLoadBalancingBandSelectEnabled>
          <advancedLoadBalancingEnabled>true</advancedLoadBalancingEnabled>
          <advancedMaximumClients>1</advancedMaximumClients>
          <advancedMdnsProfileName>String value</advancedMdnsProfileName>
          <advancedMdnsSnoopingEnabled>true</advancedMdnsSnoopingEnabled>
          <advancedMediaSessionSnoopingEnabled>true</advancedMediaSessionSnoopingEnabled>
          <advancedMfpClientProtection>DISABLED</advancedMfpClientProtection>
          <advancedMfpSignatureGenerationEnabled>true</advancedMfpSignatureGenerationEnabled>
          <advancedMfpVersion>1</advancedMfpVersion>
          <advancedOverrideInterfaceAclName>String value</advancedOverrideInterfaceAclName>
          <advancedOverrideInterfaceIpv6AclName>String value</advancedOverrideInterfaceIpv6AclName>
          <advancedPassiveClientEnabled>true</advancedPassiveClientEnabled>
          <advancedPeerToPeerBlocking>DISABLE</advancedPeerToPeerBlocking>
          <advancedPmipMobilityType>NONE</advancedPmipMobilityType>
          <advancedPmipProfile>String value</advancedPmipProfile>
          <advancedPmipRealm>String value</advancedPmipRealm>
          <advancedScanDeferPriority0>true</advancedScanDeferPriority0>
          <advancedScanDeferPriority1>true</advancedScanDeferPriority1>
          <advancedScanDeferPriority2>true</advancedScanDeferPriority2>
          <advancedScanDeferPriority3>true</advancedScanDeferPriority3>
          <advancedScanDeferPriority4>true</advancedScanDeferPriority4>
          <advancedScanDeferPriority5>true</advancedScanDeferPriority5>
          <advancedScanDeferPriority6>true</advancedScanDeferPriority6>
          <advancedScanDeferPriority7>true</advancedScanDeferPriority7>
          <advancedScanDeferTime>1</advancedScanDeferTime>
          <advancedSessionTimeout>1</advancedSessionTimeout>
          <advancedWifiDirectClientsPolicy>DISABLED</advancedWifiDirectClientsPolicy>
          <broadcastSsidEnabled>true</broadcastSsidEnabled>
          <ckipKeyIndex>1</ckipKeyIndex>
          <ckipKeyPermutationEnabled>true</ckipKeyPermutationEnabled>
          <ckipKeySize>NONE</ckipKeySize>
          <ckipMmhModeEnabled>true</ckipMmhModeEnabled>
          <ckipSecurityEnabled>true</ckipSecurityEnabled>
          <interfaceName>String value</interfaceName>
          <interfaceType>INTERFACE</interfaceType>
          <isWiredLan>true</isWiredLan>
          <lanType>WIRELESS</lanType>
          <layer2FastTransitionEnabled>true</layer2FastTransitionEnabled>
          <layer2FastTransitionOverDsEnabled>true</layer2FastTransitionOverDsEnabled>
          <layer2FastTransitionReassociationTimeout>1</layer2FastTransitionReassociationTimeout>
          <layer2MacFilteringEnabled>true</layer2MacFilteringEnabled>
          <layer3GlobalWebAuthEnabled>true</layer3GlobalWebAuthEnabled>
          <layer3PreauthenticationAcl>String value</layer3PreauthenticationAcl>
          <layer3PreauthenticationIpv6Acl>String value</layer3PreauthenticationIpv6Acl>
          <layer3VpnPassthroughEnabled>true</layer3VpnPassthroughEnabled>
          <layer3WebAuthFlexAcl>String value</layer3WebAuthFlexAcl>
          <layer3WebAuthType>DEFAULT</layer3WebAuthType>
          <layer3WebPolicyAuthenticationEnabled>true</layer3WebPolicyAuthenticationEnabled>
          <layer3WebPolicyConditionalRedirectEnabled>true</layer3WebPolicyConditionalRedirectEnabled>
          <layer3WebPolicyOnMacFailureEnabled>true</layer3WebPolicyOnMacFailureEnabled>
          <layer3WebPolicyPassthroughEnabled>true</layer3WebPolicyPassthroughEnabled>
          <multicastVlanEnabled>true</multicastVlanEnabled>
          <multicastVlanInterface>String value</multicastVlanInterface>
          <profileName>String value</profileName>
          <qos7920Cac>DISABLED</qos7920Cac>
          <qosAvcProfileName>String value</qosAvcProfileName>
          <qosNbarVisibilityEnabled>true</qosNbarVisibilityEnabled>
          <qosNetflowMonitor>String value</qosNetflowMonitor>
          <qosPerSSidBurstRealTimeUpstreamRate>1</qosPerSSidBurstRealTimeUpstreamRate>
          <qosPerSsidAverageDownstreamRate>1</qosPerSsidAverageDownstreamRate>
          <qosPerSsidAverageRealTimeDownstreamRate>1</qosPerSsidAverageRealTimeDownstreamRate>
          <qosPerSsidAverageRealTimeUpstreamRate>1</qosPerSsidAverageRealTimeUpstreamRate>
          <qosPerSsidAverageUpstreamRate>1</qosPerSsidAverageUpstreamRate>
          <qosPerSsidBurstDownstreamRate>1</qosPerSsidBurstDownstreamRate>
          <qosPerSsidBurstRealTimeDownstreamRate>1</qosPerSsidBurstRealTimeDownstreamRate>
          <qosPerSsidBurstUpstreamRate>1</qosPerSsidBurstUpstreamRate>
          <qosPerUserAverageDownstreamRate>1</qosPerUserAverageDownstreamRate>
          <qosPerUserAverageRealTimeDownstreamRate>1</qosPerUserAverageRealTimeDownstreamRate>
          <qosPerUserAverageRealTimeUpstreamRate>1</qosPerUserAverageRealTimeUpstreamRate>
          <qosPerUserAverageUpstreamRate>1</qosPerUserAverageUpstreamRate>
          <qosPerUserBurstDownstreamRate>1</qosPerUserBurstDownstreamRate>
          <qosPerUserBurstRealTimeDownstreamRate>1</qosPerUserBurstRealTimeDownstreamRate>
          <qosPerUserBurstRealTimeUpstreamRate>1</qosPerUserBurstRealTimeUpstreamRate>
          <qosPerUserBurstUpstreamRate>1</qosPerUserBurstUpstreamRate>
          <qosProfile>BRONZE</qosProfile>
          <qosWmmPolicy>DISABLED</qosWmmPolicy>
          <radioPolicy>ALL</radioPolicy>
          <ssid>String value</ssid>
          <vpnPassThroughGatewayAddress>
            <address>192.168.115.243</address>
          </vpnPassThroughGatewayAddress>
          <webAuthExternalUrl>String value</webAuthExternalUrl>
          <webAuthLoginFailurePage>String value</webAuthLoginFailurePage>
          <webAuthLoginPage>String value</webAuthLoginPage>
          <webAuthLogoutPage>String value</webAuthLogoutPage>
          <webPassthruEmailInputEnabled>true</webPassthruEmailInputEnabled>
          <wepAllowSharedKeyAuthentication>true</wepAllowSharedKeyAuthentication>
          <wepKeyIndex>1</wepKeyIndex>
          <wepKeySize>WEP104</wepKeySize>
          <wepSecurityEnabled>true</wepSecurityEnabled>
          <wpa2Enabled>true</wpa2Enabled>
          <wpa2EncryptionProtocolAes>true</wpa2EncryptionProtocolAes>
          <wpa2EncryptionProtocolTkip>true</wpa2EncryptionProtocolTkip>
          <wpaAuthenticationKeyManagement8021x>true</wpaAuthenticationKeyManagement8021x>
          <wpaAuthenticationKeyManagementCckm>true</wpaAuthenticationKeyManagementCckm>
          <wpaAuthenticationKeyManagementFt8021x>true</wpaAuthenticationKeyManagementFt8021x>
          <wpaAuthenticationKeyManagementFtPsk>true</wpaAuthenticationKeyManagementFtPsk>
          <wpaAuthenticationKeyManagementPmf8021x>true</wpaAuthenticationKeyManagementPmf8021x>
          <wpaAuthenticationKeyManagementPmfPsk>true</wpaAuthenticationKeyManagementPmfPsk>
          <wpaAuthenticationKeyManagementPsk>true</wpaAuthenticationKeyManagementPsk>
          <wpaEnabled>true</wpaEnabled>
          <wpaEncryptionProtocolAes>true</wpaEncryptionProtocolAes>
          <wpaEncryptionProtocolTkip>true</wpaEncryptionProtocolTkip>
          <wpaPresharedKey>String value</wpaPresharedKey>
          <wpaPresharedKeyFormat>DEFAULT</wpaPresharedKeyFormat>
          <wpaSecurityEnabled>true</wpaSecurityEnabled>
          <x8021KeySize>WEP104</x8021KeySize>
          <x8021SecurityEnabled>true</x8021SecurityEnabled>
          <aaaRadiusAccountingWlcSpecificEnabled>true</aaaRadiusAccountingWlcSpecificEnabled>
          <aaaRadiusAuthenticationWlcSpecificEnabled>true</aaaRadiusAuthenticationWlcSpecificEnabled>
          <advancedSessionTimeoutEnabled>true</advancedSessionTimeoutEnabled>
          <hotspot2Enable>
            <hotSpot2Enabled>true</hotSpot2Enabled>
          </hotspot2Enable>
          <hotspot2Operators>
            <hotspot2Operator>
              <operatorId>1</operatorId>
              <operatorLang>String value</operatorLang>
              <operatorName>String value</operatorName>
            </hotspot2Operator>
            <hotspot2Operator>
              <operatorId>11</operatorId>
              <operatorLang>Another string value</operatorLang>
              <operatorName>Another string value</operatorName>
            </hotspot2Operator>
          </hotspot2Operators>
          <hotspot2Ports>
            <hotspot2Port>
              <portConfigId>1</portConfigId>
              <portNo>ICMPESP</portNo>
              <portStatus>CLOSED</portStatus>
              <protocolName>ICMP</protocolName>
            </hotspot2Port>
            <hotspot2Port>
              <portConfigId>11</portConfigId>
              <portNo>FTP</portNo>
              <portStatus>OPEN</portStatus>
              <protocolName>FTP</protocolName>
            </hotspot2Port>
          </hotspot2Ports>
          <hotspot2Wan>
            <downLinkSpeed>1</downLinkSpeed>
            <upLinkSpeed>1</upLinkSpeed>
            <wanLinkStatus>LINKUP</wanLinkStatus>
            <wanSymLinkStatus>SAME</wanSymLinkStatus>
          </hotspot2Wan>
          <hotspotCellularNetworks>
            <hotspotCellularNetwork>
              <countryCode>String value</countryCode>
              <gppIndex>1</gppIndex>
              <networkCode>String value</networkCode>
            </hotspotCellularNetwork>
            <hotspotCellularNetwork>
              <countryCode>Another string value</countryCode>
              <gppIndex>11</gppIndex>
              <networkCode>Another string value</networkCode>
            </hotspotCellularNetwork>
          </hotspotCellularNetworks>
          <hotspotDomains>
            <hotspotDomain>
              <domainId>1</domainId>
              <domainName>String value</domainName>
            </hotspotDomain>
            <hotspotDomain>
              <domainId>11</domainId>
              <domainName>Another string value</domainName>
            </hotspotDomain>
          </hotspotDomains>
          <hotspotGeneral>
            <heSsid>
              <octets>000a959d6816</octets>
            </heSsid>
            <internetAccess>true</internetAccess>
            <ipv4AddressAvailType>NOTAVAILABLE</ipv4AddressAvailType>
            <ipv6AddressAvailType>NOTAVAILABLE</ipv6AddressAvailType>
            <networkAuthType>ACCEPTANCE</networkAuthType>
            <networkType>PRIVATE</networkType>
            <status>true</status>
          </hotspotGeneral>
          <hotspotOuiTemplates>
            <hotspotOuiTemplate>
              <oui>String value</oui>
              <ouiId>1</ouiId>
              <ouiInBeacon>true</ouiInBeacon>
            </hotspotOuiTemplate>
            <hotspotOuiTemplate>
              <oui>Another string value</oui>
              <ouiId>11</ouiId>
              <ouiInBeacon>false</ouiInBeacon>
            </hotspotOuiTemplate>
          </hotspotOuiTemplates>
          <hotspotRealms>
            <hotspotRealm>
              <realmEapMethods>
                <realmEapMethod>
                  <innerAuthMethods>
                    <innerAuthMethod>
                      <realmEapAuthId>1</realmEapAuthId>
                      <realmEapAuthMethod>NONEAPINNERAUTH</realmEapAuthMethod>
                      <realmEapAuthParam>NONE</realmEapAuthParam>
                    </innerAuthMethod>
                    <innerAuthMethod>
                      <realmEapAuthId>11</realmEapAuthId>
                      <realmEapAuthMethod>INNERAUTHEAP</realmEapAuthMethod>
                      <realmEapAuthParam>PAP</realmEapAuthParam>
                    </innerAuthMethod>
                  </innerAuthMethods>
                  <realmEapId>1</realmEapId>
                  <realmEapMethod>NONE</realmEapMethod>
                </realmEapMethod>
                <realmEapMethod>
                  <innerAuthMethods>
                    <innerAuthMethod>
                      <realmEapAuthId>1</realmEapAuthId>
                      <realmEapAuthMethod>NONEAPINNERAUTH</realmEapAuthMethod>
                      <realmEapAuthParam>NONE</realmEapAuthParam>
                    </innerAuthMethod>
                    <innerAuthMethod>
                      <realmEapAuthId>11</realmEapAuthId>
                      <realmEapAuthMethod>INNERAUTHEAP</realmEapAuthMethod>
                      <realmEapAuthParam>PAP</realmEapAuthParam>
                    </innerAuthMethod>
                  </innerAuthMethods>
                  <realmEapId>11</realmEapId>
                  <realmEapMethod>LEAP</realmEapMethod>
                </realmEapMethod>
              </realmEapMethods>
              <realmId>1</realmId>
              <realmName>String value</realmName>
            </hotspotRealm>
            <hotspotRealm>
              <realmEapMethods>
                <realmEapMethod>
                  <innerAuthMethods>
                    <innerAuthMethod>
                      <realmEapAuthId>1</realmEapAuthId>
                      <realmEapAuthMethod>NONEAPINNERAUTH</realmEapAuthMethod>
                      <realmEapAuthParam>NONE</realmEapAuthParam>
                    </innerAuthMethod>
                    <innerAuthMethod>
                      <realmEapAuthId>11</realmEapAuthId>
                      <realmEapAuthMethod>INNERAUTHEAP</realmEapAuthMethod>
                      <realmEapAuthParam>PAP</realmEapAuthParam>
                    </innerAuthMethod>
                  </innerAuthMethods>
                  <realmEapId>1</realmEapId>
                  <realmEapMethod>NONE</realmEapMethod>
                </realmEapMethod>
                <realmEapMethod>
                  <innerAuthMethods>
                    <innerAuthMethod>
                      <realmEapAuthId>1</realmEapAuthId>
                      <realmEapAuthMethod>NONEAPINNERAUTH</realmEapAuthMethod>
                      <realmEapAuthParam>NONE</realmEapAuthParam>
                    </innerAuthMethod>
                    <innerAuthMethod>
                      <realmEapAuthId>11</realmEapAuthId>
                      <realmEapAuthMethod>INNERAUTHEAP</realmEapAuthMethod>
                      <realmEapAuthParam>PAP</realmEapAuthParam>
                    </innerAuthMethod>
                  </innerAuthMethods>
                  <realmEapId>11</realmEapId>
                  <realmEapMethod>LEAP</realmEapMethod>
                </realmEapMethod>
              </realmEapMethods>
              <realmId>11</realmId>
              <realmName>Another string value</realmName>
            </hotspotRealm>
          </hotspotRealms>
          <hotspotServiceAdvertisement>
            <msapEnable>true</msapEnable>
            <serverIndex>1</serverIndex>
          </hotspotServiceAdvertisement>
          <lastModified>2</lastModified>
          <templateName>String value</templateName>
          <wpaControllerSpecificPresharedKeyEnabled>true</wpaControllerSpecificPresharedKeyEnabled>
        </wlanTemplatesDTO>
      </entity>
    </queryResponse>

### Sample JSON Payload

https://10.64.88.203/webacs/api/v2/data/WlanTemplates/15.json

    {
      "queryResponse" : {
        "@type" : "WlanTemplates",
        "@requestUrl" : "https://10.64.88.203/webacs/api/v2/data/WlanTemplates/15",
        "@responseType" : "getEntity",
        "@rootUrl" : "https://10.64.88.203/webacs/api/v2/data",
        "entity" : [ {
          "@dtoType" : "wlanTemplatesDTO",
          "@type" : "WlanTemplates",
          "@url" : "https://10.64.88.203/webacs/api/v2/data/WlanTemplates/15",
          "wlanTemplatesDTO" : {
            "@displayName" : "String value",
            "@id" : 15,
            "@uuid" : "String value",
            "aaaAllowOverride" : true,
            "aaaLdapPrimaryServer" : "String value",
            "aaaLdapSecondaryServer" : "String value",
            "aaaLdapTertiaryServer" : "String value",
            "aaaLocalEapAuthenticationEnabled" : true,
            "aaaLocalEapAuthenticationProfileName" : "String value",
            "aaaRadiusAccountingPrimaryServer" : "String value",
            "aaaRadiusAccountingSecondaryServer" : "String value",
            "aaaRadiusAccountingServersEnabled" : true,
            "aaaRadiusAccountingTertiaryServer" : "String value",
            "aaaRadiusAccountingWlcSpecificEnabled" : true,
            "aaaRadiusAuthenticationPrimaryServer" : "String value",
            "aaaRadiusAuthenticationSecondaryServer" : "String value",
            "aaaRadiusAuthenticationServersEnabled" : true,
            "aaaRadiusAuthenticationTertiaryServer" : "String value",
            "aaaRadiusAuthenticationWlcSpecificEnabled" : true,
            "aaaRadiusInterimUpdateEnabled" : true,
            "aaaRadiusInterimUpdateInterval" : 1,
            "adminStatus" : true,
            "advancedAironetIeEnabled" : true,
            "advancedClientExclusionEnabled" : true,
            "advancedClientExclusionTimeout" : 1,
            "advancedCoverageHoleDetectionEnabled" : true,
            "advancedDhcpAddressAssignmentRequired" : true,
            "advancedDhcpProfilingEnabled" : true,
            "advancedDhcpServerIpAddress" : {
              "address" : "192.168.115.243"
            },
            "advancedDiagnosticChannelEnabled" : true,
            "advancedDot11anDtimPeriod" : 1,
            "advancedDot11bgnDtimPeriod" : 1,
            "advancedFlexConnectCentralDhcpProcessingEnabled" : true,
            "advancedFlexConnectLearnClientIpEnabled" : true,
            "advancedFlexConnectLocalAuthEnabled" : true,
            "advancedFlexConnectLocalSwitchingEnabled" : true,
            "advancedFlexConnectNatPatEnabled" : true,
            "advancedFlexConnectOverrideDnsEnabled" : true,
            "advancedFlexConnectReapCentralAssociation" : true,
            "advancedFlexConnectVlanCentralSwitchingEnabled" : true,
            "advancedHttpProfilingEnabled" : true,
            "advancedIpv6Enabled" : true,
            "advancedKtsCacEnabled" : true,
            "advancedLoadBalancingBandSelectEnabled" : true,
            "advancedLoadBalancingEnabled" : true,
            "advancedMaximumClients" : 1,
            "advancedMdnsProfileName" : "String value",
            "advancedMdnsSnoopingEnabled" : true,
            "advancedMediaSessionSnoopingEnabled" : true,
            "advancedMfpClientProtection" : "DISABLED",
            "advancedMfpSignatureGenerationEnabled" : true,
            "advancedMfpVersion" : 1,
            "advancedOverrideInterfaceAclName" : "String value",
            "advancedOverrideInterfaceIpv6AclName" : "String value",
            "advancedPassiveClientEnabled" : true,
            "advancedPeerToPeerBlocking" : "DISABLE",
            "advancedPmipMobilityType" : "NONE",
            "advancedPmipProfile" : "String value",
            "advancedPmipRealm" : "String value",
            "advancedScanDeferPriority0" : true,
            "advancedScanDeferPriority1" : true,
            "advancedScanDeferPriority2" : true,
            "advancedScanDeferPriority3" : true,
            "advancedScanDeferPriority4" : true,
            "advancedScanDeferPriority5" : true,
            "advancedScanDeferPriority6" : true,
            "advancedScanDeferPriority7" : true,
            "advancedScanDeferTime" : 1,
            "advancedSessionTimeout" : 1,
            "advancedSessionTimeoutEnabled" : true,
            "advancedWifiDirectClientsPolicy" : "DISABLED",
            "broadcastSsidEnabled" : true,
            "ckipKeyIndex" : 1,
            "ckipKeyPermutationEnabled" : true,
            "ckipKeySize" : "NONE",
            "ckipMmhModeEnabled" : true,
            "ckipSecurityEnabled" : true,
            "hotspot2Enable" : {
              "hotSpot2Enabled" : true
            },
            "hotspot2Operators" : {
              "hotspot2Operator" : [ {
                "operatorId" : 1,
                "operatorLang" : "String value",
                "operatorName" : "String value"
              }, {
                "operatorId" : 11,
                "operatorLang" : "Another string value",
                "operatorName" : "Another string value"
              } ]
            },
            "hotspot2Ports" : {
              "hotspot2Port" : [ {
                "portConfigId" : 1,
                "portNo" : "ICMPESP",
                "portStatus" : "CLOSED",
                "protocolName" : "ICMP"
              }, {
                "portConfigId" : 11,
                "portNo" : "FTP",
                "portStatus" : "OPEN",
                "protocolName" : "FTP"
              } ]
            },
            "hotspot2Wan" : {
              "downLinkSpeed" : 1,
              "upLinkSpeed" : 1,
              "wanLinkStatus" : "LINKUP",
              "wanSymLinkStatus" : "SAME"
            },
            "hotspotCellularNetworks" : {
              "hotspotCellularNetwork" : [ {
                "countryCode" : "String value",
                "gppIndex" : 1,
                "networkCode" : "String value"
              }, {
                "countryCode" : "Another string value",
                "gppIndex" : 11,
                "networkCode" : "Another string value"
              } ]
            },
            "hotspotDomains" : {
              "hotspotDomain" : [ {
                "domainId" : 1,
                "domainName" : "String value"
              }, {
                "domainId" : 11,
                "domainName" : "Another string value"
              } ]
            },
            "hotspotGeneral" : {
              "heSsid" : {
                "octets" : "000a959d6816"
              },
              "internetAccess" : true,
              "ipv4AddressAvailType" : "NOTAVAILABLE",
              "ipv6AddressAvailType" : "NOTAVAILABLE",
              "networkAuthType" : "ACCEPTANCE",
              "networkType" : "PRIVATE",
              "status" : true
            },
            "hotspotOuiTemplates" : {
              "hotspotOuiTemplate" : [ {
                "oui" : "String value",
                "ouiId" : 1,
                "ouiInBeacon" : true
              }, {
                "oui" : "Another string value",
                "ouiId" : 11,
                "ouiInBeacon" : false
              } ]
            },
            "hotspotRealms" : {
              "hotspotRealm" : [ {
                "realmEapMethods" : {
                  "realmEapMethod" : [ {
                    "innerAuthMethods" : {
                      "innerAuthMethod" : [ {
                        "realmEapAuthId" : 1,
                        "realmEapAuthMethod" : "NONEAPINNERAUTH",
                        "realmEapAuthParam" : "NONE"
                      }, {
                        "realmEapAuthId" : 11,
                        "realmEapAuthMethod" : "INNERAUTHEAP",
                        "realmEapAuthParam" : "PAP"
                      } ]
                    },
                    "realmEapId" : 1,
                    "realmEapMethod" : "NONE"
                  }, {
                    "innerAuthMethods" : {
                      "innerAuthMethod" : [ {
                        "realmEapAuthId" : 1,
                        "realmEapAuthMethod" : "NONEAPINNERAUTH",
                        "realmEapAuthParam" : "NONE"
                      }, {
                        "realmEapAuthId" : 11,
                        "realmEapAuthMethod" : "INNERAUTHEAP",
                        "realmEapAuthParam" : "PAP"
                      } ]
                    },
                    "realmEapId" : 11,
                    "realmEapMethod" : "LEAP"
                  } ]
                },
                "realmId" : 1,
                "realmName" : "String value"
              }, {
                "realmEapMethods" : {
                  "realmEapMethod" : [ {
                    "innerAuthMethods" : {
                      "innerAuthMethod" : [ {
                        "realmEapAuthId" : 1,
                        "realmEapAuthMethod" : "NONEAPINNERAUTH",
                        "realmEapAuthParam" : "NONE"
                      }, {
                        "realmEapAuthId" : 11,
                        "realmEapAuthMethod" : "INNERAUTHEAP",
                        "realmEapAuthParam" : "PAP"
                      } ]
                    },
                    "realmEapId" : 1,
                    "realmEapMethod" : "NONE"
                  }, {
                    "innerAuthMethods" : {
                      "innerAuthMethod" : [ {
                        "realmEapAuthId" : 1,
                        "realmEapAuthMethod" : "NONEAPINNERAUTH",
                        "realmEapAuthParam" : "NONE"
                      }, {
                        "realmEapAuthId" : 11,
                        "realmEapAuthMethod" : "INNERAUTHEAP",
                        "realmEapAuthParam" : "PAP"
                      } ]
                    },
                    "realmEapId" : 11,
                    "realmEapMethod" : "LEAP"
                  } ]
                },
                "realmId" : 11,
                "realmName" : "Another string value"
              } ]
            },
            "hotspotServiceAdvertisement" : {
              "msapEnable" : true,
              "serverIndex" : 1
            },
            "interfaceName" : "String value",
            "interfaceType" : "INTERFACE",
            "isWiredLan" : true,
            "lanType" : "WIRELESS",
            "lastModified" : 2,
            "layer2FastTransitionEnabled" : true,
            "layer2FastTransitionOverDsEnabled" : true,
            "layer2FastTransitionReassociationTimeout" : 1,
            "layer2MacFilteringEnabled" : true,
            "layer3GlobalWebAuthEnabled" : true,
            "layer3PreauthenticationAcl" : "String value",
            "layer3PreauthenticationIpv6Acl" : "String value",
            "layer3VpnPassthroughEnabled" : true,
            "layer3WebAuthFlexAcl" : "String value",
            "layer3WebAuthType" : "DEFAULT",
            "layer3WebPolicyAuthenticationEnabled" : true,
            "layer3WebPolicyConditionalRedirectEnabled" : true,
            "layer3WebPolicyOnMacFailureEnabled" : true,
            "layer3WebPolicyPassthroughEnabled" : true,
            "multicastVlanEnabled" : true,
            "multicastVlanInterface" : "String value",
            "profileName" : "String value",
            "qos7920Cac" : "DISABLED",
            "qosAvcProfileName" : "String value",
            "qosNbarVisibilityEnabled" : true,
            "qosNetflowMonitor" : "String value",
            "qosPerSSidBurstRealTimeUpstreamRate" : 1,
            "qosPerSsidAverageDownstreamRate" : 1,
            "qosPerSsidAverageRealTimeDownstreamRate" : 1,
            "qosPerSsidAverageRealTimeUpstreamRate" : 1,
            "qosPerSsidAverageUpstreamRate" : 1,
            "qosPerSsidBurstDownstreamRate" : 1,
            "qosPerSsidBurstRealTimeDownstreamRate" : 1,
            "qosPerSsidBurstUpstreamRate" : 1,
            "qosPerUserAverageDownstreamRate" : 1,
            "qosPerUserAverageRealTimeDownstreamRate" : 1,
            "qosPerUserAverageRealTimeUpstreamRate" : 1,
            "qosPerUserAverageUpstreamRate" : 1,
            "qosPerUserBurstDownstreamRate" : 1,
            "qosPerUserBurstRealTimeDownstreamRate" : 1,
            "qosPerUserBurstRealTimeUpstreamRate" : 1,
            "qosPerUserBurstUpstreamRate" : 1,
            "qosProfile" : "BRONZE",
            "qosWmmPolicy" : "DISABLED",
            "radioPolicy" : "ALL",
            "ssid" : "String value",
            "templateName" : "String value",
            "vpnPassThroughGatewayAddress" : {
              "address" : "192.168.115.243"
            },
            "webAuthExternalUrl" : "String value",
            "webAuthLoginFailurePage" : "String value",
            "webAuthLoginPage" : "String value",
            "webAuthLogoutPage" : "String value",
            "webPassthruEmailInputEnabled" : true,
            "wepAllowSharedKeyAuthentication" : true,
            "wepKeyIndex" : 1,
            "wepKeySize" : "WEP104",
            "wepSecurityEnabled" : true,
            "wpa2Enabled" : true,
            "wpa2EncryptionProtocolAes" : true,
            "wpa2EncryptionProtocolTkip" : true,
            "wpaAuthenticationKeyManagement8021x" : true,
            "wpaAuthenticationKeyManagementCckm" : true,
            "wpaAuthenticationKeyManagementFt8021x" : true,
            "wpaAuthenticationKeyManagementFtPsk" : true,
            "wpaAuthenticationKeyManagementPmf8021x" : true,
            "wpaAuthenticationKeyManagementPmfPsk" : true,
            "wpaAuthenticationKeyManagementPsk" : true,
            "wpaControllerSpecificPresharedKeyEnabled" : true,
            "wpaEnabled" : true,
            "wpaEncryptionProtocolAes" : true,
            "wpaEncryptionProtocolTkip" : true,
            "wpaPresharedKey" : "String value",
            "wpaPresharedKeyFormat" : "DEFAULT",
            "wpaSecurityEnabled" : true,
            "x8021KeySize" : "WEP104",
            "x8021SecurityEnabled" : true
          }
        } ]
      }
    }

### Resource Information

Rate Limiting? | Yes
Sorting? | Yes
Paging? | Yes
Filtering? | Yes
Group Filtering? | No
Aggregation? | No
Response Formats | xml json
User Group | NBI Read
HTTP Methods | GET

## Resource URL

/webacs/api/v3/data/WlanTemplates

Unmodified

This resource has not been modified since the previous API version.

## Response Parameters

Attribute | Description
--- | ---
aaaAllowOverride boolean | Is allow AAA override enabled?
aaaLdapPrimaryServer String | Primary LDAP server.
aaaLdapSecondaryServer String | Secondary LDAP server.
aaaLdapTertiaryServer String | Tertiary LDAP server.
aaaLocalEapAuthenticationEnabled boolean | Is local EAP authentication enabled?
aaaLocalEapAuthenticationProfileName String | When aaaLocalEapAuthenticationEnabled is true, this defines the EAP profile that will be used.
aaaRadiusAccountingPrimaryServer String | When aaaRadiusAccountingServersEnabled is true, this is the primary RADIUS accounting server.
aaaRadiusAccountingSecondaryServer String | When aaaRadiusAccountingServersEnabled is true, this is the secondary RADIUS accounting server.
aaaRadiusAccountingServersEnabled boolean | Is RADIUS accounting enabled?
aaaRadiusAccountingTertiaryServer String | When aaaRadiusAccountingServersEnabled is true, this is the tertiary RADIUS accounting server.
aaaRadiusAccountingWlcSpecificEnabled boolean | Is controller specific RADIUS accounting servers enabled?
aaaRadiusAuthenticationPrimaryServer String | When aaaRadiusAuthenticationServersEnabled is true, this is the primary RADIUS authentication server.
aaaRadiusAuthenticationSecondaryServer String | When aaaRadiusAuthenticationServersEnabled is true, this is the secondary RADIUS authentication server.
aaaRadiusAuthenticationServersEnabled boolean | Is RADIUS authentication enabled?
aaaRadiusAuthenticationTertiaryServer String | When aaaRadiusAuthenticationServersEnabled is true, this is the tertiary RADIUS authentication server.
aaaRadiusAuthenticationWlcSpecificEnabled boolean | Is controller specific RADIUS authentication servers enabled?
aaaRadiusInterimUpdateEnabled boolean | Is RADIUS server accounting interim update enabled?
aaaRadiusInterimUpdateInterval int | When aaaRadiusInterimUpdateEnabled is true, this determines the update interval. Measured in seconds.
adminStatus boolean | Is the WLAN administratively enabled?
advancedAironetIeEnabled boolean | Is Aironet Information Elements (IEs) enabled for this WLAN?
advancedClientExclusionEnabled boolean | Is automatic client exclusion enabled for this WLAN?
advancedClientExclusionTimeout int | When advancedClientExclusionEnabled is true, this denotes the length of the timeout. A value of zero represents an infinite timeout. Measured in seconds.
advancedCoverageHoleDetectionEnabled boolean | Is Coverage Hole Detection enabled for this WLAN?
advancedDhcpAddressAssignmentRequired boolean | Are all clients required to obtain an IP address from the DHCP server for this WLAN?
advancedDhcpProfilingEnabled boolean | Should the wireless controller collect the DHCP attributes of clients on this WLAN?
advancedDhcpServerIpAddress InetAddress | If this contains a valid address, an IPv4 DHCP server has been specified for this WLAN.
advancedDiagnosticChannelEnabled boolean | Is the diagnostic channel available for this WLAN?
advancedDot11anDtimPeriod int | Denotes the Delivery Traffic Indication Map (DTIM) interval for 802.11a/n radios, during which broadcast and multicast frames will be transmitted. A value of one results in a broadcast after every beacon, two for every other beacon, and so on.
advancedDot11bgnDtimPeriod int | Denotes the Delivery Traffic Indication Map (DTIM) interval for 802.11b/g/n radios, during which broadcast and multicast frames will be transmitted. A value of one results in a broadcast after every beacon, two for every other beacon, and so on.
advancedFlexConnectCentralDhcpProcessingEnabled boolean | Are DHCP packets received by the access point sent to the controller then forwarded to the WLAN's corresponding VLAN?
advancedFlexConnectLearnClientIpEnabled boolean | Is client IP address learning enabled?
advancedFlexConnectLocalAuthEnabled boolean | Is local authentication enabled?
advancedFlexConnectLocalSwitchingEnabled boolean | When true, access points will locally switch traffic, rather than forwarding to the wireless controller.
advancedFlexConnectNatPatEnabled boolean | Is Network Address Translation (NAT) and Port Address Translation (PAT) enabled?
advancedFlexConnectOverrideDnsEnabled boolean | When true, clients are given the DNS server of the access point rather than of the WLAN's configured interface.
advancedFlexConnectReapCentralAssociation boolean | Is Reap Central Association enabled?
advancedFlexConnectVlanCentralSwitchingEnabled boolean | Is VLAN based central switching enabled?
advancedHttpProfilingEnabled boolean | Should the wireless controller collect the HTTP attributes of clients on this WLAN?
advancedIpv6Enabled boolean | Is IPv6 enabled?
advancedKtsCacEnabled boolean | Is CAC based on the Key Telephone System (KTS) enabled on this WLAN?
advancedLoadBalancingBandSelectEnabled boolean | Is client band select enabled?
advancedLoadBalancingEnabled boolean | Is client load balancing enabled?
advancedMaximumClients int | Denotes the maximum number of clients. A value of zero means unlimited.
advancedMdnsProfileName String | When advancedMdnsSnoopingEnabled is true, this denotes the mDNS profile. Clients receive service advertisements only for the services associated with the profile.
advancedMdnsSnoopingEnabled boolean | Is mDNS snooping enabled?
advancedMediaSessionSnoopingEnabled boolean | Should the access point snoop on Session Initiation Protocol (SIP) traffic, and report back to the controller the establishment termination and failure of voice calls?
advancedMfpClientProtection DisabledEnabledRequiredEnum | Denotes whether client management frame protection (MFP) is enabled (optional), required, or disabled for this WLAN. Allowed values DISABLED ENABLED REQUIRED
advancedMfpSignatureGenerationEnabled boolean | Do 802.11 management frames transmitted by the access point have a signature to verify authenticity?
advancedMfpVersion int | Denotes the version of management frame protection (MFP).
advancedOverrideInterfaceAclName String | Denotes an IPv4 ACL that overrides the ACL configured for the WLAN's interface.
advancedOverrideInterfaceIpv6AclName String | Denotes an IPv6 ACL that overrides the ACL configured for the WLAN's interface.
advancedPassiveClientEnabled boolean | Should the controller forward ARP requests out to the WLAN for passive clients?
advancedPeerToPeerBlocking Peer2PeerBlockingEnum | Denotes whether peer-to-peer blocking is disabled, enabled, or if the packets are forwarded to the next device. Allowed values DISABLE DROP FORWARDUP ALLOWPRIVATEGROUP
advancedPmipMobilityType PmipMobilityTypeEnum | Denotes the Proxy Mobile IP (PMIP) type for this WLAN. Allowed values NONE PMIP
advancedPmipProfile String | Denotes the Proxy Mobile IP (PMIP) profile for this WLAN.
advancedPmipRealm String | Denotes the default realm of the Proxy Mobile IPv6 (PMIPv6) WLAN.
advancedScanDeferPriority0 boolean | Is priority 0 for the channel scan enabled?
advancedScanDeferPriority1 boolean | Is priority 1 for the channel scan enabled?
advancedScanDeferPriority2 boolean | Is priority 2 for the channel scan enabled?
advancedScanDeferPriority3 boolean | Is priority 3 for the channel scan enabled?
advancedScanDeferPriority4 boolean | Is priority 4 for the channel scan enabled?
advancedScanDeferPriority5 boolean | Is priority 5 for the channel scan enabled?
advancedScanDeferPriority6 boolean | Is priority 6 for the channel scan enabled?
advancedScanDeferPriority7 boolean | Is priority 7 for the channel scan enabled?
advancedScanDeferTime int | Denotes the channel scan defer time. Measured in milliseconds.
advancedSessionTimeout int | Denotes the maximum time for a client session before requiring reauthentication. Zero means no timeout. Measured in seconds.
advancedSessionTimeoutEnabled boolean | Is advancedSessionTimeout enabled?
advancedWifiDirectClientsPolicy DisabledAllowedNotAllowedEnum | Denotes the Wi-Fi Direct Clients Policy for this WLAN. Allowed values DISABLED ALLOWED NOTALLOWED XCONNECTNOTALLOW
broadcastSsidEnabled boolean | Is SSID broadcasting enabled?
ckipKeyIndex int | When ckipSecurityEnabled is true, this denotes the key index.
ckipKeyPermutationEnabled boolean | When ckipSecurityEnabled is true, this denotes whether key permutation is enabled.
ckipKeySize CkipEncryptionTypeEnum | When ckipSecurityEnabled is true, this denotes the key size. Allowed values NONE LEN40 LEN104
ckipMmhModeEnabled boolean | When ckipSecurityEnabled is true, this denotes whether multimodular mode hashing is enabled.
ckipSecurityEnabled boolean | Is CKIP layer 2 security enabled?
hotspot2Enable WlanMcHotSpotEnableTemplate | This attribute represents enablement of HotSpot 2.0.
Attribute | Description
--- | ---
hotSpot2Enabled boolean | Is HotSpot 2.0 enabled?
hotspot2Operators WlanMcHotSpotOperatorConfigTemplate[] | These attributes represent HotSpot 2.0 operators.
Attribute | Description
--- | ---
operatorId int | Operator index of the hotspot provider.
operatorLang String | Language code.
operatorName String | Operator name of the hotspot provider.
hotspot2Ports WlanMcHotSpotPortConfigTemplate[] | These attributes represent HotSpot 2.0 port configurations.
Attribute | Description
--- | ---
portConfigId int | Port configuration index.
portNo PortNoEnum | Port number used for the IP. Allowed values ICMPESP FTP SSH HTTP TTLSVPN PPTPVPN VOIP IKEV2 IPSECNAT
portStatus PortStatusEnum | Status of the IP port. Allowed values CLOSED OPEN UNKNOWN
protocolName ProtocolNameEnum | Internet protocol name. This parameter provides information on the connection status of the most commonly used communication protocols and ports. Allowed values ICMP FTP IKEV2 ESP
hotspot2Wan WlanMcHotSpotWanTemplate | These attributes represent HotSpot 2.0 WAN metrics configuration.
Attribute | Description
--- | ---
downLinkSpeed int | Downlink speed of the WAN backhaul link. Measured in Kbps.
upLinkSpeed int | Uplink speed of the WAN backhaul. Measured in Kbps.
wanLinkStatus WanLinkStatusEnum | WAN link status. Allowed values LINKUP LINKDOWN LINKINTESTSTATE NOTCONFIGURED
wanSymLinkStatus WanSymLinkStatusEnum | WAN symmetric link status. Allowed values SAME DIFFERENT
hotspotCellularNetworks WlanMc3GppConfigTemplate[] | These attributes represent 802.11u cellular network parameters.
Attribute | Description
--- | ---
countryCode String | Mobile country code in Binary Coded Decimal (BCD) format.
gppIndex int | Cellular index.
networkCode String | Mobile network code in Binary Coded Decimal (BCD) format.
hotspotDomains WlanMcDomainConfigTemplate[] | These attributes represent 802.11u domains.
Attribute | Description
--- | ---
domainId int | Domain index.
domainName String | Domain name operating in the WLAN network.
hotspotGeneral WlanMcGeneralConfigTemplate | These attributes represent 802.11u general parameters.
Attribute | Description
--- | ---
heSsid MacAddress | The Homogenous Extended Service Set Identifier (HESSID).
internetAccess boolean | Is Internet Access enabled?
ipv4AddressAvailType IPv4AddressAvailTypeEnum | IPv4 type address. Allowed values NOTAVAILABLE PUBLIC PORTRESTRICTED SINGLENATPRIVATE DOUBLENATPRIVATE PORTRESTRICTEDSINGLENATPRIVATE PORTRESTRICTEDDOUBLENATPRIVATE UNKNOWN
ipv6AddressAvailType IPv6AddressAvailTypeEnum | IPv6 type address. Allowed values NOTAVAILABLE AVAILABLE UNKNOWN
networkAuthType NetworkAuthTypeEnum | Network authentication type for 802.11u on this WLAN. Allowed values ACCEPTANCE ENROLLMENT REDIRECTION DNSREDIRECTION NOTCONFIGURED
networkType NetworkTypeEnum | Network type of this WLAN. Allowed values PRIVATE PRIVATEWITHGUESTACCESS PUBLICPAID PUBLICFREE PERSONALDEVICE EMERGENCYSERVICEONLY TESTEQUIPMENT WILDCARD UNKNOWN
status boolean | Is 802.11u enabled?
hotspotOuiTemplate WlanMcOuiConfigTemplate[] | These attributes represent 802.11u OUIs.
Attribute | Description
--- | ---
oui String | Organization Unique Identifier (OUI).
ouiId int | OUI index.
ouiInBeacon boolean | Are Organization Unique Identifier (OUI) beacon responses enabled?
hotspotRealms WlanMcRealmConfigTemplate[] | These attributes represent 802.11u realms.
Attribute | Description
--- | ---
realmEapMethods WlanMcRealmEapConfigTemplate[] | Extensible Authentication Protocol (EAP) list.
Attribute | Description
--- | ---
innerAuthMethods WlanMcRealmEapAuthConfigTemplate[] | Auth method list.
Attribute | Description
--- | ---
realmEapAuthId int | Auth method index.
realmEapAuthMethod RealmEapAuthMethodEnum | Inner auth method. Allowed values NONEAPINNERAUTH INNERAUTHEAP CREDENTIAL TUNNELEDEAPCREDENTIAL
realmEapAuthParam RealmEapAuthParamEnum | Auth param. Allowed values NONE PAP CHAP MSCHAP MSCHAPV2 LEAP PEAP EAPTLS EAPFAST EAPSIM EAPTTLS EAPAKA SIM USIM NFCSECURE HARDWARETOKEN SOFTTOKEN CERTIFICATE USERNAMEPASSWORD RESERVED ANONYMOUS VENDORSPECIFIC
realmEapId int | EAP index.
realmEapMethod RealmEapMethodEnum | EAP method for the realm in the WLAN. Allowed values NONE LEAP EAPPEAP EAPTLS EAPFAST EAPSIM EAPTTLS EAPAKA
realmId int | Realm index.
realmName String | Realm name.
hotspotServiceAdvertisement WlanMcServiceAdConfigTemplate | These attributes represent MSAP (Mobility Service Advertisement Protocol) parameters.
Attribute | Description
--- | ---
msapEnable boolean | Is Mobility Service Advertisement Protocol (MSAP) enabled?
serverIndex int | Server index.
interfaceName String | Denotes the interface, or interface group, for this WLAN. See interfaceType to determine if this is an interface or interface group.
interfaceType InterfaceMappingTypeEnum | Denotes whether an interface or interface group is used for this interface. See interfaceName for the name of the interface or interface group. Allowed values INTERFACE INTERFACEGROUP
isWiredLan boolean | Is this a wired LAN?
lanType LanTypeEnum | Denotes the LAN type. Allowed values WIRELESS GUEST REMOTE
lastModified long | The time the template was last modified. Measured in milliseconds since the Unix epoch.
layer2FastTransitionEnabled boolean | Is fast transition (FT) between access points enabled?
layer2FastTransitionOverDsEnabled boolean | When layer2FastTransitionEnabled is true, the denotes whether fast transition over a distributed system is enabled.
layer2FastTransitionReassociationTimeout int | When layer2FastTransitionEnabled is true, this denotes the transition timeout. Measured in seconds.
layer2MacFilteringEnabled boolean | Is MAC filtering enabled?
layer3GlobalWebAuthEnabled boolean | When a layer 3 web policy is true, this denotes whether the template uses global or template-defined Web Auth configuration.
layer3PreauthenticationAcl String | When a layer 3 web policy is true, this denotes the IPv4 ACL for traffic between the client and the wireless controller.
layer3PreauthenticationIpv6Acl String | When a layer 3 web policy is true, this denotes the IPv6 ACL for traffic between the client and the wireless controller.
layer3VpnPassthroughEnabled boolean | Is VPN passthrough enabled?
layer3WebAuthFlexAcl String | When a layer 3 web policy is true, this denotes the the FlexConnect ACL for external web authentication in locally switched WLANs.
layer3WebAuthType WlanWebAuthTypeEnum | When a layer 3 web policy is true and layer3GlobalWebAuth is false, this denotes the type of web authentication to be used. Allowed values DEFAULT CUSTOMIZED EXTERNAL
layer3WebPolicyAuthenticationEnabled boolean | Is the authentication web policy enabled?
layer3WebPolicyConditionalRedirectEnabled boolean | Is the conditional redirect web policy enabled?
layer3WebPolicyOnMacFailureEnabled boolean | Is the WebAuth on MAC failure web policy enabled?
layer3WebPolicyPassthroughEnabled boolean | Is the passthrough web policy enabled?
multicastVlanEnabled boolean | Is a multicast VLAN enabled?
multicastVlanInterface String | When multicastVlanInterface is true, this denotes the multicast VLAN.
profileName String | Profile name of the WLAN.
qos7920Cac PhoneSupport7920Enum | Denotes the Call Admission Control (CAC) configuration for Cisco 7920 phones. Allowed values DISABLED CLIENTCAC APCAC CLIENTANDAPCAC
qosAvcProfileName String | Denotes the Application Visibility and Control (AVC) profile for this WLAN.
qosNbarVisibilityEnabled boolean | Is Network Based Application Recognition (NBAR) deep packet inspection enabled on this WLAN?
qosNetflowMonitor String | Denotes the Netflow monitor configured for this WLAN.
qosPerSSidBurstRealTimeUpstreamRate int | Denotes the peak data rate limit for upstream UDP traffic for the WLAN. Zero means no restriction. Measured in Kbps.
qosPerSsidAverageDownstreamRate int | Denotes the average data rate limit for downstream TCP traffic for the WLAN. Zero means no restriction. Measured in Kbps.
qosPerSsidAverageRealTimeDownstreamRate int | Denotes the average data rate limit for downstream UDP traffic for the WLAN. Zero means no restriction. Measured in Kbps.
qosPerSsidAverageRealTimeUpstreamRate int | Denotes the average data rate limit for upstream UDP traffic for the WLAN. Zero means no restriction. Measured in Kbps.
qosPerSsidAverageUpstreamRate int | Denotes the average data rate limit for upstream TCP traffic for the WLAN. Zero means no restriction. Measured in Kbps.
qosPerSsidBurstDownstreamRate int | Denotes the peak data rate limit for downstream TCP traffic for the WLAN. Zero means no restriction. Measured in Kbps.
qosPerSsidBurstRealTimeDownstreamRate int | Denotes the peak data rate limit for downstream UDP traffic for the WLAN. Zero means no restriction. Measured in Kbps.
qosPerSsidBurstUpstreamRate int | Denotes the peak data rate limit for upstream TCP traffic for the WLAN. Zero means no restriction. Measured in Kbps.
qosPerUserAverageDownstreamRate int | Denotes the average data rate limit for downstream TCP traffic for a client. Zero means no restriction. Measured in Kbps.
qosPerUserAverageRealTimeDownstreamRate int | Denotes the average data rate limit for downstream UDP traffic for a client. Zero means no restriction. Measured in Kbps.
qosPerUserAverageRealTimeUpstreamRate int | Denotes the average data rate limit for upstream UDP traffic for a client. Zero means no restriction. Measured in Kbps.
qosPerUserAverageUpstreamRate int | Denotes the average data rate limit for upstream TCP traffic for a client. Zero means no restriction. Measured in Kbps.
qosPerUserBurstDownstreamRate int | Denotes the peak data rate limit for downstream TCP traffic for a client. Zero means no restriction. Measured in Kbps.
qosPerUserBurstRealTimeDownstreamRate int | Denotes the peak data rate limit for downstream UDP traffic for a client. Zero means no restriction. Measured in Kbps.
qosPerUserBurstRealTimeUpstreamRate int | Denotes the peak data rate limit for upstream UDP traffic for a client. Zero means no restriction. Measured in Kbps.
qosPerUserBurstUpstreamRate int | Denotes the peak data rate limit for upstream TCP traffic for a client. Zero means no restriction. Measured in Kbps.
qosProfile QosEnum | Denotes the QoS level for the WLAN. Allowed values BRONZE SILVER GOLD PLATINUM
qosWmmPolicy DisabledAllowedRequiredEnum | Denotes the state of the Wi-fi Multimedia (WMM) policy for this WLAN. Allowed values DISABLED ALLOWED REQUIRED
radioPolicy RadioPolicyEnum | Denotes the WLAN radio policy. Allowed values ALL ONLY80211A ONLY80211B ONLY80211G ONLY80211BG ONLY80211AG ONLY80211AB NONE REMOTELAN
ssid String | SSID of the WLAN.
templateName String | The name of the WLAN template.
vpnPassThroughGatewayAddress InetAddress | When layer3VpnPassthroughEnabled is true, this denotes the IP address of the VPN gateway.
webAuthExternalUrl String | When a layer 3 web policy is enabled, layer3GlobalWebAuthEnabled is false, and layer3WebAuthType is set to "External", this denotes the URL of the authentication server.
webAuthLoginFailurePage String | When a layer 3 web policy is enabled, layer3GlobalWebAuthEnabled is false, and layer3WebAuthType is set to "Customized", this denotes the page for authentication failures.
webAuthLoginPage String | When a layer 3 web policy is enabled, layer3GlobalWebAuthEnabled is false, and layer3WebAuthType is set to "Customized", this denotes the page for authentication.
webAuthLogoutPage String | When a layer 3 web policy is enabled, layer3GlobalWebAuthEnabled is false, and layer3WebAuthType is set to "Customized", this denotes the page for logout.
webPassthruEmailInputEnabled boolean | When layer3WebPolicyPassthroughEnabled is true, this denotes whether the client is prompted to enter an email address when connecting.
wepAllowSharedKeyAuthentication boolean | When wepSecurityEnabled is true, this denotes whether shared key authentication is enabled.
wepKeyIndex int | When wepSecurityEnabled is true, this denotes the key index.
wepKeySize WepEncryptionTypeEnum | When wepSecurityEnabled is true, this denotes whether shared key authentication is enabled. Allowed values WEP104 NONE WEP40 WEP128 AESOCB128 WEP_40 WEP_104
wepSecurityEnabled boolean | Is WEP layer 2 security enabled?
wpa2Enabled boolean | When wpaSecurityEnabled is true, this denotes whether the WPA2 policy is enabled.
wpa2EncryptionProtocolAes boolean | When wpaSecurityEnabled and wpa2Enabled are true, this denotes whether AES encryption is supported for the WPA2 policy.
wpa2EncryptionProtocolTkip boolean | When wpaSecurityEnabled and wpa2Enabled are true, this denotes whether TKIP encryption is supported for the WPA2 policy.
wpaAuthenticationKeyManagement8021x boolean | When wpaSecurityEnabled is true, this denotes whether 802.1X key management is enabled.
wpaAuthenticationKeyManagementCckm boolean | When wpaSecurityEnabled is true, this denotes whether Cisco Centralized Key Management (CCKM) is enabled.
wpaAuthenticationKeyManagementFt8021x boolean | When wpaSecurityEnabled is true, this denotes whether Fast Transition (FT) 802.1X key management is enabled.
wpaAuthenticationKeyManagementFtPsk boolean | When wpaSecurityEnabled is true, this denotes whether Fast Transition (FT) preshared key management is enabled.
wpaAuthenticationKeyManagementPmf8021x boolean | When wpaSecurityEnabled is true, this denotes whether Protected Management Frame (PMF) 802.1X key management is enabled.
wpaAuthenticationKeyManagementPmfPsk boolean | When wpaSecurityEnabled is true, this denotes whether Protected Management Frame (PMF) preshared key management is enabled.
wpaAuthenticationKeyManagementPsk boolean | When wpaSecurityEnabled is true, this denotes whether preshared key management is enabled.
wpaControllerSpecificPresharedKeyEnabled boolean | Is controller specific preshared key enabled?
wpaEnabled boolean | When wpaSecurityEnabled is true, this denotes whether the WPA1 policy is enabled.
wpaEncryptionProtocolAes boolean | When wpaSecurityEnabled and wpaEnabled are both true, this denotes whether AES encryption is supported for the WPA1 policy.
wpaEncryptionProtocolTkip boolean | When wpaSecurityEnabled and wpaEnabled are both true, this denotes whether TKIP encryption is supported for the WPA1 policy.
wpaPresharedKey String | When wpaSecurityEnabled is true, this contains preshared key in HEX or ASCII format.
wpaPresharedKeyFormat PskFormatEnum | When wpaSecurityEnabled is true, this denotes preshared key format. Allowed values DEFAULT HEX ASCII
wpaSecurityEnabled boolean | Is WPA layer 2 security enabled?
x8021KeySize x8021EncryptionTypeEnum | When x8021SecurityEnabled is true, this denotes the 802.1X key size. Allowed values WEP104 WEP40 WEP128 NONE WEP_40 WEP_104
x8021SecurityEnabled boolean | Is 802.1X layer 2 security enabled?

## Sample Payloads

Sample payloads are for information only. They are automatically generated and the values included may not be representative of actual valid data values.

### Sample XML Payload

https://10.64.88.203/webacs/api/v3/data/WlanTemplates/15

    <?xml version="1.0" ?>
    <queryResponse type="WlanTemplates" responseType="getEntity" requestUrl="https://10.64.88.203/webacs/api/v3/data/WlanTemplates/15" rootUrl="https://10.64.88.203/webacs/api/v3/data">
      <entity dtoType="wlanTemplatesDTO" type="WlanTemplates" url="https://10.64.88.203/webacs/api/v3/data/WlanTemplates/15">
        <wlanTemplatesDTO displayName="String value" id="15" uuid="String value">
          <aaaAllowOverride>true</aaaAllowOverride>
          <aaaLdapPrimaryServer>String value</aaaLdapPrimaryServer>
          <aaaLdapSecondaryServer>String value</aaaLdapSecondaryServer>
          <aaaLdapTertiaryServer>String value</aaaLdapTertiaryServer>
          <aaaLocalEapAuthenticationEnabled>true</aaaLocalEapAuthenticationEnabled>
          <aaaLocalEapAuthenticationProfileName>String value</aaaLocalEapAuthenticationProfileName>
          <aaaRadiusAccountingPrimaryServer>String value</aaaRadiusAccountingPrimaryServer>
          <aaaRadiusAccountingSecondaryServer>String value</aaaRadiusAccountingSecondaryServer>
          <aaaRadiusAccountingServersEnabled>true</aaaRadiusAccountingServersEnabled>
          <aaaRadiusAccountingTertiaryServer>String value</aaaRadiusAccountingTertiaryServer>
          <aaaRadiusAuthenticationPrimaryServer>String value</aaaRadiusAuthenticationPrimaryServer>
          <aaaRadiusAuthenticationSecondaryServer>String value</aaaRadiusAuthenticationSecondaryServer>
          <aaaRadiusAuthenticationServersEnabled>true</aaaRadiusAuthenticationServersEnabled>
          <aaaRadiusAuthenticationTertiaryServer>String value</aaaRadiusAuthenticationTertiaryServer>
          <aaaRadiusInterimUpdateEnabled>true</aaaRadiusInterimUpdateEnabled>
          <aaaRadiusInterimUpdateInterval>1</aaaRadiusInterimUpdateInterval>
          <adminStatus>true</adminStatus>
          <advancedAironetIeEnabled>true</advancedAironetIeEnabled>
          <advancedClientExclusionEnabled>true</advancedClientExclusionEnabled>
          <advancedClientExclusionTimeout>1</advancedClientExclusionTimeout>
          <advancedCoverageHoleDetectionEnabled>true</advancedCoverageHoleDetectionEnabled>
          <advancedDhcpAddressAssignmentRequired>true</advancedDhcpAddressAssignmentRequired>
          <advancedDhcpProfilingEnabled>true</advancedDhcpProfilingEnabled>
          <advancedDhcpServerIpAddress>
            <address>192.168.115.243</address>
          </advancedDhcpServerIpAddress>
          <advancedDiagnosticChannelEnabled>true</advancedDiagnosticChannelEnabled>
          <advancedDot11anDtimPeriod>1</advancedDot11anDtimPeriod>
          <advancedDot11bgnDtimPeriod>1</advancedDot11bgnDtimPeriod>
          <advancedFlexConnectCentralDhcpProcessingEnabled>true</advancedFlexConnectCentralDhcpProcessingEnabled>
          <advancedFlexConnectLearnClientIpEnabled>true</advancedFlexConnectLearnClientIpEnabled>
          <advancedFlexConnectLocalAuthEnabled>true</advancedFlexConnectLocalAuthEnabled>
          <advancedFlexConnectLocalSwitchingEnabled>true</advancedFlexConnectLocalSwitchingEnabled>
          <advancedFlexConnectNatPatEnabled>true</advancedFlexConnectNatPatEnabled>
          <advancedFlexConnectOverrideDnsEnabled>true</advancedFlexConnectOverrideDnsEnabled>
          <advancedFlexConnectReapCentralAssociation>true</advancedFlexConnectReapCentralAssociation>
          <advancedFlexConnectVlanCentralSwitchingEnabled>true</advancedFlexConnectVlanCentralSwitchingEnabled>
          <advancedHttpProfilingEnabled>true</advancedHttpProfilingEnabled>
          <advancedIpv6Enabled>true</advancedIpv6Enabled>
          <advancedKtsCacEnabled>true</advancedKtsCacEnabled>
          <advancedLoadBalancingBandSelectEnabled>true</advancedLoadBalancingBandSelectEnabled>
          <advancedLoadBalancingEnabled>true</advancedLoadBalancingEnabled>
          <advancedMaximumClients>1</advancedMaximumClients>
          <advancedMdnsProfileName>String value</advancedMdnsProfileName>
          <advancedMdnsSnoopingEnabled>true</advancedMdnsSnoopingEnabled>
          <advancedMediaSessionSnoopingEnabled>true</advancedMediaSessionSnoopingEnabled>
          <advancedMfpClientProtection>DISABLED</advancedMfpClientProtection>
          <advancedMfpSignatureGenerationEnabled>true</advancedMfpSignatureGenerationEnabled>
          <advancedMfpVersion>1</advancedMfpVersion>
          <advancedOverrideInterfaceAclName>String value</advancedOverrideInterfaceAclName>
          <advancedOverrideInterfaceIpv6AclName>String value</advancedOverrideInterfaceIpv6AclName>
          <advancedPassiveClientEnabled>true</advancedPassiveClientEnabled>
          <advancedPeerToPeerBlocking>DISABLE</advancedPeerToPeerBlocking>
          <advancedPmipMobilityType>NONE</advancedPmipMobilityType>
          <advancedPmipProfile>String value</advancedPmipProfile>
          <advancedPmipRealm>String value</advancedPmipRealm>
          <advancedScanDeferPriority0>true</advancedScanDeferPriority0>
          <advancedScanDeferPriority1>true</advancedScanDeferPriority1>
          <advancedScanDeferPriority2>true</advancedScanDeferPriority2>
          <advancedScanDeferPriority3>true</advancedScanDeferPriority3>
          <advancedScanDeferPriority4>true</advancedScanDeferPriority4>
          <advancedScanDeferPriority5>true</advancedScanDeferPriority5>
          <advancedScanDeferPriority6>true</advancedScanDeferPriority6>
          <advancedScanDeferPriority7>true</advancedScanDeferPriority7>
          <advancedScanDeferTime>1</advancedScanDeferTime>
          <advancedSessionTimeout>1</advancedSessionTimeout>
          <advancedWifiDirectClientsPolicy>DISABLED</advancedWifiDirectClientsPolicy>
          <broadcastSsidEnabled>true</broadcastSsidEnabled>
          <ckipKeyIndex>1</ckipKeyIndex>
          <ckipKeyPermutationEnabled>true</ckipKeyPermutationEnabled>
          <ckipKeySize>NONE</ckipKeySize>
          <ckipMmhModeEnabled>true</ckipMmhModeEnabled>
          <ckipSecurityEnabled>true</ckipSecurityEnabled>
          <interfaceName>String value</interfaceName>
          <interfaceType>INTERFACE</interfaceType>
          <isWiredLan>true</isWiredLan>
          <lanType>WIRELESS</lanType>
          <layer2FastTransitionEnabled>true</layer2FastTransitionEnabled>
          <layer2FastTransitionOverDsEnabled>true</layer2FastTransitionOverDsEnabled>
          <layer2FastTransitionReassociationTimeout>1</layer2FastTransitionReassociationTimeout>
          <layer2MacFilteringEnabled>true</layer2MacFilteringEnabled>
          <layer3GlobalWebAuthEnabled>true</layer3GlobalWebAuthEnabled>
          <layer3PreauthenticationAcl>String value</layer3PreauthenticationAcl>
          <layer3PreauthenticationIpv6Acl>String value</layer3PreauthenticationIpv6Acl>
          <layer3VpnPassthroughEnabled>true</layer3VpnPassthroughEnabled>
          <layer3WebAuthFlexAcl>String value</layer3WebAuthFlexAcl>
          <layer3WebAuthType>DEFAULT</layer3WebAuthType>
          <layer3WebPolicyAuthenticationEnabled>true</layer3WebPolicyAuthenticationEnabled>
          <layer3WebPolicyConditionalRedirectEnabled>true</layer3WebPolicyConditionalRedirectEnabled>
          <layer3WebPolicyOnMacFailureEnabled>true</layer3WebPolicyOnMacFailureEnabled>
          <layer3WebPolicyPassthroughEnabled>true</layer3WebPolicyPassthroughEnabled>
          <multicastVlanEnabled>true</multicastVlanEnabled>
          <multicastVlanInterface>String value</multicastVlanInterface>
          <profileName>String value</profileName>
          <qos7920Cac>DISABLED</qos7920Cac>
          <qosAvcProfileName>String value</qosAvcProfileName>
          <qosNbarVisibilityEnabled>true</qosNbarVisibilityEnabled>
          <qosNetflowMonitor>String value</qosNetflowMonitor>
          <qosPerSSidBurstRealTimeUpstreamRate>1</qosPerSSidBurstRealTimeUpstreamRate>
          <qosPerSsidAverageDownstreamRate>1</qosPerSsidAverageDownstreamRate>
          <qosPerSsidAverageRealTimeDownstreamRate>1</qosPerSsidAverageRealTimeDownstreamRate>
          <qosPerSsidAverageRealTimeUpstreamRate>1</qosPerSsidAverageRealTimeUpstreamRate>
          <qosPerSsidAverageUpstreamRate>1</qosPerSsidAverageUpstreamRate>
          <qosPerSsidBurstDownstreamRate>1</qosPerSsidBurstDownstreamRate>
          <qosPerSsidBurstRealTimeDownstreamRate>1</qosPerSsidBurstRealTimeDownstreamRate>
          <qosPerSsidBurstUpstreamRate>1</qosPerSsidBurstUpstreamRate>
          <qosPerUserAverageDownstreamRate>1</qosPerUserAverageDownstreamRate>
          <qosPerUserAverageRealTimeDownstreamRate>1</qosPerUserAverageRealTimeDownstreamRate>
          <qosPerUserAverageRealTimeUpstreamRate>1</qosPerUserAverageRealTimeUpstreamRate>
          <qosPerUserAverageUpstreamRate>1</qosPerUserAverageUpstreamRate>
          <qosPerUserBurstDownstreamRate>1</qosPerUserBurstDownstreamRate>
          <qosPerUserBurstRealTimeDownstreamRate>1</qosPerUserBurstRealTimeDownstreamRate>
          <qosPerUserBurstRealTimeUpstreamRate>1</qosPerUserBurstRealTimeUpstreamRate>
          <qosPerUserBurstUpstreamRate>1</qosPerUserBurstUpstreamRate>
          <qosProfile>BRONZE</qosProfile>
          <qosWmmPolicy>DISABLED</qosWmmPolicy>
          <radioPolicy>ALL</radioPolicy>
          <ssid>String value</ssid>
          <vpnPassThroughGatewayAddress>
            <address>192.168.115.243</address>
          </vpnPassThroughGatewayAddress>
          <webAuthExternalUrl>String value</webAuthExternalUrl>
          <webAuthLoginFailurePage>String value</webAuthLoginFailurePage>
          <webAuthLoginPage>String value</webAuthLoginPage>
          <webAuthLogoutPage>String value</webAuthLogoutPage>
          <webPassthruEmailInputEnabled>true</webPassthruEmailInputEnabled>
          <wepAllowSharedKeyAuthentication>true</wepAllowSharedKeyAuthentication>
          <wepKeyIndex>1</wepKeyIndex>
          <wepKeySize>WEP104</wepKeySize>
          <wepSecurityEnabled>true</wepSecurityEnabled>
          <wpa2Enabled>true</wpa2Enabled>
          <wpa2EncryptionProtocolAes>true</wpa2EncryptionProtocolAes>
          <wpa2EncryptionProtocolTkip>true</wpa2EncryptionProtocolTkip>
          <wpaAuthenticationKeyManagement8021x>true</wpaAuthenticationKeyManagement8021x>
          <wpaAuthenticationKeyManagementCckm>true</wpaAuthenticationKeyManagementCckm>
          <wpaAuthenticationKeyManagementFt8021x>true</wpaAuthenticationKeyManagementFt8021x>
          <wpaAuthenticationKeyManagementFtPsk>true</wpaAuthenticationKeyManagementFtPsk>
          <wpaAuthenticationKeyManagementPmf8021x>true</wpaAuthenticationKeyManagementPmf8021x>
          <wpaAuthenticationKeyManagementPmfPsk>true</wpaAuthenticationKeyManagementPmfPsk>
          <wpaAuthenticationKeyManagementPsk>true</wpaAuthenticationKeyManagementPsk>
          <wpaEnabled>true</wpaEnabled>
          <wpaEncryptionProtocolAes>true</wpaEncryptionProtocolAes>
          <wpaEncryptionProtocolTkip>true</wpaEncryptionProtocolTkip>
          <wpaPresharedKey>String value</wpaPresharedKey>
          <wpaPresharedKeyFormat>DEFAULT</wpaPresharedKeyFormat>
          <wpaSecurityEnabled>true</wpaSecurityEnabled>
          <x8021KeySize>WEP104</x8021KeySize>
          <x8021SecurityEnabled>true</x8021SecurityEnabled>
          <aaaRadiusAccountingWlcSpecificEnabled>true</aaaRadiusAccountingWlcSpecificEnabled>
          <aaaRadiusAuthenticationWlcSpecificEnabled>true</aaaRadiusAuthenticationWlcSpecificEnabled>
          <advancedSessionTimeoutEnabled>true</advancedSessionTimeoutEnabled>
          <hotspot2Enable>
            <hotSpot2Enabled>true</hotSpot2Enabled>
          </hotspot2Enable>
          <hotspot2Operators>
            <hotspot2Operator>
              <operatorId>1</operatorId>
              <operatorLang>String value</operatorLang>
              <operatorName>String value</operatorName>
            </hotspot2Operator>
            <hotspot2Operator>
              <operatorId>11</operatorId>
              <operatorLang>Another string value</operatorLang>
              <operatorName>Another string value</operatorName>
            </hotspot2Operator>
          </hotspot2Operators>
          <hotspot2Ports>
            <hotspot2Port>
              <portConfigId>1</portConfigId>
              <portNo>ICMPESP</portNo>
              <portStatus>CLOSED</portStatus>
              <protocolName>ICMP</protocolName>
            </hotspot2Port>
            <hotspot2Port>
              <portConfigId>11</portConfigId>
              <portNo>FTP</portNo>
              <portStatus>OPEN</portStatus>
              <protocolName>FTP</protocolName>
            </hotspot2Port>
          </hotspot2Ports>
          <hotspot2Wan>
            <downLinkSpeed>1</downLinkSpeed>
            <upLinkSpeed>1</upLinkSpeed>
            <wanLinkStatus>LINKUP</wanLinkStatus>
            <wanSymLinkStatus>SAME</wanSymLinkStatus>
          </hotspot2Wan>
          <hotspotCellularNetworks>
            <hotspotCellularNetwork>
              <countryCode>String value</countryCode>
              <gppIndex>1</gppIndex>
              <networkCode>String value</networkCode>
            </hotspotCellularNetwork>
            <hotspotCellularNetwork>
              <countryCode>Another string value</countryCode>
              <gppIndex>11</gppIndex>
              <networkCode>Another string value</networkCode>
            </hotspotCellularNetwork>
          </hotspotCellularNetworks>
          <hotspotDomains>
            <hotspotDomain>
              <domainId>1</domainId>
              <domainName>String value</domainName>
            </hotspotDomain>
            <hotspotDomain>
              <domainId>11</domainId>
              <domainName>Another string value</domainName>
            </hotspotDomain>
          </hotspotDomains>
          <hotspotGeneral>
            <heSsid>
              <octets>000a959d6816</octets>
            </heSsid>
            <internetAccess>true</internetAccess>
            <ipv4AddressAvailType>NOTAVAILABLE</ipv4AddressAvailType>
            <ipv6AddressAvailType>NOTAVAILABLE</ipv6AddressAvailType>
            <networkAuthType>ACCEPTANCE</networkAuthType>
            <networkType>PRIVATE</networkType>
            <status>true</status>
          </hotspotGeneral>
          <hotspotOuiTemplates>
            <hotspotOuiTemplate>
              <oui>String value</oui>
              <ouiId>1</ouiId>
              <ouiInBeacon>true</ouiInBeacon>
            </hotspotOuiTemplate>
            <hotspotOuiTemplate>
              <oui>Another string value</oui>
              <ouiId>11</ouiId>
              <ouiInBeacon>false</ouiInBeacon>
            </hotspotOuiTemplate>
          </hotspotOuiTemplates>
          <hotspotRealms>
            <hotspotRealm>
              <realmEapMethods>
                <realmEapMethod>
                  <innerAuthMethods>
                    <innerAuthMethod>
                      <realmEapAuthId>1</realmEapAuthId>
                      <realmEapAuthMethod>NONEAPINNERAUTH</realmEapAuthMethod>
                      <realmEapAuthParam>NONE</realmEapAuthParam>
                    </innerAuthMethod>
                    <innerAuthMethod>
                      <realmEapAuthId>11</realmEapAuthId>
                      <realmEapAuthMethod>INNERAUTHEAP</realmEapAuthMethod>
                      <realmEapAuthParam>PAP</realmEapAuthParam>
                    </innerAuthMethod>
                  </innerAuthMethods>
                  <realmEapId>1</realmEapId>
                  <realmEapMethod>NONE</realmEapMethod>
                </realmEapMethod>
                <realmEapMethod>
                  <innerAuthMethods>
                    <innerAuthMethod>
                      <realmEapAuthId>1</realmEapAuthId>
                      <realmEapAuthMethod>NONEAPINNERAUTH</realmEapAuthMethod>
                      <realmEapAuthParam>NONE</realmEapAuthParam>
                    </innerAuthMethod>
                    <innerAuthMethod>
                      <realmEapAuthId>11</realmEapAuthId>
                      <realmEapAuthMethod>INNERAUTHEAP</realmEapAuthMethod>
                      <realmEapAuthParam>PAP</realmEapAuthParam>
                    </innerAuthMethod>
                  </innerAuthMethods>
                  <realmEapId>11</realmEapId>
                  <realmEapMethod>LEAP</realmEapMethod>
                </realmEapMethod>
              </realmEapMethods>
              <realmId>1</realmId>
              <realmName>String value</realmName>
            </hotspotRealm>
            <hotspotRealm>
              <realmEapMethods>
                <realmEapMethod>
                  <innerAuthMethods>
                    <innerAuthMethod>
                      <realmEapAuthId>1</realmEapAuthId>
                      <realmEapAuthMethod>NONEAPINNERAUTH</realmEapAuthMethod>
                      <realmEapAuthParam>NONE</realmEapAuthParam>
                    </innerAuthMethod>
                    <innerAuthMethod>
                      <realmEapAuthId>11</realmEapAuthId>
                      <realmEapAuthMethod>INNERAUTHEAP</realmEapAuthMethod>
                      <realmEapAuthParam>PAP</realmEapAuthParam>
                    </innerAuthMethod>
                  </innerAuthMethods>
                  <realmEapId>1</realmEapId>
                  <realmEapMethod>NONE</realmEapMethod>
                </realmEapMethod>
                <realmEapMethod>
                  <innerAuthMethods>
                    <innerAuthMethod>
                      <realmEapAuthId>1</realmEapAuthId>
                      <realmEapAuthMethod>NONEAPINNERAUTH</realmEapAuthMethod>
                      <realmEapAuthParam>NONE</realmEapAuthParam>
                    </innerAuthMethod>
                    <innerAuthMethod>
                      <realmEapAuthId>11</realmEapAuthId>
                      <realmEapAuthMethod>INNERAUTHEAP</realmEapAuthMethod>
                      <realmEapAuthParam>PAP</realmEapAuthParam>
                    </innerAuthMethod>
                  </innerAuthMethods>
                  <realmEapId>11</realmEapId>
                  <realmEapMethod>LEAP</realmEapMethod>
                </realmEapMethod>
              </realmEapMethods>
              <realmId>11</realmId>
              <realmName>Another string value</realmName>
            </hotspotRealm>
          </hotspotRealms>
          <hotspotServiceAdvertisement>
            <msapEnable>true</msapEnable>
            <serverIndex>1</serverIndex>
          </hotspotServiceAdvertisement>
          <lastModified>2</lastModified>
          <templateName>String value</templateName>
          <wpaControllerSpecificPresharedKeyEnabled>true</wpaControllerSpecificPresharedKeyEnabled>
        </wlanTemplatesDTO>
      </entity>
    </queryResponse>

### Sample JSON Payload

https://10.64.88.203/webacs/api/v3/data/WlanTemplates/15.json

    {
      "queryResponse" : {
        "@type" : "WlanTemplates",
        "@requestUrl" : "https://10.64.88.203/webacs/api/v3/data/WlanTemplates/15",
        "@responseType" : "getEntity",
        "@rootUrl" : "https://10.64.88.203/webacs/api/v3/data",
        "entity" : [ {
          "@dtoType" : "wlanTemplatesDTO",
          "@type" : "WlanTemplates",
          "@url" : "https://10.64.88.203/webacs/api/v3/data/WlanTemplates/15",
          "wlanTemplatesDTO" : {
            "@displayName" : "String value",
            "@id" : 15,
            "@uuid" : "String value",
            "aaaAllowOverride" : true,
            "aaaLdapPrimaryServer" : "String value",
            "aaaLdapSecondaryServer" : "String value",
            "aaaLdapTertiaryServer" : "String value",
            "aaaLocalEapAuthenticationEnabled" : true,
            "aaaLocalEapAuthenticationProfileName" : "String value",
            "aaaRadiusAccountingPrimaryServer" : "String value",
            "aaaRadiusAccountingSecondaryServer" : "String value",
            "aaaRadiusAccountingServersEnabled" : true,
            "aaaRadiusAccountingTertiaryServer" : "String value",
            "aaaRadiusAccountingWlcSpecificEnabled" : true,
            "aaaRadiusAuthenticationPrimaryServer" : "String value",
            "aaaRadiusAuthenticationSecondaryServer" : "String value",
            "aaaRadiusAuthenticationServersEnabled" : true,
            "aaaRadiusAuthenticationTertiaryServer" : "String value",
            "aaaRadiusAuthenticationWlcSpecificEnabled" : true,
            "aaaRadiusInterimUpdateEnabled" : true,
            "aaaRadiusInterimUpdateInterval" : 1,
            "adminStatus" : true,
            "advancedAironetIeEnabled" : true,
            "advancedClientExclusionEnabled" : true,
            "advancedClientExclusionTimeout" : 1,
            "advancedCoverageHoleDetectionEnabled" : true,
            "advancedDhcpAddressAssignmentRequired" : true,
            "advancedDhcpProfilingEnabled" : true,
            "advancedDhcpServerIpAddress" : {
              "address" : "192.168.115.243"
            },
            "advancedDiagnosticChannelEnabled" : true,
            "advancedDot11anDtimPeriod" : 1,
            "advancedDot11bgnDtimPeriod" : 1,
            "advancedFlexConnectCentralDhcpProcessingEnabled" : true,
            "advancedFlexConnectLearnClientIpEnabled" : true,
            "advancedFlexConnectLocalAuthEnabled" : true,
            "advancedFlexConnectLocalSwitchingEnabled" : true,
            "advancedFlexConnectNatPatEnabled" : true,
            "advancedFlexConnectOverrideDnsEnabled" : true,
            "advancedFlexConnectReapCentralAssociation" : true,
            "advancedFlexConnectVlanCentralSwitchingEnabled" : true,
            "advancedHttpProfilingEnabled" : true,
            "advancedIpv6Enabled" : true,
            "advancedKtsCacEnabled" : true,
            "advancedLoadBalancingBandSelectEnabled" : true,
            "advancedLoadBalancingEnabled" : true,
            "advancedMaximumClients" : 1,
            "advancedMdnsProfileName" : "String value",
            "advancedMdnsSnoopingEnabled" : true,
            "advancedMediaSessionSnoopingEnabled" : true,
            "advancedMfpClientProtection" : "DISABLED",
            "advancedMfpSignatureGenerationEnabled" : true,
            "advancedMfpVersion" : 1,
            "advancedOverrideInterfaceAclName" : "String value",
            "advancedOverrideInterfaceIpv6AclName" : "String value",
            "advancedPassiveClientEnabled" : true,
            "advancedPeerToPeerBlocking" : "DISABLE",
            "advancedPmipMobilityType" : "NONE",
            "advancedPmipProfile" : "String value",
            "advancedPmipRealm" : "String value",
            "advancedScanDeferPriority0" : true,
            "advancedScanDeferPriority1" : true,
            "advancedScanDeferPriority2" : true,
            "advancedScanDeferPriority3" : true,
            "advancedScanDeferPriority4" : true,
            "advancedScanDeferPriority5" : true,
            "advancedScanDeferPriority6" : true,
            "advancedScanDeferPriority7" : true,
            "advancedScanDeferTime" : 1,
            "advancedSessionTimeout" : 1,
            "advancedSessionTimeoutEnabled" : true,
            "advancedWifiDirectClientsPolicy" : "DISABLED",
            "broadcastSsidEnabled" : true,
            "ckipKeyIndex" : 1,
            "ckipKeyPermutationEnabled" : true,
            "ckipKeySize" : "NONE",
            "ckipMmhModeEnabled" : true,
            "ckipSecurityEnabled" : true,
            "hotspot2Enable" : {
              "hotSpot2Enabled" : true
            },
            "hotspot2Operators" : {
              "hotspot2Operator" : [ {
                "operatorId" : 1,
                "operatorLang" : "String value",
                "operatorName" : "String value"
              }, {
                "operatorId" : 11,
                "operatorLang" : "Another string value",
                "operatorName" : "Another string value"
              } ]
            },
            "hotspot2Ports" : {
              "hotspot2Port" : [ {
                "portConfigId" : 1,
                "portNo" : "ICMPESP",
                "portStatus" : "CLOSED",
                "protocolName" : "ICMP"
              }, {
                "portConfigId" : 11,
                "portNo" : "FTP",
                "portStatus" : "OPEN",
                "protocolName" : "FTP"
              } ]
            },
            "hotspot2Wan" : {
              "downLinkSpeed" : 1,
              "upLinkSpeed" : 1,
              "wanLinkStatus" : "LINKUP",
              "wanSymLinkStatus" : "SAME"
            },
            "hotspotCellularNetworks" : {
              "hotspotCellularNetwork" : [ {
                "countryCode" : "String value",
                "gppIndex" : 1,
                "networkCode" : "String value"
              }, {
                "countryCode" : "Another string value",
                "gppIndex" : 11,
                "networkCode" : "Another string value"
              } ]
            },
            "hotspotDomains" : {
              "hotspotDomain" : [ {
                "domainId" : 1,
                "domainName" : "String value"
              }, {
                "domainId" : 11,
                "domainName" : "Another string value"
              } ]
            },
            "hotspotGeneral" : {
              "heSsid" : {
                "octets" : "000a959d6816"
              },
              "internetAccess" : true,
              "ipv4AddressAvailType" : "NOTAVAILABLE",
              "ipv6AddressAvailType" : "NOTAVAILABLE",
              "networkAuthType" : "ACCEPTANCE",
              "networkType" : "PRIVATE",
              "status" : true
            },
            "hotspotOuiTemplates" : {
              "hotspotOuiTemplate" : [ {
                "oui" : "String value",
                "ouiId" : 1,
                "ouiInBeacon" : true
              }, {
                "oui" : "Another string value",
                "ouiId" : 11,
                "ouiInBeacon" : false
              } ]
            },
            "hotspotRealms" : {
              "hotspotRealm" : [ {
                "realmEapMethods" : {
                  "realmEapMethod" : [ {
                    "innerAuthMethods" : {
                      "innerAuthMethod" : [ {
                        "realmEapAuthId" : 1,
                        "realmEapAuthMethod" : "NONEAPINNERAUTH",
                        "realmEapAuthParam" : "NONE"
                      }, {
                        "realmEapAuthId" : 11,
                        "realmEapAuthMethod" : "INNERAUTHEAP",
                        "realmEapAuthParam" : "PAP"
                      } ]
                    },
                    "realmEapId" : 1,
                    "realmEapMethod" : "NONE"
                  }, {
                    "innerAuthMethods" : {
                      "innerAuthMethod" : [ {
                        "realmEapAuthId" : 1,
                        "realmEapAuthMethod" : "NONEAPINNERAUTH",
                        "realmEapAuthParam" : "NONE"
                      }, {
                        "realmEapAuthId" : 11,
                        "realmEapAuthMethod" : "INNERAUTHEAP",
                        "realmEapAuthParam" : "PAP"
                      } ]
                    },
                    "realmEapId" : 11,
                    "realmEapMethod" : "LEAP"
                  } ]
                },
                "realmId" : 1,
                "realmName" : "String value"
              }, {
                "realmEapMethods" : {
                  "realmEapMethod" : [ {
                    "innerAuthMethods" : {
                      "innerAuthMethod" : [ {
                        "realmEapAuthId" : 1,
                        "realmEapAuthMethod" : "NONEAPINNERAUTH",
                        "realmEapAuthParam" : "NONE"
                      }, {
                        "realmEapAuthId" : 11,
                        "realmEapAuthMethod" : "INNERAUTHEAP",
                        "realmEapAuthParam" : "PAP"
                      } ]
                    },
                    "realmEapId" : 1,
                    "realmEapMethod" : "NONE"
                  }, {
                    "innerAuthMethods" : {
                      "innerAuthMethod" : [ {
                        "realmEapAuthId" : 1,
                        "realmEapAuthMethod" : "NONEAPINNERAUTH",
                        "realmEapAuthParam" : "NONE"
                      }, {
                        "realmEapAuthId" : 11,
                        "realmEapAuthMethod" : "INNERAUTHEAP",
                        "realmEapAuthParam" : "PAP"
                      } ]
                    },
                    "realmEapId" : 11,
                    "realmEapMethod" : "LEAP"
                  } ]
                },
                "realmId" : 11,
                "realmName" : "Another string value"
              } ]
            },
            "hotspotServiceAdvertisement" : {
              "msapEnable" : true,
              "serverIndex" : 1
            },
            "interfaceName" : "String value",
            "interfaceType" : "INTERFACE",
            "isWiredLan" : true,
            "lanType" : "WIRELESS",
            "lastModified" : 2,
            "layer2FastTransitionEnabled" : true,
            "layer2FastTransitionOverDsEnabled" : true,
            "layer2FastTransitionReassociationTimeout" : 1,
            "layer2MacFilteringEnabled" : true,
            "layer3GlobalWebAuthEnabled" : true,
            "layer3PreauthenticationAcl" : "String value",
            "layer3PreauthenticationIpv6Acl" : "String value",
            "layer3VpnPassthroughEnabled" : true,
            "layer3WebAuthFlexAcl" : "String value",
            "layer3WebAuthType" : "DEFAULT",
            "layer3WebPolicyAuthenticationEnabled" : true,
            "layer3WebPolicyConditionalRedirectEnabled" : true,
            "layer3WebPolicyOnMacFailureEnabled" : true,
            "layer3WebPolicyPassthroughEnabled" : true,
            "multicastVlanEnabled" : true,
            "multicastVlanInterface" : "String value",
            "profileName" : "String value",
            "qos7920Cac" : "DISABLED",
            "qosAvcProfileName" : "String value",
            "qosNbarVisibilityEnabled" : true,
            "qosNetflowMonitor" : "String value",
            "qosPerSSidBurstRealTimeUpstreamRate" : 1,
            "qosPerSsidAverageDownstreamRate" : 1,
            "qosPerSsidAverageRealTimeDownstreamRate" : 1,
            "qosPerSsidAverageRealTimeUpstreamRate" : 1,
            "qosPerSsidAverageUpstreamRate" : 1,
            "qosPerSsidBurstDownstreamRate" : 1,
            "qosPerSsidBurstRealTimeDownstreamRate" : 1,
            "qosPerSsidBurstUpstreamRate" : 1,
            "qosPerUserAverageDownstreamRate" : 1,
            "qosPerUserAverageRealTimeDownstreamRate" : 1,
            "qosPerUserAverageRealTimeUpstreamRate" : 1,
            "qosPerUserAverageUpstreamRate" : 1,
            "qosPerUserBurstDownstreamRate" : 1,
            "qosPerUserBurstRealTimeDownstreamRate" : 1,
            "qosPerUserBurstRealTimeUpstreamRate" : 1,
            "qosPerUserBurstUpstreamRate" : 1,
            "qosProfile" : "BRONZE",
            "qosWmmPolicy" : "DISABLED",
            "radioPolicy" : "ALL",
            "ssid" : "String value",
            "templateName" : "String value",
            "vpnPassThroughGatewayAddress" : {
              "address" : "192.168.115.243"
            },
            "webAuthExternalUrl" : "String value",
            "webAuthLoginFailurePage" : "String value",
            "webAuthLoginPage" : "String value",
            "webAuthLogoutPage" : "String value",
            "webPassthruEmailInputEnabled" : true,
            "wepAllowSharedKeyAuthentication" : true,
            "wepKeyIndex" : 1,
            "wepKeySize" : "WEP104",
            "wepSecurityEnabled" : true,
            "wpa2Enabled" : true,
            "wpa2EncryptionProtocolAes" : true,
            "wpa2EncryptionProtocolTkip" : true,
            "wpaAuthenticationKeyManagement8021x" : true,
            "wpaAuthenticationKeyManagementCckm" : true,
            "wpaAuthenticationKeyManagementFt8021x" : true,
            "wpaAuthenticationKeyManagementFtPsk" : true,
            "wpaAuthenticationKeyManagementPmf8021x" : true,
            "wpaAuthenticationKeyManagementPmfPsk" : true,
            "wpaAuthenticationKeyManagementPsk" : true,
            "wpaControllerSpecificPresharedKeyEnabled" : true,
            "wpaEnabled" : true,
            "wpaEncryptionProtocolAes" : true,
            "wpaEncryptionProtocolTkip" : true,
            "wpaPresharedKey" : "String value",
            "wpaPresharedKeyFormat" : "DEFAULT",
            "wpaSecurityEnabled" : true,
            "x8021KeySize" : "WEP104",
            "x8021SecurityEnabled" : true
          }
        } ]
      }
    }

### Resource Information

Rate Limiting? | Yes
Sorting? | Yes
Paging? | Yes
Filtering? | Yes
Group Filtering? | No
Aggregation? | No
Response Formats | xml json
User Group | NBI Read
HTTP Methods | GET

## Resource URL

/webacs/api/v4/data/WlanTemplates

Unmodified

This resource has not been modified since the previous API version.

## Response Parameters

Attribute | Description
--- | ---
aaaAllowOverride boolean | Is allow AAA override enabled?
aaaLdapPrimaryServer String | Primary LDAP server.
aaaLdapSecondaryServer String | Secondary LDAP server.
aaaLdapTertiaryServer String | Tertiary LDAP server.
aaaLocalEapAuthenticationEnabled boolean | Is local EAP authentication enabled?
aaaLocalEapAuthenticationProfileName String | When aaaLocalEapAuthenticationEnabled is true, this defines the EAP profile that will be used.
aaaRadiusAccountingPrimaryServer String | When aaaRadiusAccountingServersEnabled is true, this is the primary RADIUS accounting server.
aaaRadiusAccountingSecondaryServer String | When aaaRadiusAccountingServersEnabled is true, this is the secondary RADIUS accounting server.
aaaRadiusAccountingServersEnabled boolean | Is RADIUS accounting enabled?
aaaRadiusAccountingTertiaryServer String | When aaaRadiusAccountingServersEnabled is true, this is the tertiary RADIUS accounting server.
aaaRadiusAccountingWlcSpecificEnabled boolean | Is controller specific RADIUS accounting servers enabled?
aaaRadiusAuthenticationPrimaryServer String | When aaaRadiusAuthenticationServersEnabled is true, this is the primary RADIUS authentication server.
aaaRadiusAuthenticationSecondaryServer String | When aaaRadiusAuthenticationServersEnabled is true, this is the secondary RADIUS authentication server.
aaaRadiusAuthenticationServersEnabled boolean | Is RADIUS authentication enabled?
aaaRadiusAuthenticationTertiaryServer String | When aaaRadiusAuthenticationServersEnabled is true, this is the tertiary RADIUS authentication server.
aaaRadiusAuthenticationWlcSpecificEnabled boolean | Is controller specific RADIUS authentication servers enabled?
aaaRadiusInterimUpdateEnabled boolean | Is RADIUS server accounting interim update enabled?
aaaRadiusInterimUpdateInterval int | When aaaRadiusInterimUpdateEnabled is true, this determines the update interval. Measured in seconds.
adminStatus boolean | Is the WLAN administratively enabled?
advancedAironetIeEnabled boolean | Is Aironet Information Elements (IEs) enabled for this WLAN?
advancedClientExclusionEnabled boolean | Is automatic client exclusion enabled for this WLAN?
advancedClientExclusionTimeout int | When advancedClientExclusionEnabled is true, this denotes the length of the timeout. A value of zero represents an infinite timeout. Measured in seconds.
advancedCoverageHoleDetectionEnabled boolean | Is Coverage Hole Detection enabled for this WLAN?
advancedDhcpAddressAssignmentRequired boolean | Are all clients required to obtain an IP address from the DHCP server for this WLAN?
advancedDhcpProfilingEnabled boolean | Should the wireless controller collect the DHCP attributes of clients on this WLAN?
advancedDhcpServerIpAddress InetAddress | If this contains a valid address, an IPv4 DHCP server has been specified for this WLAN.
advancedDiagnosticChannelEnabled boolean | Is the diagnostic channel available for this WLAN?
advancedDot11anDtimPeriod int | Denotes the Delivery Traffic Indication Map (DTIM) interval for 802.11a/n radios, during which broadcast and multicast frames will be transmitted. A value of one results in a broadcast after every beacon, two for every other beacon, and so on.
advancedDot11bgnDtimPeriod int | Denotes the Delivery Traffic Indication Map (DTIM) interval for 802.11b/g/n radios, during which broadcast and multicast frames will be transmitted. A value of one results in a broadcast after every beacon, two for every other beacon, and so on.
advancedFlexConnectCentralDhcpProcessingEnabled boolean | Are DHCP packets received by the access point sent to the controller then forwarded to the WLAN's corresponding VLAN?
advancedFlexConnectLearnClientIpEnabled boolean | Is client IP address learning enabled?
advancedFlexConnectLocalAuthEnabled boolean | Is local authentication enabled?
advancedFlexConnectLocalSwitchingEnabled boolean | When true, access points will locally switch traffic, rather than forwarding to the wireless controller.
advancedFlexConnectNatPatEnabled boolean | Is Network Address Translation (NAT) and Port Address Translation (PAT) enabled?
advancedFlexConnectOverrideDnsEnabled boolean | When true, clients are given the DNS server of the access point rather than of the WLAN's configured interface.
advancedFlexConnectReapCentralAssociation boolean | Is Reap Central Association enabled?
advancedFlexConnectVlanCentralSwitchingEnabled boolean | Is VLAN based central switching enabled?
advancedHttpProfilingEnabled boolean | Should the wireless controller collect the HTTP attributes of clients on this WLAN?
advancedIpv6Enabled boolean | Is IPv6 enabled?
advancedKtsCacEnabled boolean | Is CAC based on the Key Telephone System (KTS) enabled on this WLAN?
advancedLoadBalancingBandSelectEnabled boolean | Is client band select enabled?
advancedLoadBalancingEnabled boolean | Is client load balancing enabled?
advancedMaximumClients int | Denotes the maximum number of clients. A value of zero means unlimited.
advancedMdnsProfileName String | When advancedMdnsSnoopingEnabled is true, this denotes the mDNS profile. Clients receive service advertisements only for the services associated with the profile.
advancedMdnsSnoopingEnabled boolean | Is mDNS snooping enabled?
advancedMediaSessionSnoopingEnabled boolean | Should the access point snoop on Session Initiation Protocol (SIP) traffic, and report back to the controller the establishment termination and failure of voice calls?
advancedMfpClientProtection DisabledEnabledRequiredEnum | Denotes whether client management frame protection (MFP) is enabled (optional), required, or disabled for this WLAN. Allowed values DISABLED ENABLED REQUIRED
advancedMfpSignatureGenerationEnabled boolean | Do 802.11 management frames transmitted by the access point have a signature to verify authenticity?
advancedMfpVersion int | Denotes the version of management frame protection (MFP).
advancedOverrideInterfaceAclName String | Denotes an IPv4 ACL that overrides the ACL configured for the WLAN's interface.
advancedOverrideInterfaceIpv6AclName String | Denotes an IPv6 ACL that overrides the ACL configured for the WLAN's interface.
advancedPassiveClientEnabled boolean | Should the controller forward ARP requests out to the WLAN for passive clients?
advancedPeerToPeerBlocking Peer2PeerBlockingEnum | Denotes whether peer-to-peer blocking is disabled, enabled, or if the packets are forwarded to the next device. Allowed values DISABLE DROP FORWARDUP ALLOWPRIVATEGROUP
advancedPmipMobilityType PmipMobilityTypeEnum | Denotes the Proxy Mobile IP (PMIP) type for this WLAN. Allowed values NONE PMIP
advancedPmipProfile String | Denotes the Proxy Mobile IP (PMIP) profile for this WLAN.
advancedPmipRealm String | Denotes the default realm of the Proxy Mobile IPv6 (PMIPv6) WLAN.
advancedScanDeferPriority0 boolean | Is priority 0 for the channel scan enabled?
advancedScanDeferPriority1 boolean | Is priority 1 for the channel scan enabled?
advancedScanDeferPriority2 boolean | Is priority 2 for the channel scan enabled?
advancedScanDeferPriority3 boolean | Is priority 3 for the channel scan enabled?
advancedScanDeferPriority4 boolean | Is priority 4 for the channel scan enabled?
advancedScanDeferPriority5 boolean | Is priority 5 for the channel scan enabled?
advancedScanDeferPriority6 boolean | Is priority 6 for the channel scan enabled?
advancedScanDeferPriority7 boolean | Is priority 7 for the channel scan enabled?
advancedScanDeferTime int | Denotes the channel scan defer time. Measured in milliseconds.
advancedSessionTimeout int | Denotes the maximum time for a client session before requiring reauthentication. Zero means no timeout. Measured in seconds.
advancedSessionTimeoutEnabled boolean | Is advancedSessionTimeout enabled?
advancedWifiDirectClientsPolicy DisabledAllowedNotAllowedEnum | Denotes the Wi-Fi Direct Clients Policy for this WLAN. Allowed values DISABLED ALLOWED NOTALLOWED XCONNECTNOTALLOW
broadcastSsidEnabled boolean | Is SSID broadcasting enabled?
ckipKeyIndex int | When ckipSecurityEnabled is true, this denotes the key index.
ckipKeyPermutationEnabled boolean | When ckipSecurityEnabled is true, this denotes whether key permutation is enabled.
ckipKeySize CkipEncryptionTypeEnum | When ckipSecurityEnabled is true, this denotes the key size. Allowed values NONE LEN40 LEN104
ckipMmhModeEnabled boolean | When ckipSecurityEnabled is true, this denotes whether multimodular mode hashing is enabled.
ckipSecurityEnabled boolean | Is CKIP layer 2 security enabled?
hotspot2Enable WlanMcHotSpotEnableTemplate | This attribute represents enablement of HotSpot 2.0.
Attribute | Description
--- | ---
hotSpot2Enabled boolean | Is HotSpot 2.0 enabled?
hotspot2Operators WlanMcHotSpotOperatorConfigTemplate[] | These attributes represent HotSpot 2.0 operators.
Attribute | Description
--- | ---
operatorId int | Operator index of the hotspot provider.
operatorLang String | Language code.
operatorName String | Operator name of the hotspot provider.
hotspot2Ports WlanMcHotSpotPortConfigTemplate[] | These attributes represent HotSpot 2.0 port configurations.
Attribute | Description
--- | ---
portConfigId int | Port configuration index.
portNo PortNoEnum | Port number used for the IP. Allowed values ICMPESP FTP SSH HTTP TTLSVPN PPTPVPN VOIP IKEV2 IPSECNAT
portStatus PortStatusEnum | Status of the IP port. Allowed values CLOSED OPEN UNKNOWN
protocolName ProtocolNameEnum | Internet protocol name. This parameter provides information on the connection status of the most commonly used communication protocols and ports. Allowed values ICMP FTP IKEV2 ESP
hotspot2Wan WlanMcHotSpotWanTemplate | These attributes represent HotSpot 2.0 WAN metrics configuration.
Attribute | Description
--- | ---
downLinkSpeed int | Downlink speed of the WAN backhaul link. Measured in Kbps.
upLinkSpeed int | Uplink speed of the WAN backhaul. Measured in Kbps.
wanLinkStatus WanLinkStatusEnum | WAN link status. Allowed values LINKUP LINKDOWN LINKINTESTSTATE NOTCONFIGURED
wanSymLinkStatus WanSymLinkStatusEnum | WAN symmetric link status. Allowed values SAME DIFFERENT
hotspotCellularNetworks WlanMc3GppConfigTemplate[] | These attributes represent 802.11u cellular network parameters.
Attribute | Description
--- | ---
countryCode String | Mobile country code in Binary Coded Decimal (BCD) format.
gppIndex int | Cellular index.
networkCode String | Mobile network code in Binary Coded Decimal (BCD) format.
hotspotDomains WlanMcDomainConfigTemplate[] | These attributes represent 802.11u domains.
Attribute | Description
--- | ---
domainId int | Domain index.
domainName String | Domain name operating in the WLAN network.
hotspotGeneral WlanMcGeneralConfigTemplate | These attributes represent 802.11u general parameters.
Attribute | Description
--- | ---
heSsid MacAddress | The Homogenous Extended Service Set Identifier (HESSID).
internetAccess boolean | Is Internet Access enabled?
ipv4AddressAvailType IPv4AddressAvailTypeEnum | IPv4 type address. Allowed values NOTAVAILABLE PUBLIC PORTRESTRICTED SINGLENATPRIVATE DOUBLENATPRIVATE PORTRESTRICTEDSINGLENATPRIVATE PORTRESTRICTEDDOUBLENATPRIVATE UNKNOWN
ipv6AddressAvailType IPv6AddressAvailTypeEnum | IPv6 type address. Allowed values NOTAVAILABLE AVAILABLE UNKNOWN
networkAuthType NetworkAuthTypeEnum | Network authentication type for 802.11u on this WLAN. Allowed values ACCEPTANCE ENROLLMENT REDIRECTION DNSREDIRECTION NOTCONFIGURED
networkType NetworkTypeEnum | Network type of this WLAN. Allowed values PRIVATE PRIVATEWITHGUESTACCESS PUBLICPAID PUBLICFREE PERSONALDEVICE EMERGENCYSERVICEONLY TESTEQUIPMENT WILDCARD UNKNOWN
status boolean | Is 802.11u enabled?
hotspotOuiTemplate WlanMcOuiConfigTemplate[] | These attributes represent 802.11u OUIs.
Attribute | Description
--- | ---
oui String | Organization Unique Identifier (OUI).
ouiId int | OUI index.
ouiInBeacon boolean | Are Organization Unique Identifier (OUI) beacon responses enabled?
hotspotRealms WlanMcRealmConfigTemplate[] | These attributes represent 802.11u realms.
Attribute | Description
--- | ---
realmEapMethods WlanMcRealmEapConfigTemplate[] | Extensible Authentication Protocol (EAP) list.
Attribute | Description
--- | ---
innerAuthMethods WlanMcRealmEapAuthConfigTemplate[] | Auth method list.
Attribute | Description
--- | ---
realmEapAuthId int | Auth method index.
realmEapAuthMethod RealmEapAuthMethodEnum | Inner auth method. Allowed values NONEAPINNERAUTH INNERAUTHEAP CREDENTIAL TUNNELEDEAPCREDENTIAL
realmEapAuthParam RealmEapAuthParamEnum | Auth param. Allowed values NONE PAP CHAP MSCHAP MSCHAPV2 LEAP PEAP EAPTLS EAPFAST EAPSIM EAPTTLS EAPAKA SIM USIM NFCSECURE HARDWARETOKEN SOFTTOKEN CERTIFICATE USERNAMEPASSWORD RESERVED ANONYMOUS VENDORSPECIFIC
realmEapId int | EAP index.
realmEapMethod RealmEapMethodEnum | EAP method for the realm in the WLAN. Allowed values NONE LEAP EAPPEAP EAPTLS EAPFAST EAPSIM EAPTTLS EAPAKA
realmId int | Realm index.
realmName String | Realm name.
hotspotServiceAdvertisement WlanMcServiceAdConfigTemplate | These attributes represent MSAP (Mobility Service Advertisement Protocol) parameters.
Attribute | Description
--- | ---
msapEnable boolean | Is Mobility Service Advertisement Protocol (MSAP) enabled?
serverIndex int | Server index.
interfaceName String | Denotes the interface, or interface group, for this WLAN. See interfaceType to determine if this is an interface or interface group.
interfaceType InterfaceMappingTypeEnum | Denotes whether an interface or interface group is used for this interface. See interfaceName for the name of the interface or interface group. Allowed values INTERFACE INTERFACEGROUP
isWiredLan boolean | Is this a wired LAN?
lanType LanTypeEnum | Denotes the LAN type. Allowed values WIRELESS GUEST REMOTE
lastModified long | The time the template was last modified. Measured in milliseconds since the Unix epoch.
layer2FastTransitionEnabled boolean | Is fast transition (FT) between access points enabled?
layer2FastTransitionOverDsEnabled boolean | When layer2FastTransitionEnabled is true, the denotes whether fast transition over a distributed system is enabled.
layer2FastTransitionReassociationTimeout int | When layer2FastTransitionEnabled is true, this denotes the transition timeout. Measured in seconds.
layer2MacFilteringEnabled boolean | Is MAC filtering enabled?
layer3GlobalWebAuthEnabled boolean | When a layer 3 web policy is true, this denotes whether the template uses global or template-defined Web Auth configuration.
layer3PreauthenticationAcl String | When a layer 3 web policy is true, this denotes the IPv4 ACL for traffic between the client and the wireless controller.
layer3PreauthenticationIpv6Acl String | When a layer 3 web policy is true, this denotes the IPv6 ACL for traffic between the client and the wireless controller.
layer3VpnPassthroughEnabled boolean | Is VPN passthrough enabled?
layer3WebAuthFlexAcl String | When a layer 3 web policy is true, this denotes the the FlexConnect ACL for external web authentication in locally switched WLANs.
layer3WebAuthType WlanWebAuthTypeEnum | When a layer 3 web policy is true and layer3GlobalWebAuth is false, this denotes the type of web authentication to be used. Allowed values DEFAULT CUSTOMIZED EXTERNAL
layer3WebPolicyAuthenticationEnabled boolean | Is the authentication web policy enabled?
layer3WebPolicyConditionalRedirectEnabled boolean | Is the conditional redirect web policy enabled?
layer3WebPolicyOnMacFailureEnabled boolean | Is the WebAuth on MAC failure web policy enabled?
layer3WebPolicyPassthroughEnabled boolean | Is the passthrough web policy enabled?
multicastVlanEnabled boolean | Is a multicast VLAN enabled?
multicastVlanInterface String | When multicastVlanInterface is true, this denotes the multicast VLAN.
profileName String | Profile name of the WLAN.
qos7920Cac PhoneSupport7920Enum | Denotes the Call Admission Control (CAC) configuration for Cisco 7920 phones. Allowed values DISABLED CLIENTCAC APCAC CLIENTANDAPCAC
qosAvcProfileName String | Denotes the Application Visibility and Control (AVC) profile for this WLAN.
qosNbarVisibilityEnabled boolean | Is Network Based Application Recognition (NBAR) deep packet inspection enabled on this WLAN?
qosNetflowMonitor String | Denotes the Netflow monitor configured for this WLAN.
qosPerSSidBurstRealTimeUpstreamRate int | Denotes the peak data rate limit for upstream UDP traffic for the WLAN. Zero means no restriction. Measured in Kbps.
qosPerSsidAverageDownstreamRate int | Denotes the average data rate limit for downstream TCP traffic for the WLAN. Zero means no restriction. Measured in Kbps.
qosPerSsidAverageRealTimeDownstreamRate int | Denotes the average data rate limit for downstream UDP traffic for the WLAN. Zero means no restriction. Measured in Kbps.
qosPerSsidAverageRealTimeUpstreamRate int | Denotes the average data rate limit for upstream UDP traffic for the WLAN. Zero means no restriction. Measured in Kbps.
qosPerSsidAverageUpstreamRate int | Denotes the average data rate limit for upstream TCP traffic for the WLAN. Zero means no restriction. Measured in Kbps.
qosPerSsidBurstDownstreamRate int | Denotes the peak data rate limit for downstream TCP traffic for the WLAN. Zero means no restriction. Measured in Kbps.
qosPerSsidBurstRealTimeDownstreamRate int | Denotes the peak data rate limit for downstream UDP traffic for the WLAN. Zero means no restriction. Measured in Kbps.
qosPerSsidBurstUpstreamRate int | Denotes the peak data rate limit for upstream TCP traffic for the WLAN. Zero means no restriction. Measured in Kbps.
qosPerUserAverageDownstreamRate int | Denotes the average data rate limit for downstream TCP traffic for a client. Zero means no restriction. Measured in Kbps.
qosPerUserAverageRealTimeDownstreamRate int | Denotes the average data rate limit for downstream UDP traffic for a client. Zero means no restriction. Measured in Kbps.
qosPerUserAverageRealTimeUpstreamRate int | Denotes the average data rate limit for upstream UDP traffic for a client. Zero means no restriction. Measured in Kbps.
qosPerUserAverageUpstreamRate int | Denotes the average data rate limit for upstream TCP traffic for a client. Zero means no restriction. Measured in Kbps.
qosPerUserBurstDownstreamRate int | Denotes the peak data rate limit for downstream TCP traffic for a client. Zero means no restriction. Measured in Kbps.
qosPerUserBurstRealTimeDownstreamRate int | Denotes the peak data rate limit for downstream UDP traffic for a client. Zero means no restriction. Measured in Kbps.
qosPerUserBurstRealTimeUpstreamRate int | Denotes the peak data rate limit for upstream UDP traffic for a client. Zero means no restriction. Measured in Kbps.
qosPerUserBurstUpstreamRate int | Denotes the peak data rate limit for upstream TCP traffic for a client. Zero means no restriction. Measured in Kbps.
qosProfile QosEnum | Denotes the QoS level for the WLAN. Allowed values BRONZE SILVER GOLD PLATINUM
qosWmmPolicy DisabledAllowedRequiredEnum | Denotes the state of the Wi-fi Multimedia (WMM) policy for this WLAN. Allowed values DISABLED ALLOWED REQUIRED
radioPolicy RadioPolicyEnum | Denotes the WLAN radio policy. Allowed values ALL ONLY80211A ONLY80211B ONLY80211G ONLY80211BG ONLY80211AG ONLY80211AB NONE REMOTELAN
ssid String | SSID of the WLAN.
templateName String | The name of the WLAN template.
vpnPassThroughGatewayAddress InetAddress | When layer3VpnPassthroughEnabled is true, this denotes the IP address of the VPN gateway.
webAuthExternalUrl String | When a layer 3 web policy is enabled, layer3GlobalWebAuthEnabled is false, and layer3WebAuthType is set to "External", this denotes the URL of the authentication server.
webAuthLoginFailurePage String | When a layer 3 web policy is enabled, layer3GlobalWebAuthEnabled is false, and layer3WebAuthType is set to "Customized", this denotes the page for authentication failures.
webAuthLoginPage String | When a layer 3 web policy is enabled, layer3GlobalWebAuthEnabled is false, and layer3WebAuthType is set to "Customized", this denotes the page for authentication.
webAuthLogoutPage String | When a layer 3 web policy is enabled, layer3GlobalWebAuthEnabled is false, and layer3WebAuthType is set to "Customized", this denotes the page for logout.
webPassthruEmailInputEnabled boolean | When layer3WebPolicyPassthroughEnabled is true, this denotes whether the client is prompted to enter an email address when connecting.
wepAllowSharedKeyAuthentication boolean | When wepSecurityEnabled is true, this denotes whether shared key authentication is enabled.
wepKeyIndex int | When wepSecurityEnabled is true, this denotes the key index.
wepKeySize WepEncryptionTypeEnum | When wepSecurityEnabled is true, this denotes whether shared key authentication is enabled. Allowed values WEP104 NONE WEP40 WEP128 AESOCB128 WEP_40 WEP_104
wepSecurityEnabled boolean | Is WEP layer 2 security enabled?
wpa2Enabled boolean | When wpaSecurityEnabled is true, this denotes whether the WPA2 policy is enabled.
wpa2EncryptionProtocolAes boolean | When wpaSecurityEnabled and wpa2Enabled are true, this denotes whether AES encryption is supported for the WPA2 policy.
wpa2EncryptionProtocolTkip boolean | When wpaSecurityEnabled and wpa2Enabled are true, this denotes whether TKIP encryption is supported for the WPA2 policy.
wpaAuthenticationKeyManagement8021x boolean | When wpaSecurityEnabled is true, this denotes whether 802.1X key management is enabled.
wpaAuthenticationKeyManagementCckm boolean | When wpaSecurityEnabled is true, this denotes whether Cisco Centralized Key Management (CCKM) is enabled.
wpaAuthenticationKeyManagementFt8021x boolean | When wpaSecurityEnabled is true, this denotes whether Fast Transition (FT) 802.1X key management is enabled.
wpaAuthenticationKeyManagementFtPsk boolean | When wpaSecurityEnabled is true, this denotes whether Fast Transition (FT) preshared key management is enabled.
wpaAuthenticationKeyManagementPmf8021x boolean | When wpaSecurityEnabled is true, this denotes whether Protected Management Frame (PMF) 802.1X key management is enabled.
wpaAuthenticationKeyManagementPmfPsk boolean | When wpaSecurityEnabled is true, this denotes whether Protected Management Frame (PMF) preshared key management is enabled.
wpaAuthenticationKeyManagementPsk boolean | When wpaSecurityEnabled is true, this denotes whether preshared key management is enabled.
wpaControllerSpecificPresharedKeyEnabled boolean | Is controller specific preshared key enabled?
wpaEnabled boolean | When wpaSecurityEnabled is true, this denotes whether the WPA1 policy is enabled.
wpaEncryptionProtocolAes boolean | When wpaSecurityEnabled and wpaEnabled are both true, this denotes whether AES encryption is supported for the WPA1 policy.
wpaEncryptionProtocolTkip boolean | When wpaSecurityEnabled and wpaEnabled are both true, this denotes whether TKIP encryption is supported for the WPA1 policy.
wpaPresharedKey String | When wpaSecurityEnabled is true, this contains preshared key in HEX or ASCII format.
wpaPresharedKeyFormat PskFormatEnum | When wpaSecurityEnabled is true, this denotes preshared key format. Allowed values DEFAULT HEX ASCII
wpaSecurityEnabled boolean | Is WPA layer 2 security enabled?
x8021KeySize x8021EncryptionTypeEnum | When x8021SecurityEnabled is true, this denotes the 802.1X key size. Allowed values WEP104 WEP40 WEP128 NONE WEP_40 WEP_104
x8021SecurityEnabled boolean | Is 802.1X layer 2 security enabled?

## Sample Payloads

Sample payloads are for information only. They are automatically generated and the values included may not be representative of actual valid data values.

### Sample XML Payload

https://10.64.88.203/webacs/api/v4/data/WlanTemplates/15

    <?xml version="1.0" ?>
    <queryResponse type="WlanTemplates" responseType="getEntity" requestUrl="https://10.64.88.203/webacs/api/v4/data/WlanTemplates/15" rootUrl="https://10.64.88.203/webacs/api/v4/data">
      <entity dtoType="wlanTemplatesDTO" type="WlanTemplates" url="https://10.64.88.203/webacs/api/v4/data/WlanTemplates/15">
        <wlanTemplatesDTO displayName="String value" id="15" uuid="String value">
          <aaaAllowOverride>true</aaaAllowOverride>
          <aaaLdapPrimaryServer>String value</aaaLdapPrimaryServer>
          <aaaLdapSecondaryServer>String value</aaaLdapSecondaryServer>
          <aaaLdapTertiaryServer>String value</aaaLdapTertiaryServer>
          <aaaLocalEapAuthenticationEnabled>true</aaaLocalEapAuthenticationEnabled>
          <aaaLocalEapAuthenticationProfileName>String value</aaaLocalEapAuthenticationProfileName>
          <aaaRadiusAccountingPrimaryServer>String value</aaaRadiusAccountingPrimaryServer>
          <aaaRadiusAccountingSecondaryServer>String value</aaaRadiusAccountingSecondaryServer>
          <aaaRadiusAccountingServersEnabled>true</aaaRadiusAccountingServersEnabled>
          <aaaRadiusAccountingTertiaryServer>String value</aaaRadiusAccountingTertiaryServer>
          <aaaRadiusAuthenticationPrimaryServer>String value</aaaRadiusAuthenticationPrimaryServer>
          <aaaRadiusAuthenticationSecondaryServer>String value</aaaRadiusAuthenticationSecondaryServer>
          <aaaRadiusAuthenticationServersEnabled>true</aaaRadiusAuthenticationServersEnabled>
          <aaaRadiusAuthenticationTertiaryServer>String value</aaaRadiusAuthenticationTertiaryServer>
          <aaaRadiusInterimUpdateEnabled>true</aaaRadiusInterimUpdateEnabled>
          <aaaRadiusInterimUpdateInterval>1</aaaRadiusInterimUpdateInterval>
          <adminStatus>true</adminStatus>
          <advancedAironetIeEnabled>true</advancedAironetIeEnabled>
          <advancedClientExclusionEnabled>true</advancedClientExclusionEnabled>
          <advancedClientExclusionTimeout>1</advancedClientExclusionTimeout>
          <advancedCoverageHoleDetectionEnabled>true</advancedCoverageHoleDetectionEnabled>
          <advancedDhcpAddressAssignmentRequired>true</advancedDhcpAddressAssignmentRequired>
          <advancedDhcpProfilingEnabled>true</advancedDhcpProfilingEnabled>
          <advancedDhcpServerIpAddress>
            <address>192.168.115.243</address>
          </advancedDhcpServerIpAddress>
          <advancedDiagnosticChannelEnabled>true</advancedDiagnosticChannelEnabled>
          <advancedDot11anDtimPeriod>1</advancedDot11anDtimPeriod>
          <advancedDot11bgnDtimPeriod>1</advancedDot11bgnDtimPeriod>
          <advancedFlexConnectCentralDhcpProcessingEnabled>true</advancedFlexConnectCentralDhcpProcessingEnabled>
          <advancedFlexConnectLearnClientIpEnabled>true</advancedFlexConnectLearnClientIpEnabled>
          <advancedFlexConnectLocalAuthEnabled>true</advancedFlexConnectLocalAuthEnabled>
          <advancedFlexConnectLocalSwitchingEnabled>true</advancedFlexConnectLocalSwitchingEnabled>
          <advancedFlexConnectNatPatEnabled>true</advancedFlexConnectNatPatEnabled>
          <advancedFlexConnectOverrideDnsEnabled>true</advancedFlexConnectOverrideDnsEnabled>
          <advancedFlexConnectReapCentralAssociation>true</advancedFlexConnectReapCentralAssociation>
          <advancedFlexConnectVlanCentralSwitchingEnabled>true</advancedFlexConnectVlanCentralSwitchingEnabled>
          <advancedHttpProfilingEnabled>true</advancedHttpProfilingEnabled>
          <advancedIpv6Enabled>true</advancedIpv6Enabled>
          <advancedKtsCacEnabled>true</advancedKtsCacEnabled>
          <advancedLoadBalancingBandSelectEnabled>true</advancedLoadBalancingBandSelectEnabled>
          <advancedLoadBalancingEnabled>true</advancedLoadBalancingEnabled>
          <advancedMaximumClients>1</advancedMaximumClients>
          <advancedMdnsProfileName>String value</advancedMdnsProfileName>
          <advancedMdnsSnoopingEnabled>true</advancedMdnsSnoopingEnabled>
          <advancedMediaSessionSnoopingEnabled>true</advancedMediaSessionSnoopingEnabled>
          <advancedMfpClientProtection>DISABLED</advancedMfpClientProtection>
          <advancedMfpSignatureGenerationEnabled>true</advancedMfpSignatureGenerationEnabled>
          <advancedMfpVersion>1</advancedMfpVersion>
          <advancedOverrideInterfaceAclName>String value</advancedOverrideInterfaceAclName>
          <advancedOverrideInterfaceIpv6AclName>String value</advancedOverrideInterfaceIpv6AclName>
          <advancedPassiveClientEnabled>true</advancedPassiveClientEnabled>
          <advancedPeerToPeerBlocking>DISABLE</advancedPeerToPeerBlocking>
          <advancedPmipMobilityType>NONE</advancedPmipMobilityType>
          <advancedPmipProfile>String value</advancedPmipProfile>
          <advancedPmipRealm>String value</advancedPmipRealm>
          <advancedScanDeferPriority0>true</advancedScanDeferPriority0>
          <advancedScanDeferPriority1>true</advancedScanDeferPriority1>
          <advancedScanDeferPriority2>true</advancedScanDeferPriority2>
          <advancedScanDeferPriority3>true</advancedScanDeferPriority3>
          <advancedScanDeferPriority4>true</advancedScanDeferPriority4>
          <advancedScanDeferPriority5>true</advancedScanDeferPriority5>
          <advancedScanDeferPriority6>true</advancedScanDeferPriority6>
          <advancedScanDeferPriority7>true</advancedScanDeferPriority7>
          <advancedScanDeferTime>1</advancedScanDeferTime>
          <advancedSessionTimeout>1</advancedSessionTimeout>
          <advancedWifiDirectClientsPolicy>DISABLED</advancedWifiDirectClientsPolicy>
          <broadcastSsidEnabled>true</broadcastSsidEnabled>
          <ckipKeyIndex>1</ckipKeyIndex>
          <ckipKeyPermutationEnabled>true</ckipKeyPermutationEnabled>
          <ckipKeySize>NONE</ckipKeySize>
          <ckipMmhModeEnabled>true</ckipMmhModeEnabled>
          <ckipSecurityEnabled>true</ckipSecurityEnabled>
          <interfaceName>String value</interfaceName>
          <interfaceType>INTERFACE</interfaceType>
          <isWiredLan>true</isWiredLan>
          <lanType>WIRELESS</lanType>
          <layer2FastTransitionEnabled>true</layer2FastTransitionEnabled>
          <layer2FastTransitionOverDsEnabled>true</layer2FastTransitionOverDsEnabled>
          <layer2FastTransitionReassociationTimeout>1</layer2FastTransitionReassociationTimeout>
          <layer2MacFilteringEnabled>true</layer2MacFilteringEnabled>
          <layer3GlobalWebAuthEnabled>true</layer3GlobalWebAuthEnabled>
          <layer3PreauthenticationAcl>String value</layer3PreauthenticationAcl>
          <layer3PreauthenticationIpv6Acl>String value</layer3PreauthenticationIpv6Acl>
          <layer3VpnPassthroughEnabled>true</layer3VpnPassthroughEnabled>
          <layer3WebAuthFlexAcl>String value</layer3WebAuthFlexAcl>
          <layer3WebAuthType>DEFAULT</layer3WebAuthType>
          <layer3WebPolicyAuthenticationEnabled>true</layer3WebPolicyAuthenticationEnabled>
          <layer3WebPolicyConditionalRedirectEnabled>true</layer3WebPolicyConditionalRedirectEnabled>
          <layer3WebPolicyOnMacFailureEnabled>true</layer3WebPolicyOnMacFailureEnabled>
          <layer3WebPolicyPassthroughEnabled>true</layer3WebPolicyPassthroughEnabled>
          <multicastVlanEnabled>true</multicastVlanEnabled>
          <multicastVlanInterface>String value</multicastVlanInterface>
          <profileName>String value</profileName>
          <qos7920Cac>DISABLED</qos7920Cac>
          <qosAvcProfileName>String value</qosAvcProfileName>
          <qosNbarVisibilityEnabled>true</qosNbarVisibilityEnabled>
          <qosNetflowMonitor>String value</qosNetflowMonitor>
          <qosPerSSidBurstRealTimeUpstreamRate>1</qosPerSSidBurstRealTimeUpstreamRate>
          <qosPerSsidAverageDownstreamRate>1</qosPerSsidAverageDownstreamRate>
          <qosPerSsidAverageRealTimeDownstreamRate>1</qosPerSsidAverageRealTimeDownstreamRate>
          <qosPerSsidAverageRealTimeUpstreamRate>1</qosPerSsidAverageRealTimeUpstreamRate>
          <qosPerSsidAverageUpstreamRate>1</qosPerSsidAverageUpstreamRate>
          <qosPerSsidBurstDownstreamRate>1</qosPerSsidBurstDownstreamRate>
          <qosPerSsidBurstRealTimeDownstreamRate>1</qosPerSsidBurstRealTimeDownstreamRate>
          <qosPerSsidBurstUpstreamRate>1</qosPerSsidBurstUpstreamRate>
          <qosPerUserAverageDownstreamRate>1</qosPerUserAverageDownstreamRate>
          <qosPerUserAverageRealTimeDownstreamRate>1</qosPerUserAverageRealTimeDownstreamRate>
          <qosPerUserAverageRealTimeUpstreamRate>1</qosPerUserAverageRealTimeUpstreamRate>
          <qosPerUserAverageUpstreamRate>1</qosPerUserAverageUpstreamRate>
          <qosPerUserBurstDownstreamRate>1</qosPerUserBurstDownstreamRate>
          <qosPerUserBurstRealTimeDownstreamRate>1</qosPerUserBurstRealTimeDownstreamRate>
          <qosPerUserBurstRealTimeUpstreamRate>1</qosPerUserBurstRealTimeUpstreamRate>
          <qosPerUserBurstUpstreamRate>1</qosPerUserBurstUpstreamRate>
          <qosProfile>BRONZE</qosProfile>
          <qosWmmPolicy>DISABLED</qosWmmPolicy>
          <radioPolicy>ALL</radioPolicy>
          <ssid>String value</ssid>
          <vpnPassThroughGatewayAddress>
            <address>192.168.115.243</address>
          </vpnPassThroughGatewayAddress>
          <webAuthExternalUrl>String value</webAuthExternalUrl>
          <webAuthLoginFailurePage>String value</webAuthLoginFailurePage>
          <webAuthLoginPage>String value</webAuthLoginPage>
          <webAuthLogoutPage>String value</webAuthLogoutPage>
          <webPassthruEmailInputEnabled>true</webPassthruEmailInputEnabled>
          <wepAllowSharedKeyAuthentication>true</wepAllowSharedKeyAuthentication>
          <wepKeyIndex>1</wepKeyIndex>
          <wepKeySize>WEP104</wepKeySize>
          <wepSecurityEnabled>true</wepSecurityEnabled>
          <wpa2Enabled>true</wpa2Enabled>
          <wpa2EncryptionProtocolAes>true</wpa2EncryptionProtocolAes>
          <wpa2EncryptionProtocolTkip>true</wpa2EncryptionProtocolTkip>
          <wpaAuthenticationKeyManagement8021x>true</wpaAuthenticationKeyManagement8021x>
          <wpaAuthenticationKeyManagementCckm>true</wpaAuthenticationKeyManagementCckm>
          <wpaAuthenticationKeyManagementFt8021x>true</wpaAuthenticationKeyManagementFt8021x>
          <wpaAuthenticationKeyManagementFtPsk>true</wpaAuthenticationKeyManagementFtPsk>
          <wpaAuthenticationKeyManagementPmf8021x>true</wpaAuthenticationKeyManagementPmf8021x>
          <wpaAuthenticationKeyManagementPmfPsk>true</wpaAuthenticationKeyManagementPmfPsk>
          <wpaAuthenticationKeyManagementPsk>true</wpaAuthenticationKeyManagementPsk>
          <wpaEnabled>true</wpaEnabled>
          <wpaEncryptionProtocolAes>true</wpaEncryptionProtocolAes>
          <wpaEncryptionProtocolTkip>true</wpaEncryptionProtocolTkip>
          <wpaPresharedKey>String value</wpaPresharedKey>
          <wpaPresharedKeyFormat>DEFAULT</wpaPresharedKeyFormat>
          <wpaSecurityEnabled>true</wpaSecurityEnabled>
          <x8021KeySize>WEP104</x8021KeySize>
          <x8021SecurityEnabled>true</x8021SecurityEnabled>
          <aaaRadiusAccountingWlcSpecificEnabled>true</aaaRadiusAccountingWlcSpecificEnabled>
          <aaaRadiusAuthenticationWlcSpecificEnabled>true</aaaRadiusAuthenticationWlcSpecificEnabled>
          <advancedSessionTimeoutEnabled>true</advancedSessionTimeoutEnabled>
          <hotspot2Enable>
            <hotSpot2Enabled>true</hotSpot2Enabled>
          </hotspot2Enable>
          <hotspot2Operators>
            <hotspot2Operator>
              <operatorId>1</operatorId>
              <operatorLang>String value</operatorLang>
              <operatorName>String value</operatorName>
            </hotspot2Operator>
            <hotspot2Operator>
              <operatorId>11</operatorId>
              <operatorLang>Another string value</operatorLang>
              <operatorName>Another string value</operatorName>
            </hotspot2Operator>
          </hotspot2Operators>
          <hotspot2Ports>
            <hotspot2Port>
              <portConfigId>1</portConfigId>
              <portNo>ICMPESP</portNo>
              <portStatus>CLOSED</portStatus>
              <protocolName>ICMP</protocolName>
            </hotspot2Port>
            <hotspot2Port>
              <portConfigId>11</portConfigId>
              <portNo>FTP</portNo>
              <portStatus>OPEN</portStatus>
              <protocolName>FTP</protocolName>
            </hotspot2Port>
          </hotspot2Ports>
          <hotspot2Wan>
            <downLinkSpeed>1</downLinkSpeed>
            <upLinkSpeed>1</upLinkSpeed>
            <wanLinkStatus>LINKUP</wanLinkStatus>
            <wanSymLinkStatus>SAME</wanSymLinkStatus>
          </hotspot2Wan>
          <hotspotCellularNetworks>
            <hotspotCellularNetwork>
              <countryCode>String value</countryCode>
              <gppIndex>1</gppIndex>
              <networkCode>String value</networkCode>
            </hotspotCellularNetwork>
            <hotspotCellularNetwork>
              <countryCode>Another string value</countryCode>
              <gppIndex>11</gppIndex>
              <networkCode>Another string value</networkCode>
            </hotspotCellularNetwork>
          </hotspotCellularNetworks>
          <hotspotDomains>
            <hotspotDomain>
              <domainId>1</domainId>
              <domainName>String value</domainName>
            </hotspotDomain>
            <hotspotDomain>
              <domainId>11</domainId>
              <domainName>Another string value</domainName>
            </hotspotDomain>
          </hotspotDomains>
          <hotspotGeneral>
            <heSsid>
              <octets>000a959d6816</octets>
            </heSsid>
            <internetAccess>true</internetAccess>
            <ipv4AddressAvailType>NOTAVAILABLE</ipv4AddressAvailType>
            <ipv6AddressAvailType>NOTAVAILABLE</ipv6AddressAvailType>
            <networkAuthType>ACCEPTANCE</networkAuthType>
            <networkType>PRIVATE</networkType>
            <status>true</status>
          </hotspotGeneral>
          <hotspotOuiTemplates>
            <hotspotOuiTemplate>
              <oui>String value</oui>
              <ouiId>1</ouiId>
              <ouiInBeacon>true</ouiInBeacon>
            </hotspotOuiTemplate>
            <hotspotOuiTemplate>
              <oui>Another string value</oui>
              <ouiId>11</ouiId>
              <ouiInBeacon>false</ouiInBeacon>
            </hotspotOuiTemplate>
          </hotspotOuiTemplates>
          <hotspotRealms>
            <hotspotRealm>
              <realmEapMethods>
                <realmEapMethod>
                  <innerAuthMethods>
                    <innerAuthMethod>
                      <realmEapAuthId>1</realmEapAuthId>
                      <realmEapAuthMethod>NONEAPINNERAUTH</realmEapAuthMethod>
                      <realmEapAuthParam>NONE</realmEapAuthParam>
                    </innerAuthMethod>
                    <innerAuthMethod>
                      <realmEapAuthId>11</realmEapAuthId>
                      <realmEapAuthMethod>INNERAUTHEAP</realmEapAuthMethod>
                      <realmEapAuthParam>PAP</realmEapAuthParam>
                    </innerAuthMethod>
                  </innerAuthMethods>
                  <realmEapId>1</realmEapId>
                  <realmEapMethod>NONE</realmEapMethod>
                </realmEapMethod>
                <realmEapMethod>
                  <innerAuthMethods>
                    <innerAuthMethod>
                      <realmEapAuthId>1</realmEapAuthId>
                      <realmEapAuthMethod>NONEAPINNERAUTH</realmEapAuthMethod>
                      <realmEapAuthParam>NONE</realmEapAuthParam>
                    </innerAuthMethod>
                    <innerAuthMethod>
                      <realmEapAuthId>11</realmEapAuthId>
                      <realmEapAuthMethod>INNERAUTHEAP</realmEapAuthMethod>
                      <realmEapAuthParam>PAP</realmEapAuthParam>
                    </innerAuthMethod>
                  </innerAuthMethods>
                  <realmEapId>11</realmEapId>
                  <realmEapMethod>LEAP</realmEapMethod>
                </realmEapMethod>
              </realmEapMethods>
              <realmId>1</realmId>
              <realmName>String value</realmName>
            </hotspotRealm>
            <hotspotRealm>
              <realmEapMethods>
                <realmEapMethod>
                  <innerAuthMethods>
                    <innerAuthMethod>
                      <realmEapAuthId>1</realmEapAuthId>
                      <realmEapAuthMethod>NONEAPINNERAUTH</realmEapAuthMethod>
                      <realmEapAuthParam>NONE</realmEapAuthParam>
                    </innerAuthMethod>
                    <innerAuthMethod>
                      <realmEapAuthId>11</realmEapAuthId>
                      <realmEapAuthMethod>INNERAUTHEAP</realmEapAuthMethod>
                      <realmEapAuthParam>PAP</realmEapAuthParam>
                    </innerAuthMethod>
                  </innerAuthMethods>
                  <realmEapId>1</realmEapId>
                  <realmEapMethod>NONE</realmEapMethod>
                </realmEapMethod>
                <realmEapMethod>
                  <innerAuthMethods>
                    <innerAuthMethod>
                      <realmEapAuthId>1</realmEapAuthId>
                      <realmEapAuthMethod>NONEAPINNERAUTH</realmEapAuthMethod>
                      <realmEapAuthParam>NONE</realmEapAuthParam>
                    </innerAuthMethod>
                    <innerAuthMethod>
                      <realmEapAuthId>11</realmEapAuthId>
                      <realmEapAuthMethod>INNERAUTHEAP</realmEapAuthMethod>
                      <realmEapAuthParam>PAP</realmEapAuthParam>
                    </innerAuthMethod>
                  </innerAuthMethods>
                  <realmEapId>11</realmEapId>
                  <realmEapMethod>LEAP</realmEapMethod>
                </realmEapMethod>
              </realmEapMethods>
              <realmId>11</realmId>
              <realmName>Another string value</realmName>
            </hotspotRealm>
          </hotspotRealms>
          <hotspotServiceAdvertisement>
            <msapEnable>true</msapEnable>
            <serverIndex>1</serverIndex>
          </hotspotServiceAdvertisement>
          <lastModified>2</lastModified>
          <templateName>String value</templateName>
          <wpaControllerSpecificPresharedKeyEnabled>true</wpaControllerSpecificPresharedKeyEnabled>
        </wlanTemplatesDTO>
      </entity>
    </queryResponse>

### Sample JSON Payload

https://10.64.88.203/webacs/api/v4/data/WlanTemplates/15.json

    {
      "queryResponse" : {
        "@type" : "WlanTemplates",
        "@requestUrl" : "https://10.64.88.203/webacs/api/v4/data/WlanTemplates/15",
        "@responseType" : "getEntity",
        "@rootUrl" : "https://10.64.88.203/webacs/api/v4/data",
        "entity" : [ {
          "@dtoType" : "wlanTemplatesDTO",
          "@type" : "WlanTemplates",
          "@url" : "https://10.64.88.203/webacs/api/v4/data/WlanTemplates/15",
          "wlanTemplatesDTO" : {
            "@displayName" : "String value",
            "@id" : 15,
            "@uuid" : "String value",
            "aaaAllowOverride" : true,
            "aaaLdapPrimaryServer" : "String value",
            "aaaLdapSecondaryServer" : "String value",
            "aaaLdapTertiaryServer" : "String value",
            "aaaLocalEapAuthenticationEnabled" : true,
            "aaaLocalEapAuthenticationProfileName" : "String value",
            "aaaRadiusAccountingPrimaryServer" : "String value",
            "aaaRadiusAccountingSecondaryServer" : "String value",
            "aaaRadiusAccountingServersEnabled" : true,
            "aaaRadiusAccountingTertiaryServer" : "String value",
            "aaaRadiusAccountingWlcSpecificEnabled" : true,
            "aaaRadiusAuthenticationPrimaryServer" : "String value",
            "aaaRadiusAuthenticationSecondaryServer" : "String value",
            "aaaRadiusAuthenticationServersEnabled" : true,
            "aaaRadiusAuthenticationTertiaryServer" : "String value",
            "aaaRadiusAuthenticationWlcSpecificEnabled" : true,
            "aaaRadiusInterimUpdateEnabled" : true,
            "aaaRadiusInterimUpdateInterval" : 1,
            "adminStatus" : true,
            "advancedAironetIeEnabled" : true,
            "advancedClientExclusionEnabled" : true,
            "advancedClientExclusionTimeout" : 1,
            "advancedCoverageHoleDetectionEnabled" : true,
            "advancedDhcpAddressAssignmentRequired" : true,
            "advancedDhcpProfilingEnabled" : true,
            "advancedDhcpServerIpAddress" : {
              "address" : "192.168.115.243"
            },
            "advancedDiagnosticChannelEnabled" : true,
            "advancedDot11anDtimPeriod" : 1,
            "advancedDot11bgnDtimPeriod" : 1,
            "advancedFlexConnectCentralDhcpProcessingEnabled" : true,
            "advancedFlexConnectLearnClientIpEnabled" : true,
            "advancedFlexConnectLocalAuthEnabled" : true,
            "advancedFlexConnectLocalSwitchingEnabled" : true,
            "advancedFlexConnectNatPatEnabled" : true,
            "advancedFlexConnectOverrideDnsEnabled" : true,
            "advancedFlexConnectReapCentralAssociation" : true,
            "advancedFlexConnectVlanCentralSwitchingEnabled" : true,
            "advancedHttpProfilingEnabled" : true,
            "advancedIpv6Enabled" : true,
            "advancedKtsCacEnabled" : true,
            "advancedLoadBalancingBandSelectEnabled" : true,
            "advancedLoadBalancingEnabled" : true,
            "advancedMaximumClients" : 1,
            "advancedMdnsProfileName" : "String value",
            "advancedMdnsSnoopingEnabled" : true,
            "advancedMediaSessionSnoopingEnabled" : true,
            "advancedMfpClientProtection" : "DISABLED",
            "advancedMfpSignatureGenerationEnabled" : true,
            "advancedMfpVersion" : 1,
            "advancedOverrideInterfaceAclName" : "String value",
            "advancedOverrideInterfaceIpv6AclName" : "String value",
            "advancedPassiveClientEnabled" : true,
            "advancedPeerToPeerBlocking" : "DISABLE",
            "advancedPmipMobilityType" : "NONE",
            "advancedPmipProfile" : "String value",
            "advancedPmipRealm" : "String value",
            "advancedScanDeferPriority0" : true,
            "advancedScanDeferPriority1" : true,
            "advancedScanDeferPriority2" : true,
            "advancedScanDeferPriority3" : true,
            "advancedScanDeferPriority4" : true,
            "advancedScanDeferPriority5" : true,
            "advancedScanDeferPriority6" : true,
            "advancedScanDeferPriority7" : true,
            "advancedScanDeferTime" : 1,
            "advancedSessionTimeout" : 1,
            "advancedSessionTimeoutEnabled" : true,
            "advancedWifiDirectClientsPolicy" : "DISABLED",
            "broadcastSsidEnabled" : true,
            "ckipKeyIndex" : 1,
            "ckipKeyPermutationEnabled" : true,
            "ckipKeySize" : "NONE",
            "ckipMmhModeEnabled" : true,
            "ckipSecurityEnabled" : true,
            "hotspot2Enable" : {
              "hotSpot2Enabled" : true
            },
            "hotspot2Operators" : {
              "hotspot2Operator" : [ {
                "operatorId" : 1,
                "operatorLang" : "String value",
                "operatorName" : "String value"
              }, {
                "operatorId" : 11,
                "operatorLang" : "Another string value",
                "operatorName" : "Another string value"
              } ]
            },
            "hotspot2Ports" : {
              "hotspot2Port" : [ {
                "portConfigId" : 1,
                "portNo" : "ICMPESP",
                "portStatus" : "CLOSED",
                "protocolName" : "ICMP"
              }, {
                "portConfigId" : 11,
                "portNo" : "FTP",
                "portStatus" : "OPEN",
                "protocolName" : "FTP"
              } ]
            },
            "hotspot2Wan" : {
              "downLinkSpeed" : 1,
              "upLinkSpeed" : 1,
              "wanLinkStatus" : "LINKUP",
              "wanSymLinkStatus" : "SAME"
            },
            "hotspotCellularNetworks" : {
              "hotspotCellularNetwork" : [ {
                "countryCode" : "String value",
                "gppIndex" : 1,
                "networkCode" : "String value"
              }, {
                "countryCode" : "Another string value",
                "gppIndex" : 11,
                "networkCode" : "Another string value"
              } ]
            },
            "hotspotDomains" : {
              "hotspotDomain" : [ {
                "domainId" : 1,
                "domainName" : "String value"
              }, {
                "domainId" : 11,
                "domainName" : "Another string value"
              } ]
            },
            "hotspotGeneral" : {
              "heSsid" : {
                "octets" : "000a959d6816"
              },
              "internetAccess" : true,
              "ipv4AddressAvailType" : "NOTAVAILABLE",
              "ipv6AddressAvailType" : "NOTAVAILABLE",
              "networkAuthType" : "ACCEPTANCE",
              "networkType" : "PRIVATE",
              "status" : true
            },
            "hotspotOuiTemplates" : {
              "hotspotOuiTemplate" : [ {
                "oui" : "String value",
                "ouiId" : 1,
                "ouiInBeacon" : true
              }, {
                "oui" : "Another string value",
                "ouiId" : 11,
                "ouiInBeacon" : false
              } ]
            },
            "hotspotRealms" : {
              "hotspotRealm" : [ {
                "realmEapMethods" : {
                  "realmEapMethod" : [ {
                    "innerAuthMethods" : {
                      "innerAuthMethod" : [ {
                        "realmEapAuthId" : 1,
                        "realmEapAuthMethod" : "NONEAPINNERAUTH",
                        "realmEapAuthParam" : "NONE"
                      }, {
                        "realmEapAuthId" : 11,
                        "realmEapAuthMethod" : "INNERAUTHEAP",
                        "realmEapAuthParam" : "PAP"
                      } ]
                    },
                    "realmEapId" : 1,
                    "realmEapMethod" : "NONE"
                  }, {
                    "innerAuthMethods" : {
                      "innerAuthMethod" : [ {
                        "realmEapAuthId" : 1,
                        "realmEapAuthMethod" : "NONEAPINNERAUTH",
                        "realmEapAuthParam" : "NONE"
                      }, {
                        "realmEapAuthId" : 11,
                        "realmEapAuthMethod" : "INNERAUTHEAP",
                        "realmEapAuthParam" : "PAP"
                      } ]
                    },
                    "realmEapId" : 11,
                    "realmEapMethod" : "LEAP"
                  } ]
                },
                "realmId" : 1,
                "realmName" : "String value"
              }, {
                "realmEapMethods" : {
                  "realmEapMethod" : [ {
                    "innerAuthMethods" : {
                      "innerAuthMethod" : [ {
                        "realmEapAuthId" : 1,
                        "realmEapAuthMethod" : "NONEAPINNERAUTH",
                        "realmEapAuthParam" : "NONE"
                      }, {
                        "realmEapAuthId" : 11,
                        "realmEapAuthMethod" : "INNERAUTHEAP",
                        "realmEapAuthParam" : "PAP"
                      } ]
                    },
                    "realmEapId" : 1,
                    "realmEapMethod" : "NONE"
                  }, {
                    "innerAuthMethods" : {
                      "innerAuthMethod" : [ {
                        "realmEapAuthId" : 1,
                        "realmEapAuthMethod" : "NONEAPINNERAUTH",
                        "realmEapAuthParam" : "NONE"
                      }, {
                        "realmEapAuthId" : 11,
                        "realmEapAuthMethod" : "INNERAUTHEAP",
                        "realmEapAuthParam" : "PAP"
                      } ]
                    },
                    "realmEapId" : 11,
                    "realmEapMethod" : "LEAP"
                  } ]
                },
                "realmId" : 11,
                "realmName" : "Another string value"
              } ]
            },
            "hotspotServiceAdvertisement" : {
              "msapEnable" : true,
              "serverIndex" : 1
            },
            "interfaceName" : "String value",
            "interfaceType" : "INTERFACE",
            "isWiredLan" : true,
            "lanType" : "WIRELESS",
            "lastModified" : 2,
            "layer2FastTransitionEnabled" : true,
            "layer2FastTransitionOverDsEnabled" : true,
            "layer2FastTransitionReassociationTimeout" : 1,
            "layer2MacFilteringEnabled" : true,
            "layer3GlobalWebAuthEnabled" : true,
            "layer3PreauthenticationAcl" : "String value",
            "layer3PreauthenticationIpv6Acl" : "String value",
            "layer3VpnPassthroughEnabled" : true,
            "layer3WebAuthFlexAcl" : "String value",
            "layer3WebAuthType" : "DEFAULT",
            "layer3WebPolicyAuthenticationEnabled" : true,
            "layer3WebPolicyConditionalRedirectEnabled" : true,
            "layer3WebPolicyOnMacFailureEnabled" : true,
            "layer3WebPolicyPassthroughEnabled" : true,
            "multicastVlanEnabled" : true,
            "multicastVlanInterface" : "String value",
            "profileName" : "String value",
            "qos7920Cac" : "DISABLED",
            "qosAvcProfileName" : "String value",
            "qosNbarVisibilityEnabled" : true,
            "qosNetflowMonitor" : "String value",
            "qosPerSSidBurstRealTimeUpstreamRate" : 1,
            "qosPerSsidAverageDownstreamRate" : 1,
            "qosPerSsidAverageRealTimeDownstreamRate" : 1,
            "qosPerSsidAverageRealTimeUpstreamRate" : 1,
            "qosPerSsidAverageUpstreamRate" : 1,
            "qosPerSsidBurstDownstreamRate" : 1,
            "qosPerSsidBurstRealTimeDownstreamRate" : 1,
            "qosPerSsidBurstUpstreamRate" : 1,
            "qosPerUserAverageDownstreamRate" : 1,
            "qosPerUserAverageRealTimeDownstreamRate" : 1,
            "qosPerUserAverageRealTimeUpstreamRate" : 1,
            "qosPerUserAverageUpstreamRate" : 1,
            "qosPerUserBurstDownstreamRate" : 1,
            "qosPerUserBurstRealTimeDownstreamRate" : 1,
            "qosPerUserBurstRealTimeUpstreamRate" : 1,
            "qosPerUserBurstUpstreamRate" : 1,
            "qosProfile" : "BRONZE",
            "qosWmmPolicy" : "DISABLED",
            "radioPolicy" : "ALL",
            "ssid" : "String value",
            "templateName" : "String value",
            "vpnPassThroughGatewayAddress" : {
              "address" : "192.168.115.243"
            },
            "webAuthExternalUrl" : "String value",
            "webAuthLoginFailurePage" : "String value",
            "webAuthLoginPage" : "String value",
            "webAuthLogoutPage" : "String value",
            "webPassthruEmailInputEnabled" : true,
            "wepAllowSharedKeyAuthentication" : true,
            "wepKeyIndex" : 1,
            "wepKeySize" : "WEP104",
            "wepSecurityEnabled" : true,
            "wpa2Enabled" : true,
            "wpa2EncryptionProtocolAes" : true,
            "wpa2EncryptionProtocolTkip" : true,
            "wpaAuthenticationKeyManagement8021x" : true,
            "wpaAuthenticationKeyManagementCckm" : true,
            "wpaAuthenticationKeyManagementFt8021x" : true,
            "wpaAuthenticationKeyManagementFtPsk" : true,
            "wpaAuthenticationKeyManagementPmf8021x" : true,
            "wpaAuthenticationKeyManagementPmfPsk" : true,
            "wpaAuthenticationKeyManagementPsk" : true,
            "wpaControllerSpecificPresharedKeyEnabled" : true,
            "wpaEnabled" : true,
            "wpaEncryptionProtocolAes" : true,
            "wpaEncryptionProtocolTkip" : true,
            "wpaPresharedKey" : "String value",
            "wpaPresharedKeyFormat" : "DEFAULT",
            "wpaSecurityEnabled" : true,
            "x8021KeySize" : "WEP104",
            "x8021SecurityEnabled" : true
          }
        } ]
      }
    }