
Cisco Evolved Programmable Network Manager API
Evolved Programmable Network Manager API Documentation

# GET RadioDetails

Represents detail information of a radio interfaces on lightweight access point.

Since Product Version: 1.2

- Jump To

- v1
- v2
- v3
- v4

### Resource Information

Rate Limiting? | Yes
Sorting? | Yes
Paging? | Yes
Filtering? | Yes
Group Filtering? | No
Aggregation? | No
Response Formats | xml json
User Group | NBI Read
HTTP Methods | GET

API version v1 is deprecated

This API version has been deprecated. It will be removed in a future release of the product. Please develop new clients using the latest API version. Please modify your existing clients to use a later API version.

## Resource URL

/webacs/api/v1/data/RadioDetails

Deprecated

This version has been deprecated. Please use v4.

## Response Parameters

Attribute | Description
--- | ---
adminStatus RadioAdminStatusEnum | Administrative status of the radio interface Allowed values UNKNOWN ENABLE DISABLE
alarmStatus AlarmSeverityEnum | Allowed values CRITICAL MAJOR MINOR WARNING CLEARED INFORMATION
antennaAzimAngle Float | Displays the horizontal angle of the antenna
antennaDiversity String | Displays if antenna diversity is enabled or disabled. Antenna diversity refers to the access point sampling the radio signal from two integrated antenna ports to choose the preferred antenna. Allowed values: 'Connector A', 'Connector B', 'Enabled', 'NA'
antennaElevAngle Float | Displays the elevation angle of the antenna.
antennaGain Integer | The external antenna gain, measured in 0.5 dBi units. This is the raw value from device. It is different from displayed in the UI. An integer value 7 means 7 x 0.5 = 3.5 dBm of gain.
antennaMode String | Displays the antenna mode. Allowed values: Sector A, Sector B, Omni, NA (non-applicable).
antennaName String | Antenna name
antennaType String | Antenna type. Allowed values: Internal, External, Circular, Linear, NA
apIpAddress String | IP address of the access point
apName String | Name of the access point
baseRadioMac String | Base radio MAC address
channelControl String | Radio channel control. Allowed values: Automatic, Custom, NA
channelNumber Integer | Current operational channel number
channelWidth String | Channel width. Allowed values: 5 MHz, 10 MHz, 20 MHz, 40 MHz, 80 MHz, 160 MHz, Above 40 MHz, Below 40 MHz, NA
cleanAirCapable String | Capability of clean air feature. Allowed values: Yes, No
cleanAirSensorStatus String | Clean air sensor status. Allowed values: Up, Down, NA
cleanAirStatus String | Clean air status. Allowed values: Yes, No
clientCount String | Client count connected to the radio interface
controllerIpAddress String | Registered controller IP address for CAPWAP AP only
dot11nCapable boolean | 802.11n capability
ethernetMac String | MAC address of the ethernet interface on the AP
operStatus RadioOperStatusEnum | Operational status of the radio interface Allowed values DOWN UP NOTASSOCIATED UNKNOWN
port int | Controller port number
powerLevel Integer | Power level of the radio
radioBand RadioBandEnum | Radio band of the radio interface Allowed values 2.4 GHz 5 GHz Unknown
radioRole RadioRoleEnum | Radio role Allowed values SHUTDOWN UPDOWNLINK UPLINK DOWNLINK ACCESS UPLINKACCESS DOWNLINKACCESS UPDOWNLINKACCESS NOTAPPLICABLE
radioType String | Radio type of the interface. Allowed values: 802.11a, 802.11ac, 802.11a/n, 802.11a/n/ac, 802.11a/n/ac/ax, 802.11b/g, 802.11b/g/n, 802.11b/g/n/ax, 802.11a/b/g/n, 802.11a/b/g/n/ac, 802.11a/b/g/n/ac/ax, XOR (Monitor Mode), XOR (2.4GHz), XOR (5GHz), UWB, BLE, Unknown
slotId Integer | Slot ID of the radio in the AP
txPowerControl String | Tranmission power control. Allowed values: Automatic, Custom, NA
txPowerOutput Integer | The txPower currently being used to transmit data, in dBm

## Sample Payloads

Sample payloads are for information only. They are automatically generated and the values included may not be representative of actual valid data values.

### Sample XML Payload

https://10.64.88.203/webacs/api/v1/data/RadioDetails/15

    <?xml version="1.0" ?>
    <queryResponse type="RadioDetails" responseType="getEntity" requestUrl="https://10.64.88.203/webacs/api/v1/data/RadioDetails/15" rootUrl="https://10.64.88.203/webacs/api/v1/data">
      <entity dtoType="radioDetailsDTO" type="RadioDetails" url="https://10.64.88.203/webacs/api/v1/data/RadioDetails/15">
        <radioDetailsDTO displayName="String value" id="15" uuid="String value">
          <adminStatus>UNKNOWN</adminStatus>
          <alarmStatus>CRITICAL</alarmStatus>
          <antennaAzimAngle>15.0</antennaAzimAngle>
          <antennaElevAngle>15.0</antennaElevAngle>
          <antennaGain>15</antennaGain>
          <antennaName>String value</antennaName>
          <apName>String value</apName>
          <dot11nCapable>true</dot11nCapable>
          <operStatus>DOWN</operStatus>
          <port>1</port>
          <powerLevel>15</powerLevel>
          <radioBand>2.4 GHz</radioBand>
          <radioRole>SHUTDOWN</radioRole>
          <slotId>15</slotId>
          <txPowerOutput>15</txPowerOutput>
          <antennaDiversity>String value</antennaDiversity>
          <antennaMode>String value</antennaMode>
          <antennaType>String value</antennaType>
          <apIpAddress>String value</apIpAddress>
          <baseRadioMac>String value</baseRadioMac>
          <channelControl>String value</channelControl>
          <channelNumber>15</channelNumber>
          <channelWidth>String value</channelWidth>
          <cleanAirCapable>String value</cleanAirCapable>
          <cleanAirSensorStatus>String value</cleanAirSensorStatus>
          <cleanAirStatus>String value</cleanAirStatus>
          <clientCount>String value</clientCount>
          <controllerIpAddress>String value</controllerIpAddress>
          <ethernetMac>String value</ethernetMac>
          <radioType>String value</radioType>
          <txPowerControl>String value</txPowerControl>
        </radioDetailsDTO>
      </entity>
    </queryResponse>

### Sample JSON Payload

https://10.64.88.203/webacs/api/v1/data/RadioDetails/15.json

    {
      "queryResponse" : {
        "@type" : "RadioDetails",
        "@responseType" : "getEntity",
        "@requestUrl" : "https : //10.64.88.203/webacs/api/v1/data/RadioDetails/15",
        "@rootUrl" : "https : //10.64.88.203/webacs/api/v1/data",
        "entity" : {
          "@dtoType" : "radioDetailsDTO",
          "@type" : "RadioDetails",
          "@url" : "https : //10.64.88.203/webacs/api/v1/data/RadioDetails/15",
          "radioDetailsDTO" : {
            "@displayName" : "String value",
            "@id" : 15,
            "@uuid" : "String value",
            "adminStatus" : "UNKNOWN",
            "alarmStatus" : "CRITICAL",
            "antennaAzimAngle" : 15,
            "antennaElevAngle" : 15,
            "antennaGain" : 15,
            "antennaName" : "String value",
            "apName" : "String value",
            "dot11nCapable" : true,
            "operStatus" : "DOWN",
            "port" : 1,
            "powerLevel" : 15,
            "radioBand" : "2.4 GHz",
            "radioRole" : "SHUTDOWN",
            "slotId" : 15,
            "txPowerOutput" : 15,
            "antennaDiversity" : "String value",
            "antennaMode" : "String value",
            "antennaType" : "String value",
            "apIpAddress" : "String value",
            "baseRadioMac" : "String value",
            "channelControl" : "String value",
            "channelNumber" : 15,
            "channelWidth" : "String value",
            "cleanAirCapable" : "String value",
            "cleanAirSensorStatus" : "String value",
            "cleanAirStatus" : "String value",
            "clientCount" : "String value",
            "controllerIpAddress" : "String value",
            "ethernetMac" : "String value",
            "radioType" : "String value",
            "txPowerControl" : "String value"
          }
        }
      }
    }

### Resource Information

Rate Limiting? | Yes
Sorting? | Yes
Paging? | Yes
Filtering? | Yes
Group Filtering? | No
Aggregation? | No
Response Formats | xml json
User Group | NBI Read
HTTP Methods | GET

## Resource URL

/webacs/api/v2/data/RadioDetails

Unmodified

This resource has not been modified since the previous API version.

Deprecated

This version has been deprecated. Please use v4.

## Response Parameters

Attribute | Description
--- | ---
adminStatus RadioAdminStatusEnum | Administrative status of the radio interface Allowed values UNKNOWN ENABLE DISABLE
alarmStatus AlarmSeverityEnum | Allowed values CRITICAL MAJOR MINOR WARNING CLEARED INFORMATION
antennaAzimAngle Float | Displays the horizontal angle of the antenna
antennaDiversity String | Displays if antenna diversity is enabled or disabled. Antenna diversity refers to the access point sampling the radio signal from two integrated antenna ports to choose the preferred antenna. Allowed values: 'Connector A', 'Connector B', 'Enabled', 'NA'
antennaElevAngle Float | Displays the elevation angle of the antenna.
antennaGain Integer | The external antenna gain, measured in 0.5 dBi units. This is the raw value from device. It is different from displayed in the UI. An integer value 7 means 7 x 0.5 = 3.5 dBm of gain.
antennaMode String | Displays the antenna mode. Allowed values: Sector A, Sector B, Omni, NA (non-applicable).
antennaName String | Antenna name
antennaType String | Antenna type. Allowed values: Internal, External, Circular, Linear, NA
apIpAddress String | IP address of the access point
apName String | Name of the access point
baseRadioMac String | Base radio MAC address
channelControl String | Radio channel control. Allowed values: Automatic, Custom, NA
channelNumber Integer | Current operational channel number
channelWidth String | Channel width. Allowed values: 5 MHz, 10 MHz, 20 MHz, 40 MHz, 80 MHz, 160 MHz, Above 40 MHz, Below 40 MHz, NA
cleanAirCapable String | Capability of clean air feature. Allowed values: Yes, No
cleanAirSensorStatus String | Clean air sensor status. Allowed values: Up, Down, NA
cleanAirStatus String | Clean air status. Allowed values: Yes, No
clientCount String | Client count connected to the radio interface
controllerIpAddress String | Registered controller IP address for CAPWAP AP only
dot11nCapable boolean | 802.11n capability
ethernetMac String | MAC address of the ethernet interface on the AP
operStatus RadioOperStatusEnum | Operational status of the radio interface Allowed values DOWN UP NOTASSOCIATED UNKNOWN
port int | Controller port number
powerLevel Integer | Power level of the radio
radioBand RadioBandEnum | Radio band of the radio interface Allowed values 2.4 GHz 5 GHz Unknown
radioRole RadioRoleEnum | Radio role Allowed values SHUTDOWN UPDOWNLINK UPLINK DOWNLINK ACCESS UPLINKACCESS DOWNLINKACCESS UPDOWNLINKACCESS NOTAPPLICABLE
radioType String | Radio type of the interface. Allowed values: 802.11a, 802.11ac, 802.11a/n, 802.11a/n/ac, 802.11a/n/ac/ax, 802.11b/g, 802.11b/g/n, 802.11b/g/n/ax, 802.11a/b/g/n, 802.11a/b/g/n/ac, 802.11a/b/g/n/ac/ax, XOR (Monitor Mode), XOR (2.4GHz), XOR (5GHz), UWB, BLE, Unknown
slotId Integer | Slot ID of the radio in the AP
txPowerControl String | Tranmission power control. Allowed values: Automatic, Custom, NA
txPowerOutput Integer | The txPower currently being used to transmit data, in dBm

## Sample Payloads

Sample payloads are for information only. They are automatically generated and the values included may not be representative of actual valid data values.

### Sample XML Payload

https://10.64.88.203/webacs/api/v2/data/RadioDetails/15

    <?xml version="1.0" ?>
    <queryResponse type="RadioDetails" responseType="getEntity" requestUrl="https://10.64.88.203/webacs/api/v2/data/RadioDetails/15" rootUrl="https://10.64.88.203/webacs/api/v2/data">
      <entity dtoType="radioDetailsDTO" type="RadioDetails" url="https://10.64.88.203/webacs/api/v2/data/RadioDetails/15">
        <radioDetailsDTO displayName="String value" id="15" uuid="String value">
          <adminStatus>UNKNOWN</adminStatus>
          <alarmStatus>CRITICAL</alarmStatus>
          <antennaAzimAngle>15.0</antennaAzimAngle>
          <antennaElevAngle>15.0</antennaElevAngle>
          <antennaGain>15</antennaGain>
          <antennaName>String value</antennaName>
          <apName>String value</apName>
          <dot11nCapable>true</dot11nCapable>
          <operStatus>DOWN</operStatus>
          <port>1</port>
          <powerLevel>15</powerLevel>
          <radioBand>2.4 GHz</radioBand>
          <radioRole>SHUTDOWN</radioRole>
          <slotId>15</slotId>
          <txPowerOutput>15</txPowerOutput>
          <antennaDiversity>String value</antennaDiversity>
          <antennaMode>String value</antennaMode>
          <antennaType>String value</antennaType>
          <apIpAddress>String value</apIpAddress>
          <baseRadioMac>String value</baseRadioMac>
          <channelControl>String value</channelControl>
          <channelNumber>15</channelNumber>
          <channelWidth>String value</channelWidth>
          <cleanAirCapable>String value</cleanAirCapable>
          <cleanAirSensorStatus>String value</cleanAirSensorStatus>
          <cleanAirStatus>String value</cleanAirStatus>
          <clientCount>String value</clientCount>
          <controllerIpAddress>String value</controllerIpAddress>
          <ethernetMac>String value</ethernetMac>
          <radioType>String value</radioType>
          <txPowerControl>String value</txPowerControl>
        </radioDetailsDTO>
      </entity>
    </queryResponse>

### Sample JSON Payload

https://10.64.88.203/webacs/api/v2/data/RadioDetails/15.json

    {
      "queryResponse" : {
        "@type" : "RadioDetails",
        "@requestUrl" : "https://10.64.88.203/webacs/api/v2/data/RadioDetails/15",
        "@responseType" : "getEntity",
        "@rootUrl" : "https://10.64.88.203/webacs/api/v2/data",
        "entity" : [ {
          "@dtoType" : "radioDetailsDTO",
          "@type" : "RadioDetails",
          "@url" : "https://10.64.88.203/webacs/api/v2/data/RadioDetails/15",
          "radioDetailsDTO" : {
            "@displayName" : "String value",
            "@id" : 15,
            "@uuid" : "String value",
            "adminStatus" : "UNKNOWN",
            "alarmStatus" : "CRITICAL",
            "antennaAzimAngle" : 15.0,
            "antennaDiversity" : "String value",
            "antennaElevAngle" : 15.0,
            "antennaGain" : 15,
            "antennaMode" : "String value",
            "antennaName" : "String value",
            "antennaType" : "String value",
            "apIpAddress" : "String value",
            "apName" : "String value",
            "baseRadioMac" : "String value",
            "channelControl" : "String value",
            "channelNumber" : 15,
            "channelWidth" : "String value",
            "cleanAirCapable" : "String value",
            "cleanAirSensorStatus" : "String value",
            "cleanAirStatus" : "String value",
            "clientCount" : "String value",
            "controllerIpAddress" : "String value",
            "dot11nCapable" : true,
            "ethernetMac" : "String value",
            "operStatus" : "DOWN",
            "port" : 1,
            "powerLevel" : 15,
            "radioBand" : "2.4 GHz",
            "radioRole" : "SHUTDOWN",
            "radioType" : "String value",
            "slotId" : 15,
            "txPowerControl" : "String value",
            "txPowerOutput" : 15
          }
        } ]
      }
    }

### Resource Information

Rate Limiting? | Yes
Sorting? | Yes
Paging? | Yes
Filtering? | Yes
Group Filtering? | No
Aggregation? | No
Response Formats | xml json
User Group | NBI Read
HTTP Methods | GET

## Resource URL

/webacs/api/v3/data/RadioDetails

Unmodified

This resource has not been modified since the previous API version.

Deprecated

This version has been deprecated. Please use v4.

## Response Parameters

Attribute | Description
--- | ---
adminStatus RadioAdminStatusEnum | Administrative status of the radio interface Allowed values UNKNOWN ENABLE DISABLE
alarmStatus AlarmSeverityEnum | Allowed values CRITICAL MAJOR MINOR WARNING CLEARED INFORMATION
antennaAzimAngle Float | Displays the horizontal angle of the antenna
antennaDiversity String | Displays if antenna diversity is enabled or disabled. Antenna diversity refers to the access point sampling the radio signal from two integrated antenna ports to choose the preferred antenna. Allowed values: 'Connector A', 'Connector B', 'Enabled', 'NA'
antennaElevAngle Float | Displays the elevation angle of the antenna.
antennaGain Integer | The external antenna gain, measured in 0.5 dBi units. This is the raw value from device. It is different from displayed in the UI. An integer value 7 means 7 x 0.5 = 3.5 dBm of gain.
antennaMode String | Displays the antenna mode. Allowed values: Sector A, Sector B, Omni, NA (non-applicable).
antennaName String | Antenna name
antennaType String | Antenna type. Allowed values: Internal, External, Circular, Linear, NA
apIpAddress String | IP address of the access point
apName String | Name of the access point
baseRadioMac String | Base radio MAC address
channelControl String | Radio channel control. Allowed values: Automatic, Custom, NA
channelNumber Integer | Current operational channel number
channelWidth String | Channel width. Allowed values: 5 MHz, 10 MHz, 20 MHz, 40 MHz, 80 MHz, 160 MHz, Above 40 MHz, Below 40 MHz, NA
cleanAirCapable String | Capability of clean air feature. Allowed values: Yes, No
cleanAirSensorStatus String | Clean air sensor status. Allowed values: Up, Down, NA
cleanAirStatus String | Clean air status. Allowed values: Yes, No
clientCount String | Client count connected to the radio interface
controllerIpAddress String | Registered controller IP address for CAPWAP AP only
dot11nCapable boolean | 802.11n capability
ethernetMac String | MAC address of the ethernet interface on the AP
operStatus RadioOperStatusEnum | Operational status of the radio interface Allowed values DOWN UP NOTASSOCIATED UNKNOWN
port int | Controller port number
powerLevel Integer | Power level of the radio
radioBand RadioBandEnum | Radio band of the radio interface Allowed values 2.4 GHz 5 GHz Unknown
radioRole RadioRoleEnum | Radio role Allowed values SHUTDOWN UPDOWNLINK UPLINK DOWNLINK ACCESS UPLINKACCESS DOWNLINKACCESS UPDOWNLINKACCESS NOTAPPLICABLE
radioType String | Radio type of the interface. Allowed values: 802.11a, 802.11ac, 802.11a/n, 802.11a/n/ac, 802.11a/n/ac/ax, 802.11b/g, 802.11b/g/n, 802.11b/g/n/ax, 802.11a/b/g/n, 802.11a/b/g/n/ac, 802.11a/b/g/n/ac/ax, XOR (Monitor Mode), XOR (2.4GHz), XOR (5GHz), UWB, BLE, Unknown
slotId Integer | Slot ID of the radio in the AP
txPowerControl String | Tranmission power control. Allowed values: Automatic, Custom, NA
txPowerOutput Integer | The txPower currently being used to transmit data, in dBm

## Sample Payloads

Sample payloads are for information only. They are automatically generated and the values included may not be representative of actual valid data values.

### Sample XML Payload

https://10.64.88.203/webacs/api/v3/data/RadioDetails/15

    <?xml version="1.0" ?>
    <queryResponse type="RadioDetails" responseType="getEntity" requestUrl="https://10.64.88.203/webacs/api/v3/data/RadioDetails/15" rootUrl="https://10.64.88.203/webacs/api/v3/data">
      <entity dtoType="radioDetailsDTO" type="RadioDetails" url="https://10.64.88.203/webacs/api/v3/data/RadioDetails/15">
        <radioDetailsDTO displayName="String value" id="15" uuid="String value">
          <adminStatus>UNKNOWN</adminStatus>
          <alarmStatus>CRITICAL</alarmStatus>
          <antennaAzimAngle>15.0</antennaAzimAngle>
          <antennaElevAngle>15.0</antennaElevAngle>
          <antennaGain>15</antennaGain>
          <antennaName>String value</antennaName>
          <apName>String value</apName>
          <dot11nCapable>true</dot11nCapable>
          <operStatus>DOWN</operStatus>
          <port>1</port>
          <powerLevel>15</powerLevel>
          <radioBand>2.4 GHz</radioBand>
          <radioRole>SHUTDOWN</radioRole>
          <slotId>15</slotId>
          <txPowerOutput>15</txPowerOutput>
          <antennaDiversity>String value</antennaDiversity>
          <antennaMode>String value</antennaMode>
          <antennaType>String value</antennaType>
          <apIpAddress>String value</apIpAddress>
          <baseRadioMac>String value</baseRadioMac>
          <channelControl>String value</channelControl>
          <channelNumber>15</channelNumber>
          <channelWidth>String value</channelWidth>
          <cleanAirCapable>String value</cleanAirCapable>
          <cleanAirSensorStatus>String value</cleanAirSensorStatus>
          <cleanAirStatus>String value</cleanAirStatus>
          <clientCount>String value</clientCount>
          <controllerIpAddress>String value</controllerIpAddress>
          <ethernetMac>String value</ethernetMac>
          <radioType>String value</radioType>
          <txPowerControl>String value</txPowerControl>
        </radioDetailsDTO>
      </entity>
    </queryResponse>

### Sample JSON Payload

https://10.64.88.203/webacs/api/v3/data/RadioDetails/15.json

    {
      "queryResponse" : {
        "@type" : "RadioDetails",
        "@requestUrl" : "https://10.64.88.203/webacs/api/v3/data/RadioDetails/15",
        "@responseType" : "getEntity",
        "@rootUrl" : "https://10.64.88.203/webacs/api/v3/data",
        "entity" : [ {
          "@dtoType" : "radioDetailsDTO",
          "@type" : "RadioDetails",
          "@url" : "https://10.64.88.203/webacs/api/v3/data/RadioDetails/15",
          "radioDetailsDTO" : {
            "@displayName" : "String value",
            "@id" : 15,
            "@uuid" : "String value",
            "adminStatus" : "UNKNOWN",
            "alarmStatus" : "CRITICAL",
            "antennaAzimAngle" : 15.0,
            "antennaDiversity" : "String value",
            "antennaElevAngle" : 15.0,
            "antennaGain" : 15,
            "antennaMode" : "String value",
            "antennaName" : "String value",
            "antennaType" : "String value",
            "apIpAddress" : "String value",
            "apName" : "String value",
            "baseRadioMac" : "String value",
            "channelControl" : "String value",
            "channelNumber" : 15,
            "channelWidth" : "String value",
            "cleanAirCapable" : "String value",
            "cleanAirSensorStatus" : "String value",
            "cleanAirStatus" : "String value",
            "clientCount" : "String value",
            "controllerIpAddress" : "String value",
            "dot11nCapable" : true,
            "ethernetMac" : "String value",
            "operStatus" : "DOWN",
            "port" : 1,
            "powerLevel" : 15,
            "radioBand" : "2.4 GHz",
            "radioRole" : "SHUTDOWN",
            "radioType" : "String value",
            "slotId" : 15,
            "txPowerControl" : "String value",
            "txPowerOutput" : 15
          }
        } ]
      }
    }

### Resource Information

Rate Limiting? | Yes
Sorting? | Yes
Paging? | Yes
Filtering? | Yes
Group Filtering? | No
Aggregation? | No
Response Formats | xml json
User Group | NBI Read
HTTP Methods | GET

## Resource URL

/webacs/api/v4/data/RadioDetails

Updated

Since version 4 types of attributes apIpAddress, controllerIpAddress, channelNumber, clientCount have been changed.

## Response Parameters

Attribute | Description
--- | ---
adminStatus RadioAdminStatusEnum | Administrative status of the radio interface Allowed values UNKNOWN ENABLE DISABLE
alarmStatus AlarmSeverityEnum | Allowed values CRITICAL MAJOR MINOR WARNING CLEARED INFORMATION
antennaAzimAngle Float | Displays the horizontal angle of the antenna
antennaDiversity AntennaDiversityEnum | Displays if antenna diversity is enabled or disabled. Antenna diversity refers to the access point sampling the radio signal from two integrated antenna ports to choose the preferred antenna. Allowed values CONNECTOR_A CONNECTOR_B ENABLED NOT_APPLICABLE
antennaElevAngle Float | Displays the elevation angle of the antenna.
antennaGain Integer | The external antenna gain, measured in 0.5 dBi units. This is the raw value from device. It is different from displayed in the UI. An integer value 7 means 7 x 0.5 = 3.5 dBm of gain.
antennaMode AntennaModeEnum | Displays the antenna mode such as Omni, Directional, or NA (non-applicable). Allowed values SECTOR_A SECTOR_B OMNI NOTAPPLICABLE
antennaName String | Antenna name
antennaType AntennaTypeEnum | Antenna type Allowed values INTERNAL EXTERNAL CIRCULAR LINEAR NOT_APPLICABLE
apIpAddress InetAddress | IP address of the access point
apName String | Name of the access point
baseRadioMac MacAddress | Base radio MAC address
channelControl ChannelAssignmentEnum | Radio channel control Allowed values UNKNOWN AUTOMATIC CUSTOM
channelNumber ChannelNumberEnum | Current operational channel number Allowed values UNKNOWN _1 _2 _3 _4 _5 _6 _7 _8 _9 _10 _11 _12 _13 _14 _20 _21 _22 _23 _24 _25 _26 _34 _36 _38 _40 _42 _44 _46 _48 _52 _56 _60 _64 _100 _104 _108 _112 _116 _120 _124 _128 _132 _136 _140 _144 _149 _153 _157 _161 _165 _169 _173
channelWidth ChannelBandwidthEnum | Channel width Allowed values 5 MHz 10 MHz 20 MHz 40 MHz Below 40 MHz Above 40 MHz 80 MHz 160 MHz NOTAPPLICABLE
cleanAirCapable Boolean | Capability of clean air feature.
cleanAirSensorStatus CleanAirSensorStatus | Clean air sensor status Allowed values UP DOWN NOTAPPLICABLE
cleanAirStatus Boolean | Clean air enablement status.
clientCount int | Client count connected to the radio interface
controllerIpAddress InetAddress | Registered controller IP address for CAPWAP AP only
dot11nCapable boolean | 802.11n capability
ethernetMac MacAddress | MAC address of the ethernet interface on the AP
operStatus RadioOperStatusEnum | Operational status of the radio interface Allowed values DOWN UP NOTASSOCIATED UNKNOWN
port int | Controller port number
powerLevel Integer | Power level of the radio
radioBand RadioBandEnum | Radio band of the radio interface Allowed values 2.4 GHz 5 GHz Unknown
radioRole RadioRoleEnum | Radio role Allowed values SHUTDOWN UPDOWNLINK UPLINK DOWNLINK ACCESS UPLINKACCESS DOWNLINKACCESS UPDOWNLINKACCESS NOTAPPLICABLE
radioType UnifiedRadioTypeEnum | Radio type ot the interface Allowed values 802.11a 802.11a/n 802.11ac 802.11a/n/ac 802.11a/n/ac/ax 802.11b/g 802.11b/g/n 802.11b/g/n/ax 802.11a/b/g/n 802.11a/b/g/n/ac 802.11a/b/g/n/ac/ax XOR (2.4GHz) XOR (5GHz) XOR (Monitor Mode) UWB BLE Unknown
slotId Integer | Slot ID of the radio in the AP
txPowerControl TxPowerControlEnum | Tranmission power control Allowed values UNKNOWN AUTOMATIC CUSTOM
txPowerOutput Integer | The txPower currently being used to transmit data, in dBm

## Sample Payloads

Sample payloads are for information only. They are automatically generated and the values included may not be representative of actual valid data values.

### Sample XML Payload

https://10.64.88.203/webacs/api/v4/data/RadioDetails/15

    <?xml version="1.0" ?>
    <queryResponse type="RadioDetails" responseType="getEntity" requestUrl="https://10.64.88.203/webacs/api/v4/data/RadioDetails/15" rootUrl="https://10.64.88.203/webacs/api/v4/data">
      <entity dtoType="radioDetailsDTO" type="RadioDetails" url="https://10.64.88.203/webacs/api/v4/data/RadioDetails/15">
        <radioDetailsDTO displayName="String value" id="15" uuid="String value">
          <adminStatus>UNKNOWN</adminStatus>
          <alarmStatus>CRITICAL</alarmStatus>
          <antennaAzimAngle>15.0</antennaAzimAngle>
          <antennaElevAngle>15.0</antennaElevAngle>
          <antennaGain>15</antennaGain>
          <antennaName>String value</antennaName>
          <apName>String value</apName>
          <dot11nCapable>true</dot11nCapable>
          <operStatus>DOWN</operStatus>
          <port>1</port>
          <powerLevel>15</powerLevel>
          <radioBand>2.4 GHz</radioBand>
          <radioRole>SHUTDOWN</radioRole>
          <slotId>15</slotId>
          <txPowerOutput>15</txPowerOutput>
          <antennaDiversity>CONNECTOR_A</antennaDiversity>
          <antennaMode>SECTOR_A</antennaMode>
          <antennaType>INTERNAL</antennaType>
          <apIpAddress>
            <address>192.168.115.243</address>
          </apIpAddress>
          <baseRadioMac>
            <octets>000a959d6816</octets>
          </baseRadioMac>
          <channelControl>UNKNOWN</channelControl>
          <channelNumber>UNKNOWN</channelNumber>
          <channelWidth>5 MHz</channelWidth>
          <cleanAirCapable>true</cleanAirCapable>
          <cleanAirSensorStatus>UP</cleanAirSensorStatus>
          <cleanAirStatus>true</cleanAirStatus>
          <clientCount>1</clientCount>
          <controllerIpAddress>
            <address>192.168.115.243</address>
          </controllerIpAddress>
          <ethernetMac>
            <octets>000a959d6816</octets>
          </ethernetMac>
          <radioType>802.11a</radioType>
          <txPowerControl>UNKNOWN</txPowerControl>
        </radioDetailsDTO>
      </entity>
    </queryResponse>

### Sample JSON Payload

https://10.64.88.203/webacs/api/v4/data/RadioDetails/15.json

    {
      "queryResponse" : {
        "@type" : "RadioDetails",
        "@requestUrl" : "https://10.64.88.203/webacs/api/v4/data/RadioDetails/15",
        "@responseType" : "getEntity",
        "@rootUrl" : "https://10.64.88.203/webacs/api/v4/data",
        "entity" : [ {
          "@dtoType" : "radioDetailsDTO",
          "@type" : "RadioDetails",
          "@url" : "https://10.64.88.203/webacs/api/v4/data/RadioDetails/15",
          "radioDetailsDTO" : {
            "@displayName" : "String value",
            "@id" : 15,
            "@uuid" : "String value",
            "adminStatus" : "UNKNOWN",
            "alarmStatus" : "CRITICAL",
            "antennaAzimAngle" : 15.0,
            "antennaDiversity" : "CONNECTOR_A",
            "antennaElevAngle" : 15.0,
            "antennaGain" : 15,
            "antennaMode" : "SECTOR_A",
            "antennaName" : "String value",
            "antennaType" : "INTERNAL",
            "apIpAddress" : {
              "address" : "192.168.115.243"
            },
            "apName" : "String value",
            "baseRadioMac" : {
              "octets" : "000a959d6816"
            },
            "channelControl" : "UNKNOWN",
            "channelNumber" : "UNKNOWN",
            "channelWidth" : "5 MHz",
            "cleanAirCapable" : true,
            "cleanAirSensorStatus" : "UP",
            "cleanAirStatus" : true,
            "clientCount" : 1,
            "controllerIpAddress" : {
              "address" : "192.168.115.243"
            },
            "dot11nCapable" : true,
            "ethernetMac" : {
              "octets" : "000a959d6816"
            },
            "operStatus" : "DOWN",
            "port" : 1,
            "powerLevel" : 15,
            "radioBand" : "2.4 GHz",
            "radioRole" : "SHUTDOWN",
            "radioType" : "802.11a",
            "slotId" : 15,
            "txPowerControl" : "UNKNOWN",
            "txPowerOutput" : 15
          }
        } ]
      }
    }