
Cisco Evolved Programmable Network Manager API
Evolved Programmable Network Manager API Documentation

# GET nfv/getOvsBridges

Get OVS bridges.

Since Product Version: 3.1

- Jump To

- v1
- v2
- v3
- v4

### Resource Information

Rate Limiting? | No
Sorting? | No
Paging? | No
Filtering? | No
Group Filtering? | No
Aggregation? | No
Response Formats | xml json
User Group | NBI Read
HTTP Methods | GET

API version v1 is deprecated

This API version has been deprecated. It will be removed in a future release of the product. Please develop new clients using the latest API version. Please modify your existing clients to use a later API version.

## Resource URL

/webacs/api/v1/op/nfv/getOvsBridges

## Request Parameters

Attribute | Source | Description
--- | --- | ---
deviceIp String | query | Optional Device management address

## Response Parameters

Attribute | Description
--- | ---
admin_state Boolean | Specifies whether the admin state is up or down. Set to true for up and false for down. If down, the network does not forward packets.
akey_name String | Name of the network to be created. The name will be appended with the deployment id during actual creation during deployment to maintain uniqueness. These are given before vm_group so that ESC can create the network before actually deploying any VMs on the network in one pass.
bridge String | Attach this network to a bridge.
mirror Boolean | Mirror traffic to this network from other network.
mirror_src String | Mirror traffic from a specific source.
provider_network_type String | Specifies the physical mechanism by which the virtual network is implemented.
provider_physical_network String | Specifies the name of the physical network over which the virtual network is implemented.
provider_segmentation_id Integer | ID or tunnel ID of the underlying physical network.
router_external Boolean | Indicates whether this netework is externally accessible.
shared Boolean | Whether the network is shared among other tenants.
sriov String | Attach this network using SR-IOV.
subnet Subnet[] | Subnet DTO.
Attribute | Description
--- | ---
address String | Subnet address for this network. E.g.: 10.4.4.0
akey_name String | Name of the subnet.
dhcp Boolean | true if IP addresses are assigned by DHCP.
gateway String | Default gateway for the network. If unspecified ESC will try to determine the gateway for the network.
ipversion String | ipv4 or ipv6
netmask String | Netmask for the network
trunk Boolean | Set to trunk mode.
vlan Short[] | The list of vLANs for this network.

## Sample Payloads

Sample payloads are for information only. They are automatically generated and the values included may not be representative of actual valid data values.

### Sample XML Response Payload

https://10.64.88.203/webacs/api/v1/op/nfv/getOvsBridges

    <?xml version="1.0" ?>
    <mgmtResponse responseType="operation" requestUrl="../../../../../pages/common/login.jsp.html" rootUrl="https://10.64.88.203/webacs/api/v1/op">
      <network>
        <admin_state>true</admin_state>
        <akey_name>String value</akey_name>
        <bridge>String value</bridge>
        <mirror>true</mirror>
        <mirror_src>String value</mirror_src>
        <provider_network_type>String value</provider_network_type>
        <provider_physical_network>String value</provider_physical_network>
        <provider_segmentation_id>15</provider_segmentation_id>
        <router_external>true</router_external>
        <shared>true</shared>
        <sriov>String value</sriov>
        <subnets>
          <subnet>
            <address>String value</address>
            <akey_name>String value</akey_name>
            <dhcp>true</dhcp>
            <gateway>String value</gateway>
            <ipversion>String value</ipversion>
            <netmask>String value</netmask>
          </subnet>
          <subnet>
            <address>Another string value</address>
            <akey_name>Another string value</akey_name>
            <dhcp>false</dhcp>
            <gateway>Another string value</gateway>
            <ipversion>Another string value</ipversion>
            <netmask>Another string value</netmask>
          </subnet>
        </subnets>
        <trunk>true</trunk>
        <vlans>
          <vlan>15</vlan>
          <vlan>25</vlan>
        </vlans>
      </network>
      <network>
        <admin_state>false</admin_state>
        <akey_name>Another string value</akey_name>
        <bridge>Another string value</bridge>
        <mirror>false</mirror>
        <mirror_src>Another string value</mirror_src>
        <provider_network_type>Another string value</provider_network_type>
        <provider_physical_network>Another string value</provider_physical_network>
        <provider_segmentation_id>25</provider_segmentation_id>
        <router_external>false</router_external>
        <shared>false</shared>
        <sriov>Another string value</sriov>
        <subnets>
          <subnet>
            <address>String value</address>
            <akey_name>String value</akey_name>
            <dhcp>true</dhcp>
            <gateway>String value</gateway>
            <ipversion>String value</ipversion>
            <netmask>String value</netmask>
          </subnet>
          <subnet>
            <address>Another string value</address>
            <akey_name>Another string value</akey_name>
            <dhcp>false</dhcp>
            <gateway>Another string value</gateway>
            <ipversion>Another string value</ipversion>
            <netmask>Another string value</netmask>
          </subnet>
        </subnets>
        <trunk>false</trunk>
        <vlans>
          <vlan>15</vlan>
          <vlan>25</vlan>
        </vlans>
      </network>
    </mgmtResponse>

### Sample JSON Response Payload

https://10.64.88.203/webacs/api/v1/op/nfv/getOvsBridges.json

    {
      "mgmtResponse" : {
        "@responseType" : "operation",
        "@requestUrl" : "https : //10.64.88.203/webacs/api/v1/op/nfv/getOvsBridges",
        "@rootUrl" : "https : //10.64.88.203/webacs/api/v1/op",
        "network" : [{
          "admin_state" : true,
          "akey_name" : "String value",
          "bridge" : "String value",
          "mirror" : true,
          "mirror_src" : "String value",
          "provider_network_type" : "String value",
          "provider_physical_network" : "String value",
          "provider_segmentation_id" : 15,
          "router_external" : true,
          "shared" : true,
          "sriov" : "String value",
          "subnets" : {
            "subnet" : [{
              "address" : "String value",
              "akey_name" : "String value",
              "dhcp" : true,
              "gateway" : "String value",
              "ipversion" : "String value",
              "netmask" : "String value"
            },
            {
              "address" : "Another string value",
              "akey_name" : "Another string value",
              "dhcp" : false,
              "gateway" : "Another string value",
              "ipversion" : "Another string value",
              "netmask" : "Another string value"
            }]
          },
          "trunk" : true,
          "vlans" : {
            "vlan" : [15,
            25]
          }
        },
        {
          "admin_state" : false,
          "akey_name" : "Another string value",
          "bridge" : "Another string value",
          "mirror" : false,
          "mirror_src" : "Another string value",
          "provider_network_type" : "Another string value",
          "provider_physical_network" : "Another string value",
          "provider_segmentation_id" : 25,
          "router_external" : false,
          "shared" : false,
          "sriov" : "Another string value",
          "subnets" : {
            "subnet" : [{
              "address" : "String value",
              "akey_name" : "String value",
              "dhcp" : true,
              "gateway" : "String value",
              "ipversion" : "String value",
              "netmask" : "String value"
            },
            {
              "address" : "Another string value",
              "akey_name" : "Another string value",
              "dhcp" : false,
              "gateway" : "Another string value",
              "ipversion" : "Another string value",
              "netmask" : "Another string value"
            }]
          },
          "trunk" : false,
          "vlans" : {
            "vlan" : [15,
            25]
          }
        }]
      }
    }

### Resource Information

Rate Limiting? | No
Sorting? | No
Paging? | No
Filtering? | No
Group Filtering? | No
Aggregation? | No
Response Formats | xml json
User Group | NBI Read
HTTP Methods | GET

## Resource URL

/webacs/api/v2/op/nfv/getOvsBridges

Unmodified

This resource has not been modified since the previous API version.

## Request Parameters

Attribute | Source | Description
--- | --- | ---
deviceIp String | query | Optional Device management address

## Response Parameters

Attribute | Description
--- | ---
admin_state Boolean | Specifies whether the admin state is up or down. Set to true for up and false for down. If down, the network does not forward packets.
akey_name String | Name of the network to be created. The name will be appended with the deployment id during actual creation during deployment to maintain uniqueness. These are given before vm_group so that ESC can create the network before actually deploying any VMs on the network in one pass.
bridge String | Attach this network to a bridge.
mirror Boolean | Mirror traffic to this network from other network.
mirror_src String | Mirror traffic from a specific source.
provider_network_type String | Specifies the physical mechanism by which the virtual network is implemented.
provider_physical_network String | Specifies the name of the physical network over which the virtual network is implemented.
provider_segmentation_id Integer | ID or tunnel ID of the underlying physical network.
router_external Boolean | Indicates whether this netework is externally accessible.
shared Boolean | Whether the network is shared among other tenants.
sriov String | Attach this network using SR-IOV.
subnet Subnet[] | Subnet DTO.
Attribute | Description
--- | ---
address String | Subnet address for this network. E.g.: 10.4.4.0
akey_name String | Name of the subnet.
dhcp Boolean | true if IP addresses are assigned by DHCP.
gateway String | Default gateway for the network. If unspecified ESC will try to determine the gateway for the network.
ipversion String | ipv4 or ipv6
netmask String | Netmask for the network
trunk Boolean | Set to trunk mode.
vlan Short[] | The list of vLANs for this network.

## Sample Payloads

Sample payloads are for information only. They are automatically generated and the values included may not be representative of actual valid data values.

### Sample XML Response Payload

https://10.64.88.203/webacs/api/v2/op/nfv/getOvsBridges

    <?xml version="1.0" ?>
    <mgmtResponse responseType="operation" requestUrl="../../../../../pages/common/login.jsp.html" rootUrl="https://10.64.88.203/webacs/api/v2/op">
      <network>
        <admin_state>true</admin_state>
        <akey_name>String value</akey_name>
        <bridge>String value</bridge>
        <mirror>true</mirror>
        <mirror_src>String value</mirror_src>
        <provider_network_type>String value</provider_network_type>
        <provider_physical_network>String value</provider_physical_network>
        <provider_segmentation_id>15</provider_segmentation_id>
        <router_external>true</router_external>
        <shared>true</shared>
        <sriov>String value</sriov>
        <subnets>
          <subnet>
            <address>String value</address>
            <akey_name>String value</akey_name>
            <dhcp>true</dhcp>
            <gateway>String value</gateway>
            <ipversion>String value</ipversion>
            <netmask>String value</netmask>
          </subnet>
          <subnet>
            <address>Another string value</address>
            <akey_name>Another string value</akey_name>
            <dhcp>false</dhcp>
            <gateway>Another string value</gateway>
            <ipversion>Another string value</ipversion>
            <netmask>Another string value</netmask>
          </subnet>
        </subnets>
        <trunk>true</trunk>
        <vlans>
          <vlan>15</vlan>
          <vlan>25</vlan>
        </vlans>
      </network>
      <network>
        <admin_state>false</admin_state>
        <akey_name>Another string value</akey_name>
        <bridge>Another string value</bridge>
        <mirror>false</mirror>
        <mirror_src>Another string value</mirror_src>
        <provider_network_type>Another string value</provider_network_type>
        <provider_physical_network>Another string value</provider_physical_network>
        <provider_segmentation_id>25</provider_segmentation_id>
        <router_external>false</router_external>
        <shared>false</shared>
        <sriov>Another string value</sriov>
        <subnets>
          <subnet>
            <address>String value</address>
            <akey_name>String value</akey_name>
            <dhcp>true</dhcp>
            <gateway>String value</gateway>
            <ipversion>String value</ipversion>
            <netmask>String value</netmask>
          </subnet>
          <subnet>
            <address>Another string value</address>
            <akey_name>Another string value</akey_name>
            <dhcp>false</dhcp>
            <gateway>Another string value</gateway>
            <ipversion>Another string value</ipversion>
            <netmask>Another string value</netmask>
          </subnet>
        </subnets>
        <trunk>false</trunk>
        <vlans>
          <vlan>15</vlan>
          <vlan>25</vlan>
        </vlans>
      </network>
    </mgmtResponse>

### Sample JSON Response Payload

https://10.64.88.203/webacs/api/v2/op/nfv/getOvsBridges.json

    {
      "mgmtResponse" : {
        "@requestUrl" : "../../../../../pages/common/login.jsp.html",
        "@responseType" : "operation",
        "@rootUrl" : "https://10.64.88.203/webacs/api/v2/op",
        "network" : [ {
          "admin_state" : true,
          "akey_name" : "String value",
          "bridge" : "String value",
          "mirror" : true,
          "mirror_src" : "String value",
          "provider_network_type" : "String value",
          "provider_physical_network" : "String value",
          "provider_segmentation_id" : 15,
          "router_external" : true,
          "shared" : true,
          "sriov" : "String value",
          "subnets" : {
            "subnet" : [ {
              "address" : "String value",
              "akey_name" : "String value",
              "dhcp" : true,
              "gateway" : "String value",
              "ipversion" : "String value",
              "netmask" : "String value"
            }, {
              "address" : "Another string value",
              "akey_name" : "Another string value",
              "dhcp" : false,
              "gateway" : "Another string value",
              "ipversion" : "Another string value",
              "netmask" : "Another string value"
            } ]
          },
          "trunk" : true,
          "vlans" : {
            "vlan" : [ 15, 25 ]
          }
        }, {
          "admin_state" : false,
          "akey_name" : "Another string value",
          "bridge" : "Another string value",
          "mirror" : false,
          "mirror_src" : "Another string value",
          "provider_network_type" : "Another string value",
          "provider_physical_network" : "Another string value",
          "provider_segmentation_id" : 25,
          "router_external" : false,
          "shared" : false,
          "sriov" : "Another string value",
          "subnets" : {
            "subnet" : [ {
              "address" : "String value",
              "akey_name" : "String value",
              "dhcp" : true,
              "gateway" : "String value",
              "ipversion" : "String value",
              "netmask" : "String value"
            }, {
              "address" : "Another string value",
              "akey_name" : "Another string value",
              "dhcp" : false,
              "gateway" : "Another string value",
              "ipversion" : "Another string value",
              "netmask" : "Another string value"
            } ]
          },
          "trunk" : false,
          "vlans" : {
            "vlan" : [ 15, 25 ]
          }
        } ]
      }
    }

### Resource Information

Rate Limiting? | No
Sorting? | No
Paging? | No
Filtering? | No
Group Filtering? | No
Aggregation? | No
Response Formats | xml json
User Group | NBI Read
HTTP Methods | GET

## Resource URL

/webacs/api/v3/op/nfv/getOvsBridges

Unmodified

This resource has not been modified since the previous API version.

## Request Parameters

Attribute | Source | Description
--- | --- | ---
deviceIp String | query | Optional Device management address

## Response Parameters

Attribute | Description
--- | ---
admin_state Boolean | Specifies whether the admin state is up or down. Set to true for up and false for down. If down, the network does not forward packets.
akey_name String | Name of the network to be created. The name will be appended with the deployment id during actual creation during deployment to maintain uniqueness. These are given before vm_group so that ESC can create the network before actually deploying any VMs on the network in one pass.
bridge String | Attach this network to a bridge.
mirror Boolean | Mirror traffic to this network from other network.
mirror_src String | Mirror traffic from a specific source.
provider_network_type String | Specifies the physical mechanism by which the virtual network is implemented.
provider_physical_network String | Specifies the name of the physical network over which the virtual network is implemented.
provider_segmentation_id Integer | ID or tunnel ID of the underlying physical network.
router_external Boolean | Indicates whether this netework is externally accessible.
shared Boolean | Whether the network is shared among other tenants.
sriov String | Attach this network using SR-IOV.
subnet Subnet[] | Subnet DTO.
Attribute | Description
--- | ---
address String | Subnet address for this network. E.g.: 10.4.4.0
akey_name String | Name of the subnet.
dhcp Boolean | true if IP addresses are assigned by DHCP.
gateway String | Default gateway for the network. If unspecified ESC will try to determine the gateway for the network.
ipversion String | ipv4 or ipv6
netmask String | Netmask for the network
trunk Boolean | Set to trunk mode.
vlan Short[] | The list of vLANs for this network.

## Sample Payloads

Sample payloads are for information only. They are automatically generated and the values included may not be representative of actual valid data values.

### Sample XML Response Payload

https://10.64.88.203/webacs/api/v3/op/nfv/getOvsBridges

    <?xml version="1.0" ?>
    <mgmtResponse responseType="operation" requestUrl="../../../../../pages/common/login.jsp.html" rootUrl="https://10.64.88.203/webacs/api/v3/op">
      <network>
        <admin_state>true</admin_state>
        <akey_name>String value</akey_name>
        <bridge>String value</bridge>
        <mirror>true</mirror>
        <mirror_src>String value</mirror_src>
        <provider_network_type>String value</provider_network_type>
        <provider_physical_network>String value</provider_physical_network>
        <provider_segmentation_id>15</provider_segmentation_id>
        <router_external>true</router_external>
        <shared>true</shared>
        <sriov>String value</sriov>
        <subnets>
          <subnet>
            <address>String value</address>
            <akey_name>String value</akey_name>
            <dhcp>true</dhcp>
            <gateway>String value</gateway>
            <ipversion>String value</ipversion>
            <netmask>String value</netmask>
          </subnet>
          <subnet>
            <address>Another string value</address>
            <akey_name>Another string value</akey_name>
            <dhcp>false</dhcp>
            <gateway>Another string value</gateway>
            <ipversion>Another string value</ipversion>
            <netmask>Another string value</netmask>
          </subnet>
        </subnets>
        <trunk>true</trunk>
        <vlans>
          <vlan>15</vlan>
          <vlan>25</vlan>
        </vlans>
      </network>
      <network>
        <admin_state>false</admin_state>
        <akey_name>Another string value</akey_name>
        <bridge>Another string value</bridge>
        <mirror>false</mirror>
        <mirror_src>Another string value</mirror_src>
        <provider_network_type>Another string value</provider_network_type>
        <provider_physical_network>Another string value</provider_physical_network>
        <provider_segmentation_id>25</provider_segmentation_id>
        <router_external>false</router_external>
        <shared>false</shared>
        <sriov>Another string value</sriov>
        <subnets>
          <subnet>
            <address>String value</address>
            <akey_name>String value</akey_name>
            <dhcp>true</dhcp>
            <gateway>String value</gateway>
            <ipversion>String value</ipversion>
            <netmask>String value</netmask>
          </subnet>
          <subnet>
            <address>Another string value</address>
            <akey_name>Another string value</akey_name>
            <dhcp>false</dhcp>
            <gateway>Another string value</gateway>
            <ipversion>Another string value</ipversion>
            <netmask>Another string value</netmask>
          </subnet>
        </subnets>
        <trunk>false</trunk>
        <vlans>
          <vlan>15</vlan>
          <vlan>25</vlan>
        </vlans>
      </network>
    </mgmtResponse>

### Sample JSON Response Payload

https://10.64.88.203/webacs/api/v3/op/nfv/getOvsBridges.json

    {
      "mgmtResponse" : {
        "@requestUrl" : "../../../../../pages/common/login.jsp.html",
        "@responseType" : "operation",
        "@rootUrl" : "https://10.64.88.203/webacs/api/v3/op",
        "network" : [ {
          "admin_state" : true,
          "akey_name" : "String value",
          "bridge" : "String value",
          "mirror" : true,
          "mirror_src" : "String value",
          "provider_network_type" : "String value",
          "provider_physical_network" : "String value",
          "provider_segmentation_id" : 15,
          "router_external" : true,
          "shared" : true,
          "sriov" : "String value",
          "subnets" : {
            "subnet" : [ {
              "address" : "String value",
              "akey_name" : "String value",
              "dhcp" : true,
              "gateway" : "String value",
              "ipversion" : "String value",
              "netmask" : "String value"
            }, {
              "address" : "Another string value",
              "akey_name" : "Another string value",
              "dhcp" : false,
              "gateway" : "Another string value",
              "ipversion" : "Another string value",
              "netmask" : "Another string value"
            } ]
          },
          "trunk" : true,
          "vlans" : {
            "vlan" : [ 15, 25 ]
          }
        }, {
          "admin_state" : false,
          "akey_name" : "Another string value",
          "bridge" : "Another string value",
          "mirror" : false,
          "mirror_src" : "Another string value",
          "provider_network_type" : "Another string value",
          "provider_physical_network" : "Another string value",
          "provider_segmentation_id" : 25,
          "router_external" : false,
          "shared" : false,
          "sriov" : "Another string value",
          "subnets" : {
            "subnet" : [ {
              "address" : "String value",
              "akey_name" : "String value",
              "dhcp" : true,
              "gateway" : "String value",
              "ipversion" : "String value",
              "netmask" : "String value"
            }, {
              "address" : "Another string value",
              "akey_name" : "Another string value",
              "dhcp" : false,
              "gateway" : "Another string value",
              "ipversion" : "Another string value",
              "netmask" : "Another string value"
            } ]
          },
          "trunk" : false,
          "vlans" : {
            "vlan" : [ 15, 25 ]
          }
        } ]
      }
    }

### Resource Information

Rate Limiting? | No
Sorting? | No
Paging? | No
Filtering? | No
Group Filtering? | No
Aggregation? | No
Response Formats | xml json
User Group | NBI Read
HTTP Methods | GET

## Resource URL

/webacs/api/v4/op/nfv/getOvsBridges

Unmodified

This resource has not been modified since the previous API version.

## Request Parameters

Attribute | Source | Description
--- | --- | ---
deviceIp String | query | Optional Device management address

## Response Parameters

Attribute | Description
--- | ---
admin_state Boolean | Specifies whether the admin state is up or down. Set to true for up and false for down. If down, the network does not forward packets.
akey_name String | Name of the network to be created. The name will be appended with the deployment id during actual creation during deployment to maintain uniqueness. These are given before vm_group so that ESC can create the network before actually deploying any VMs on the network in one pass.
bridge String | Attach this network to a bridge.
mirror Boolean | Mirror traffic to this network from other network.
mirror_src String | Mirror traffic from a specific source.
provider_network_type String | Specifies the physical mechanism by which the virtual network is implemented.
provider_physical_network String | Specifies the name of the physical network over which the virtual network is implemented.
provider_segmentation_id Integer | ID or tunnel ID of the underlying physical network.
router_external Boolean | Indicates whether this netework is externally accessible.
shared Boolean | Whether the network is shared among other tenants.
sriov String | Attach this network using SR-IOV.
subnet Subnet[] | Subnet DTO.
Attribute | Description
--- | ---
address String | Subnet address for this network. E.g.: 10.4.4.0
akey_name String | Name of the subnet.
dhcp Boolean | true if IP addresses are assigned by DHCP.
gateway String | Default gateway for the network. If unspecified ESC will try to determine the gateway for the network.
ipversion String | ipv4 or ipv6
netmask String | Netmask for the network
trunk Boolean | Set to trunk mode.
vlan Short[] | The list of vLANs for this network.

## Sample Payloads

Sample payloads are for information only. They are automatically generated and the values included may not be representative of actual valid data values.

### Sample XML Response Payload

https://10.64.88.203/webacs/api/v4/op/nfv/getOvsBridges

    <?xml version="1.0" ?>
    <mgmtResponse responseType="operation" requestUrl="../../../../../pages/common/login.jsp.html" rootUrl="https://10.64.88.203/webacs/api/v4/op">
      <network>
        <admin_state>true</admin_state>
        <akey_name>String value</akey_name>
        <bridge>String value</bridge>
        <mirror>true</mirror>
        <mirror_src>String value</mirror_src>
        <provider_network_type>String value</provider_network_type>
        <provider_physical_network>String value</provider_physical_network>
        <provider_segmentation_id>15</provider_segmentation_id>
        <router_external>true</router_external>
        <shared>true</shared>
        <sriov>String value</sriov>
        <subnets>
          <subnet>
            <address>String value</address>
            <akey_name>String value</akey_name>
            <dhcp>true</dhcp>
            <gateway>String value</gateway>
            <ipversion>String value</ipversion>
            <netmask>String value</netmask>
          </subnet>
          <subnet>
            <address>Another string value</address>
            <akey_name>Another string value</akey_name>
            <dhcp>false</dhcp>
            <gateway>Another string value</gateway>
            <ipversion>Another string value</ipversion>
            <netmask>Another string value</netmask>
          </subnet>
        </subnets>
        <trunk>true</trunk>
        <vlans>
          <vlan>15</vlan>
          <vlan>25</vlan>
        </vlans>
      </network>
      <network>
        <admin_state>false</admin_state>
        <akey_name>Another string value</akey_name>
        <bridge>Another string value</bridge>
        <mirror>false</mirror>
        <mirror_src>Another string value</mirror_src>
        <provider_network_type>Another string value</provider_network_type>
        <provider_physical_network>Another string value</provider_physical_network>
        <provider_segmentation_id>25</provider_segmentation_id>
        <router_external>false</router_external>
        <shared>false</shared>
        <sriov>Another string value</sriov>
        <subnets>
          <subnet>
            <address>String value</address>
            <akey_name>String value</akey_name>
            <dhcp>true</dhcp>
            <gateway>String value</gateway>
            <ipversion>String value</ipversion>
            <netmask>String value</netmask>
          </subnet>
          <subnet>
            <address>Another string value</address>
            <akey_name>Another string value</akey_name>
            <dhcp>false</dhcp>
            <gateway>Another string value</gateway>
            <ipversion>Another string value</ipversion>
            <netmask>Another string value</netmask>
          </subnet>
        </subnets>
        <trunk>false</trunk>
        <vlans>
          <vlan>15</vlan>
          <vlan>25</vlan>
        </vlans>
      </network>
    </mgmtResponse>

### Sample JSON Response Payload

https://10.64.88.203/webacs/api/v4/op/nfv/getOvsBridges.json

    {
      "mgmtResponse" : {
        "@requestUrl" : "../../../../../pages/common/login.jsp.html",
        "@responseType" : "operation",
        "@rootUrl" : "https://10.64.88.203/webacs/api/v4/op",
        "network" : [ {
          "admin_state" : true,
          "akey_name" : "String value",
          "bridge" : "String value",
          "mirror" : true,
          "mirror_src" : "String value",
          "provider_network_type" : "String value",
          "provider_physical_network" : "String value",
          "provider_segmentation_id" : 15,
          "router_external" : true,
          "shared" : true,
          "sriov" : "String value",
          "subnets" : {
            "subnet" : [ {
              "address" : "String value",
              "akey_name" : "String value",
              "dhcp" : true,
              "gateway" : "String value",
              "ipversion" : "String value",
              "netmask" : "String value"
            }, {
              "address" : "Another string value",
              "akey_name" : "Another string value",
              "dhcp" : false,
              "gateway" : "Another string value",
              "ipversion" : "Another string value",
              "netmask" : "Another string value"
            } ]
          },
          "trunk" : true,
          "vlans" : {
            "vlan" : [ 15, 25 ]
          }
        }, {
          "admin_state" : false,
          "akey_name" : "Another string value",
          "bridge" : "Another string value",
          "mirror" : false,
          "mirror_src" : "Another string value",
          "provider_network_type" : "Another string value",
          "provider_physical_network" : "Another string value",
          "provider_segmentation_id" : 25,
          "router_external" : false,
          "shared" : false,
          "sriov" : "Another string value",
          "subnets" : {
            "subnet" : [ {
              "address" : "String value",
              "akey_name" : "String value",
              "dhcp" : true,
              "gateway" : "String value",
              "ipversion" : "String value",
              "netmask" : "String value"
            }, {
              "address" : "Another string value",
              "akey_name" : "Another string value",
              "dhcp" : false,
              "gateway" : "Another string value",
              "ipversion" : "Another string value",
              "netmask" : "Another string value"
            } ]
          },
          "trunk" : false,
          "vlans" : {
            "vlan" : [ 15, 25 ]
          }
        } ]
      }
    }