
Cisco Evolved Programmable Network Manager API
Evolved Programmable Network Manager API Documentation

# GET ClientTraffics

Represents clients traffic information collected during the last polling cycle.

Since Product Version: 1.2

- Jump To

- v1
- v2
- v3
- v4

### Resource Information

Rate Limiting? | Yes
Sorting? | Yes
Paging? | Yes
Filtering? | Yes
Group Filtering? | No
Aggregation? | No
Response Formats | xml json
User Group | NBI Read
HTTP Methods | GET

API version v1 is deprecated

This API version has been deprecated. It will be removed in a future release of the product. Please develop new clients using the latest API version. Please modify your existing clients to use a later API version.

## Resource URL

/webacs/api/v1/data/ClientTraffics

Deprecated

This version has been deprecated. Please use v4.

## Response Parameters

Attribute | Description
--- | ---
collectionTime long | The time collection of this record was finished, measured in milliseconds since the Unix epoch.
dot11aReceived String | Total bytes received using 802.11a protocol
dot11aSent long | Total bytes sent using 802.11a protocol
dot11aThroughput long | Total throughput in Kbps using 802.11a protocol
dot11acReceived long | Total bytes received using 802.11ac protocol
dot11acSent long | Total bytes sent using 802.11ac protocol
dot11acThroughput long | Total throughput in Kbps using 802.11ac protocol
dot11ax2_4Received long | Total bytes received using 802.11ax protocol in 2.4GHz band
dot11ax2_4Sent long | Total bytes sent using 802.11ax protocol in 2.4GHz band
dot11ax2_4Throughput long | Total throughput in Kbps using 802.11ax protocol in 2.4GHz band
dot11ax5Received long | Total bytes received using 802.11ax protocol in 5GHz band
dot11ax5Sent long | Total bytes sent using 802.11ax protocol in 5GHz band
dot11ax5Throughput long | Total throughput in Kbps using 802.11ax protocol in 5GHz band
dot11bReceived String | Total bytes received using 802.11b protocol
dot11bSent long | Total bytes sent using 802.11b protocol
dot11bThroughput long | Total throughput in Kbps using 802.11b protocol
dot11gReceived String | Total bytes received using 802.11g protocol
dot11gSent long | Total bytes sent using 802.11g protocol
dot11gThroughput long | Total throughput in Kbps using 802.11g protocol
dot11n2_4Received String | Total bytes received using 802.11n protocol in 2.4GHz band
dot11n2_4Sent long | Total bytes sent using 802.11n protocol in 2.4GHz band
dot11n2_4Throughput long | Total throughput in Kbps using 802.11n protocol in 2.4GHz band
dot11n5Received String | Total bytes received using 802.11n protocol in 5GHz band
dot11n5Sent long | Total bytes sent using 802.11n protocol in 5GHz band
dot11n5Throughput long | Total throughput in Kbps using 802.11n protocol in 5GHz band
key String | Key represents the element
received String | Total bytes received
sent long | Total bytes sent
subkey String | Subkey is used to further categorize client count
throughput long | Total throughput in Kbps
type ClientCountTypeEnum | Type of count element Allowed values DEVICE ACCESSPOINT MAPLOCATION SSID VIRTUALDOMAIN GUEST
wired100MReceived String | Total bytes sent from wired clients connected to wired switch on 100Mbps port
wired100MSent long | Total bytes send from wired clients connected to wired switch on 100Mbps port
wired100MThroughput long | Total throughput from wired clients connected to wired switch on 100Mbps port
wired10GReceived long | Total bytes received by wired clients connected to wired switch on 10Gbps port
wired10GSent long | Total bytes send from wired clients connected to wired switch on 10Gbps port
wired10GThroughput long | Total throughput from wired clients connected to wired switch on 10Gbps port
wired10MReceived String | Total bytes sent from wired clients connected to wired switch on 10Mbps port
wired10MSent long | Total bytes send from wired clients connected to wired switch on 10Mbps port
wired10MThroughput long | Total throughput from wired clients connected to wired switch on 10Mbps port
wired1GReceived String | Total bytes sent from wired clients connected to wired switch on 1Gbps port
wired1GSent long | Total bytes send from wired clients connected to wired switch on 1Gbps port
wired1GThroughput long | Total throughput from wired clients connected to wired switch on 1Gbps port

## Sample Payloads

Sample payloads are for information only. They are automatically generated and the values included may not be representative of actual valid data values.

### Sample XML Payload

https://10.64.88.203/webacs/api/v1/data/ClientTraffics/15

    <?xml version="1.0" ?>
    <queryResponse type="ClientTraffics" responseType="getEntity" requestUrl="https://10.64.88.203/webacs/api/v1/data/ClientTraffics/15" rootUrl="https://10.64.88.203/webacs/api/v1/data">
      <entity dtoType="clientTrafficsDTO" type="ClientTraffics" url="https://10.64.88.203/webacs/api/v1/data/ClientTraffics/15">
        <clientTrafficsDTO displayName="String value" id="15" uuid="String value">
          <collectionTime>2</collectionTime>
          <dot11aSent>2</dot11aSent>
          <dot11aThroughput>2</dot11aThroughput>
          <dot11acReceived>2</dot11acReceived>
          <dot11acSent>2</dot11acSent>
          <dot11acThroughput>2</dot11acThroughput>
          <dot11ax2_4Received>2</dot11ax2_4Received>
          <dot11ax2_4Sent>2</dot11ax2_4Sent>
          <dot11ax2_4Throughput>2</dot11ax2_4Throughput>
          <dot11ax5Received>2</dot11ax5Received>
          <dot11ax5Sent>2</dot11ax5Sent>
          <dot11ax5Throughput>2</dot11ax5Throughput>
          <dot11bSent>2</dot11bSent>
          <dot11bThroughput>2</dot11bThroughput>
          <dot11gSent>2</dot11gSent>
          <dot11gThroughput>2</dot11gThroughput>
          <dot11n2_4Sent>2</dot11n2_4Sent>
          <dot11n2_4Throughput>2</dot11n2_4Throughput>
          <dot11n5Sent>2</dot11n5Sent>
          <dot11n5Throughput>2</dot11n5Throughput>
          <key>String value</key>
          <sent>2</sent>
          <subkey>String value</subkey>
          <throughput>2</throughput>
          <type>DEVICE</type>
          <wired100MSent>2</wired100MSent>
          <wired100MThroughput>2</wired100MThroughput>
          <wired10GReceived>2</wired10GReceived>
          <wired10GSent>2</wired10GSent>
          <wired10GThroughput>2</wired10GThroughput>
          <wired10MSent>2</wired10MSent>
          <wired10MThroughput>2</wired10MThroughput>
          <wired1GSent>2</wired1GSent>
          <wired1GThroughput>2</wired1GThroughput>
          <dot11aReceived>String value</dot11aReceived>
          <dot11bReceived>String value</dot11bReceived>
          <dot11gReceived>String value</dot11gReceived>
          <dot11n2_4Received>String value</dot11n2_4Received>
          <dot11n5Received>String value</dot11n5Received>
          <received>String value</received>
          <wired100MReceived>String value</wired100MReceived>
          <wired10MReceived>String value</wired10MReceived>
          <wired1GReceived>String value</wired1GReceived>
        </clientTrafficsDTO>
      </entity>
    </queryResponse>

### Sample JSON Payload

https://10.64.88.203/webacs/api/v1/data/ClientTraffics/15.json

    {
      "queryResponse" : {
        "@type" : "ClientTraffics",
        "@responseType" : "getEntity",
        "@requestUrl" : "https : //10.64.88.203/webacs/api/v1/data/ClientTraffics/15",
        "@rootUrl" : "https : //10.64.88.203/webacs/api/v1/data",
        "entity" : {
          "@dtoType" : "clientTrafficsDTO",
          "@type" : "ClientTraffics",
          "@url" : "https : //10.64.88.203/webacs/api/v1/data/ClientTraffics/15",
          "clientTrafficsDTO" : {
            "@displayName" : "String value",
            "@id" : 15,
            "@uuid" : "String value",
            "collectionTime" : 2,
            "dot11aSent" : 2,
            "dot11aThroughput" : 2,
            "dot11acReceived" : 2,
            "dot11acSent" : 2,
            "dot11acThroughput" : 2,
            "dot11ax2_4Received" : 2,
            "dot11ax2_4Sent" : 2,
            "dot11ax2_4Throughput" : 2,
            "dot11ax5Received" : 2,
            "dot11ax5Sent" : 2,
            "dot11ax5Throughput" : 2,
            "dot11bSent" : 2,
            "dot11bThroughput" : 2,
            "dot11gSent" : 2,
            "dot11gThroughput" : 2,
            "dot11n2_4Sent" : 2,
            "dot11n2_4Throughput" : 2,
            "dot11n5Sent" : 2,
            "dot11n5Throughput" : 2,
            "key" : "String value",
            "sent" : 2,
            "subkey" : "String value",
            "throughput" : 2,
            "type" : "DEVICE",
            "wired100MSent" : 2,
            "wired100MThroughput" : 2,
            "wired10GReceived" : 2,
            "wired10GSent" : 2,
            "wired10GThroughput" : 2,
            "wired10MSent" : 2,
            "wired10MThroughput" : 2,
            "wired1GSent" : 2,
            "wired1GThroughput" : 2,
            "dot11aReceived" : "String value",
            "dot11bReceived" : "String value",
            "dot11gReceived" : "String value",
            "dot11n2_4Received" : "String value",
            "dot11n5Received" : "String value",
            "received" : "String value",
            "wired100MReceived" : "String value",
            "wired10MReceived" : "String value",
            "wired1GReceived" : "String value"
          }
        }
      }
    }

### Resource Information

Rate Limiting? | Yes
Sorting? | Yes
Paging? | Yes
Filtering? | Yes
Group Filtering? | No
Aggregation? | No
Response Formats | xml json
User Group | NBI Read
HTTP Methods | GET

## Resource URL

/webacs/api/v2/data/ClientTraffics

Unmodified

This resource has not been modified since the previous API version.

Deprecated

This version has been deprecated. Please use v4.

## Response Parameters

Attribute | Description
--- | ---
collectionTime long | The time collection of this record was finished, measured in milliseconds since the Unix epoch.
dot11aReceived String | Total bytes received using 802.11a protocol
dot11aSent long | Total bytes sent using 802.11a protocol
dot11aThroughput long | Total throughput in Kbps using 802.11a protocol
dot11acReceived long | Total bytes received using 802.11ac protocol
dot11acSent long | Total bytes sent using 802.11ac protocol
dot11acThroughput long | Total throughput in Kbps using 802.11ac protocol
dot11ax2_4Received long | Total bytes received using 802.11ax protocol in 2.4GHz band
dot11ax2_4Sent long | Total bytes sent using 802.11ax protocol in 2.4GHz band
dot11ax2_4Throughput long | Total throughput in Kbps using 802.11ax protocol in 2.4GHz band
dot11ax5Received long | Total bytes received using 802.11ax protocol in 5GHz band
dot11ax5Sent long | Total bytes sent using 802.11ax protocol in 5GHz band
dot11ax5Throughput long | Total throughput in Kbps using 802.11ax protocol in 5GHz band
dot11bReceived String | Total bytes received using 802.11b protocol
dot11bSent long | Total bytes sent using 802.11b protocol
dot11bThroughput long | Total throughput in Kbps using 802.11b protocol
dot11gReceived String | Total bytes received using 802.11g protocol
dot11gSent long | Total bytes sent using 802.11g protocol
dot11gThroughput long | Total throughput in Kbps using 802.11g protocol
dot11n2_4Received String | Total bytes received using 802.11n protocol in 2.4GHz band
dot11n2_4Sent long | Total bytes sent using 802.11n protocol in 2.4GHz band
dot11n2_4Throughput long | Total throughput in Kbps using 802.11n protocol in 2.4GHz band
dot11n5Received String | Total bytes received using 802.11n protocol in 5GHz band
dot11n5Sent long | Total bytes sent using 802.11n protocol in 5GHz band
dot11n5Throughput long | Total throughput in Kbps using 802.11n protocol in 5GHz band
key String | Key represents the element
received String | Total bytes received
sent long | Total bytes sent
subkey String | Subkey is used to further categorize client count
throughput long | Total throughput in Kbps
type ClientCountTypeEnum | Type of count element Allowed values DEVICE ACCESSPOINT MAPLOCATION SSID VIRTUALDOMAIN GUEST
wired100MReceived String | Total bytes sent from wired clients connected to wired switch on 100Mbps port
wired100MSent long | Total bytes send from wired clients connected to wired switch on 100Mbps port
wired100MThroughput long | Total throughput from wired clients connected to wired switch on 100Mbps port
wired10GReceived long | Total bytes received by wired clients connected to wired switch on 10Gbps port
wired10GSent long | Total bytes send from wired clients connected to wired switch on 10Gbps port
wired10GThroughput long | Total throughput from wired clients connected to wired switch on 10Gbps port
wired10MReceived String | Total bytes sent from wired clients connected to wired switch on 10Mbps port
wired10MSent long | Total bytes send from wired clients connected to wired switch on 10Mbps port
wired10MThroughput long | Total throughput from wired clients connected to wired switch on 10Mbps port
wired1GReceived String | Total bytes sent from wired clients connected to wired switch on 1Gbps port
wired1GSent long | Total bytes send from wired clients connected to wired switch on 1Gbps port
wired1GThroughput long | Total throughput from wired clients connected to wired switch on 1Gbps port

## Sample Payloads

Sample payloads are for information only. They are automatically generated and the values included may not be representative of actual valid data values.

### Sample XML Payload

https://10.64.88.203/webacs/api/v2/data/ClientTraffics/15

    <?xml version="1.0" ?>
    <queryResponse type="ClientTraffics" responseType="getEntity" requestUrl="https://10.64.88.203/webacs/api/v2/data/ClientTraffics/15" rootUrl="https://10.64.88.203/webacs/api/v2/data">
      <entity dtoType="clientTrafficsDTO" type="ClientTraffics" url="https://10.64.88.203/webacs/api/v2/data/ClientTraffics/15">
        <clientTrafficsDTO displayName="String value" id="15" uuid="String value">
          <collectionTime>2</collectionTime>
          <dot11aSent>2</dot11aSent>
          <dot11aThroughput>2</dot11aThroughput>
          <dot11acReceived>2</dot11acReceived>
          <dot11acSent>2</dot11acSent>
          <dot11acThroughput>2</dot11acThroughput>
          <dot11ax2_4Received>2</dot11ax2_4Received>
          <dot11ax2_4Sent>2</dot11ax2_4Sent>
          <dot11ax2_4Throughput>2</dot11ax2_4Throughput>
          <dot11ax5Received>2</dot11ax5Received>
          <dot11ax5Sent>2</dot11ax5Sent>
          <dot11ax5Throughput>2</dot11ax5Throughput>
          <dot11bSent>2</dot11bSent>
          <dot11bThroughput>2</dot11bThroughput>
          <dot11gSent>2</dot11gSent>
          <dot11gThroughput>2</dot11gThroughput>
          <dot11n2_4Sent>2</dot11n2_4Sent>
          <dot11n2_4Throughput>2</dot11n2_4Throughput>
          <dot11n5Sent>2</dot11n5Sent>
          <dot11n5Throughput>2</dot11n5Throughput>
          <key>String value</key>
          <sent>2</sent>
          <subkey>String value</subkey>
          <throughput>2</throughput>
          <type>DEVICE</type>
          <wired100MSent>2</wired100MSent>
          <wired100MThroughput>2</wired100MThroughput>
          <wired10GReceived>2</wired10GReceived>
          <wired10GSent>2</wired10GSent>
          <wired10GThroughput>2</wired10GThroughput>
          <wired10MSent>2</wired10MSent>
          <wired10MThroughput>2</wired10MThroughput>
          <wired1GSent>2</wired1GSent>
          <wired1GThroughput>2</wired1GThroughput>
          <dot11aReceived>String value</dot11aReceived>
          <dot11bReceived>String value</dot11bReceived>
          <dot11gReceived>String value</dot11gReceived>
          <dot11n2_4Received>String value</dot11n2_4Received>
          <dot11n5Received>String value</dot11n5Received>
          <received>String value</received>
          <wired100MReceived>String value</wired100MReceived>
          <wired10MReceived>String value</wired10MReceived>
          <wired1GReceived>String value</wired1GReceived>
        </clientTrafficsDTO>
      </entity>
    </queryResponse>

### Sample JSON Payload

https://10.64.88.203/webacs/api/v2/data/ClientTraffics/15.json

    {
      "queryResponse" : {
        "@type" : "ClientTraffics",
        "@requestUrl" : "https://10.64.88.203/webacs/api/v2/data/ClientTraffics/15",
        "@responseType" : "getEntity",
        "@rootUrl" : "https://10.64.88.203/webacs/api/v2/data",
        "entity" : [ {
          "@dtoType" : "clientTrafficsDTO",
          "@type" : "ClientTraffics",
          "@url" : "https://10.64.88.203/webacs/api/v2/data/ClientTraffics/15",
          "clientTrafficsDTO" : {
            "@displayName" : "String value",
            "@id" : 15,
            "@uuid" : "String value",
            "collectionTime" : 2,
            "dot11aReceived" : "String value",
            "dot11aSent" : 2,
            "dot11aThroughput" : 2,
            "dot11acReceived" : 2,
            "dot11acSent" : 2,
            "dot11acThroughput" : 2,
            "dot11ax2_4Received" : 2,
            "dot11ax2_4Sent" : 2,
            "dot11ax2_4Throughput" : 2,
            "dot11ax5Received" : 2,
            "dot11ax5Sent" : 2,
            "dot11ax5Throughput" : 2,
            "dot11bReceived" : "String value",
            "dot11bSent" : 2,
            "dot11bThroughput" : 2,
            "dot11gReceived" : "String value",
            "dot11gSent" : 2,
            "dot11gThroughput" : 2,
            "dot11n2_4Received" : "String value",
            "dot11n2_4Sent" : 2,
            "dot11n2_4Throughput" : 2,
            "dot11n5Received" : "String value",
            "dot11n5Sent" : 2,
            "dot11n5Throughput" : 2,
            "key" : "String value",
            "received" : "String value",
            "sent" : 2,
            "subkey" : "String value",
            "throughput" : 2,
            "type" : "DEVICE",
            "wired100MReceived" : "String value",
            "wired100MSent" : 2,
            "wired100MThroughput" : 2,
            "wired10GReceived" : 2,
            "wired10GSent" : 2,
            "wired10GThroughput" : 2,
            "wired10MReceived" : "String value",
            "wired10MSent" : 2,
            "wired10MThroughput" : 2,
            "wired1GReceived" : "String value",
            "wired1GSent" : 2,
            "wired1GThroughput" : 2
          }
        } ]
      }
    }

### Resource Information

Rate Limiting? | Yes
Sorting? | Yes
Paging? | Yes
Filtering? | Yes
Group Filtering? | No
Aggregation? | No
Response Formats | xml json
User Group | NBI Read
HTTP Methods | GET

## Resource URL

/webacs/api/v3/data/ClientTraffics

Unmodified

This resource has not been modified since the previous API version.

Deprecated

This version has been deprecated. Please use v4.

## Response Parameters

Attribute | Description
--- | ---
collectionTime long | The time collection of this record was finished, measured in milliseconds since the Unix epoch.
dot11aReceived String | Total bytes received using 802.11a protocol
dot11aSent long | Total bytes sent using 802.11a protocol
dot11aThroughput long | Total throughput in Kbps using 802.11a protocol
dot11acReceived long | Total bytes received using 802.11ac protocol
dot11acSent long | Total bytes sent using 802.11ac protocol
dot11acThroughput long | Total throughput in Kbps using 802.11ac protocol
dot11ax2_4Received long | Total bytes received using 802.11ax protocol in 2.4GHz band
dot11ax2_4Sent long | Total bytes sent using 802.11ax protocol in 2.4GHz band
dot11ax2_4Throughput long | Total throughput in Kbps using 802.11ax protocol in 2.4GHz band
dot11ax5Received long | Total bytes received using 802.11ax protocol in 5GHz band
dot11ax5Sent long | Total bytes sent using 802.11ax protocol in 5GHz band
dot11ax5Throughput long | Total throughput in Kbps using 802.11ax protocol in 5GHz band
dot11bReceived String | Total bytes received using 802.11b protocol
dot11bSent long | Total bytes sent using 802.11b protocol
dot11bThroughput long | Total throughput in Kbps using 802.11b protocol
dot11gReceived String | Total bytes received using 802.11g protocol
dot11gSent long | Total bytes sent using 802.11g protocol
dot11gThroughput long | Total throughput in Kbps using 802.11g protocol
dot11n2_4Received String | Total bytes received using 802.11n protocol in 2.4GHz band
dot11n2_4Sent long | Total bytes sent using 802.11n protocol in 2.4GHz band
dot11n2_4Throughput long | Total throughput in Kbps using 802.11n protocol in 2.4GHz band
dot11n5Received String | Total bytes received using 802.11n protocol in 5GHz band
dot11n5Sent long | Total bytes sent using 802.11n protocol in 5GHz band
dot11n5Throughput long | Total throughput in Kbps using 802.11n protocol in 5GHz band
key String | Key represents the element
received String | Total bytes received
sent long | Total bytes sent
subkey String | Subkey is used to further categorize client count
throughput long | Total throughput in Kbps
type ClientCountTypeEnum | Type of count element Allowed values DEVICE ACCESSPOINT MAPLOCATION SSID VIRTUALDOMAIN GUEST
wired100MReceived String | Total bytes sent from wired clients connected to wired switch on 100Mbps port
wired100MSent long | Total bytes send from wired clients connected to wired switch on 100Mbps port
wired100MThroughput long | Total throughput from wired clients connected to wired switch on 100Mbps port
wired10GReceived long | Total bytes received by wired clients connected to wired switch on 10Gbps port
wired10GSent long | Total bytes send from wired clients connected to wired switch on 10Gbps port
wired10GThroughput long | Total throughput from wired clients connected to wired switch on 10Gbps port
wired10MReceived String | Total bytes sent from wired clients connected to wired switch on 10Mbps port
wired10MSent long | Total bytes send from wired clients connected to wired switch on 10Mbps port
wired10MThroughput long | Total throughput from wired clients connected to wired switch on 10Mbps port
wired1GReceived String | Total bytes sent from wired clients connected to wired switch on 1Gbps port
wired1GSent long | Total bytes send from wired clients connected to wired switch on 1Gbps port
wired1GThroughput long | Total throughput from wired clients connected to wired switch on 1Gbps port

## Sample Payloads

Sample payloads are for information only. They are automatically generated and the values included may not be representative of actual valid data values.

### Sample XML Payload

https://10.64.88.203/webacs/api/v3/data/ClientTraffics/15

    <?xml version="1.0" ?>
    <queryResponse type="ClientTraffics" responseType="getEntity" requestUrl="https://10.64.88.203/webacs/api/v3/data/ClientTraffics/15" rootUrl="https://10.64.88.203/webacs/api/v3/data">
      <entity dtoType="clientTrafficsDTO" type="ClientTraffics" url="https://10.64.88.203/webacs/api/v3/data/ClientTraffics/15">
        <clientTrafficsDTO displayName="String value" id="15" uuid="String value">
          <collectionTime>2</collectionTime>
          <dot11aSent>2</dot11aSent>
          <dot11aThroughput>2</dot11aThroughput>
          <dot11acReceived>2</dot11acReceived>
          <dot11acSent>2</dot11acSent>
          <dot11acThroughput>2</dot11acThroughput>
          <dot11ax2_4Received>2</dot11ax2_4Received>
          <dot11ax2_4Sent>2</dot11ax2_4Sent>
          <dot11ax2_4Throughput>2</dot11ax2_4Throughput>
          <dot11ax5Received>2</dot11ax5Received>
          <dot11ax5Sent>2</dot11ax5Sent>
          <dot11ax5Throughput>2</dot11ax5Throughput>
          <dot11bSent>2</dot11bSent>
          <dot11bThroughput>2</dot11bThroughput>
          <dot11gSent>2</dot11gSent>
          <dot11gThroughput>2</dot11gThroughput>
          <dot11n2_4Sent>2</dot11n2_4Sent>
          <dot11n2_4Throughput>2</dot11n2_4Throughput>
          <dot11n5Sent>2</dot11n5Sent>
          <dot11n5Throughput>2</dot11n5Throughput>
          <key>String value</key>
          <sent>2</sent>
          <subkey>String value</subkey>
          <throughput>2</throughput>
          <type>DEVICE</type>
          <wired100MSent>2</wired100MSent>
          <wired100MThroughput>2</wired100MThroughput>
          <wired10GReceived>2</wired10GReceived>
          <wired10GSent>2</wired10GSent>
          <wired10GThroughput>2</wired10GThroughput>
          <wired10MSent>2</wired10MSent>
          <wired10MThroughput>2</wired10MThroughput>
          <wired1GSent>2</wired1GSent>
          <wired1GThroughput>2</wired1GThroughput>
          <dot11aReceived>String value</dot11aReceived>
          <dot11bReceived>String value</dot11bReceived>
          <dot11gReceived>String value</dot11gReceived>
          <dot11n2_4Received>String value</dot11n2_4Received>
          <dot11n5Received>String value</dot11n5Received>
          <received>String value</received>
          <wired100MReceived>String value</wired100MReceived>
          <wired10MReceived>String value</wired10MReceived>
          <wired1GReceived>String value</wired1GReceived>
        </clientTrafficsDTO>
      </entity>
    </queryResponse>

### Sample JSON Payload

https://10.64.88.203/webacs/api/v3/data/ClientTraffics/15.json

    {
      "queryResponse" : {
        "@type" : "ClientTraffics",
        "@requestUrl" : "https://10.64.88.203/webacs/api/v3/data/ClientTraffics/15",
        "@responseType" : "getEntity",
        "@rootUrl" : "https://10.64.88.203/webacs/api/v3/data",
        "entity" : [ {
          "@dtoType" : "clientTrafficsDTO",
          "@type" : "ClientTraffics",
          "@url" : "https://10.64.88.203/webacs/api/v3/data/ClientTraffics/15",
          "clientTrafficsDTO" : {
            "@displayName" : "String value",
            "@id" : 15,
            "@uuid" : "String value",
            "collectionTime" : 2,
            "dot11aReceived" : "String value",
            "dot11aSent" : 2,
            "dot11aThroughput" : 2,
            "dot11acReceived" : 2,
            "dot11acSent" : 2,
            "dot11acThroughput" : 2,
            "dot11ax2_4Received" : 2,
            "dot11ax2_4Sent" : 2,
            "dot11ax2_4Throughput" : 2,
            "dot11ax5Received" : 2,
            "dot11ax5Sent" : 2,
            "dot11ax5Throughput" : 2,
            "dot11bReceived" : "String value",
            "dot11bSent" : 2,
            "dot11bThroughput" : 2,
            "dot11gReceived" : "String value",
            "dot11gSent" : 2,
            "dot11gThroughput" : 2,
            "dot11n2_4Received" : "String value",
            "dot11n2_4Sent" : 2,
            "dot11n2_4Throughput" : 2,
            "dot11n5Received" : "String value",
            "dot11n5Sent" : 2,
            "dot11n5Throughput" : 2,
            "key" : "String value",
            "received" : "String value",
            "sent" : 2,
            "subkey" : "String value",
            "throughput" : 2,
            "type" : "DEVICE",
            "wired100MReceived" : "String value",
            "wired100MSent" : 2,
            "wired100MThroughput" : 2,
            "wired10GReceived" : 2,
            "wired10GSent" : 2,
            "wired10GThroughput" : 2,
            "wired10MReceived" : "String value",
            "wired10MSent" : 2,
            "wired10MThroughput" : 2,
            "wired1GReceived" : "String value",
            "wired1GSent" : 2,
            "wired1GThroughput" : 2
          }
        } ]
      }
    }

### Resource Information

Rate Limiting? | Yes
Sorting? | Yes
Paging? | Yes
Filtering? | Yes
Group Filtering? | No
Aggregation? | No
Response Formats | xml json
User Group | NBI Read
HTTP Methods | GET

## Resource URL

/webacs/api/v4/data/ClientTraffics

Updated

Since version 4 type of attributes representing received traffic is long instead of String.

## Response Parameters

Attribute | Description
--- | ---
collectionTime long | The time collection of this record was finished, measured in milliseconds since the Unix epoch.
dot11aReceived long | Total bytes received using 802.11a protocol
dot11aSent long | Total bytes sent using 802.11a protocol
dot11aThroughput long | Total throughput in Kbps using 802.11a protocol
dot11acReceived long | Total bytes received using 802.11ac protocol
dot11acSent long | Total bytes sent using 802.11ac protocol
dot11acThroughput long | Total throughput in Kbps using 802.11ac protocol
dot11ax2_4Received long | Total bytes received using 802.11ax protocol in 2.4GHz band
dot11ax2_4Sent long | Total bytes sent using 802.11ax protocol in 2.4GHz band
dot11ax2_4Throughput long | Total throughput in Kbps using 802.11ax protocol in 2.4GHz band
dot11ax5Received long | Total bytes received using 802.11ax protocol in 5GHz band
dot11ax5Sent long | Total bytes sent using 802.11ax protocol in 5GHz band
dot11ax5Throughput long | Total throughput in Kbps using 802.11ax protocol in 5GHz band
dot11bReceived long | Total bytes received using 802.11b protocol
dot11bSent long | Total bytes sent using 802.11b protocol
dot11bThroughput long | Total throughput in Kbps using 802.11b protocol
dot11gReceived long | Total bytes received using 802.11g protocol
dot11gSent long | Total bytes sent using 802.11g protocol
dot11gThroughput long | Total throughput in Kbps using 802.11g protocol
dot11n2_4Received long | Total bytes received using 802.11n protocol in 2.4GHz band
dot11n2_4Sent long | Total bytes sent using 802.11n protocol in 2.4GHz band
dot11n2_4Throughput long | Total throughput in Kbps using 802.11n protocol in 2.4GHz band
dot11n5Received long | Total bytes received using 802.11n protocol in 5GHz band
dot11n5Sent long | Total bytes sent using 802.11n protocol in 5GHz band
dot11n5Throughput long | Total throughput in Kbps using 802.11n protocol in 5GHz band
key String | Key represents the element
received long | Total bytes received
sent long | Total bytes sent
subkey String | Subkey is used to further categorize client count
throughput long | Total throughput in Kbps
type ClientCountTypeEnum | Type of count element Allowed values DEVICE ACCESSPOINT MAPLOCATION SSID VIRTUALDOMAIN GUEST
wired100MReceived long | Total bytes sent from wired clients connected to wired switch on 100Mbps port
wired100MSent long | Total bytes send from wired clients connected to wired switch on 100Mbps port
wired100MThroughput long | Total throughput from wired clients connected to wired switch on 100Mbps port
wired10GReceived long | Total bytes received by wired clients connected to wired switch on 10Gbps port
wired10GSent long | Total bytes send from wired clients connected to wired switch on 10Gbps port
wired10GThroughput long | Total throughput from wired clients connected to wired switch on 10Gbps port
wired10MReceived long | Total bytes sent from wired clients connected to wired switch on 10Mbps port
wired10MSent long | Total bytes send from wired clients connected to wired switch on 10Mbps port
wired10MThroughput long | Total throughput from wired clients connected to wired switch on 10Mbps port
wired1GReceived long | Total bytes sent from wired clients connected to wired switch on 1Gbps port
wired1GSent long | Total bytes send from wired clients connected to wired switch on 1Gbps port
wired1GThroughput long | Total throughput from wired clients connected to wired switch on 1Gbps port

## Sample Payloads

Sample payloads are for information only. They are automatically generated and the values included may not be representative of actual valid data values.

### Sample XML Payload

https://10.64.88.203/webacs/api/v4/data/ClientTraffics/15

    <?xml version="1.0" ?>
    <queryResponse type="ClientTraffics" responseType="getEntity" requestUrl="https://10.64.88.203/webacs/api/v4/data/ClientTraffics/15" rootUrl="https://10.64.88.203/webacs/api/v4/data">
      <entity dtoType="clientTrafficsDTO" type="ClientTraffics" url="https://10.64.88.203/webacs/api/v4/data/ClientTraffics/15">
        <clientTrafficsDTO displayName="String value" id="15" uuid="String value">
          <collectionTime>2</collectionTime>
          <dot11aSent>2</dot11aSent>
          <dot11aThroughput>2</dot11aThroughput>
          <dot11acReceived>2</dot11acReceived>
          <dot11acSent>2</dot11acSent>
          <dot11acThroughput>2</dot11acThroughput>
          <dot11ax2_4Received>2</dot11ax2_4Received>
          <dot11ax2_4Sent>2</dot11ax2_4Sent>
          <dot11ax2_4Throughput>2</dot11ax2_4Throughput>
          <dot11ax5Received>2</dot11ax5Received>
          <dot11ax5Sent>2</dot11ax5Sent>
          <dot11ax5Throughput>2</dot11ax5Throughput>
          <dot11bSent>2</dot11bSent>
          <dot11bThroughput>2</dot11bThroughput>
          <dot11gSent>2</dot11gSent>
          <dot11gThroughput>2</dot11gThroughput>
          <dot11n2_4Sent>2</dot11n2_4Sent>
          <dot11n2_4Throughput>2</dot11n2_4Throughput>
          <dot11n5Sent>2</dot11n5Sent>
          <dot11n5Throughput>2</dot11n5Throughput>
          <key>String value</key>
          <sent>2</sent>
          <subkey>String value</subkey>
          <throughput>2</throughput>
          <type>DEVICE</type>
          <wired100MSent>2</wired100MSent>
          <wired100MThroughput>2</wired100MThroughput>
          <wired10GReceived>2</wired10GReceived>
          <wired10GSent>2</wired10GSent>
          <wired10GThroughput>2</wired10GThroughput>
          <wired10MSent>2</wired10MSent>
          <wired10MThroughput>2</wired10MThroughput>
          <wired1GSent>2</wired1GSent>
          <wired1GThroughput>2</wired1GThroughput>
          <dot11aReceived>2</dot11aReceived>
          <dot11bReceived>2</dot11bReceived>
          <dot11gReceived>2</dot11gReceived>
          <dot11n2_4Received>2</dot11n2_4Received>
          <dot11n5Received>2</dot11n5Received>
          <received>2</received>
          <wired100MReceived>2</wired100MReceived>
          <wired10MReceived>2</wired10MReceived>
          <wired1GReceived>2</wired1GReceived>
        </clientTrafficsDTO>
      </entity>
    </queryResponse>

### Sample JSON Payload

https://10.64.88.203/webacs/api/v4/data/ClientTraffics/15.json

    {
      "queryResponse" : {
        "@type" : "ClientTraffics",
        "@requestUrl" : "https://10.64.88.203/webacs/api/v4/data/ClientTraffics/15",
        "@responseType" : "getEntity",
        "@rootUrl" : "https://10.64.88.203/webacs/api/v4/data",
        "entity" : [ {
          "@dtoType" : "clientTrafficsDTO",
          "@type" : "ClientTraffics",
          "@url" : "https://10.64.88.203/webacs/api/v4/data/ClientTraffics/15",
          "clientTrafficsDTO" : {
            "@displayName" : "String value",
            "@id" : 15,
            "@uuid" : "String value",
            "collectionTime" : 2,
            "dot11aReceived" : 2,
            "dot11aSent" : 2,
            "dot11aThroughput" : 2,
            "dot11acReceived" : 2,
            "dot11acSent" : 2,
            "dot11acThroughput" : 2,
            "dot11ax2_4Received" : 2,
            "dot11ax2_4Sent" : 2,
            "dot11ax2_4Throughput" : 2,
            "dot11ax5Received" : 2,
            "dot11ax5Sent" : 2,
            "dot11ax5Throughput" : 2,
            "dot11bReceived" : 2,
            "dot11bSent" : 2,
            "dot11bThroughput" : 2,
            "dot11gReceived" : 2,
            "dot11gSent" : 2,
            "dot11gThroughput" : 2,
            "dot11n2_4Received" : 2,
            "dot11n2_4Sent" : 2,
            "dot11n2_4Throughput" : 2,
            "dot11n5Received" : 2,
            "dot11n5Sent" : 2,
            "dot11n5Throughput" : 2,
            "key" : "String value",
            "received" : 2,
            "sent" : 2,
            "subkey" : "String value",
            "throughput" : 2,
            "type" : "DEVICE",
            "wired100MReceived" : 2,
            "wired100MSent" : 2,
            "wired100MThroughput" : 2,
            "wired10GReceived" : 2,
            "wired10GSent" : 2,
            "wired10GThroughput" : 2,
            "wired10MReceived" : 2,
            "wired10MSent" : 2,
            "wired10MThroughput" : 2,
            "wired1GReceived" : 2,
            "wired1GSent" : 2,
            "wired1GThroughput" : 2
          }
        } ]
      }
    }