Media Routing Peripheral Gateway

The media routing peripheral gateway (MR-PG) is an ICM peripheral gateway that is capable of routing media requests of different kinds, such as e-mail and Web callback. The MR-PG supports multiple media routing clients by accommodating multiple, independent peripheral interface managers (PIMs) on a PG platform. A single MR-PIM is required for each application instance connected to the ICM system. For example, when connecting an E-Mail Manager instance and a Collaboration Server instance, two MR-PIMs are needed on the PG.