> S-GW Node Level Schema Statistics
> This schema provides the following type of statistics:

> • | Counter: A counter records incremental data cumulatively and rolls over when the counter limit is reached. The limit depends upon the counter data type.

> • | Gauge: A gauge statistic indicates a single value representative of a single instance. This type is often used to track particular events in time.

> Important: The format string syntax is described by Schema Format String Syntax in the Bulk Statistics Overview chapter.
> Important: Unless otherwise indicated, all statistics are counters. For statistics with the Int32 data type, the roll-over to zero limit is 4,294,967,295. For statistics with the Int64 data type, the roll-over to zero limit is 18,446,744,073,709,551,615. All statistics are cumulative and reset only by one of the following methods: roll-over (as described above), after a system restart, or after a clear command is performed. All statistics are considered standards-based unless otherwise described.
> The following variables are supported:
> S-GW Node Level Schema Statistics

> Statistic | Description | Data Type
> vpnname | The name of the context configured on the system that is currently facilitating the S-GW service. | String / Static
> vpnid | The identification number of the context configured on the system that is currently facilitating the S-GW service. This is an internal reference number. | Gauge / Int32
> servname | Displays the name of the S-GW service for which the statistics are displayed. | String / Static
> servid | The identification number of the service configured on the system that is currently facilitating the S-GW service. This is an internal reference number. | Gauge / Int32
> sess-cur | The total number of sessions currently established on this system. | Counter / Int32
> sessstat-totcur-ueidle | Session Statistics - Total Current - UE Idle | Counter / Int32
> sessstat-totcur-ueactive | Session Statistics - Total Current - UE Active | Counter / Int32
> sessstat-totcur-pdn | Session Statistics - Total Current - PDN | Counter / Int32
> sessstat-totcur-bearers | Session Statistics - Total Current - Bearers | Counter / Int32
> sessstat-totsetup-ue | Session Statistics - Total Setup - UE | Counter / Int32
> sessstat-totsetup-pdn | Session Statistics - Total Setup - PDN | Counter / Int32
> sessstat-totsetup-bearers | Session Statistics - Total Setup - Bearers | Counter / Int32
> sessstat-pdnsetuptype-ipv4 | Session Statistics - Total PDNs Setup Per PDN-type - IPv4 | Counter / Int32
> sessstat-pdnsetuptype-ipv6 | Session Statistics - Total PDNs Setup Per PDN-type - IPv6 | Counter / Int32
> sessstat-pdnsetuptype-ipv4v6 | Session Statistics - Total PDNs Setup Per PDN-type - IPv4v6 | Counter / Int32
> sessstat-pdnsetupintrface-s11 | Session Statistics - Total PDNs Setup Per Interface - S11 | Counter / Int32
> sessstat-pdnsetupintrface-s4 | Session Statistics - Total PDNs Setup Per Interface - S4 | Counter / Int32
> sessstat-pdnsetups5proto-gtp | Session Statistics - Total PDNs Setup Per S5 Proto - GTP | Counter / Int32
> sessstat-pdnsetups5proto-pmip | Session Statistics - Total PDNs Setup Per S5 Proto - PMIP | Counter / Int32
> sessstat-pdnrel-ipv4 | Session Statistics - Total PDNs Released - IPv4 | Counter / Int32
> sessstat-pdnrel-ipv6 | Session Statistics - Total PDNs Released - IPv6 | Counter / Int32
> sessstat-pdnrel-ipv4v6 | Session Statistics - Total PDNs Released - IPv4v6 | Counter / Int32
> sessstat-pdnrelrsn-mme | Session Statistics - Total PDNs Released reason - MME Initiated | Counter / Int32
> sessstat-pdnrelrsn-pgw | Session Statistics - Total PDNs Released reason - PGW Initiated | Counter / Int32
> sessstat-pdnrelrsn-pcrf | Session Statistics - Total PDNs Released reason - PCRF Initiated | Counter / Int32
> sessstat-pdnrelrsn-local | Session Statistics - Total PDNs Released reason - Local | Counter / Int32
> sessstat-pdnrelrsn-s1err | Session Statistics - Total PDNs Released reason - S1 Error Ind | Counter / Int32
> sessstat-pdnrelrsn-s5err | Session Statistics - Total PDNs Released reason - S5 Error Ind | Counter / Int32
> sessstat-pdnrelrsn-pathfail-S11 | Session Statistics - Total PDNs Released reason - S11 Path Failure | Counter / Int32
> sessstat-pdnrelrsn-pathfail-S5 | Session Statistics - Total PDNs Released reason - S5 Path Failure | Counter / Int32
> sessstat-pdnrelrsn-pathfail-S5-u | Session Statistics - Total PDNs Released reason - Path Failure S5-U | Counter / Int32
> sessstat-pdnrelrsn-pathfail-S1-u | Session Statistics - Total PDNs Released reason - Path Failure S1-U | Counter / Int32
> sessstat-pdnrelrsn-other | Session Statistics - Total PDNs Released reason - Other | Counter / Int32
> sessstat-pdnrej-ipv4 | Session Statistics - Total PDNs Rejected - IPv4 | Counter / Int32
> sessstat-pdnrej-ipv6 | Session Statistics - Total PDNs Rejected - IPv6 | Counter / Int32
> sessstat-pdnrej-ipv4v6 | Session Statistics - Total PDNs Rejected - IPv4v6 | Counter / Int32
> sessstat-pdnrejrsn-pgw | Session Statistics - Total PDNs Rejected Reason - PGW Reject | Counter / Int32
> sessstat-pdnrejrsn-license | Session Statistics - Total PDNs Rejected Reason - License | Counter / Int32
> sessstat-pdnrejrsn-newcall-policy | Session Statistics - Total PDNs Rejected Reason - Newcall Policy | Counter / Int32
> sessstat-pdnrejrsn-overload | Session Statistics - Total PDNs Rejected Reason - Overload | Counter / Int32
> sessstat-pdnrejrsn-cong | Session Statistics - Total PDNs Rejected Reason - Congestion | Counter / Int32
> sessstat-pdnrejrsn-other | Session Statistics - Total PDNs Rejected Reason - Other | Counter / Int32
> totepsbearsetup-qci1 | Total EPS Bearers Setup - QCI 1 | Counter / Int32
> totepsbearsetup-qci2 | Total EPS Bearers Setup - QCI 2 | Counter / Int32
> totepsbearsetup-qci3 | Total EPS Bearers Setup - QCI 3 | Counter / Int32
> totepsbearsetup-qci4 | Total EPS Bearers Setup - QCI 4 | Counter / Int32
> totepsbearsetup-qci5 | Total EPS Bearers Setup - QCI 5 | Counter / Int32
> totepsbearsetup-qci6 | Total EPS Bearers Setup - QCI 6 | Counter / Int32
> totepsbearsetup-qci7 | Total EPS Bearers Setup - QCI 7 | Counter / Int32
> totepsbearsetup-qci8 | Total EPS Bearers Setup - QCI 8 | Counter / Int32
> totepsbearsetup-qci9 | Total EPS Bearers Setup - QCI 9 | Counter / Int32
> totepsbearsetup-other | Total EPS Bearers Setup - Other | Counter / Int32
> totepsbearmod | Total EPS Bearers Modified | Counter / Int32
> totepsbearrel-qci1 | Total EPS Bearers Released - QCI 1 | Counter / Int32
> totepsbearrel-qci2 | Total EPS Bearers Released - QCI 2 | Counter / Int32
> totepsbearrel-qci3 | Total EPS Bearers Released - QCI 3 | Counter / Int32
> totepsbearrel-qci4 | Total EPS Bearers Released - QCI 4 | Counter / Int32
> totepsbearrel-qci5 | Total EPS Bearers Released - QCI 5 | Counter / Int32
> totepsbearrel-qci6 | Total EPS Bearers Released - QCI 6 | Counter / Int32
> totepsbearrel-qci7 | Total EPS Bearers Released - QCI 7 | Counter / Int32
> totepsbearrel-qci8 | Total EPS Bearers Released - QCI 8 | Counter / Int32
> totepsbearrel-qci9 | Total EPS Bearers Released - QCI 9 | Counter / Int32
> totepsbearrel-other | Total EPS Bearers Released - Other | Counter / Int32
> totepsbearmod-qci1 | Total EPS Bearers Modified - QCI 1 | Counter / Int32
> totepsbearmod-qci2 | Total EPS Bearers Modified - QCI 2 | Counter / Int32
> totepsbearmod-qci3 | Total EPS Bearers Modified - QCI 3 | Counter / Int32
> totepsbearmod-qci4 | Total EPS Bearers Modified - QCI 4 | Counter / Int32
> totepsbearmod-qci5 | Total EPS Bearers Modified - QCI 5 | Counter / Int32
> totepsbearmod-qci6 | Total EPS Bearers Modified - QCI 6 | Counter / Int32
> totepsbearmod-qci7 | Total EPS Bearers Modified - QCI 7 | Counter / Int32
> totepsbearmod-qci8 | Total EPS Bearers Modified - QCI 8 | Counter / Int32
> totepsbearmod-qci9 | Total EPS Bearers Modified - QCI 9 | Counter / Int32
> totepsbearmod-other | Total EPS Bearers Modified - Other | Counter / Int32
> totepsbearrel-dedrsn-pgw | Total EPS Bearers Released - Dedicated Bearers Released Reason - PGW Ini | Counter / Int32
> totepsbearrel-dedrsn-pcrf | Total EPS Bearers Released - Dedicated Bearers Released Reason - PCRF Ini | Counter / Int32
> totepsbearrel-dedrsn-s1err | Total EPS Bearers Released - Dedicated Bearers Released Reason - S1 Error Ind | Counter / Int32
> totepsbearrel-dedrsn-s5err | Total EPS Bearers Released - Dedicated Bearers Released Reason - S5 Error Ind | Counter / Int32
> totepsbearrel-dedrsn-local | Total EPS Bearers Released - Dedicated Bearers Released Reason - Local | Counter / Int32
> totepsbearrel-dedrsn-pdn | Total EPS Bearers Released - Dedicated Bearers Released Reason - PDN Down | Counter / Int32
> totepsbearrel-dedrsn-pathfail-s1-u | Total EPS Bearers Released - Total Dedicated Bearers Released Reason - Path Failure S1-U | Counter / Int32
> totepsbearrel-dedrsn-pathfail-s5-u | Total EPS Bearers Released - Total Dedicated Bearers Released Reason - Path Failure S5-U | Counter / Int32
> totepsbearrel-dedrsn-other | Total EPS Bearers Released - Dedicated Bearers Released Reason - Other | Counter / Int32
> datastat-uplink-qci1totbyte | Data Statistics - Uplink Stats - QCI 1 Total-Bytes | Counter / Int32
> datastat-uplink-qci1totpkt | Data Statistics - Uplink Stats - QCI 1 Total-Packets | Counter / Int32
> datastat-uplink-qci2totbyte | Data Statistics - Uplink Stats - QCI 2 Total-Bytes | Counter / Int32
> datastat-uplink-qci2totpkt | Data Statistics - Uplink Stats - QCI 2 Total-Packets | Counter / Int32
> datastat-uplink-qci3totbyte | Data Statistics - Uplink Stats - QCI 3 Total-Bytes | Counter / Int32
> datastat-uplink-qci3totpkt | Data Statistics - Uplink Stats - QCI 3 Total-Packets | Counter / Int32
> datastat-uplink-qci4totbyte | Data Statistics - Uplink Stats - QCI 4 Total-Bytes | Counter / Int32
> datastat-uplink-qci4totpkt | Data Statistics - Uplink Stats - QCI 4 Total-Packets | Counter / Int32
> datastat-uplink-qci5totbyte | Data Statistics - Uplink Stats - QCI 5 Total-Bytes | Counter / Int32
> datastat-uplink-qci5totpkt | Data Statistics - Uplink Stats - QCI 5 Total-Packets | Counter / Int32
> datastat-uplink-qci6totbyte | Data Statistics - Uplink Stats - QCI 6 Total-Bytes | Counter / Int32
> datastat-uplink-qci6totpkt | Data Statistics - Uplink Stats - QCI 6 Total-Packets | Counter / Int32
> datastat-uplink-qci7totbyte | Data Statistics - Uplink Stats - QCI 7 Total-Bytes | Counter / Int32
> datastat-uplink-qci7totpkt | Data Statistics - Uplink Stats - QCI 7 Total-Packets | Counter / Int32
> datastat-uplink-qci8totbyte | Data Statistics - Uplink Stats - QCI 8 Total-Bytes | Counter / Int32
> datastat-uplink-qci8totpkt | Data Statistics - Uplink Stats - QCI 8 Total-Packets | Counter / Int32
> datastat-uplink-qci9totbyte | Data Statistics - Uplink Stats - QCI 9 Total-Bytes | Counter / Int32
> datastat-uplink-qci9totpkt | Data Statistics - Uplink Stats - QCI 9 Total-Packets | Counter / Int32
> datastat-uplink-othertotbyte | Data Statistics - Uplink Stats - Other Total-Bytes | Counter / Int32
> datastat-uplink-othertotpkt | Data Statistics - Uplink Stats - Other Total-Packets | Counter / Int32
> datastat-uplink-dropstat-qci1totbyte | Data Statistics - Uplink Bytes Dropped - QCI 1 Total-Bytes | Counter / Int32
> datastat-uplink-dropstat-qci1totpkt | Data Statistics - Uplink Packets Dropped - QCI 1 Total-Packets | Counter / Int32
> datastat-uplink-dropstat-qci2totbyte | Data Statistics - Uplink Bytes Dropped - QCI 2 Total-Bytes | Counter / Int32
> datastat-uplink-dropstat-qci2totpkt | Data Statistics - Uplink Packets Dropped - QCI 2 Total-Packets | Counter / Int32
> datastat-uplink-dropstat-qci3totbyte | Data Statistics - Uplink Bytes Dropped - QCI 3 Total-Bytes | Counter / Int32
> datastat-uplink-dropstat-qci3totpkt | Data Statistics - Uplink Packets Dropped - QCI 3 Total-Packets | Counter / Int32
> datastat-uplink-dropstat-qci4totbyte | Data Statistics - Uplink Bytes Dropped - QCI 4 Total-Bytes | Counter / Int32
> datastat-uplink-dropstat-qci4totpkt | Data Statistics - Uplink Packets Dropped - QCI 4 Total-Packets | Counter / Int32
> datastat-uplink-dropstat-qci5totbyte | Data Statistics - Uplink Bytes Dropped - QCI 5 Total-Bytes | Counter / Int32
> datastat-uplink-dropstat-qci5totpkt | Data Statistics - Uplink Packets Dropped - QCI 5 Total-Packets | Counter / Int32
> datastat-uplink-dropstat-qci6totbyte | Data Statistics - Uplink Bytes Dropped - QCI 6 Total-Bytes | Counter / Int32
> datastat-uplink-dropstat-qci6totpkt | Data Statistics - Uplink Packets Dropped - QCI 6 Total-Packets | Counter / Int32
> datastat-uplink-dropstat- qci7totbyte | Data Statistics - Uplink Bytes Dropped - QCI 7 Total-Bytes | Counter / Int32
> datastat-uplink-dropstat-qci7totpkt | Data Statistics - Uplink Packets Dropped - QCI 7 Total-Packets | Counter / Int32
> datastat-uplink-dropstat-qci8totbyte | Data Statistics - Uplink Bytes Dropped - QCI 8 Total-Bytes | Counter / Int32
> datastat-uplink-dropstat-qci8totpkt | Data Statistics - Uplink Packets Dropped - QCI 8 Total-Packets | Counter / Int32
> datastat-uplink-dropstat-qci9totbyte | Data Statistics - Uplink Bytes Dropped - QCI 9 Total-Bytes | Counter / Int32
> datastat-uplink-dropstat-qci9totpkt | Data Statistics - Uplink Packets Dropped - QCI 9 Total-Packets | Counter / Int32
> datastat-uplink-dropstat-othertotbyte | Data Statistics - Uplink Bytes Dropped - Other Total-Bytes | Counter / Int32
> datastat-uplink-dropstat-othertotpkt | Data Statistics - Uplink Packets Dropped - Other Total-Packets | Counter / Int32
> datastat-downlink-qci1totbyte | Data Statistics - Downlink Stats - QCI 1 Total-Bytes | Counter / Int32
> datastat-downlink-qci1totpkt | Data Statistics - Downlink Stats - QCI 1 Total-Packets | Counter / Int32
> datastat-downlink-qci2totbyte | Data Statistics - Downlink Stats - QCI 2 Total-Bytes | Counter / Int32
> datastat-downlink-qci2totpkt | Data Statistics - Downlink Stats - QCI 2 Total-Packets | Counter / Int32
> datastat-downlink-qci3totbyte | Data Statistics - Downlink Stats - QCI 3 Total-Bytes | Counter / Int32
> datastat-downlink-qci3totpkt | Data Statistics - Downlink Stats - QCI 3 Total-Packets | Counter / Int32
> datastat-downlink-qci4totbyte | Data Statistics - Downlink Stats - QCI 4 Total-Bytes | Counter / Int32
> datastat-downlink-qci4totpkt | Data Statistics - Downlink Stats - QCI 4 Total-Packets | Counter / Int32
> datastat-downlink-qci5totbyte | Data Statistics - Downlink Stats - QCI 5 Total-Bytes | Counter / Int32
> datastat-downlink-qci5totpkt | Data Statistics - Downlink Stats - QCI 5 Total-Packets | Counter / Int32
> datastat-downlink-qci6totbyte | Data Statistics - Downlink Stats - QCI 6 Total-Bytes | Counter / Int32
> datastat-downlink-qci6totpkt | Data Statistics - Downlink Stats - QCI 6 Total-Packets | Counter / Int32
> datastat-downlink-qci7totbyte | Data Statistics - Downlink Stats - QCI 7 Total-Bytes | Counter / Int32
> datastat-downlink-qci7totpkt | Data Statistics - Downlink Stats - QCI 7 Total-Packets | Counter / Int32
> datastat-downlink-qci8totbyte | Data Statistics - Downlink Stats - QCI 8 Total-Bytes | Counter / Int32
> datastat-downlink-qci8totpkt | Data Statistics - Downlink Stats - QCI 8 Total-Packets | Counter / Int32
> datastat-downlink-qci9totbyte | Data Statistics - Downlink Stats - QCI 9 Total-Bytes | Counter / Int32
> datastat-downlink-qci9totpkt | Data Statistics - Downlink Stats - QCI 9 Total-Packets | Counter / Int32
> datastat-downlink-othertotbyte | Data Statistics - Downlink Stats - Other Total-Bytes | Counter / Int32
> datastat-downlink-othertotpkt | Data Statistics - Downlink Stats - Other Total-Packets | Counter / Int32
> datastat-downlink-dropstat-qci1totbyte | Data Statistics - Downlink Bytes Dropped - QCI 1 Total-Bytes | Counter / Int32
> datastat-downlink-dropstat-qci1totpkt | Data Statistics - Downlink Packets Dropped - QCI 1 Total-Packets | Counter / Int32
> datastat-downlink-dropstat-qci2totbyte | Data Statistics - Downlink Bytes Dropped - QCI 2 Total-Bytes | Counter / Int32
> datastat-downlink-dropstat-qci2totpkt | Data Statistics - Downlink Packets Dropped - QCI 2 Total-Packets | Counter / Int32
> datastat-downlink-dropstat-qci3totbyte | Data Statistics - Downlink Bytes Dropped - QCI 3 Total-Bytes | Counter / Int32
> datastat-downlink-dropstat-qci3totpkt | Data Statistics - Downlink Packets Dropped - QCI 3 Total-Packets | Counter / Int32
> datastat-downlink-dropstat-qci4totbyte | Data Statistics - Downlink Bytes Dropped - QCI 4 Total-Bytes | Counter / Int32
> datastat-downlink-dropstat-qci4totpkt | Data Statistics - Downlink Packets Dropped - QCI 4 Total-Packets | Counter / Int32
> datastat-downlink-dropstat-qci5totbyte | Data Statistics - Downlink Bytes Dropped - QCI 5 Total-Bytes | Counter / Int32
> datastat-downlink-dropstat-qci5totpkt | Data Statistics - Downlink Packets Dropped - QCI 5 Total-Packets | Counter / Int32
> datastat-downlink-dropstat-qci6totbyte | Data Statistics - Downlink Bytes Dropped - QCI 6 Total-Bytes | Counter / Int32
> datastat-downlink-dropstat-qci6totpkt | Data Statistics - Downlink Packets Dropped - QCI 6 Total-Packets | Counter / Int32
> datastat-downlink-dropstat-qci7totbyte | Data Statistics - Downlink Bytes Dropped - QCI 7 Total-Bytes | Counter / Int32
> datastat-downlink-dropstat-qci7totpkt | Data Statistics - Downlink Packets Dropped - QCI 7 Total-Packets | Counter / Int32
> datastat-downlink-dropstat-qci8totbyte | Data Statistics - Downlink Bytes Dropped - QCI 8 Total-Bytes | Counter / Int32
> datastat-downlink-dropstat-qci8totpkt | Data Statistics - Downlink Packets Dropped - QCI 8 Total-Packets | Counter / Int32
> datastat-downlink-dropstat-qci9totbyte | Data Statistics - Downlink Bytes Dropped - QCI 9 Total-Bytes | Counter / Int32
> datastat-downlink-dropstat-qci9totpkt | Data Statistics - Downlink Packets Dropped - QCI 9 Total-Packets | Counter / Int32
> datastat-downlink-dropstat-othertotbyte | Data Statistics - Downlink Bytes Dropped - Other Total-Bytes | Counter / Int32
> datastat-downlink-dropstat-othertotpkt | Data Statistics - Downlink Packets Dropped - Other Total-Packets | Counter / Int32
> interhaovstat-pdnin-x2 | Inter-SGW Handover Statistics - Total PDNs Incoming - X2 based | Counter / Int32
> interhaovstat-pdnin-idletau | Inter-SGW Handover Statistics - Total PDNs Incoming - Idle-mode TAU | Counter / Int32
> interhaovstat-pdnin-s1 | Inter-SGW Handover Statistics - Total PDNs Incoming - S1 Based | Counter / Int32
> interhaovstat-pdnout | Inter-SGW Handover Statistics - Total PDNs Outgoing | Counter / Int32
> interhaovstat-intra-intramme | Intra-SGW Handover Stats - Intra-MME | Counter / Int32
> interhaovstat-intra-intermme | Intra-SGW Handover Stats - Inter-MME | Counter / Int32
> pagingstat-req | Paging Statistics - Requests | Counter / Int32
> pagingstat-rej | Paging Statistics - Rejects | Counter / Int32
> pagingstat-fail | Paging Statistics - Failures | Counter / Int32
> pagingstat-actidleuetrans | Paging Statistics - Active-Idle UE Transitions | Counter / Int32
> pagingstat-idleactuetrans | Paging Statistics - Idle-Active UE Transitions | Counter / Int32
> pagingreldatastat-totbytebuff | Paging Related Data Statistics - Total Bytes Buffered | Counter / Int32
> pagingreldatastat-disc | Paging Related Data Statistics - Discarded | Counter / Int32
> misc-updatabeformbreq | Miscellaneous - Uplink Data Before MBreq | Counter / Int32
> misc-cbreqrcvbeforcsrsp | Miscellaneous - CBReq Rcvd Before CSRsp | Counter / Int32
> indftstat-totcur-tunnels | Indirecect forward tunneling: The total number of current tunnels. | Counter / Int32
> indftstat-totcur-bearers | Indirect forward tunneling: The total number of current bearers. | Counter / Int32
> indftstat-totsetup-tunnels | Indirect forward tunneling: The total number of tunnels set up. | Counter / Int32
> indftstat-totsetup-bearers | Indirect forward tunneling: The total number of bearers set up. | Counter / Int32
> indftstat-totrel-tunnels | Indirect forward tunneling: The total number of released tunnels. | Counter / Int32
> indftstat-totrel-bearers | Indirect forward tunneling: The total number of released bearers. | Counter / Int32
> indftstat-totfail-tunnels | Indirect forward tunneling: The total number of failed tunnel set ups. | Counter / Int32
> indftstat-data-fwd-pkts | Indirect forward tunneling: The total number of forwarded packets. | Counter / Int32
> indftstat-data-fwd-bytes | Indirect forward tunneling: The total number of forwarded bytes. | Counter / Int32
> Important: See Bulk Statistics Overview for statistics that are common to all schema.

> ‌

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883