> P-GW Node Level Schema Statistics
> This schema provides the following type of statistics:

> • | Counter: A counter records incremental data cumulatively and rolls over when the counter limit is reached. The limit depends upon the counter data type.

> • | Gauge: A gauge statistic indicates a single value representative of a single instance. This type is often used to track particular events in time.

> Important: The format string syntax is described by Schema Format String Syntax in the Bulk Statistics Overview chapter.
> Important: Unless otherwise indicated, all statistics are counters. For statistics with the Int32 data type, the roll-over to zero limit is 4,294,967,295. For statistics with the Int64 data type, the roll-over to zero limit is 18,446,744,073,709,551,615. All statistics are cumulative and reset only by one of the following methods: roll-over (as described above), after a system restart, or after a clear command is performed. All statistics are considered standards-based unless otherwise described.
> The following variables are supported:
> P-GW Service Schema Statistics

> Statistic | Description | Data Type
> vpnname | The name of the context configured on the system that is currently facilitating the P-GW service. | String / Static
> vpnid | The identification number of the context configured on the system that is currently facilitating the P-GW service. This is an internal reference number. | Gauge / Int32
> servname | Displays the name of the P-GW service for which the statistics are displayed. | String / Static
> servid | The identification number of the service configured on the system that is currently facilitating the P-GW service. This is an internal reference number. | Gauge / Int32
> sess-cur | The total number of sessions currently established on this system. | Counter / Int32
> sessstat-bearact-def | Session Statistics - Total default bearers active | Counter / Int32
> sessstat-bearact-ded | Session Statistics - Total dedicated bearers active | Counter / Int32
> sessstat-bearact-ue-init-ded | Session Statistics - Total bearers active - UE-initiated | Counter / Int32
> sessstat-bearact-nw-init-ded | Session Statistics - Total bearers active - Network-initiated | Counter / Int32
> sessstat-bearact-nw-init-ded-att | Session Statistics - Total bearers active - Network-initiated dedicated bearers | Counter / Int32
> sessstat-bearsetup-def | Session Statistics - Total default bearers setup | Counter / Int32
> sessstat-bearsetup-ded | Session Statistics - Total dedicated bearers setup | Counter / Int32
> sessstat-bearsetup-ue-init-ded | Session Statistics - Total bearers rejected - Network-req reject - No Resource | Counter / Int32
> sessstat-bearsetup-nw-init-ded | Session Statistics - Total bearers setup - Dedicated bearers - Network-initiated | Counter / Int32
> sessstat-bearrel-def | Session Statistics - Total default bearers released | Counter / Int32
> sessstat-bearrel-ded | Session Statistics - Total dedicated bearers released | Counter / Int32
> sessstat-bearrel-nwdefadmin | Session Statistics - Total bearers released - Network Default Admin disconnect | Counter / Int32
> sessstat-bearrel-nwdefgtp | Session Statistics - Total bearers released - Network Default GTP-U error ind | Counter / Int32
> sessstat-bearrel-nwdefsgw | Session Statistics - Total bearers released - Network Default SGW Path failure | Counter / Int32
> sessstat-bearrel-nwdefmme | Session Statistics - Total bearers released - Network Default MME initiated release | Counter / Int32
> sessstat-bearrel-nwdedadmin | Session Statistics - Total bearers released - Network Dedicated Admin disconnect | Counter / Int32
> sessstat-bearrel-nwdedgtp | Session Statistics - Total bearers released - Network Dedicated GTP-U error ind | Counter / Int32
> sessstat-bearrel-nwdedmme | Session Statistics - Total bearers released - Network Dedicated MME initiated release | Counter / Int32
> sessstat-bearrel-nwdeddefbear | Session Statistics - Total bearers released - Network Dedicated Default bearer release | Counter / Int32
> sessstat-bearrel-nwdedgxdisc | Session Statistics - Total bearers released - Network Dedicated GX Disconnect | Counter / Int32
> sessstat-bearrelfail-def | Session Statistics - Total bearers release failure - Default bearers | Counter / Int32
> sessstat-bearrelfail-ded | Session Statistics - Total bearers release failure - Dedicated bearers | Counter / Int32
> sessstat-bearrej-def | Session Statistics - Total bearers rejected - Default bearers | Counter / Int32
> sessstat-bearrej-ded | Session Statistics - Total bearers rejected - Dedicated bearers | Counter / Int32
> sessstat-bearrej-nores | Session Statistics - Total bearers rejected - No Resource | Counter / Int32
> sessstat-bearrej-uereq | Session Statistics - Total bearers rejected - UE-req reject | Counter / Int32
> sessstat-bearrej-uereq-nores | Session Statistics - Total bearers rejected - UE-req reject - No Resource | Counter / Int32
> sessstat-bearrej-misapn | Session Statistics - Total bearers rejected - Missing or unknown APN | Counter / Int32
> sessstat-bearrej-nwreq | Session Statistics - Total bearers rejected - Network-req reject | Counter / Int32
> sessstat-bearrej-nwreq-nores | Session Statistics - Total bearers rejected - Network-req reject - No Resource | Counter / Int32
> sessstat-bearrej-nwreq-nomem | Session Statistics - Total bearers rejected - Network-req reject - No memory available | Counter / Int32
> sessstat-bearrej-nwreq-sysfail | Session Statistics - Total bearers rejected - Network-req reject - System failure | Counter / Int32
> sessstat-bearrej-apnmode | Session Statistics - Total bearers rejected - APN selection -Mode mismatch | Counter / Int32
> sessstat-bearrej-pdn | Session Statistics - Total bearers rejected - Pref PDN -Type not supported | Counter / Int32
> sessstat-bearrej-apnrestr | Session Statistics - Total bearers rejected - APN restr violation | Counter / Int32
> sessstat-bearrej-subsauth | Session Statistics - Total bearers rejected - Subs auth failed | Counter / Int32
> sessstat-bearrej-subsaddrnotallow | Session Statistics - Total bearers rejected - Subscriber’s static address not allowed | Counter / Int32
> sessstat-bearrej-subsaddrnotalloc | Session Statistics - Total bearers rejected - Subscriber’s static address not allocated | Counter / Int32
> sessstat-bearrej-dynaddrnotalloc | Session Statistics - Total bearers rejected - Dynamic address not allocated | Counter / Int32
> sessstat-bearrej-subsaddrnotpres | Session Statistics - Total bearers rejected - Subscriber’s static address not present | Counter / Int32
> sessstat-bearmod-ueinit | Session Statistics - Total bearers modified - UE-initiated modification | Counter / Int32
> sessstat-bearmod-nwinit | Session Statistics - Total bearers modified - Network-initiated modification | Counter / Int32
> sessstat-bearmod-ueqos | Session Statistics - Total bearers modified - UE-initiated QoS modification | Counter / Int32
> sessstat-bearmod-uetft | Session Statistics - Total bearers modified - UE-initiated TFT modification | Counter / Int32
> sessstat-bearmod-nwqos | Session Statistics - Total bearers modified - Network-initiated QoS modification | Counter / Int32
> sessstat-bearmod-nwtft | Session Statistics - Total bearers modified - Network-initiated TFT modification | Counter / Int32
> sessstat-bearmodfail-ueinit | Session Statistics - Total bearers modification failure - UE-initiated modification failed | Counter / Int32
> sessstat-bearmodfail-nwinit | Session Statistics - Total bearers modification failure - Network-initiated modification failed | Counter / Int32
> sessstat-bearmodfail-uenores | Session Statistics - Total bearers modification failure - UE-initiated No res available | Counter / Int32
> sessstat-bearmodfail-uesemtft | Session Statistics - Total bearers modification failure - UE-initiated Semantic error in TFT oper | Counter / Int32
> sessstat-bearmodfail-uesyntft | Session Statistics - Total bearers modification failure - UE-initiated Syntax error in TFT oper | Counter / Int32
> sessstat-bearmodfail-uesempkt | Session Statistics - Total bearers modification failure - UE-initiated Semantic error in packet filter | Counter / Int32
> sessstat-bearmodfail-uesynpkt | Session Statistics - Total bearers modification failure - UE-initiated syntaxt error in packet filter | Counter / Int32
> sessstat-bearmodfail-nwnores | Session Statistics - Total bearers modification failure - Network-initiated - No res available | Counter / Int32
> sessstat-bearmodfail-nwnomem | Session Statistics - Total bearers modification failure - Network-initiated - No memory available | Counter / Int32
> sessstat-bearmodfail-nwsysfail | Session Statistics - Total bearers modification failure - Network-initiated - System failure | Counter / Int32
> sessstat-bearmodfail-nwsemtft | Session Statistics - Total bearers modification failure - Network-initiated Semantic error in TFT oper | Counter / Int32
> sessstat-bearmodfail-nwsyntft | Session Statistics - Total bearers modification failure - Network-initiated syntax error in TFT oper | Counter / Int32
> sessstat-bearmodfail-nwsempkt | Session Statistics - Total bearers modification failure - Network-initiated Semantic error in packet filter | Counter / Int32
> sessstat-bearmodfail-nwsynpkt | Session Statistics - Total bearers modification failure - Network-initiated syntax error in packet filter | Counter / Int32
> sessstat-bearmodfail-qos-uenores | Session Statistics - Total bearer modification failures - User equipment quality of service no response errors | Counter / Int32
> sessstat-bearmodfail-qos-uesemtft | Session Statistics - Total bearer modification failures - User equipment quality of service TFT semantics errors | Counter / Int32
> sessstat-bearmodfail-qos-uesyntft | Session Statistics - Total bearer modification failures - User equipment quality of service TFT syntax errors | Counter / Int32
> sessstat-bearmodfail-qos-uesempkt | Session Statistics - Total bearer modification failures - User equipment quality of service packet semantics errors | Counter / Int32
> sessstat-bearmodfail-qos-uesynpkt | Session Statistics - Total bearer modification failures - User equipment quality of service packet syntax errors | Counter / Int32
> sessstat-bearmodfail-qos-nwnores | Session Statistics - Total bearer modification failures - Network-initiated quality of service no response | Counter / Int32
> sessstat-bearmodfail-qos-nwnomem | Session Statistics - Total bearer modification failures - Network-initiated quality of service no memory | Counter / Int32
> sessstat-bearmodfail-qos-nwsysfail | Session Statistics - Total bearer modification failures - Network-initiated quality of service system failures | Counter / Int32
> sessstat-bearmodfail-qos-nwsemtft | Session Statistics - Total becarer modification failures - Network-initiated quality of service semantics of TFT | Counter / Int32
> sessstat-bearmodfail-qos-nwsyntft | Session Statistics - Total modified bearer failures - Network-initiated TFT syntax | Counter / Int32
> sessstat-bearmodfail-qos-nwsempkt | Session Statistics - Total modified bearer failures - Network quality of service semantics packets | Counter / Int32
> sessstat-bearmodfail-qos-nwsynpkt | Session Statistics - Total modified bearer failures - Network quality of service syntax of packets | Counter / Int32
> sessstat-beardel-ded | Session Statistics - Total deleted dedicated bearers | Counter / Int32
> sessstat-nw-init-qos-update-att | Session Statistics - Session Statistics - Total network initiated quality of service updates attempted | Counter / Int32
> sessstat-nw-init-bearer-fail-cause | Session Statistics - Total bearers modification failure - Network-initiated Syntax error in packet filter | Counter / Int32
> sessstat-pdn-ipv4active | Session Statistics - Total PDN-Type stats - IPv4 Active | Counter / Int32
> sessstat-pdn-ipv4setup | Session Statistics - Total PDN-Type stats - IPv4 Setup | Counter / Int32
> sessstat-pdn-ipv4rel | Session Statistics - Total PDN-Type stats - IPv4 Released | Counter / Int32
> sessstat-pdn-ipv6active | Session Statistics - Total PDN-Type stats - IPv6 Active | Counter / Int32
> sessstat-pdn-ipv6setup | Session Statistics - Total PDN-Type stats - IPv6 Setup | Counter / Int32
> sessstat-pdn-ipv6rel | Session Statistics - Total PDN-Type stats - IPv6 Released | Counter / Int32
> sessstat-pdn-ipv4v6active | Session Statistics - Total PDN-Type stats - IPv4v6 Active | Counter / Int32
> sessstat-pdn-ipv4v6setup | Session Statistics - Total PDN-Type stats - IPv4v6 Setup | Counter / Int32
> sessstat-pdn-ipv4v6rel | Session Statistics - Total PDN-Type stats - IPv4v6 Released | Counter / Int32
> sessstat-ipv4addaloc | Session Statistics - IPv4 address allocation | Counter / Int32
> sessstat-ipaddaloc-ipv4loacalpool | Session Statistics - IP address allocation stats - IPv4 Local pool address assign | Counter / Int32
> sessstat-ipaddaloc-ipv4staticaddr | Session Statistics - IP address allocation stats - IPv4 Static address assign | Counter / Int32
> sessstat-ipaddaloc-ipv4radaddr | Session Statistics - IP address allocation stats - IPv4 Radius provided address assign | Counter / Int32
> sessstat-ipv6addaloc | Session Statistics - IPv6 address allocation | Counter / Int32
> sessstat-ipaddaloc-ipv6auto | Session Statistics - IP address allocation stats - IPv6 Stateless auto config | Counter / Int32
> subplmnstat-homesubact | Subscriber PLMN Statistics - Home subscribers sessions active | Counter / Int32
> subplmnstat-homesubsetup | Subscriber PLMN Statistics - Home subscribers sessions setup | Counter / Int32
> subplmnstat-homesubrel | Subscriber PLMN Statistics - Home subscribers sessions released | Counter / Int32
> subplmnstat-roamsubact | Subscriber PLMN Statistics - Roaming subscribers sessions active | Counter / Int32
> subplmnstat-roamsubsetup | Subscriber PLMN Statistics - Roaming subscribers sessions setup | Counter / Int32
> subplmnstat-roamsubrel | Subscriber PLMN Statistics - Roaming subscribers sessions released | Counter / Int32
> subplmnstat-visitsubact | Subscriber PLMN Statistics - Visiting subscribers sessions active | Counter / Int32
> subplmnstat-visitsubsetup | Subscriber PLMN Statistics - Visiting subscribers sessions setup | Counter / Int32
> subplmnstat-visitsubrel | Subscriber PLMN Statistics - Visiting subscribers sessions released | Counter / Int32
> sgitunstat-ipv4sessact | SGi tunneling Statistics - IPv4 IP-in-IP tunnel sessions active | Counter / Int32
> sgitunstat-ipv4sesssetup | SGi tunneling Statistics - IPv4 IP-in-IP tunnel sessions setup | Counter / Int32
> sgitunstat-ipv4sessrel | SGi tunneling Statistics - IPv4 IP-in-IP tunnel sessions released | Counter / Int32
> sgitunstat-ipv4gresessact | SGi tunneling Statistics - IPv4 GRE tunnel sessions active | Counter / Int32
> sgitunstat-ipv4gresesssetup | SGi tunneling Statistics - IPv4 GRE tunnel sessions setup | Counter / Int32
> sgitunstat-ipv4gresessrel | SGi tunneling Statistics - IPv4 GRE tunnel sessions released | Counter / Int32
> sgitunstat-ipv6sessact | SGi tunneling Statistics - IPv6 6to4 tunnel sessions active | Counter / Int32
> sgitunstat-ipv6sesssetup | SGi tunneling Statistics - IPv6 6to4 tunnel sessions setup | Counter / Int32
> handoverstat-ersgsnatt | Handover Statistics - Total number of inter-SGSN handover attempts | Counter / Int32
> handoverstat-ersgsnsucc | Handover Statistics - Total number of successful inter-SGSN handovers | Counter / Int32
> handoverstat-ersgsnfail | Total number of failed inter-SGSN handovers | Counter / Int32
> handoverstat-ersgwatt | Total number of inter-SGW handover attempts | Counter / Int32
> handoverstat-ersgwsucc | Total number of successful inter-SGW handovers | Counter / Int32
> handoverstat-ersgwfail | Total number of failed inter-SGW handovers | Counter / Int32
> handoverstat-erhsgwsucc | Handover Statistics - Total number of successful inter-HSGW handovers | Counter / Int32
> handoverstat-erhsgwsucc | Total number of successful inter-HSGW handovers | Counter / Int32
> handoverstat-erhsgwfail | Handover Statistics - Total number of failed inter-HSGW handovers | Counter / Int32
> handoverstat-gngptolteatt | Handover Statistics - Number of GN/GP to LTE attempted handovers | Counter / Int32
> handoverstat-gngptoltesucc | Handover Statistics - Number of GN/GP to LTE successful handovers | Counter / Int32
> handoverstat-gngptoltefail | Handover Statistics - Number of GN/GP to LTE failed handovers | Counter / Int32
> handoverstat-ltetogngpatt | Handover Statistics - Number of LTE to GN/GP attempted handovers | Counter / Int32
> handoverstat-ltetogngpsucc | Handover Statistics - Number of LTE to GN/GP successful handovers | Counter / Int32
> handoverstat-ltetogngpfail | Handover Statistics - Number of LTE to GN/GP failed handovers | Counter / Int32
> handoverstat-ltetoehrpdatt | Handover Statistics -Number of LTE to eHPRD attempted handovers | Counter / Int32
> handoverstat-ltetoehrpdsucc | Handover Statistics - Number of LTE to eHPRD successful handovers | Counter / Int32
> handoverstat-ltetoehrpdfail | Handover Statistics - Number of eHPRD to LTE failed handovers | Counter / Int32
> handoverstat-ehrpdtolteatt | Handover Statistics - Number of eHPRD to LTE attempted handovers | Counter / Int32
> handoverstat-ehrpdtoltesucc | Handover Statistics - Number of eHPRD to LTE successful handovers | Counter / Int32
> handoverstat-ehrpdtoltefail | Handover Statistics - Number of eHPRD to LTE failed handovers | Counter / Int32
> sgitunstat-ipv6sessrel | SGi tunneling Statistics - IPv6 6to4 tunnel sessions released | Counter / Int32
> subqosstat-bearact-qci1 | Subscriber QoS Statistics - Total bearers active - QCI 1 | Counter / Int32
> subqosstat-bearact-qci2 | Subscriber QoS Statistics - Total bearers active - QCI 2 | Counter / Int32
> subqosstat-bearact-qci3 | Subscriber QoS Statistics - Total bearers active - QCI 3 | Counter / Int32
> subqosstat-bearact-qci4 | Subscriber QoS Statistics - Total bearers active - QCI 4 | Counter / Int32
> subqosstat-bearact-qci5 | Subscriber QoS Statistics - Total bearers active - QCI 5 | Counter / Int32
> subqosstat-bearact-qci6 | Subscriber QoS Statistics - Total bearers active - QCI 6 | Counter / Int32
> subqosstat-bearact-qci7 | Subscriber QoS Statistics - Total bearers active - QCI 7 | Counter / Int32
> subqosstat-bearact-qci8 | Subscriber QoS Statistics - Total bearers active - QCI 8 | Counter / Int32
> subqosstat-bearact-qci9 | Subscriber QoS Statistics - Total bearers active - QCI 9 | Counter / Int32
> subqosstat-bearact-qcinongbr | Subscriber QoS Statistics - Total bearers active - Non-Standard QCI (Non-GBR) | Counter / Int32
> subqosstat-bearact-qcigbr | Subscriber QoS Statistics - Total bearers active - Non-Standard QCI (GBR) | Counter / Int32
> subqosstat-bearsetup-qci1 | Subscriber QoS Statistics - Total bearers setup - QCI 1 | Counter / Int32
> subqosstat-bearsetup-qci2 | Subscriber QoS Statistics - Total bearers setup - QCI 2 | Counter / Int32
> subqosstat-bearsetup-qci3 | Subscriber QoS Statistics - Total bearers setup - QCI 3 | Counter / Int32
> subqosstat-bearsetup-qci4 | Subscriber QoS Statistics - Total bearers setup - QCI 4 | Counter / Int32
> subqosstat-bearsetup-qci5 | Subscriber QoS Statistics - Total bearers setup - QCI 5 | Counter / Int32
> subqosstat-bearsetup-qci6 | Subscriber QoS Statistics - Total bearers setup - QCI 6 | Counter / Int32
> subqosstat-bearsetup-qci7 | Subscriber QoS Statistics - Total bearers setup - QCI 7 | Counter / Int32
> subqosstat-bearsetup-qci8 | Subscriber QoS Statistics - Total bearers setup - QCI 8 | Counter / Int32
> subqosstat-bearsetup-qci9 | Subscriber QoS Statistics - Total bearers setup - QCI 9 | Counter / Int32
> subqosstat-bearsetup-qcinongbr | Subscriber QoS Statistics - Total bearers setup - Non-Standard QCI (Non-GBR) | Counter / Int32
> subqosstat-bearsetup-qcigbr | Subscriber QoS Statistics - Total bearers setup - Non-Standard QCI (GBR) | Counter / Int32
> subqosstat-bearrel-qci1 | Subscriber QoS Statistics - Total bearers released - QCI 1 | Counter / Int32
> subqosstat-bearrel-qci2 | Subscriber QoS Statistics - Total bearers released - QCI 2 | Counter / Int32
> subqosstat-bearrel-qci3 | Subscriber QoS Statistics - Total bearers released - QCI 3 | Counter / Int32
> subqosstat-bearrel-qci4 | Subscriber QoS Statistics - Total bearers released - QCI 4 | Counter / Int32
> subqosstat-bearrel-qci5 | Subscriber QoS Statistics - Total bearers released - QCI 5 | Counter / Int32
> subqosstat-bearrel-qci6 | Subscriber QoS Statistics - Total bearers released - QCI 6 | Counter / Int32
> subqosstat-bearrel-qci7 | Subscriber QoS Statistics - Total bearers released - QCI 7 | Counter / Int32
> subqosstat-bearrel-qci8 | Subscriber QoS Statistics - Total bearers released - QCI 8 | Counter / Int32
> subqosstat-bearrel-qci9 | Subscriber QoS Statistics - Total bearers released - QCI 9 | Counter / Int32
> subqosstat-bearrel-qcinongbr | Subscriber QoS Statistics - Total bearers released - Non-Standard QCI (Non-GBR) | Counter / Int32
> subqosstat-bearrel-qcigbr | Subscriber QoS Statistics - Total bearers released - Non-Standard QCI (GBR) | Counter / Int32
> subdatastat-totuppktfwd | Subscriber Data Statistics - Total Uplink packets forwarded | Counter / Int32
> subdatastat-uppktfwd-qci1 | Subscriber Data Statistics -Uplink packets forwarded - QCI 1 | Counter / Int32
> subdatastat-uppktfwd-qci2 | Subscriber Data Statistics -Uplink packets forwarded - QCI 2 | Counter / Int32
> subdatastat-uppktfwd-qci3 | Subscriber Data Statistics -Uplink packets forwarded - QCI 3 | Counter / Int32
> subdatastat-uppktfwd-qci4 | Subscriber Data Statistics -Uplink packets forwarded - QCI 4 | Counter / Int32
> subdatastat-uppktfwd-qci5 | Subscriber Data Statistics -Uplink packets forwarded - QCI 5 | Counter / Int32
> subdatastat-uppktfwd-qci6 | Subscriber Data Statistics -Uplink packets forwarded - QCI 6 | Counter / Int32
> subdatastat-uppktfwd-qci7 | Subscriber Data Statistics -Uplink packets forwarded - QCI 7 | Counter / Int32
> subdatastat-uppktfwd-qci8 | Subscriber Data Statistics -Uplink packets forwarded - QCI 8 | Counter / Int32
> subdatastat-uppktfwd-qci9 | Subscriber Data Statistics -Uplink packets forwarded - QCI 9 | Counter / Int32
> subdatastat-uppktfwd-stdqcinongbr | Subscriber Data Statistics - Uplink packets forwarded - Standard QCI (Non-GBR) | Counter / Int32
> subdatastat-uppktfwd-stdqcigbr | Subscriber Data Statistics - Uplink packets forwarded - Standard QCI (GBR) | Counter / Int32
> subdatastat-uppktfwd-qcinongbr | Subscriber Data Statistics - Uplink packets forwarded - Non-Standard QCI (Non-GBR) | Counter / Int32
> subdatastat-uppktfwd-qcigbr | Subscriber Data Statistics - Uplink packets forwarded - Non-Standard QCI (GBR) | Counter / Int32
> subdatastat-uppktfwd-totgbr | Subscriber Data Statistics - Uplink packets forwarded - Total GBR | Counter / Int32
> subdatastat-uppktfwd-totnongbr | Subscriber Data Statistics - Uplink packets forwarded - Total NON-GBR | Counter / Int32
> subdatastat-totupbytefwd | Subscriber Data Statistics - Total Uplink bytes forwarded | Counter / Int64
> subdatastat-upbytefwd-qci1 | Subscriber Data Statistics - Uplink bytes forwarded - QCI 1 | Counter / Int64
> subdatastat-upbytefwd-qci2 | Subscriber Data Statistics - Uplink bytes forwarded - QCI 2 | Counter / Int64
> subdatastat-upbytefwd-qci3 | Subscriber Data Statistics - Uplink bytes forwarded - QCI 3 | Counter / Int64
> subdatastat-upbytefwd-qci4 | Subscriber Data Statistics - Uplink bytes forwarded - QCI 4 | Counter / Int64
> subdatastat-upbytefwd-qci5 | Subscriber Data Statistics - Uplink bytes forwarded - QCI 5 | Counter / Int64
> subdatastat-upbytefwd-qci6 | Subscriber Data Statistics - Uplink bytes forwarded - QCI 6 | Counter / Int64
> subdatastat-upbytefwd-qci7 | Subscriber Data Statistics - Uplink bytes forwarded - QCI 7 | Counter / Int64
> subdatastat-upbytefwd-qci8 | Subscriber Data Statistics - Uplink bytes forwarded - QCI 8 | Counter / Int64
> subdatastat-upbytefwd-qci9 | Subscriber Data Statistics - Uplink bytes forwarded - QCI 9 | Counter / Int64
> subdatastat-upbytefwd-stdqcinongbr | Subscriber Data Statistics - Uplink bytes forwarded - Standard QCI (Non-GBR) | Counter / Int64
> subdatastat-upbytefwd-stdqcigbr | Subscriber Data Statistics - Uplink bytes forwarded - Standard QCI (GBR) | Counter / Int64
> subdatastat-upbytefwd-qcinongbr | Subscriber Data Statistics - Uplink bytes forwarded - Non-Standard QCI (Non-GBR) | Counter / Int64
> subdatastat-upbytefwd-qcigbr | Subscriber Data Statistics - Uplink bytes forwarded - Non-Standard QCI (GBR) | Counter / Int64
> subdatastat-upbytefwd-totgbr | Subscriber Data Statistics - Uplink bytes forwarded - Total GBR | Counter / Int64
> subdatastat-upbytefwd-totnongbr | Subscriber Data Statistics - Uplink bytes forwarded - Total NON-GBR | Counter / Int64
> subdatastat-totdownpktfwd | Subscriber Data Statistics - Total Downlink packets forwarded | Counter / Int64
> subdatastat-downpktfwd-qci1 | Subscriber Data Statistics - Downlink packets forwarded - QCI 1 | Counter / Int32
> subdatastat-downpktfwd-qci2 | Subscriber Data Statistics - Downlink packets forwarded - QCI 2 | Counter / Int32
> subdatastat-downpktfwd-qci3 | Subscriber Data Statistics - Downlink packets forwarded - QCI 3 | Counter / Int32
> subdatastat-downpktfwd-qci4 | Subscriber Data Statistics - Downlink packets forwarded - QCI 4 | Counter / Int32
> subdatastat-downpktfwd-qci5 | Subscriber Data Statistics - Downlink packets forwarded - QCI 5 | Counter / Int32
> subdatastat-downpktfwd-qci6 | Subscriber Data Statistics - Downlink packets forwarded - QCI 6 | Counter / Int32
> subdatastat-downpktfwd-qci7 | Subscriber Data Statistics - Downlink packets forwarded - QCI 7 | Counter / Int32
> subdatastat-downpktfwd-qci8 | Subscriber Data Statistics - Downlink packets forwarded - QCI 8 | Counter / Int32
> subdatastat-downpktfwd-qci9 | Subscriber Data Statistics - Downlink packets forwarded - QCI 9 | Counter / Int32
> subdatastat-downpktfwd-stdqcinongbr | Subscriber Data Statistics - Downlink packets forwarded - Standard QCI (Non-GBR) | Counter / Int32
> subdatastat-downpktfwd-stdqcigbr | Subscriber Data Statistics - Downlink packets forwarded - Standard QCI (GBR) | Counter / Int32
> subdatastat-downpktfwd-qcinongbr | Subscriber Data Statistics - Downlink packets forwarded - Non-Standard QCI (Non-GBR) | Counter / Int32
> subdatastat-downpktfwd-qcigbr | Subscriber Data Statistics - Downlink packets forwarded - Non-Standard QCI (GBR) | Counter / Int32
> subdatastat-downpktfwd-totgbr | Subscriber Data Statistics - Downlink packets forwarded - Total GBR | Counter / Int32
> subdatastat-downpktfwd-totnongbr | Subscriber Data Statistics - Downlink packets forwarded - Total NON-GBR | Counter / Int32
> subdatastat-totdownbytefwd | Subscriber Data Statistics - Total Downlink bytes forwarded | Counter / Int64
> subdatastat-downbytefwd-qci1 | Subscriber Data Statistics - Downlink bytes forwarded - QCI 1 | Counter / Int64
> subdatastat-downbytefwd-qci2 | Subscriber Data Statistics - Downlink bytes forwarded - QCI 2 | Counter / Int64
> subdatastat-downbytefwd-qci3 | Subscriber Data Statistics - Downlink bytes forwarded - QCI 3 | Counter / Int64
> subdatastat-downbytefwd-qci4 | Subscriber Data Statistics - Downlink bytes forwarded - QCI 4 | Counter / Int64
> subdatastat-downbytefwd-qci5 | Subscriber Data Statistics - Downlink bytes forwarded - QCI 5 | Counter / Int64
> subdatastat-downbytefwd-qci6 | Subscriber Data Statistics - Downlink bytes forwarded - QCI 6 | Counter / Int64
> subdatastat-downbytefwd-qci7 | Subscriber Data Statistics - Downlink bytes forwarded - QCI 7 | Counter / Int64
> subdatastat-downbytefwd-qci8 | Subscriber Data Statistics - Downlink bytes forwarded - QCI 8 | Counter / Int64
> subdatastat-downbytefwd-qci9 | Subscriber Data Statistics - Downlink bytes forwarded - QCI 9 | Counter / Int64
> subdatastat-downbytefwd-stdqcinongbr | Subscriber Data Statistics - Downlink bytes forwarded - Standard QCI (Non-GBR) | Counter / Int64
> subdatastat-downbytefwd-stdqcigbr | Subscriber Data Statistics - Downlink bytes forwarded - Standard QCI (GBR) | Counter / Int64
> subdatastat-downbytefwd-qcinongbr | Subscriber Data Statistics - Downlink bytes forwarded - Non-Standard QCI (Non-GBR) | Counter / Int64
> subdatastat-downbytefwd-qcigbr | Subscriber Data Statistics - Downlink bytes forwarded - Non-Standard QCI (GBR) | Counter / Int64
> subdatastat-downbytefwd-totgbr | Subscriber Data Statistics - Downlink bytes forwarded - Total GBR | Counter / Int64
> subdatastat-downbytefwd-totnongbr | Subscriber Data Statistics - Downlink bytes forwarded - Total NON-GBR | Counter / Int64
> subdatastat-totuppktdrop | Subscriber Data Statistics - Total Uplink packets dropped | Counter / Int32
> subdatastat-uppktdrop-qci1 | Subscriber Data Statistics -Uplink packets dropped - QCI 1 | Counter / Int32
> subdatastat-uppktdrop-qci2 | Subscriber Data Statistics -Uplink packets dropped - QCI 2 | Counter / Int32
> subdatastat-uppktdrop-qci3 | Subscriber Data Statistics -Uplink packets dropped - QCI 3 | Counter / Int32
> subdatastat-uppktdrop-qci4 | Subscriber Data Statistics -Uplink packets dropped - QCI 4 | Counter / Int32
> subdatastat-uppktdrop-qci5 | Subscriber Data Statistics -Uplink packets dropped - QCI 5 | Counter / Int32
> subdatastat-uppktdrop-qci6 | Subscriber Data Statistics -Uplink packets dropped - QCI 6 | Counter / Int32
> subdatastat-uppktdrop-qci7 | Subscriber Data Statistics -Uplink packets dropped - QCI 7 | Counter / Int32
> subdatastat-uppktdrop-qci8 | Subscriber Data Statistics -Uplink packets dropped - QCI 8 | Counter / Int32
> subdatastat-uppktdrop-qci9 | Subscriber Data Statistics -Uplink packets dropped - QCI 9 | Counter / Int32
> subdatastat-uppktdrop-stdqcinongbr | Subscriber Data Statistics - Uplink packets dropped - Standard QCI (Non-GBR) | Counter / Int32
> subdatastat-uppktdrop-stdqcigbr | Subscriber Data Statistics - Uplink packets dropped - Standard QCI (GBR) | Counter / Int32
> subdatastat-uppktdrop-qcinongbr | Subscriber Data Statistics - Uplink packets dropped - Non-Standard QCI (Non-GBR) | Counter / Int32
> subdatastat-uppktdrop-qcigbr | Subscriber Data Statistics - Uplink packets dropped - Non-Standard QCI (GBR) | Counter / Int32
> subdatastat-uppktdrop-totgbr | Subscriber Data Statistics - Uplink packets dropped - Total GBR | Counter / Int32
> subdatastat-uppktdrop-totnongbr | Subscriber Data Statistics - Uplink packets dropped - Total NON-GBR | Counter / Int32
> subdatastat-totupbytedrop | Subscriber Data Statistics - Total Uplink bytes dropped | Counter / Int64
> subdatastat-upbytedrop-qci1 | Subscriber Data Statistics - Uplink bytes dropped - QCI 1 | Counter / Int64
> subdatastat-upbytedrop-qci2 | Subscriber Data Statistics - Uplink bytes dropped - QCI 2 | Counter / Int64
> subdatastat-upbytedrop-qci3 | Subscriber Data Statistics - Uplink bytes dropped - QCI 3 | Counter / Int64
> subdatastat-upbytedrop-qci4 | Subscriber Data Statistics - Uplink bytes dropped - QCI 4 | Counter / Int64
> subdatastat-upbytedrop-qci5 | Subscriber Data Statistics - Uplink bytes dropped - QCI 5 | Counter / Int64
> subdatastat-upbytedrop-qci6 | Subscriber Data Statistics - Uplink bytes dropped - QCI 6 | Counter / Int64
> subdatastat-upbytedrop-qci7 | Subscriber Data Statistics - Uplink bytes dropped - QCI 7 | Counter / Int64
> subdatastat-upbytedrop-qci8 | Subscriber Data Statistics - Uplink bytes dropped - QCI 8 | Counter / Int64
> subdatastat-upbytedrop-qci9 | Subscriber Data Statistics - Uplink bytes dropped - QCI 9 | Counter / Int64
> subdatastat-upbytedrop-stdqcinongbr | Subscriber Data Statistics - Uplink bytes dropped - Standard QCI (Non-GBR) | Counter / Int64
> subdatastat-upbytedrop- stdqcigbr | Subscriber Data Statistics - Uplink bytes dropped - Standard QCI (GBR) | Counter / Int64
> subdatastat-upbytedrop-qcinongbr | Subscriber Data Statistics - Uplink bytes dropped - Non-Standard QCI (Non-GBR) | Counter / Int64
> subdatastat-upbytedrop-qcigbr | Subscriber Data Statistics - Uplink bytes dropped - Non-Standard QCI (GBR) | Counter / Int64
> subdatastat-upbytedrop-totgbr | Subscriber Data Statistics - Uplink bytes dropped - Total GBR | Counter / Int64
> subdatastat-upbytedrop-totnongbr | Subscriber Data Statistics - Uplink bytes dropped - Total NON-GBR | Counter / Int64
> subdatastat-totdownpktdrop | Subscriber Data Statistics - Total Downlink packets dropped | Counter / Int32
> subdatastat-downpktdrop-qci1 | Subscriber Data Statistics - Downlink packets dropped - QCI 1 | Counter / Int32
> subdatastat-downpktdrop-qci2 | Subscriber Data Statistics - Downlink packets dropped - QCI 2 | Counter / Int32
> subdatastat-downpktdrop-qci3 | Subscriber Data Statistics - Downlink packets dropped - QCI 3 | Counter / Int32
> subdatastat-downpktdrop-qci4 | Subscriber Data Statistics - Downlink packets dropped - QCI 4 | Counter / Int32
> subdatastat-downpktdrop-qci5 | Subscriber Data Statistics - Downlink packets dropped - QCI 5 | Counter / Int32
> subdatastat-downpktdrop-qci6 | Subscriber Data Statistics - Downlink packets dropped - QCI 6 | Counter / Int32
> subdatastat-downpktdrop-qci7 | Subscriber Data Statistics - Downlink packets dropped - QCI 7 | Counter / Int32
> subdatastat-downpktdrop-qci8 | Subscriber Data Statistics - Downlink packets dropped - QCI 8 | Counter / Int32
> subdatastat-downpktdrop-qci9 | Subscriber Data Statistics - Downlink packets dropped - QCI 9 | Counter / Int32
> subdatastat-downpktdrop-stdqcinongbr | Subscriber Data Statistics - Downlink packets dropped - Standard QCI (Non-GBR) | Counter / Int32
> subdatastat-downpktdrop-stdqcigbr | Subscriber Data Statistics - Downlink packets dropped - Standard QCI (GBR) | Counter / Int32
> subdatastat-downpktdrop-qcinongbr | Subscriber Data Statistics - Downlink packets dropped - Non-Standard QCI (Non-GBR) | Counter / Int32
> subdatastat-downpktdrop-qcigbr | Subscriber Data Statistics - Downlink packets dropped - Non-Standard QCI (GBR) | Counter / Int32
> subdatastat-downpktdrop-totgbr | Subscriber Data Statistics - Downlink packets dropped - Total GBR | Counter / Int32
> subdatastat-downpktdrop-totnongbr | Subscriber Data Statistics - Downlink packets dropped - Total NON-GBR | Counter / Int32
> subdatastat-totdownbytedrop | Subscriber Data Statistics - Total Downlink bytes dropped | Counter / Int64
> subdatastat-downbytedrop-qci1 | Subscriber Data Statistics - Downlink bytes dropped - QCI 1 | Counter / Int64
> subdatastat-downbytedrop-qci2 | Subscriber Data Statistics - Downlink bytes dropped - QCI 2 | Counter / Int64
> subdatastat-downbytedrop-qci3 | Subscriber Data Statistics - Downlink bytes dropped - QCI 3 | Counter / Int64
> subdatastat-downbytedrop-qci4 | Subscriber Data Statistics - Downlink bytes dropped - QCI 4 | Counter / Int64
> subdatastat-downbytedrop-qci5 | Subscriber Data Statistics - Downlink bytes dropped - QCI 5 | Counter / Int64
> subdatastat-downbytedrop-qci6 | Subscriber Data Statistics - Downlink bytes dropped - QCI 6 | Counter / Int64
> subdatastat-downbytedrop-qci7 | Subscriber Data Statistics - Downlink bytes dropped - QCI 7 | Counter / Int64
> subdatastat-downbytedrop-qci8 | Subscriber Data Statistics - Downlink bytes dropped - QCI 8 | Counter / Int64
> subdatastat-downbytedrop-qci9 | Subscriber Data Statistics - Downlink bytes dropped - QCI 9 | Counter / Int64
> subdatastat-downbytedrop-stdqcinongbr | Subscriber Data Statistics - Downlink bytes dropped - Standard QCI (Non-GBR) | Counter / Int64
> subdatastat-downbytedrop-stdqcigbr | Subscriber Data Statistics - Downlink bytes dropped - Standard QCI (GBR) | Counter / Int64
> subdatastat-downbytedrop-qcinongbr | Subscriber Data Statistics - Downlink bytes dropped - Non-Standard QCI (Non-GBR) | Counter / Int64
> subdatastat-downbytedrop-qcigbr | Subscriber Data Statistics - Downlink bytes dropped - Non-Standard QCI (GBR) | Counter / Int64
> subdatastat-downbytedrop-totgbr | Subscriber Data Statistics - Downlink bytes dropped - Total GBR | Counter / Int64
> subdatastat-downbytedrop-totnongbr | Subscriber Data Statistics - Downlink bytes dropped - Total NON-GBR | Counter / Int64
> subdatastat-totuppktdropmbrexc | Subscriber Data Statistics - Total Uplink packets Drop mbr exceed | Counter / Int32
> subdatastat-uppktdropmbrexc-qci1 | Subscriber Data Statistics - Uplink packets Drop mbr exceed - QCI 1 | Counter / Int32
> subdatastat-uppktdropmbrexc-qci2 | Subscriber Data Statistics - Uplink packets Drop mbr exceed - QCI 2 | Counter / Int32
> subdatastat-uppktdropmbrexc-qci3 | Subscriber Data Statistics - Uplink packets Drop mbr exceed- QCI 3 | Counter / Int32
> subdatastat-uppktdropmbrexc-qci4 | Subscriber Data Statistics - Uplink packets Drop mbr exceed - QCI 4 | Counter / Int32
> subdatastat-uppktdropmbrexc-qci5 | Subscriber Data Statistics - Uplink packets Drop mbr exceed- QCI 5 | Counter / Int32
> subdatastat-uppktdropmbrexc-qci6 | Subscriber Data Statistics - Uplink packets Drop mbr exceed - QCI 6 | Counter / Int32
> subdatastat-uppktdropmbrexc-qci7 | Subscriber Data Statistics - Uplink packets Drop mbr exceed - QCI 7 | Counter / Int32
> subdatastat-uppktdropmbrexc-qci8 | Subscriber Data Statistics - Uplink packets Drop mbr exceed - QCI 8 | Counter / Int32
> subdatastat-uppktdropmbrexc-qci9 | Subscriber Data Statistics - Uplink packets Drop mbr exceed - QCI 9 | Counter / Int32
> subdatastat-uppktdropmbrexc-stdqcinongbr | Subscriber Data Statistics - Uplink packets Drop mbr exceed - Standard QCI (Non-GBR | Counter / Int32
> subdatastat-uppktdropmbrexc-stdqcigbr | Subscriber Data Statistics - Uplink packets Drop mbr exceed - Standard QCI (GBR) | Counter / Int32
> subdatastat-uppktdropmbrexc-qcinongbr | Subscriber Data Statistics - Uplink packets Drop mbr exceed - Non-Standard QCI (Non-GBR) | Counter / Int32
> subdatastat-uppktdropmbrexc-qcigbr | Subscriber Data Statistics - Uplink packets Drop mbr exceed - Non-Standard QCI (GBR) | Counter / Int32
> subdatastat-uppktdropmbrexc-totgbr | Subscriber Data Statistics - Uplink packets Drop mbr exceed - Total GBR | Counter / Int32
> subdatastat-uppktdropmbrexc-totnongbr | Subscriber Data Statistics - Uplink packets Drop mbr exceed - Total NON-GBR | Counter / Int32
> subdatastat-totupbytedropmbrexc | Subscriber Data Statistics - Total Uplink bytes Drop mbr exceed | Counter / Int64
> subdatastat-upbytedropmbrexc-qci1 | Subscriber Data Statistics - Uplink bytes Drop mbr exceed - QCI 1 | Counter / Int64
> subdatastat-upbytedropmbrexc-qci2 | Subscriber Data Statistics - Uplink bytes Drop mbr exceed - QCI 2 | Counter / Int64
> subdatastat-upbytedropmbrexc-qci3 | Subscriber Data Statistics - Uplink bytes Drop mbr exceed- QCI 3 | Counter / Int64
> subdatastat-upbytedropmbrexc-qci4 | Subscriber Data Statistics - Uplink bytes Drop mbr exceed - QCI 4 | Counter / Int64
> subdatastat-upbytedropmbrexc-qci5 | Subscriber Data Statistics - Uplink bytes Drop mbr exceed- QCI 5 | Counter / Int64
> subdatastat-upbytedropmbrexc-qci6 | Subscriber Data Statistics - Uplink bytes Drop mbr exceed - QCI 6 | Counter / Int64
> subdatastat-upbytedropmbrexc-qci7 | Subscriber Data Statistics - Uplink bytes Drop mbr exceed - QCI 7 | Counter / Int64
> subdatastat-upbytedropmbrexc-qci8 | Subscriber Data Statistics - Uplink bytes Drop mbr exceed - QCI 8 | Counter / Int64
> subdatastat-upbytedropmbrexc-qci9 | Subscriber Data Statistics - Uplink bytes Drop mbr exceed - QCI 9 | Counter / Int64
> subdatastat-upbytedropmbrexc-stdqcinongbr | Subscriber Data Statistics - Uplink bytes Drop mbr exceed - Standard QCI (Non-GBR | Counter / Int64
> subdatastat-upbytedropmbrexc-stdqcigbr | Subscriber Data Statistics - Uplink bytes Drop mbr exceed - Standard QCI (GBR) | Counter / Int64
> subdatastat-upbytedropmbrexc-qcinongbr | Subscriber Data Statistics - Uplink bytes Drop mbr exceed - Non-Standard QCI (Non-GBR) | Counter / Int64
> subdatastat-upbytedropmbrexc-qcigbr | Subscriber Data Statistics - Uplink bytes Drop mbr exceed - Non-Standard QCI (GBR) | Counter / Int64
> subdatastat-upbytedropmbrexc-totgbr | Subscriber Data Statistics - Uplink bytes Drop mbr exceed - Total GBR | Counter / Int64
> subdatastat-upbytedropmbrexc-totnongbr | Subscriber Data Statistics - Uplink bytes Drop mbr exceed - Total NON-GBR | Counter / Int64
> subdatastat-totdownpktdropmbrexc | Subscriber Data Statistics - Total Downlink packets Drop mbr exceed | Counter / Int32
> subdatastat-downpktdropmbrexc-qci1 | Subscriber Data Statistics - Downlink packets Drop mbr exceed - QCI 1 | Counter / Int32
> subdatastat-downpktdropmbrexc-qci2 | Subscriber Data Statistics - Downlink packets Drop mbr exceed - QCI 2 | Counter / Int32
> subdatastat-downpktdropmbrexc-qci3 | Subscriber Data Statistics - Downlink packets Drop mbr exceed- QCI 3 | Counter / Int32
> subdatastat-downpktdropmbrexc-qci4 | Subscriber Data Statistics - Downlink packets Drop mbr exceed - QCI 4 | Counter / Int32
> subdatastat-downpktdropmbrexc-qci5 | Subscriber Data Statistics - Downlink packets Drop mbr exceed- QCI 5 | Counter / Int32
> subdatastat-downpktdropmbrexc-qci6 | Subscriber Data Statistics - Downlink packets Drop mbr exceed - QCI 6 | Counter / Int32
> subdatastat-downpktdropmbrexc-qci7 | Subscriber Data Statistics - Downlink packets Drop mbr exceed - QCI 7 | Counter / Int32
> subdatastat-downpktdropmbrexc-qci8 | Subscriber Data Statistics - Downlink packets Drop mbr exceed - QCI 8 | Counter / Int32
> subdatastat-downpktdropmbrexc-qci9 | Subscriber Data Statistics - Downlink packets Drop mbr exceed - QCI 9 | Counter / Int32
> subdatastat-downpktdropmbrexc-stdqcinongbr | Subscriber Data Statistics - Downlink packets Drop mbr exceed - Standard QCI (Non-GBR | Counter / Int32
> subdatastat-downpktdropmbrexc-stdqcigbr | Subscriber Data Statistics - Downlink packets Drop mbr exceed - Standard QCI (GBR) | Counter / Int32
> subdatastat-downpktdropmbrexc-qcinongbr | Subscriber Data Statistics - Downlink packets Drop mbr exceed - Non-Standard QCI (Non-GBR) | Counter / Int32
> subdatastat-downpktdropmbrexc-qcigbr | Subscriber Data Statistics - Downlink packets Drop mbr exceed - Non-Standard QCI (GBR) | Counter / Int32
> subdatastat-downpktdropmbrexc-totgbr | Subscriber Data Statistics - Downlink packets Drop mbr exceed - Total GBR | Counter / Int32
> subdatastat-downpktdropmbrexc-totnongbr | Subscriber Data Statistics - Downlink packets Drop mbr exceed - Total NON-GBR | Counter / Int32
> subdatastat-totdownbytedropmbrexc | Subscriber Data Statistics - Total Downlink bytes Drop mbr exceed | Counter / Int64
> subdatastat-downbytedropmbrexc-qci1 | Subscriber Data Statistics - Downlink bytes Drop mbr exceed - QCI 1 | Counter / Int64
> subdatastat-downbytedropmbrexc-qci2 | Subscriber Data Statistics - Downlink bytes Drop mbr exceed - QCI 2 | Counter / Int64
> subdatastat-downbytedropmbrexc-qci3 | Subscriber Data Statistics - Downlink bytes Drop mbr exceed- QCI 3 | Counter / Int64
> subdatastat-downbytedropmbrexc-qci4 | Subscriber Data Statistics - Downlink bytes Drop mbr exceed - QCI 4 | Counter / Int64
> subdatastat-downbytedropmbrexc-qci5 | Subscriber Data Statistics - Downlink bytes Drop mbr exceed- QCI 5 | Counter / Int64
> subdatastat-downbytedropmbrexc-qci6 | Subscriber Data Statistics - Downlink bytes Drop mbr exceed - QCI 6 | Counter / Int64
> subdatastat-downbytedropmbrexc-qci7 | Subscriber Data Statistics - Downlink bytes Drop mbr exceed - QCI 7 | Counter / Int64
> subdatastat-downbytedropmbrexc-qci8 | Subscriber Data Statistics - Downlink bytes Drop mbr exceed - QCI 8 | Counter / Int64
> subdatastat-downbytedropmbrexc-qci9 | Subscriber Data Statistics - Downlink bytes Drop mbr exceed - QCI 9 | Counter / Int64
> subdatastat-downbytedropmbrexc-stdqcinongbr | Subscriber Data Statistics - Downlink bytes Drop mbr exceed - Standard QCI (Non-GBR | Counter / Int64
> subdatastat-downbytedropmbrexc-stdqcigbr | Subscriber Data Statistics - Downlink bytes Drop mbr exceed - Standard QCI (GBR) | Counter / Int64
> subdatastat-downbytedropmbrexc-qcinongbr | Subscriber Data Statistics - Downlink bytes Drop mbr exceed - Non-Standard QCI (Non-GBR) | Counter / Int64
> subdatastat-downbytedropmbrexc-qcigbr | Subscriber Data Statistics - Downlink bytes Drop mbr exceed - Non-Standard QCI (GBR) | Counter / Int64
> subdatastat-downbytedropmbrexc-totgbr | Subscriber Data Statistics - Downlink bytes Drop mbr exceed - Total GBR | Counter / Int64
> subdatastat-downbytedropmbrexc-totnongbr | Subscriber Data Statistics - Downlink bytes Drop mbr exceed - Total NON-GBR | Counter / Int64
> apnambrratelimit-uppktdrop | APN AMBR Rate Limiting Statistics - Uplink packets dropped | Counter / Int32
> apnambrratelimit-downpktdrop | APN AMBR Rate Limiting Statistics - Downlink packets dropped | Counter / Int32
> apnambrratelimit-upbytedrop | APN AMBR Rate Limiting Statistics - Uplink bytes dropped | Counter / Int64
> apnambrratelimit-downbytedrop | APN AMBR Rate Limiting Statistics - Downlink bytes dropped | Counter / Int64
> Important: See Bulk Statistics Overview for statistics that are common to all schema.

> ‌

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883