> CSCF IFC Trigger Point Mode Commands
> The CSCF iFC Trigger Point Configuration Mode is used to associate an Initial Filter Criteria (iFC) Service Point Trigger (SPT) group with an iFC trigger point.
> Important: The commands or keywords/variables that are available are dependent on platform type, product version, and installed license(s).
> end
> Exits the current mode and returns to the Exec Mode.
> Product
> All
> Privilege
> Administrator
> Syntax
> end
> Usage
> Change the mode back to the Exec mode.
> exit
> Exits the current mode and returns to the previous mode.
> Product
> All
> Privilege
> Administrator
> Syntax
> exit
> Usage
> Return to the previous mode.
> spt-group
> Assigns an existing iFC SPT group to an iFC trigger point.
> Product
> SCM (S-CSCF, SIP Proxy)
> Privilege
> Administrator
> Syntax
> [ no ] spt-group name group_name
> no
> Removes the specified CSCF iFC SPT group from the iFC trigger point.
> spt-group name group_name
> Specifies the name of an existing iFC SPT group.
> group_name must be from 1 to 39 alpha and/or numeric characters in length.
> Important: An iFC SPT group can be assigned to more than one iFC trigger point.
> Usage
> Use this command to associate an iFC SPT group with an iFC trigger point.
> Example
> The following command assigns an iFC SPT group named group2 to an iFC trigger point:
> spt-group name group2

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883