> IPSG Schema Statistics
> The IPSG schema provides the following types of statistics:

> • | Counter: A counter records incremental data cumulatively and rolls over when the counter limit is reached. The limit depends upon the counter data type.

> • | Gauge: A gauge statistic indicates a single value representative of a single instance. This type is often used to track particular events in time.

> Important: The format string syntax is described by Schema Format String Syntax in the Bulk Statistics Overview chapter.
> Important: Unless otherwise indicated, all statistics are counters. For statistics with the Int32 data type, the roll-over to zero limit is 4,294,967,295. For statistics with the Int64 data type, the roll-over to zero limit is 18,446,744,073,709,551,615. All counter statistics are cumulative and reset only by one of the following methods: roll-over (as described above), after a system restart, or after a clear command is performed. All statistics are considered standards-based unless otherwise noted.
> The following variables are supported:
> IPSG Schema Statistics

> Statistic | Description | Data Type
> vpnname | The name of the VPN context where the IPSG service resides. | String
> vpnid | The identification number of the VPN context where the IPSG service resides. | Int32
> servname | The name of the IPSG service. | String
> servid | The identification number of the IPSG service. | Int32
> total-start-req-rcv | The total number of start requests received by the service. | Int32
> total-start-req-retrans-rcv | The total number of start request retransmissions received by the service. | Int32
> total-start-rsp-sent | The total number of start responses sent. | Int32
> total-interim-update-req-rcv | The total number of interim update requests received by the service. | Int32
> total-stop-req-rcv | The total number of stop requests received by the service. | Int32
> total-unknown-req-rcv | The total number of unknown requests received by the service. | Int32
> total-rsp-sent | The total number of responses sent by the service. | Int32
> total-discard-msgs-unknown-clnt | The total number of discarded messages from an unknown client. | Int32
> total-discard-msgs-ignore-interim | The total number of RADIUS-Accounting-Interim messages ignored by the IPSG since they were received for non-existing sessions. | Int32
> total-discard-msgs-ignore-stop | The total number of RADIUS-Accounting-Stop messages ignored by the IPSG since they were received for non-existing sessions. | Int32
> total-discard-msgs-incorrect-secret | The total number of messages discarded due to an incorrect secret. | Int32
> total-discard-msgs-attr-missing | The total number of discarded messages due to a missing attribute. | Int32
> rad-servaddr | The RADIUS server IP address supporting the service. | String
> rad-servport | The RADIUS server port. | Int32
> Important: See Bulk Statistics Overview for statistics that are common to all schema.

> ‌

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883