> show cscf
> This chapter includes the show cscf command output tables.
> show cscf nat media mapping all
> show cscf nat media mapping all Command Output Descriptions

> Field | Description
> UE-Origin | The IP address and port number of the UE origin.
> UE-Destination | The IP address and port number of the UE destination.
> Nwk-Origin | The IP address and port number of the network origin.
> Nwk-Destination | The IP address and port number of the network destination.
> Nwk-Core-context | The context in which the network core configuration resides.
> UE-Access-context | The context in which the UE access configuration resides.

> ‌
> show cscf peer-servers full
> show cscf peer-servers full Command Output Descriptions

> Field | Description
> Peer-Server name | The name of the peer server group.
> Context | The context in which the peer server group configuration resides.
> Server type | The type of servers in the peer server group.
> Hunting-method | The hunting method used by the servers in the peer server group.
> server | The name of the peer server.
> Address | The IP address of the peer server expressed in IPv4 or IPv6 dotted decimal notation.
> domain | The domain name of the peer server.
> Monitor status | The monitoring status of the peer servers as determined by the CLI command Enabled/Disabled.
> monitor-interval (seconds) | The time period, in seconds, between monitor intervals.
> monitor-message | The SIP message (OPTIONS) to be sent after each monitoring interval.
> monitor-response-timer (seconds) | The response wait timer, in seconds, for each monitor message.
> Server mode | The mode of the peer server as determined by the CLI command Active/Standby.
> Server status | The status of the peer server. Possible statuses are:
> • | OUT_OF_SERVICE — Peer server mode changed to standby through CLI command.
> • | AVAILABLE — Peer server mode is Active and peer server sends response to monitor message.
> • | UNAVAILABLE— Peer server mode is Active, however, peer server does not send response to monitor message.
> Network session template | Binds the nw-session-template name with the peer server.
> IMS Capable | Indicates if the peer server is ims-capable or not.
> Request Rx | The number of requests received by the sip-as peer server from S-CSCF during load balancing.

> ‌
> show cscf service li-packet-cable statistics
> show cscf service li-packet-cable statistics Command Output Descriptions

> Field | Description
> DLIA Session Stats | Diameter Lawful Intercept Application Session statistics:
> Total Current Sessions | Total number of current sessions.
> DLIA Message Stats | Diameter Lawful Intercept Application Message statistics:
> ACR Sent | Number of Accounting Request messages sent.
> ACA Received | Number of Accounting Answer messages received.
> DLIA Message Error Stats | Diameter Lawful Intercept Application Error statistics:
> Diameter Protocol Errs | Number of Diameter protocol errors.
> Bad Answers | Number of bad answers.
> ACR Send Errors | Number of Accounting Request send errors.

> ‌
> show cscf service statistics
> show cscf service statistics Command Output Descriptions

> Field | Description
> CSCF Service | The name of the service and context.
> CSCF Active Subscriptions
> Originating | The total current number of active subscriptions originating on this service.
> Terminating (UE originated) | The total current number of UE-originated active subscriptions terminating on this service.
> Terminating (PCSCF Originated) | The total current number of Proxy CSCF-originated active subscriptions terminating on this service.
> Terminating (AS Originated) | The total current number of AS-originated active subscriptions terminating on this service.
> Proxied | The total current number of active subscriptions proxied on this service.
> CSCF Calls
> Total CallSetupAttempts Rx | The total current number of call setup attempts received by this service.
> Total CallSetupAttempts Tx | The total current number of call setup attempts transmitted by this service.
> Total CallSetupSuccess Rx | The total current number of successful call setups received by this service.
> Total CallSetupSuccess Tx | The total current number of call setups successfully transmitted by this service.
> Total CallSetupFailures Rx | The total current number of call setup failures received by this service.
> Total CallSetupFailures Tx | The total current number of failed call setups transmitted by this service.
> Total 3xx Responses Rx | The total current number of 3xx responses received by this service.
> Total 3xx Responses Tx | The total current number of 3xx responses transmitted by this service.
> Total 402 Payment Required Rx | The total current number of 402 Payment Required responses received by this service.
> Total 402 Payment Required Tx | The total current number of 402 Payment Required responses transmitted by this service.
> Total 403 Forbidden Rx | The total current number of 403 Forbidden responses received by this service.
> Total 403 Forbidden Tx | The total current number of 403 Forbidden responses transmitted by this service.
> Total 404 Not Found Rx | The total current number of 404 Not Found responses received by this service.
> Total 404 Not FoundTx | The total current number of 404 Not Found responses transmitted by this service.
> Total 407 Proxy Auth Required Rx | The total current number of 407 Proxy Auth Required responses received by this service.
> Total 407 Proxy Auth Required Tx | The total current number of 407 Proxy Auth Required responses transmitted by this service.
> Total 408 Request Timeout Rx | The total current number of 408 Request Timeout responses received by this service.
> Total 408 Request Timeout Tx | The total current number of 408 Request Timeout responses transmitted by this service.
> Total 420 Bad Extension Rx | The total current number of 420 Bad Extension responses received by this service.
> Total 420 Bad Extension Tx | The total current number of 420 Bad Extension responses transmitted by this service.
> Total 421 Extension Required Rx | The total current number of 421 Extension Required responses received by this service.
> Total 421 Extension Required Tx | The total current number of 421 Extension Required responses transmitted by this service.
> Total 480 Temp Not Available Rx | The total current number of 480 Temp Not Available responses received by this service.
> Total 480 Temp Not Available Tx | The total current number of 480 Temp Not Available responses transmitted by this service.
> Total 486 Busy Here Rx | The total current number of 486 Busy Here responses received by this service.
> Total 486 Busy Here Tx | The total current number of 486 Busy Here responses transmitted by this service.
> Total 487 Request Cancel Rx | The total current number of 487 Request Cancel responses received by this service.
> Total 487 Request Cancel Tx | The total current number of 487 Request Cancel responses transmitted by this service.
> Total 488 Not Acceptable Media Rx | The total current number of 488 Not Acceptable Media responses received by this service.
> Total 488 Not Acceptable Media Tx | The total current number of 488 Not Acceptable Media responses transmitted by this service.
> Total 4xx Responses Rx | The total current number of 4xx responses received by this service.
> Total 4xx Responses Tx | The total current number of 4xx responses transmitted by this service.
> Total 5xx Responses Rx | The total current number of 5xx responses received by this service.
> Total 5xx Responses Tx | The total current number of 5xx responses transmitted by this service.
> Total 500 Internal Error Rx | The total current number of 500 Internal Error responses received by this service.
> Total 500 Internal Error Tx | The total current number of 500 Internal Error responses transmitted by this service.
> Total 503 Service Unavailable Rx | The total current number of 503 Service Unavailable responses received by this service.
> Total 503 Service Unavailable Tx | The total current number of 503 Service Unavailable responses transmitted by this service.
> Total 6xx Responses Rx | The total current number of 6xx responses received by this service.
> Total 6xx Responses Tx | The total current number of 6xx responses transmitted by this service.
> Total CallReleaseAttempts Rx | The total current number of call release attempts received by this service.
> Total CallReleaseAttempts Tx | The total current number of call release attempts transmitted by this service.
> Total CallReleaseSuccess Rx | The total current number of call releases successfully received by this service.
> Total CallReleaseSuccess Tx | The total current number of successful call releases transmitted by this service.
> Total CallReleaseFailures Rx | The total current number of call release failures received by this service.
> Total CallReleaseFailures Tx | The total current number of failed call releases transmitted by this service.
> Total Call Attempts Challenged | The total current number of call attempts challenged on this service.
> Total Session Timer Expires | The total current number of sessions on this service with expired timers.
> Total Call Rejects from PCRF/PDF | The total current number of calls rejected by the PCRF/PDF from this service.
> Total Call Rejects from Proxy (local) | The total current number of calls rejected by the local proxy from this service.
> Total Too Large SIP Messages | The total current number of too large SIP messages on this service.
> Total HSS Accesses | The total current number of HSS accesses by this service.
> Total Emergency Calls | The total current number of emergency calls made through this service.
> Total Toll Free Calls | The total current number of toll-free calls made through this service.
> Total Premium Service Calls | The total current number of premium-service calls made through this service.
> Total International Calls | The total current number of international calls made through this service.
> Total LongDistance Calls | The total current number of long distance calls made through this service.
> Total Operator Assisted Calls | The total current number of operator-assisted calls made through this service.
> Total Directory Assisted Calls | The total current number of directory-assisted calls made through this service.
> Total Media (audio) Loss Call Releases | The total current number of media (audio) loss call releases by this service.
> Total RTP Packets Sent | The total current number of RTP packets sent by this service.
> Total RTP Packets Received | The total current number of RTP packets received by this service.
> Total MSRP Packets Sent | The total current number of MSRP TCP packets sent by this service.
> Total MSRP Packets Received | The total current number of MSRP TCP packets received by this service.
> Total Call Releases initiated by UE | The total current number of UE-initiated call releases.
> • | For P-CSCF, the number of BYE initiated by UE.
> • | For S-CSCF, the number of BYE received from P-CSCF (initiated by UE/P-CSCF).
> Total Call Releases initiated by Network | The total current number of network-initiated call releases.
> • | For P-CSCF, the number of BYE received from S-CSCF.
> • | For S-CSCF, the number of BYE received from AS, etc.
> Total Call Releases initiated by Radio Loss | The total current number of Radio Loss-initiated call releases; the number of BYE originated by P-CSCF due to radio coverage loss of UE.
> Total Call Releases initiated by CSCF (Local) | The total current number of CSCF (Local)-initiated call releases; the number of BYE originated by CSCF due to CLI, radio loss, network-initiated de-registration, and internal processing failure.
> Total Calls rejected due to Concurrent Call limit exceeded | The total current number of calls rejected due to concurrent call limit exceeded by this service.
> CSCF Congestion Control Statistcs
> Registration Attempts Rejected | The total current number of registration (SIP REGISTER message) attempts rejected by CSCF service due to congestion trigger.
> Re-Registration Attempts Rejected | The total current number of re-registration (SIP REGISTER message) attempts rejected by CSCF service due to congestion trigger.
> Call Setup Attempts Rejected | The total current number of call setup attempts (SIP INVITE) rejected by CSCF service due to congestion trigger.
> Message Attempts Rejected | The total current number of SIP MESSAGE requests rejected by CSCF service due to congestion trigger.
> Subscription Attempts Rejected | The total current number of SIP SUBSCRIBE requests rejected by CSCF service due to congestion trigger.
> Notification Attempts Rejected | The total current number of SIP NOTIFY requests rejected by CSCF service due to congestion trigger.
> Publish Attempts Rejected | The total current number of SIP PUBLISH attempts rejected by CSCF service due to congestion trigger.
> Other SIP Message Attempts Rejected | The total current number of other SIP requests (excepts those mentioned above) rejected by CSCF service due to congestion trigger.
> Messages dropped due to congestion | The total current number of SIP messages dropped by CSCF service due to congestion trigger.
> TCP packets dropped due to congestion | The total current number of TCP packets dropped by CSCF service due to congestion trigger.
> Number of times congestion applied | The number of times the sessmgr congestion control is triggered.This value is collected from all sessmgrs running the CSCF service.
> Number of times congestion cleared | The number of times the sessmgr congestion control is cleared. This value is collected from all sessmgrs running the CSCF service.
> CSCF MESSAGE Statistics
> Message Attempts Received | The total current number of message attempts received by this service.
> Message Attempts Transmitted | The total current number of message attempts transmitted by this service.
> Message Success Received | The total current number of successful messages received by this service.
> Message Success Transmitted | The total current number of messages successfully transmitted by this service.
> Message Failures Received | The total current number of message failures received by this service.
> Message Failures Transmitted | The total current number of failed messages transmitted by this service.
> 3xx Response Received | The total current number of 3xx Response messages received on this service.
> 3xx Response Transmitted | The total current number of 3xx Response messages transmitted by this service.
> 400 Bad Request Received | The total current number of 400 Bad Request messages received on this service.
> 400 Bad Request Transmitted | The total current number of 400 Bad Request messages transmitted by this service.
> 403 Forbidden Received | The total current number of 403 Forbidden messages received on this service.
> 403 Forbidden Transmitted | The total current number of 403 Forbidden messages transmitted by this service.
> 404 Not Found Received | The total current number of 404 Not Found messages received on this service.
> 404 Not Found Transmitted | The total current number of 404 Not Found messages transmitted by this service.
> 415 Unsupport Media Type Received | The total current number of 415 Unsupport Media Type messages received on this service.
> 415 Unsupport Media Type Transmitted | The total current number of 415 Unsupport Media Type messages transmitted by this service.
> 416 Unsupport URI Scheme Received | The total current number of 416 Unsupport URI Scheme messages received on this service.
> 416 Unsupport URI Scheme Transmitted | The total current number of 416 Unsupport URI Scheme messages transmitted by this service.
> 420 Bad Extension Received | The total current number of 420 Bad Extension messages received on this service.
> 420 Bad Extension Transmitted | The total current number of 420 Bad Extension messages transmitted by this service.
> 421 Extension Required Received | The total current number of 421 Extension Required messages received on this service.
> 421 Extension Required Transmitted | The total current number of 421 Extension Required messages transmitted by this service.
> 480 Temp Not Available Received | The total current number of 480 Temp Not Available messages received on this service.
> 480 Temp Not Available Transmitted | The total current number of 480 Temp Not Available messages transmitted by this service.
> 488 Not Acceptable Media Received | The total current number of 488 Not Acceptable Media messages received on this service.
> 488 Not Acceptable Mediad Transmitted | The total current number of 488 Not Acceptable Media messages transmitted by this service.
> 4xx Response Received | The total current number of 4xx Response messages received on this service.
> 4xx Response Transmitted | The total current number of 4xx Response messages transmitted by this service.
> 500 Internal Error Received | The total current number of 500 Internal Error messages received on this service.
> 500 Internal Error Transmitted | The total current number of 500 Internal Error messages transmitted by this service.
> 513 Message Too Large Received | The total current number of 513 Message Too Large messages received on this service.
> 513 Message Too Large Transmitted | The total current number of 513 Message Too Large messages transmitted by this service.
> 5xx Response Received | The total current number of 5xx Response messages received on this service.
> 5xx Response Transmitted | The total current number of 5xx Response messages transmitted by this service.
> 6xx Response Received | The total current number of 6xx Response messages received on this service.
> 6xx Response Transmitted | The total current number of 6xx Response messages transmitted by this service.
> CSCF Performance
> Invite Processing Time | Minimum and maximum time (in ms) required to process an INVITE message (time elapsed between the INVITE entering the proxy and the INVITE forwarded out of the proxy).
> First Response Time | Minimum and maximum time (in ms) between sending an INVITE message out of the proxy and the first response received for the INVITE (any 1xx).
> Post Dial Delay | Minimum and maximum time (in ms) between sending an INVITE message out of the proxy and receiving the ringing message or any final response to the INVITE.
> Session Setup Delay | Minimum and maximum time (in ms) between when an INVITE message was received by the proxy and a 200 OK (invite) sent out of the proxy.
> Post Answer Delay | Minimum and maximum time (in ms) between a 200 OK INVITE message received by the proxy and the ACK message (for invite) sent out of the proxy.
> Session Release Delay | Minimum and maximum time (in ms) between when a BYE message is received by the proxy and a 200 OK BYE is sent out of the proxy.
> CSCF Registrations
> Current Registered Users | The current number of users registered to this service.
> Current Secure Connections | The current number of secure connections to this service.
> Current Unsecure Connections | The current number of unsecure connections to this service.
> Total Failed Authentications | The total current number of failed authentications for this service.
> Total Registration Expires | The total current number of expired registrations on this service.
> Total Registration from Roaming UE | The total number of registrations from Roaming UE.
> Total Successful Registration from Roaming UE | The total number 200 ok to registrations from Roaming UE.
> Total Failed Registration from Roaming UE | The total number of failed registrations from Roaming UE.
> Total 403 response to Registration from Roaming UE | The total number of 403 response to registration from Roaming UE.
> Total Re-Registration from Roaming UE | The total number of re-registration from Roaming UE.
> Total Successful Re-Registration from Roaming UE | The total number 200 ok to re-registrations from Roaming UE.
> Total Failed Re-Registration from Roaming UE | The total number of failed re-registrations from Roaming UE.
> Total 403 response to Re-Registration from Roaming UE | The total number of 403 response to re-registration from Roaming UE.
> Total De-Registration from Roaming UE | The total number of de-registration from Roaming UE.
> Total Successful De-Registration from Roaming UE | The total number 200 ok to de-registrations from Roaming UE.
> Total Failed De-Registration from Roaming UE | The total number of failed de-registrations from Roaming UE.
> Total 403 response to De-Registration from Roaming UE | The total number of 403 response to de-registration from Roaming UE.
> Total De-registrations initiated by UE | The total current number of UE-initiated de-registration requests on this service.
> Total De-registrations initiated by Network | The total current number of network-initiated de-registration requests received by P-CSCF from S-CSCF or by S-CSCF/SIP Proxy from internal/HSS trigger on this service.
> Total Secure Registrations | The total current number of secure registrations on this service.
> Total Failed Secure Registrations | The total current number of failed secure registrations on this service.
> Registration Statistics
> Registration Attempts Received | The total current number of registration attempts received on this service.
> Registration Attempts Transmitted | The total current number of registration attempts transmitted by this service.
> Registration Success Received | The total current number of registration successes received on this service.
> Registration Success Transmitted | The total current number of registration successes transmitted by this service.
> Registration Failures Received | The total current number of registration failures received on this service.
> Registration Failures Transmitted | The total current number of registration failures transmitted by this service.
> 401 Unauthorized (Registration) Received | The total current number of 401 Unauthorized responses to registration received on this service.
> 401 Unauthorized (Registration) Transmitted | The total current number of 401 Unauthorized responses to registration transmitted by this service.
> 403 Forbidden (Registration) Received | The total current number of 403 Forbidden responses to registration received on this service.
> 403 Forbidden (Registration) Transmitted | The total current number of 403 Forbidden responses to registration transmitted by this service.
> 404 Not Found (Registration) Received | The total current number of 404 Not Found responses to registration received on this service.
> 404 Not Found (Registration) Transmitted | The total current number of 404 Not Found responses to registration transmitted by this service.
> 420 Bad Extension (Registration) Received | The total current number of 420 Bad Extension responses to registration received on this service.
> 420 Bad Extension (Registration) Transmitted | The total current number of 420 Bad Extension responses to registration transmitted by this service.
> 439 First HopLackOb (Registration) Received | The total current number of 439 First Hop Lack Outbound responses to registration received on this service.
> 439 First HopLackOb (Registration) Transmitted | The total current number of 439 First Hop Lack Outbound responses to registration transmitted by this service.
> 4xx Responses (Registration) Received | The total current number of 4xx responses to registration received on this service.
> 4xx Responses (Registration) Transmitted | The total current number of 4xx responses to registration transmitted by this service.
> 500 Internal Error (Registration) Received | The total current number of 500 Internal Error responses to registration received on this service.
> 500 Internal Error (Registration) Transmitted | The total current number of 500 Internal Error responses to registration transmitted by this service.
> 5xx Responses (Registration) Received | The total current number of 5xx responses to registration received on this service.
> 5xx Responses (Registration) Transmitted | The total current number of 5xx responses to registration transmitted by this service.
> 6xx Responses (Registration) Received | The total current number of 6xx responses to registration received on this service.
> 6xx Responses (Registration) Transmitted | The total current number of 6xx responses to registration transmitted by this service.
> Re-Registration Statistics
> Re-Registration Attempts Received | The total current number of re-registration attempts received on this service.
> Re-Registration Attempts Transmitted | The total current number of re-registration attempts transmitted by this service.
> Re-Registration Success Received | The total current number of re-registration successes received on this service.
> Re-Registration Success Transmitted | The total current number of re-registration successes transmitted by this service.
> Re-Registration Failures Received | The total current number of re-registration failures received on this service.
> Re-Registration Failures Transmitted | The total current number of re-registration failures transmitted by this service.
> 401 Unauthorized (Re-Registration) Received | The total current number of 401 Unauthorized responses to re-registration received on this service.
> 401 Unauthorized (Re-Registration) Transmitted | The total current number of 401 Unauthorized responses to re-registration transmitted by this service.
> 403 Forbidden (Re-Registration) Received | The total current number of 403 Forbidden responses to re-registration received on this service.
> 403 Forbidden (Re-Registration) Transmitted | The total current number of 403 Forbidden responses to re-registration transmitted by this service.
> 404 Not Found (Re-Registration) Received | The total current number of 404 Not Found responses to re-registration received on this service.
> 404 Not Found (Re-Registration) Transmitted | The total current number of 404 Not Found responses to re-registration transmitted by this service.
> 420 Bad Extension (Re-Registration) Received | The total current number of 420 Bad Extension responses to re-registration received on this service.
> 420 Bad Extension (Re-Registration) Transmitted | The total current number of 420 Bad Extension responses to re-registration transmitted by this service.
> 439 First HopLackOb (Re-Registration) Received | The total current number of 439 First Hop Lack Outbound responses to re-registration received on this service.
> 439 First HopLackOb (Re-Registration) Transmitted | The total current number of 439 First Hop Lack Outbound responses to re-registration transmitted by this service.
> 4xx Responses (Re-Registration) Received | The total current number of 4xx responses to re-registration received on this service.
> 4xx Responses (Re-Registration) Transmitted | The total current number of 4xx responses to re-registration transmitted by this service.
> 500 Internal Error (Re-Registration) Received | The total current number of 500 Internal Error responses to re-registration received on this service.
> 500 Internal Error (Re-Registration) Transmitted | The total current number of 500 Internal Error responses to re-registration transmitted by this service.
> 5xx Responses (Re-Registration) Received | The total current number of 5xx responses to re-registration received on this service.
> 5xx Responses (Re-Registration) Transmitted | The total current number of 5xx responses to re-registration transmitted by this service.
> 6xx Responses (Re-Registration) Received | The total current number of 6xx responses to re-registration received on this service.
> 6xx Responses (Re-Registration) Transmitted | The total current number of 6xx responses to re-registration transmitted by this service.
> De-Registration Statistics
> De-Registration Attempts Received | The total current number of de-registration attempts received on this service.
> De-Registration Attempts Transmitted | The total current number of de-registration attempts transmitted by this service.
> De-Registration Success Received | The total current number of de-registration successes received on this service.
> De-Registration Success Transmitted | The total current number of de-registration successes transmitted by this service.
> De-Registration Failures Received | The total current number of de-registration failures received on this service.
> De-Registration Failures Transmitted | The total current number of de-registration failures transmitted by this service.
> 401 Unauthorized (De-Registration) Received | The total current number of 401 Unauthorized responses to de-registration received on this service.
> 401 Unauthorized (De-Registration) Transmitted | The total current number of 401 Unauthorized responses to de-registration transmitted by this service.
> 403 Forbidden (De-Registration) Received | The total current number of 403 Forbidden responses to de-registration received on this service.
> 403 Forbidden (De-Registration) Transmitted | The total current number of 403 Forbidden responses to de-registration transmitted by this service.
> 404 Not Found (De-Registration) Received | The total current number of 404 Not Found responses to de-registration received on this service.
> 404 Not Found (De-Registration) Transmitted | The total current number of 404 Not Found responses to de-registration transmitted by this service.
> 420 Bad Extension (De-Registration) Received | The total current number of 420 Bad Extension responses to de-registration received on this service.
> 420 Bad Extension (De-Registration) Transmitted | The total current number of 420 Bad Extension responses to de-registration transmitted by this service.
> 439 First HopLackOb (De-Registration) Received | The total current number of 439 First Hop Lack Outbound responses to de-registration received on this service.
> 439 First HopLackOb (De-Registration) Transmitted | The total current number of 439 First Hop Lack Outbound responses to de-registration transmitted by this service.
> 4xx Responses (De-Registration) Received | The total current number of 4xx responses to de-registration received on this service.
> 4xx Responses (De-Registration) Transmitted | The total current number of 4xx responses to de-registration transmitted by this service.
> 500 Internal Error (De-Registration) Received | The total current number of 500 Internal Error responses to de-registration received on this service.
> 500 Internal Error (De-Registration) Transmitted | The total current number of 500 Internal Error responses to de-registration transmitted by this service.
> 5xx Responses (Re-Registration) Received | The total current number of 5xx responses to de-registration received on this service.
> 5xx Responses (De-Registration) Transmitted | The total current number of 5xx responses to de-registration transmitted by this service.
> 6xx Responses (De-Registration) Received | The total current number of 6xx responses to de-registration received on this service.
> 6xx Responses (De-Registration) Transmitted | The total current number of 6xx responses to de-registration transmitted by this service.
> Unclassified Requests (Registration) Received | The total current number of unclassified request responses to registration received on this service.
> 4XX Responses (Unclassified Requests) Transmitted | The total current number of 4XX responses (Unclassified Requests) transmitted by this service.
> 5XX Responses (Unclassified Requests) Transmitted | The total current number of 5XX Responses (Unclassified Requests) transmitted by this service.
> IP-Security Statistics
> Total Secure Connection | The total number of subscribers with secure connections on this service.
> Total Unsecure Connection | The total number of subscribers with unsecure connections on this service.
> Total Security Association Rejects | The total number of security association rejections on this service.
> Total Secure Registrations | The total number of secure registrations on this service.
> Total Secure Re-registrations | The total number of secure re-registrations on this service.
> Total Secure De-registrations | The total number of secure de-registrations on this service.
> Total Failed Secure Registrations | The total number of failed secure registrations on this service.
> Total IP-Sec Packets Received | The total number of IPSec packets received on this service.
> Total IP-Sec Packets Transmitted | The total number of IPSec packets transmitted by this service.
> Total IP-Sec Octets Received | The total number of IPSec octets received on this service.
> Total IP-Sec Octets Transmitted | The total number of IPSec octets transmitted by this service.
> Total Registration Rejects Due to Sec-Agree | The total number of registration rejections due to security agreement on this service.
> Total Registration Rejects Due to Algorithm Mismatch | The total number of registration rejections due to algorithm mismatch on this service.
> Total Messages Dropped Due to Error | The total number of messages dropped due to error on this service.
> Total Messages With Incorrect Security Verify | The total number of messages with incorrect security verification on this service.
> Others
> Current CSCF Sessions | The number of currently active CSCF sessions existing on this service.
> Total CSCF Sessions | Total number of CSCF sessions created so far for originating/proxying SIP messages. This counter should not include CSCF sessions created for internal processing, like ROUTE REQUEST. Also, this counter should not get incremented for REGISTER requests received by S-CSCF as it acts as registrar and S-CSCF callleg itself can handle this.
> Current TCP Connections | The number of currently active TCP connections existing on this service.
> Current IPsec TCP Connections | The number of currently active IPSec TCP connections existing on this service.
> SigComp Statistics
> Total Requests Compressed | The total number of SIP request messages compressed by this service.
> Total Requests Decompressed | The total number of SIP request messages decompressed by this service.
> Total Responses Compressed | The total number of SIP response messages compressed by this service.
> Total Responses Decompressed | The total number of SIP response messages decompressed by this service.
> Total NACK Packets Received | The total number of NACK (negative acknowledgement) packets received by this service.
> Total NACK Packets Transmitted | The total number of NACK (negative acknowledgement) packets transmitted by this service.
> Total Compression Failures | The current total number of compression failures that occurred in this service.
> Total Decompression Failures | The current total number of decompression failures that occurred in this service.
> SigComp Effectiveness Ratio results in this section are derived using the following formula: (Sb - Sa)*100/(Sb) where Sb = the size of the message before compression and Sa = the size of the message after compression.
> Best compression ratio (Outgoing message) | The current best compression ratio achieved for messages sent by this service.
> Worst compression ratio (Outgoing message) | The current worst compression ratio achieved for messages sent by this service. Usually this will be a negative value indicating that the message had expanded instead of compressed.
> Average compression ratio (Outgoing message) | The running average compression of messages sent by this service. The average is derived using the following formula: (S(Sb) - S(Sa))*100/(S(Sb)).
> Best compression ratio (Incoming message) | The current best compression ratio achieved for messages received by this service.
> Worst compression ratio (Incoming message) | The current worst compression ratio achieved for messages received by this service. Usually this will be a negative value indicating that the message had expanded instead of compressed.
> Average compression ratio (Incoming message) | The running average compression of messages received by this service. The average is derived using the following formula: (S(Sb) - S(Sa))*100/(S(Sb)).
> SIP TCP Connection Statistics
> Active Connections | The total number of active TCP connections on this service.
> Total Connections Closed | The total number of TCP connections closed on this service.
> Total Successful Outgoing Connections | The total number of successful outgoing TCP connections on this service.
> Total Failed Outgoing Connections | The total number of failed outgoing TCP connections on this service.
> Total Successful Incoming Connections | The total number of successful incoming TCP connections on this service.
> Total Failed Incoming Connections | The total number of failed incoming TCP connections on this service.
> Total Migrated Connections | The total number of TCP conenctions migrated from Cscfmgr to Sessmgr for load balancing.
> Total Packets Sent | The total number of TCP/IP packets transmitted by CSCF service.
> Total Packets Received | The total number of TCP/IP packets received by CSCF service.
> Total Bytes Sent | The total number of bytes transmitted.
> Total Bytes Received | The total number of bytes received.
> Subscription Package
> Subscription Attempts Received | The total current number of subscription attempts received on this service.
> Subscription Attempts Transmitted | The total current number of subscription attempts transmitted by this service.
> Subscription Success Received | The total current number of subscription successes received on this service.
> Subscription Success Transmitted | The total current number of subscription successes transmitted by this service.
> Subscription Failures Received | The total current number of subscription failures received on this service.
> Subscription Failures Transmitted | The total current number of subscription failures transmitted by this service.
> 200 OK (Subscription) Received | The total current number of 200 OK responses to registration received on this service.
> 200 OK (Subscription) Transmitted | The total current number of 200 OK responses to registration transmitted by this service.
> 202 Accepted (Subscription) Received | The total current number of 202 Accepted responses to registration received on this service.
> 202 Accepted (Subscription) Transmitted | The total current number of 202 Accepted responses to registration transmitted by this service.
> 400 Bad Request (Subscription) Received | The total current number of 400 Bad Request responses to registration received on this service.
> 400 Bad Request (Subscription) Transmitted | The total current number of 400 Bad Request responses to registration transmitted by this service.
> 403 Forbidden (Subscription) Received | The total current number of 403 Forbidden responses to registration received on this service.
> 403 Forbidden (Subscription) Transmitted | The total current number of 403 Forbidden responses to registration transmitted by this service.
> 481 Trans Does Not Exist (Subscription) Received | The total current number of 481 Trans Does Not Exist responses to registration received on this service.
> 481 Trans Does Not Exist (Subscription) Transmitted | The total current number of 481 Trans Does Not Exist responses to registration transmitted by this service.
> 489 Bad Event (Subscription) Received | The total current number of 489 Bad Event responses to registration received on this service.
> 489 Bad Event (Subscription) Transmitted | The total current number of 489 Bad Event responses to registration transmitted by this service.
> 500 Internal Error (Subscription) Received | The total current number of 500 Internal Error responses to registration received on this service.
> 500 Internal Error (Subscription) Transmitted | The total current number of 500 Internal Error responses to registration transmitted by this service.
> Re-Subscription Attempts Received | The total current number of re-subscription attempts received on this service.
> Re-Subscription Attempts Transmitted | The total current number of re-subscription attempts transmitted by this service.
> Re-Subscription Success Received | The total current number of re-subscription successes received on this service.
> Re-Subscription Success Transmitted | The total current number of re-subscription successes transmitted by this service.
> Re-Subscription Failures Received | The total current number of re-subscription failures received on this service.
> Re-Subscription Failures Transmitted | The total current number of re-subscription failures transmitted by this service.
> 200 OK (Re-Subscription) Received | The total current number of 200 OK responses to re-registration received on this service.
> 200 OK (Re-Subscription) Transmitted | The total current number of 200 OK responses to re-registration transmitted by this service.
> 202 Accepted (Re-Subscription) Received | The total current number of 202 Accepted responses to re-registration received on this service.
> 202 Accepted (Re-Subscription) Transmitted | The total current number of 202 Accepted responses to re-registration transmitted by this service.
> 400 Bad Request (Re-Subscription) Received | The total current number of 400 Bad Request responses to re-registration received on this service.
> 400 Bad Request (Re-Subscription) Transmitted | The total current number of 400 Bad Request responses to re-registration transmitted by this service.
> 403 Forbidden (Re-Subscription) Received | The total current number of 403 Forbidden responses to re-registration received on this service.
> 403 Forbidden (Re-Subscription) Transmitted | The total current number of 403 Forbidden responses to re-registration transmitted by this service.
> 481 Trans Does Not Exist (Re-Subscription) Received | The total current number of 481 Trans Does Not Exist responses to re-registration received on this service.
> 481 Trans Does Not Exist (Re-Subscription) Transmitted | The total current number of 481 Trans Does Not Exist responses to re-registration transmitted by this service.
> 489 Bad Event (Re-Subscription) Received | The total current number of 489 Bad Event responses to re-registration received on this service.
> 489 Bad Event (Re-Subscription) Transmitted | The total current number of 489 Bad Event responses to re-registration transmitted by this service.
> 500 Internal Error (Re-Subscription) Received | The total current number of 500 Internal Error responses to re-registration received on this service.
> 500 Internal Error (Re-Subscription) Transmitted | The total current number of 500 Internal Error responses to re-registration transmitted by this service.
> Un-Subscription Attempts Received | The total current number of un-subscription attempts received on this service.
> Un-Subscription Attempts Transmitted | The total current number of un-subscription attempts transmitted by this service.
> Un-Subscription Success Received | The total current number of un-subscription successes received on this service.
> Un-Subscription Success Transmitted | The total current number of un-subscription successes transmitted by this service.
> Un-Subscription Failures Received | The total current number of un-subscription failures received on this service.
> Un-Subscription Failures Transmitted | The total current number of un-subscription failures transmitted by this service.
> 200 OK (Un-Subscription) Received | The total current number of 200 OK responses to un-registration received on this service.
> 200 OK (Un-Subscription) Transmitted | The total current number of 200 OK responses to un-registration transmitted by this service.
> 202 Accepted (Un-Subscription) Received | The total current number of 202 Accepted responses to un-registration received on this service.
> 202 Accepted (Un-Subscription) Transmitted | The total current number of 202 Accepted responses to un-registration transmitted by this service.
> 400 Bad Request (Un-Subscription) Received | The total current number of 400 Bad Request responses to un-registration received on this service.
> 400 Bad Request (Un-Subscription) Transmitted | The total current number of 400 Bad Request responses to un-registration transmitted by this service.
> 403 Forbidden (Un-Subscription) Received | The total current number of 403 Forbidden responses to un-registration received on this service.
> 403 Forbidden (Un-Subscription) Transmitted | The total current number of 403 Forbidden responses to un-registration transmitted by this service.
> 481 Trans Does Not Exist (Un-Subscription) Received | The total current number of 481 Trans Does Not Exist responses to un-registration received on this service.
> 481 Trans Does Not Exist (Un-Subscription) Transmitted | The total current number of 481 Trans Does Not Exist responses to un-registration transmitted by this service.
> 489 Bad Event (Un-Subscription) Received | The total current number of 489 Bad Event responses to un-registration received on this service.
> 489 Bad Event (Un-Subscription) Transmitted | The total current number of 489 Bad Event responses to un-registration transmitted by this service.
> 500 Internal Error (Un-Subscription) Received | The total current number of 500 Internal Error responses to un-registration received on this service.
> 500 Internal Error (Un-Subscription) Transmitted | The total current number of 500 Internal Error responses to un-registration transmitted by this service.
> Notify Attempts Received | The total current number of notify attempts received on this service.
> Notify Attempts Transmitted | The total current number of notify attempts transmitted by this service.
> Notify Success Received | The total current number of notify successes received on this service.
> Notify Success Transmitted | The total current number of notify successes transmitted by this service.
> Notify Failures Received | The total current number of notify failures received on this service.
> Notify Failures Transmitted | The total current number of notify failures transmitted by this service.
> Publish Attempts Received | The total current number of publish attempts received on this service.
> Publish Attempts Transmitted | The total current number of publish attempts transmitted by this service.
> Publish Success Received | The total current number of publish successes received on this service.
> Publish Success Transmitted | The total current number of publish successes transmitted by this service.
> Publish Failures Received | The total current number of publish failures received on this service.
> Publish Failures Transmitted | The total current number of publish failures transmitted by this service.
> Un-Publish Attempts Received | The total current number of un-publish attempts received on this service.
> Un-Publish Attempts Transmitted | The total current number of un-publish attempts transmitted by this service.
> Un-Publish Success Received | The total current number of un-publish successes received on this service.
> Un-Publish Success Transmitted | The total current number of un-publish successes transmitted by this service.
> Un-Publish Failures Received | The total current number of un-publish failures received on this service.
> Un-Publish Failures Transmitted | The total current number of un-publish failures transmitted by this service.
> TCP Connection Statistics
> Active IP-Sec Connections | The total number of active IPSec TCP connections on this service.
> Total IP-Sec Connections Closed | The total number of IPSec TCP connections closed on this service.
> Total Successful IP-Sec Outgoing Connections | The total number of successful outgoing IPSec TCP connections on this service.
> Total Failed IP-Sec Outgoing Connections | The total number of failed outgoing IPSec TCP connections on this service.
> Total Successful IP-Sec Incoming Connections | The total number of successful incoming IPSec TCP connections on this service.
> Total Failed IP-Sec Incoming Connections | The total number of failed incoming IPSec TCP connections on this service.

> ‌
> show cscf sessions counters
> show cscf sessions counters Command Output Descriptions

> Field | Description
> Interval
> <200ms | The number of sessions that had a duration of less than 200 millisecond.
> 200..400ms | The number of sessions that had a duration between 200 and 400 milliseconds.
> 400..600ms | The number of sessions that had a duration between 400 and 600 milliseconds.
> 600..800ms | The number of sessions that had a duration between 600 and 800 milliseconds.
> 800..1000ms | The number of sessions that had a duration between 800 and 1000 milliseconds.
> 1000..1200ms | The number of sessions that had a duration between 1000 and 1200 milliseconds.
> 1200..1400ms | The number of sessions that had a duration between 1200 and 1400 milliseconds.
> 1400..1600ms | The number of sessions that had a duration between 1400 and 1600 milliseconds.
> 1600..1800ms | The number of sessions that had a duration between 1600 and 1800 milliseconds.
> 1800..2000ms | The number of sessions that had a duration between 1800 and 2000 milliseconds.
> 2000..2200ms | The number of sessions that had a duration between 2000 and 2200 milliseconds.
> 2200..2400ms | The number of sessions that had a duration between 2200 and 2400 milliseconds.
> 2400..2600ms | The number of sessions that had a duration between 2400 and 2600 milliseconds.
> 2600..2800ms | The number of sessions that had a duration between 2600 and 2800 milliseconds.
> 2800..3000ms | The number of sessions that had a duration between 2800 and 3000 milliseconds.
> 3..5sec | The number of sessions that had a duration between three and five seconds.
> 5..7sec | The number of sessions that had a duration between five and seven seconds.
> 7..9sec | The number of sessions that had a duration between seven and nine seconds.
> 9..11sec | The number of sessions that had a duration between nine and 11 seconds.
> 11..13sec | The number of sessions that had a duration between 11 and 13 seconds.
> 13..15sec | The number of sessions that had a duration between 13 and 15 seconds.
> 15..17sec | The number of sessions that had a duration between 15 and 17 seconds.
> 17..19sec | The number of sessions that had a duration between 17 and 19 seconds.
> 19..21sec | The number of sessions that had a duration between 19 and 21 seconds.
> >21sec | The number of sessions that had a duration of more than 21 seconds.
> Count The following provide total counts for each session type per specified interval.
> Invite Processing Time | Time required to process an INVITE message (time elapsed between the INVITE entering the proxy and the INVITE forwarded out of the proxy).
> First Response Delay | Time between sending an INVITE message out of the proxy and the first response received for the INVITE (any 1xx).
> Post Dial Delay | Time between sending an INVITE message out of the proxy and receiving the ringing message or any final response to the INVITE.
> Session Setup Delay | Time between when an INVITE message was received by the proxy and a 200 OK (invite) sent out of the proxy.
> Post Answer Delay | Time between a 200 OK INVITE message received by the proxy and the ACK message (for invite) sent out of the proxy.
> Session Release Delay | Time between when a BYE message is received by the proxy and a 200 OK BYE is sent out of the proxy.

> ‌
> show cscf sessions duration
> show cscf sessions duration Command Output Descriptions

> Field | Description
> <1s | The number of sessions that had a duration of less than one second.
> 01..10sec | The number of sessions that had a duration between one and 10 seconds.
> 10..30sec | The number of sessions that had a duration between 10 and 30 seconds.
> 30..60sec | The number of sessions that had a duration between 30 and 60 seconds.
> 01..03min | The number of sessions that had a duration between one and three minutes.
> 03..05min | The number of sessions that had a duration between three and five minutes.
> 05..07min | The number of sessions that had a duration between five and seven minutes.
> 07..09min | The number of sessions that had a duration between seven and nine minutes.
> 09..11min | The number of sessions that had a duration between nine and 11 minutes.
> 11..13min | The number of sessions that had a duration between 11 and 13 minutes.
> 13..15min | The number of sessions that had a duration between 13 and 15 minutes.
> 15..17min | The number of sessions that had a duration between 15 and 17 minutes.
> 17..19min | The number of sessions that had a duration between 17 and 19 minutes.
> 19..21min | The number of sessions that had a duration between 19 and 21 minutes.
> 21..23min | The number of sessions that had a duration between 21 and 23 minutes.
> 23..25min | The number of sessions that had a duration between 23 and 25 minutes.
> 25..27min | The number of sessions that had a duration between 25 and 27 minutes.
> 27..29min | The number of sessions that had a duration between 27 and 29 minutes.
> 29..60min | The number of sessions that had a duration between 29 and 60 minutes.
> >60min | The number of sessions that had a duration of more than 60 minutes.
> <1hr | The number of sessions that had a duration of less than one hour.
> 1..2hrs | The number of sessions that had a duration between one and two hours.
> 2..3hrs | The number of sessions that had a duration between two and three hours.
> 3..4hrs | The number of sessions that had a duration between three and four hours.
> 4..5hrs | The number of sessions that had a duration between four and five hours.
> 5..6hrs | The number of sessions that had a duration between five and six hours.
> 6..7hrs | The number of sessions that had a duration between six and seven hours.
> 7..8hrs | The number of sessions that had a duration between seven and eight hours.
> 8..9hrs | The number of sessions that had a duration between eight and nine hours.
> 9..10hrs | The number of sessions that had a duration between nine and 10 hours.
> >10hrs | The number of sessions that had a duration of more than 10 hours.

> ‌
> show cscf sip statistics
> show cscf sip statistics Command Output Descriptions

> Field | Description
> CSCF Service | The name of the service and context.
> Peer IP Address | The IP address of the peer server expressed in IPv4 or IPv6 dotted decimal notation.
> SIP Request Statistics
> Register | The total number of SIP Register requests received (Rx) or transmitted (Tx) by this service.
> Invite | The total number of INVITE requests received (Rx) or transmitted (Tx) by this service.
> Ack | The total number of ACK requests received (Rx) or transmitted (Tx) by this service.
> Bye | The total number of Bye requests received (Rx) or transmitted (Tx) by this service.
> Info | The total number of Info requests received (Rx) or transmitted (Tx) by this service.
> Prack | The total number of PRACK requests received (Rx) or transmitted (Tx) by this service.
> Refer | The total number of Refer requests received (Rx) or transmitted (Tx) by this service.
> Cancel | The total number of Cancel requests received (Rx) or transmitted (Tx) by this service.
> Notify | The total number of Notify requests received (Rx) or transmitted (Tx) by this service.
> Update | The total number of Update requests received (Rx) or transmitted (Tx) by this service.
> Message | The total number of Message requests received (Rx) or transmitted (Tx) by this service.
> Options | The total number of Options requests received (Rx) or transmitted (Tx) by this service.
> Publish | The total number of Publish requests received (Rx) or transmitted (Tx) by this service.
> Subscribe | The total number of Subscribe requests received (Rx) or transmitted (Tx) by this service.
> Notify | The total number of Notify requests received (Rx) or transmitted (Tx) by this service.
> SIP Response Statistics
> 100 Trying | The total number of 100 Trying responses received (Rx) or transmitted (Tx) by this service.
> 180 Ringing | The total number of 180 Ringing responses received (Rx) or transmitted (Tx) by this service.
> 181 Forwarding | The total number of 181 Forwarded responses received (Rx) or transmitted (Tx) by this service.
> 182 Queued | The total number of 182 Queued responses received (Rx) or transmitted (Tx) by this service.
> 183 Progress | The total number of 183 Progress responses received (Rx) or transmitted (Tx) by this service.
> 200 Ok (Register) | The total number of 200 OK Register responses received (Rx) or transmitted (Tx) by this service.
> 200 Ok (Invite) | The total number of 200 OK Invite responses received (Rx) or transmitted (Tx) by this service.
> 200 Ok (Bye) | The total number of 200 OK Bye responses received (Rx) or transmitted (Tx) by this service.
> 200 Ok (Info) | The total number of 200 OK Info responses received (Rx) or transmitted (Tx) by this service.
> 200 Ok (Prack) | The total number of 200 OK PRACK responses received (Rx) or transmitted (Tx) by this service.
> 200 Ok (Refer) | The total number of 200 OK Refer responses received (Rx) or transmitted (Tx) by this service.
> 200 Ok (Cancel) | The total number of 200 OK Cancel responses received (Rx) or transmitted (Tx) by this service.
> 200 Ok (Notify) | The total number of 200 OK Notify responses received (Rx) or transmitted (Tx) by this service.
> 200 Ok (Update) | The total number of 200 OK Update responses received (Rx) or transmitted (Tx) by this service.
> 200 Ok (Message) | The total number of 200 OK Message responses received (Rx) or transmitted (Tx) by this service.
> 200 Ok (Options) | The total number of 200 OK Options responses received (Rx) or transmitted (Tx) by this service.
> 200 Ok (Publish) | The total number of 200 OK Publish responses received (Rx) or transmitted (Tx) by this service.
> 200 Ok (Subscribe) | The total number of 200 OK Subscribe responses received (Rx) or transmitted (Tx) by this service.
> 202 Accepted (Refer) | The total number of 202 Accepted Refer responses received (Rx) or transmitted (Tx) by this service.
> 202 Accepted (Subscribe) | The total number of 202 Accepted Subscribe responses received (Rx) or transmitted (Tx) by this service.
> 300 Multiple Choices | The total number of Multiple Choices responses received (Rx) or transmitted (Tx) by this service.
> 301 Moved Permanently | The total number of Moved Permanently responses received (Rx) or transmitted (Tx) by this service.
> 302 Moved Temporarily | The total number of Moved Temporarily responses received (Rx) or transmitted (Tx) by this service.
> 305 Use Proxy | The total number of Use Proxy responses received (Rx) or transmitted (Tx) by this service.
> 380 Alternative Service | The total number of Alternative Service responses received (Rx) or transmitted (Tx) by this service.
> 400 Bad Request | The total number of 400 Bad Request errors received (Rx) or transmitted (Tx) by this service.
> 401 Unauthorized | The total number of 401 Unauthorized errors received (Rx) or transmitted (Tx) by this service.
> 403 Forbidden | The total number of 403 Forbidden errors received (Rx) or transmitted (Tx) by this service.
> 404 Not Found | The total number of 404 Not Found errors received (Rx) or transmitted (Tx) by this service.
> 405 Method Not Allowed | The total number of 405 Method Not Allowed errors received (Rx) or transmitted (Tx) by this service.
> 406 Not Acceptable | The total number of 406 Not Acceptable errors received (Rx) or transmitted (Tx) by this service.
> 407 Proxy Auth Required | The total number of 407 Proxy Auth Required errors received (Rx) or transmitted (Tx) by this service.
> 408 Request Timeout | The total number of 408 Request Timeout errors received (Rx) or transmitted (Tx) by this service.
> 410 Gone | The total number of 410 Gone errors received (Rx) or transmitted (Tx) by this service.
> 412 Conditional Req Fail | The total number of 412 Conditional Request Fail errors received (Rx) or transmitted (Tx) by this service.
> 413 Req Entity Too Large | The total number of 413 Request Entity Too Large errors received (Rx) or transmitted (Tx) by this service.
> 414 Req URI Too Long | The total number of 414 Request URI Too Long errors received (Rx) or transmitted (Tx) by this service.
> 415 Unsupport Media Type | The total number of 415 Unsupported Media Type errors received (Rx) or transmitted (Tx) by this service.
> 416 Unsupport URI Scheme | The total number of 416 Unsupported URI Scheme errors received (Rx) or transmitted (Tx) by this service.
> 420 Bad Extension | The total number of 420 Bad Extension errors received (Rx) or transmitted (Tx) by this service.
> 421 Extension Required | The total number of 421 Extension Required errors received (Rx) or transmitted (Tx) by this service.
> 423 Interval Too Brief | The total number of 423 Interval Too Brief errors received (Rx) or transmitted (Tx) by this service.
> 480 Temp Not Available | The total number of 480 Temp Not Available errors received (Rx) or transmitted (Tx) by this service.
> 481 Trans Does Not Exist | The total number of 481 Transaction Does Not Exist errors received (Rx) or transmitted (Tx) by this service.
> 482 Loop Detected | The total number of 482 Loop Detected errors received (Rx) or transmitted (Tx) by this service.
> 483 Too Many Hops | The total number of 483 Too Many Hops errors received (Rx) or transmitted (Tx) by this service.
> 484 Address Incomplete | The total number of 484 Address Incomplete errors received (Rx) or transmitted (Tx) by this service.
> 485 Ambiguous | The total number of 485 Ambiguous errors received (Rx) or transmitted (Tx) by this service.
> 486 Busy Here | The total number of 486 Busy Here errors received (Rx) or transmitted (Tx) by this service.
> 487 Request Cancel | The total number of 487 Request Cancel errors received (Rx) or transmitted (Tx) by this service.
> 488 Not Acceptable Media | The total number of 488 Not Acceptable Media errors received (Rx) or transmitted (Tx) by this service.
> 489 Bad Event | The total number of 489 Bad Event errors received (Rx) or transmitted (Tx) by this service.
> 491 Request Pending | The total number of 491 Request Pending errors received (Rx) or transmitted (Tx) by this service.
> 493 Undecipherable | The total number of 493 Undecipherable errors received (Rx) or transmitted (Tx) by this service.
> 500 Internal Error | The total number of 500 Internal Error errors received (Rx) or transmitted (Tx) by this service.
> 501 Not Implemented | The total number of 501 Not Implemented errors received (Rx) or transmitted (Tx) by this service.
> 502 Bad Gateway | The total number of 502 Bad Gateway errors received (Rx) or transmitted (Tx) by this service.
> 503 Service Unavailable | The total number of 503 Service Unavailable errors received (Rx) or transmitted (Tx) by this service.
> 504 Gateway Timeout | The total number of 504 Gateway Timeout errors received (Rx) or transmitted (Tx) by this service.
> 505 Bad SIP Version | The total number of 505 Bad SIP Version errors received (Rx) or transmitted (Tx) by this service.
> 513 Message Too Large | The total number of 513 Message Too Large errors received (Rx) or transmitted (Tx) by this service.
> 580 Precondition Failure | The total number of 580 Precondition Failure errors received (Rx) or transmitted (Tx) by this service.
> 600 Busy Everywhere | The total number of 600 Busy Everywhere errors received (Rx) or transmitted (Tx) by this service.
> 603 Decline | The total number of 603 Decline errors received (Rx) or transmitted (Tx) by this service.
> 604 Not Exist Anywhere | The total number of 604 Not Exist Anywhere errors received (Rx) or transmitted (Tx) by this service.
> 606 Not Acceptable | The total number of 606 Not Acceptable errors received (Rx) or transmitted (Tx) by this service.
> Total Invalid Messages | The total number of SIP Invalid Messages received (Rx) or transmitted (Tx) by this service.
> Total Messages | The total number of SIP Messages received (Rx) or transmitted (Tx) by this service.
> TCP Request | The total number of SIP requests received (Rx) or transmitted (Tx) over TCP by this service.
> TCP Response | The total number of SIP responses received (Rx) or transmitted (Tx) over TCP by this service.
> Auto switch to TCP on MTU size limit | The total number of times CSCF switched from UDP to TCP because of message size larger than MTU.

> ‌
> show cscf tcp connections
> show cscf tcp connections Command Output Descriptions

> Field | Description
> TCP Connection Details
> LocalIp | The local IP address, expressed in IPv4 or IPv6 dotted decimal notation, of the TCP connection.
> Local Port | The local port number of the TCP connection.
> RemoteIp | The remote IP address, expressed in IPv4 or IPv6 dotted decimal notation, of the TCP connection.
> Remote Port | The remote port number of the TCP connection.
> Facility | Facility type for which connection details have to be retrieved—CscfMgr or SessMgr.
> Instance | The instance number of the facility that the connection belongs to.
> SockDesc | The socket descriptor id.
> State | The state of the connection. TCP states are:
> • | CLOSED
> • | LISTEN
> • | SYNCSENT
> • | SYNCRCVD
> • | ESTABLISHED
> • | CLOSEWAIT
> • | FINWAIT1
> • | CLOSING
> • | LASTACK
> • | FINWAIT2
> • | TIMEWAIT
> • | INVALID
> BytesInRecvQueue | Data size in the receive queue, in bytes.
> BytesInSendQueue | Data size in the send queue, in bytes.
> RecvQueueSize | Size of the receive queue, in bytes.
> SendQueueSize | Size of the send queue, in bytes.
> MaxSendWind | Maximum send window seen so far.
> SndUna | Send unacknowledged sequence value.
> SndNext | Send next sequence value.
> MaxSndNext | Highest sequence number sent.
> Iss | Initial send sequence number.
> Irs | Initial receive sequence number.
> Rto | Retransmission timeout.
> SndWL1 | Send segment sequence number used for last window update.
> SndWL2 | Send segment acknowledgment number used for last window update.
> MaxSndWind | Maximum send window seen so far.
> RecvNxt | Receive next sequence.
> RecvWind | Receive window sequence.
> RecvAdv | Sequence number of right edge of advertised window.
> CWind | Send congestion window.
> Ssthresh | Send slow start threshold size.
> BackLog | Back logs.
> DupAck | Duplicate ACKs.
> RetransSegments | Number of retransmitted segments.
> AckAfterRetrans | Number of non duplicate acks after duplicate ACK.
> TcpFlags | TCP flags.
> Total TCP sockets | The total number of TCP sockets.

> ‌

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883