> Safety, Electrical, and Environmental Certifications
> Federal Communications Commission Warning
> The ASR 5000 complies with the limits for a Class A digital device, pursuant to Part 15 of the FCC Rules and Regulations. Operation is subject to the following two conditions:

> • | This device must not cause harmful interference.

> • | This device must withstand any interference received, including interference that may cause undesired operation.

> These limits provide reasonable protection against harmful interference when this equipment is operated in a commercial environment. This equipment generates, uses, and can radiate radio-frequency energy and, if not installed and used in accordance with the instruction manual, may cause harmful interference to radio and television communications. Operation of this equipment in a residential area is likely to cause interference, in which case your organization is responsible for the expenses incurred to correct the interference.
> ICS Notice
> This Class A digital apparatus complies with Canadian ICES-003.
> Cet appareil numérique de la classe A est conforme à la norme NMB-003 du Canada.
> Laser Notice
> The lasers in this equipment are Class 1 devices. Class 1 laser devices are not considered to be hazardous.
> Safety Certifications
> The ASR 5000 complies with all safety certifications listed below.

> • | UL60950 - Standard for Safety for Information Technology Equipment, 3rd Edition

> • | European Union EN 60950 (CE Mark)

> Electrical Certifications
> The ASR 5000 complies with all electrical certifications listed below.

> • | Telcordia GR-1089-Core, Network Equipment-Building System (NEBS) Requirements: Electromagnetic Compatibility and Electrical Safety Criteria for Network Telecommunication Equipment

> • | FCC, Part 15 B, Class A Requirements for Non-residential Equipment

> • | ETSI EN 300 019

> • | ETSI 300 386

> • | ETSI/EN 300 386-2 Electrical Fast Transients

> • | SBC TP76200MP

> • | Taiwan - BMSI

> Environmental Certifications
> The ASR 5000 complies with all environmental certifications listed below.

> • | Telcordia GR-63-Core, Network Equipment-Building System (NEBS) Requirements: Physical Protection

> • | The chassis equipped with the 165A PFU is compliant to the European Union’s RoHS Directive (Directive 2002/95/EC)

> • | Waste Electrical and Electronic Equipment (WEEE) Directive 2002/96/EC

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883