# HSGW Schema Statistics

The HSGW schema provides operational statistics that can be used for monitoring and troubleshooting the following products: HSGW
This schema provides the following types of statistics:

- Counter: A counter records incremental data cumulatively and rolls over when the counter limit is reached. All counter statistics are cumulative and reset only by one of the following methods: roll-over when limit is reached, after a system restart, or after a clear command is performed. The limit depends upon the data type.
- Gauge: A gauge statistic indicates a single value; a snapshot representation of a single point in time within a defined time frame. The gauge changes to a new value with each snapshot though a value may repeat from one period to the next. The limit depends upon the data type.
- Information: This type of statistic provides information, often intended to differentiate sets of statistics; for example, a VPN name or IP address. The type of information provided depends upon the data type.

The data type defines the format of the data for the value provided by the statistic. The following data types are used in statistics for this schema:

- Int32/Int64: An integer, either 32-bit or 64-bit: For statistics with the Int32 data type, the roll-over to zero limit is 4,294,967,295. For statistics with the Int64 data type, the roll-over to zero limit is 18,446,744,073,709,551,615.
- Float: A numeric value that can be represented fractionally; for example, 1.345.
- String: A series of ASCII alphanumeric characters in a single grouping, usually pre-configured.

IMPORTANT:

Unless otherwise indicated, all statistics are counters and all statistics are standards-based.

Key Variables: Every schema has some variables which are typically referred to as 'key variables'. These key variables provide index markers to identify which object the statistics apply to. For example, in the card schema, the card number (variable %card%) uniquely identifies a card. For an HA service, the keys would be "%vpnname%" plus "%servname%", as the combination uniquely identifies an HA service. So, in a given measurement interval, one row of statistics will be generated per unique key. The schema keys are identified in the Description section of the table.
Table 1. Bulk Statistic Variables in the HSGW Schema

Variables | Description | Data Type
--- | --- | ---
vpnname | The name of the context configured on the system that is currently facilitating the HSGW service. This is a key variable. | String
vpnid | The identification number of the context configured on the system that is currently facilitating the HSGW service. This is an internal reference number. This is a key variable. Type: Gauge | Int32
servname | Displays the name of the HSGW service for which the statistics are displayed. This is a key variable. | String
servid | The identification number of the service configured on the system that is currently facilitating the HSGW service. This is an internal reference number. This is a key variable. Type: Gauge | Int32
sessstat-totcur-ue | Session Statistics - Total Current - UE Active Type: Gauge | Int32
sessstat-totcur-pdn | Session Statistics - Total Current - PDN Type: Gauge | Int32
sessstat-totcur-bearers | Session Statistics - Total Current - Bearers Type: Gauge | Int32
sessstat-totsetup-ue | Session Statistics - Total Setup - UE | Int32
sessstat-totsetup-pdn | Session Statistics - Total Setup - PDN | Int32
sessstat-totsetup-bearers | Session Statistics - Total Setup - Bearers | Int32
sessstat-pdnsetuptype-ipv4 | Session Statistics - Total PDNs Setup Per PDN-type - IPv4 | Int32
sessstat-pdnsetuptype-ipv4v6 | Session Statistics - Total PDNs Setup Per PDN-type - IPv4v6 | Int32
sessstat-pdnrel-ipv4 | Session Statistics - Total PDNs Released - IPv4Ctr32Servicesessstat | Int32
sessstat-pdnrel-ipv6 | Session Statistics - Total PDNs Released - IPv6 | Int32
sessstat-pdnrel-ipv4v6 | Session Statistics - Total PDNs Released - IPv4v6 | Int32
sessstat-pdnrelrsn-pcf | Session Statistics - Total PDNs Released Reason - PCFMME Ini | Int32
sessstat-pdnrelrsn-pgw | Session Statistics - Total PDNs Released Reason -PGW Ini | Int32
sessstat-pdnrelrsn-pcrf | Session Statistics - Total PDNs Released Reason -PCRF Ini | Int32
sessstat-pdnrelrsn-local | Session Statistics - Total PDNs Released Reason -Local | Int32
sessstat-pdnrelrsn-other | Session Statistics - Total PDNs Released Reason -Other | Int32
sessstat-pdnrej-ipv4 | Session Statistics - Total PDNs Rejected - IPv4 | Int32
sessstat-pdnrej-ipv6 | Session Statistics - Total PDNs Rejected - IPv6 | Int32
sessstat-pdnrej-ipv4v6 | Session Statistics - Total PDNs Rejected - IPv4v6 | Int32
sessstat-pdnrejrsn-pgw | Session Statistics - Total PDNs Rejected Reason - PGW Reject | Int32
sessstat-pdnrejrsn-apnauth | Session Statistics - Total PDNs Rejected Reason - APN Auth FailureLicense | Int32
sessstat-pdnrejrsn-other | Session Statistics - Total PDNs Rejected Reason - OtherNewcall Policy | Int32
sessstat-pdnrejrsn-pgwrej | Session Statistics - Total PDNs Rejected Reason - No PGW AvailableOverload | Int32
sessstat-pdnrejrsn-pdnexists | Session Statistics - Total PDNs Rejected Reason - PDN Already ExisCongestion | Int32
sessstat-pdnrejrsn-adminrej | Session Statistics - Total PDNs Rejected Reason - Admin Prohibited | Int32
sessstat-pdnrejrsn-limitexceed | Session Statistics - Total PDNs Rejected Reason - PDN Limit ExceededOther | Int32
sessstat-pdnrejrsn-unreach | Session Statistics - Total PDNs Rejected Reason - PDN GW Unreachable | Int32
sessstat-pdnrejrsn-rscunavail | Session Statistics - Total PDNs Rejected Reason - Resource Unavailable | Int32
sessstat-pdnrejrsn-sublimit | Session Statistics - Total PDNs Rejected Reason - Subscription Limitation | Int32
sessstat-totinter-ho | Session Statistics - HandOff Statistics - Total Inter HSGW HO | Int32
sessstat-totintra-ho | Session Statistics - HandOff Statistics - Total Intra HSGW HO | Int32
sessstat-active | Session Statistics - HandOff Statistics - Active | Int32
sessstat-dormant | Session Statistics - HandOff Statistics - Dormant | Int32
sessstat-a10s-totcur | Session Statistics - A10 Statistics - Total A10s Current | Int32
sessstat-a10s-maincur | Session Statistics - A10 Statistics - Main A10s Current | Int32
sessstat-a10s-auxcur | Session Statistics - A10 Statistics - Aux A10s Current | Int32
sessstat-a10s-totsetup | Session Statistics - A10 Statistics - Total A10s Setup | Int32
sessstat-a10s-mainsetup | Session Statistics - A10 Statistics - Main A10s Setup | Int32
sessstat-a10s-auxsetup | Session Statistics - A10 Statistics - Aux A10s Setup | Int32
sessstat-a10s-totrel | Session Statistics - A10 Statistics - Total A10s Released | Int32
sessstat-a10s-mainrel | Session Statistics - A10 Statistics - Main A10s Released | Int32
sessstat-a10s-auxrel | Session Statistics - A10 Statistics - Aux A10s Released | Int32
totepsbearsetup-qci1 | Total EPS Bearers Setup - QCI 1 | Int32
totepsbearsetup-qci2 | Total EPS Bearers Setup - QCI 2 | Int32
totepsbearsetup-qci3 | Total EPS Bearers Setup - QCI 3 | Int32
totepsbearsetup-qci4 | Total EPS Bearers Setup - QCI 4 | Int32
totepsbearsetup-qci5 | Total EPS Bearers Setup - QCI 5 | Int32
totepsbearsetup-qci6 | Total EPS Bearers Setup - QCI 6 | Int32
totepsbearsetup-qci7 | Total EPS Bearers Setup - QCI 7 | Int32
totepsbearsetup-qci8 | Total EPS Bearers Setup - QCI 8 | Int32
totepsbearsetup-qci9 | Total EPS Bearers Setup - QCI 9 | Int32
totepsbearsetup-other | Total EPS Bearers Setup - Other | Int32
totepsbearrel-qci1 | Total EPS Bearers Released - QCI 1 | Int32
totepsbearrel-qci2 | Total EPS Bearers Released - QCI 2 | Int32
totepsbearrel-qci3 | Total EPS Bearers Released - QCI 3 | Int32
totepsbearrel-qci4 | Total EPS Bearers Released - QCI 4 | Int32
totepsbearrel-qci5 | Total EPS Bearers Released - QCI 5 | Int32
totepsbearrel-qci6 | Total EPS Bearers Released - QCI 6 | Int32
totepsbearrel-qci7 | Total EPS Bearers Released - QCI 7 | Int32
totepsbearrel-qci8 | Total EPS Bearers Released - QCI 8 | Int32
totepsbearrel-qci9 | Total EPS Bearers Released - QCI 9 | Int32
totepsbearrel-other | Total EPS Bearers Released - Other | Int32
totepsbearmod-qci1 | Total EPS Bearers Modified - QCI 1 | Int32
totepsbearmod-qci2 | Total EPS Bearers Modified - QCI 2 | Int32
totepsbearmod-qci3 | Total EPS Bearers Modified - QCI 3 | Int32
totepsbearmod-qci4 | Total EPS Bearers Modified - QCI 4 | Int32
totepsbearmod-qci5 | Total EPS Bearers Modified - QCI 5 | Int32
totepsbearmod-qci6 | Total EPS Bearers Modified - QCI 6 | Int32
totepsbearmod-qci7 | Total EPS Bearers Modified - QCI 7 | Int32
totepsbearmod-qci8 | Total EPS Bearers Modified - QCI 8 | Int32
totepsbearmod-qci9 | Total EPS Bearers Modified - QCI 9 | Int32
totepsbearmod-other | Total EPS Bearers Modified - Other | Int32
totepsbearrelrsn-pgw | Total EPS Bearers Released - Total Dedicated Bearers Released Reason - PGW Ini | Int32
totepsbearrelrsn-pcrf | Total EPS Bearers Released - Total Dedicated Bearers Released Reason - PCRF Ini | Int32
totepsbearrelrsn-hsgw | Total EPS Bearers Released - Total Dedicated Bearers Released Reason - HSGW IniS1 Error Ind | Int32
totepsbearrelrsn-pdn | Total EPS Bearers Released - Total Dedicated Bearers Released Reason - PDN DownS5 Error Ind | Int32
totepsbearrelrsn-other | Total EPS Bearers Released - Total Dedicated Bearers Released Reason - Other | Int32
datastat-uplink-qci1totbyte | Data Statistics - Uplink Statistics - QCI 1 Total-Bytes | Int64
datastat-uplink-qci1totpkt | Data Statistics - Uplink Statistics - QCI 1 Total-Packets | Int64
datastat-uplink-qci2totbyte | Data Statistics - Uplink Statistics - QCI 2 Total-Bytes | Int64
datastat-uplink-qci2totpkt | Data Statistics - Uplink Statistics - QCI 2 Total-Packets | Int64
datastat-uplink-qci3totbyte | Data Statistics - Uplink Statistics - QCI 3 Total-Bytes | Int64
datastat-uplink-qci3totpkt | Data Statistics - Uplink Statistics - QCI 3 Total-Packets | Int64
datastat-uplink-qci4totbyte | Data Statistics - Uplink Statistics - QCI 4 Total-Bytes | Int64
datastat-uplink-qci4totpkt | Data Statistics - Uplink Statistics - QCI 4 Total-Packets | Int64
datastat-uplink-qci5totbyte | Data Statistics - Uplink Statistics - QCI 5 Total-Bytes | Int64
datastat-uplink-qci5totpkt | Data Statistics - Uplink Statistics - QCI 5 Total-Packets | Int64
datastat-uplink-qci6totbyte | Data Statistics - Uplink Statistics - QCI 6 Total-Bytes | Int64
datastat-uplink-qci6totpkt | Data Statistics - Uplink Statistics - QCI 6 Total-Packets | Int64
datastat-uplink-qci7totbyte | Data Statistics - Uplink Statistics - QCI 7 Total-Bytes | Int64
datastat-uplink-qci7totpkt | Data Statistics - Uplink Statistics - QCI 7 Total-Packets | Int64
datastat-uplink-qci8totbyte | Data Statistics - Uplink Statistics - QCI 8 Total-Bytes | Int64
datastat-uplink-qci8totpkt | Data Statistics - Uplink Statistics - QCI 8 Total-Packets | Int64
datastat-uplink-qci9totbyte | Data Statistics - Uplink Statistics - QCI 9 Total-Bytes | Int64
datastat-uplink-qci9totpkt | Data Statistics - Uplink Statistics - QCI 9 Total-Packets | Int64
datastat-uplink-othertotbyte | Data Statistics - Uplink Statistics - Other Total-Bytes | Int64
datastat-uplink-othertotpkt | Data Statistics - Uplink Statistics - Other Total-Packets | Int64
datastat-downlink-qci1totbyte | Data Statistics - Downlink Statistics - QCI 1 Total-Bytes | Int64
datastat-downlink-qci1totpkt | Data Statistics - Downlink Statistics - QCI 1 Total-Packets | Int64
datastat-downlink-qci2totbyte | Data Statistics - Downlink Statistics - QCI 2 Total-Bytes | Int64
datastat-downlink-qci2totpkt | Data Statistics - Downlink Statistics - QCI 2 Total-Packets | Int64
datastat-downlink-qci3totbyte | Data Statistics - Downlink Statistics - QCI 3 Total-Bytes | Int64
datastat-downlink-qci3totpkt | Data Statistics - Downlink Statistics - QCI 3 Total-Packets | Int64
datastat-downlink-qci4totbyte | Data Statistics - Downlink Statistics - QCI 4 Total-Bytes | Int64
datastat-downlink-qci4totpkt | Data Statistics - Downlink Statistics - QCI 4 Total-Packets | Int64
datastat-downlink-qci5totbyte | Data Statistics - Downlink Statistics - QCI 5 Total-Bytes | Int64
datastat-downlink-qci5totpkt | Data Statistics - Downlink Statistics - QCI 5 Total-Packets | Int64
datastat-downlink-qci6totbyte | Data Statistics - Downlink Statistics - QCI 6 Total-Bytes | Int64
datastat-downlink-qci6totpkt | Data Statistics - Downlink Statistics - QCI 6 Total-Packets | Int64
datastat-downlink-qci7totbyte | Data Statistics - Downlink Statistics - QCI 7 Total-Bytes | Int64
datastat-downlink-qci7totpkt | Data Statistics - Downlink Statistics - QCI 7 Total-Packets | Int64
datastat-downlink-qci8totbyte | Data Statistics - Downlink Statistics - QCI 8 Total-Bytes | Int64
datastat-downlink-qci8totpkt | Data Statistics - Downlink Statistics - QCI 8 Total-Packets | Int64
datastat-downlink-qci9totbyte | Data Statistics - Downlink Statistics - QCI 9 Total-Bytes | Int64
datastat-downlink-qci9totpkt | Data Statistics - Downlink Statistics - QCI 9 Total-Packets | Int64
datastat-downlink-othertotbyte | Data Statistics - Downlink Statistics - Other Total-Bytes | Int64
datastat-downlink-othertotpkt | Data Statistics - Downlink Statistics - Other Total-Packets | Int64
IMPORTANT: For information on statistics that are common to all schema see the Statistics and Counters Overview chapter.