# CSCF IFC Trigger Point Mode Commands

The CSCF iFC Trigger Point Configuration Mode is used to associate an Initial Filter Criteria (iFC) Service Point Trigger (SPT) group with an iFC trigger point.

IMPORTANT:

The commands or keywords/variables that are available are dependent on platform type, product version, and installed license(s).
end

Exits the current mode and returns to the Exec Mode.
Product:

All
Privilege:

Administrator
Syntax

    end

Usage:

Change the mode back to the Exec mode.
exit

Exits the current mode and returns to the previous mode.
Product:

All
Privilege:

Administrator
Syntax

    exit

Usage:

Return to the previous mode.
spt-group

Assigns an existing iFC SPT group to an iFC trigger point.
Platform:

ASR 5000
Product:

SCM (S-CSCF, SIP Proxy)
Privilege:

Administrator
Syntax

    [ no ] spt-group
    id group_id

no

Removes the specified CSCF iFC SPT group from the iFC trigger point.
spt-group id group_id

Specifies the ID of an existing iFC SPT group.

group_id must be an integer from 1 to 200.

IMPORTANT:

An iFC SPT group can be assigned to more than one iFC trigger point.
Usage:

Use this command to associate an iFC SPT group with an iFC trigger point.
Example:
The following command assigns iFC SPT group 2 to an iFC trigger point:

    spt-group id 2