# CSCF Emergency-CSCF Configuration Mode Commands

The Emergency-CSCF Configuration Mode is used to set commands supporting the role of the CSCF service as an Emergency CSCF.

IMPORTANT:

The commands or keywords/variables that are available are dependent on platform type, product version, and installed license(s).
end

Exits the current mode and returns to the Exec Mode.
Product:

All
Privilege:

Administrator
Syntax

    end

Usage:

Change the mode back to the Exec mode.
exit

Exits the current mode and returns to the previous mode.
Product:

All
Privilege:

Administrator
Syntax

    exit

Usage:

Return to the previous mode.
privacy

Enables privacy support on the E-CSCF.
Platform:

ASR 5000
Product:

SCM
Privilege:

Administrator
Syntax

    [ no | default ] privacy

no | default

Removes privacy support from the E-CSCF.
Usage:

Use this command to enable privacy support for Emergency CSCF service.