# show mag-service

This chapter includes the show mag-service command output tables.
show mag-service statistics
Table 1. show mag-service statistics Command Output Descriptions

Field | Description
--- | ---
Binding Update Sent
Total | The total number of all binding updates sent by this system or the specified service.
Init Request Xmit | The total number of initial request transmit binding updates sent by this system or the specified service.
Init Request Re-Xmit | The total number of initial request retransmit binding updates sent by this system or the specified service.
Renew Request Xmit | The total number of renew request transmit binding updates sent by this system or the specified service.
Renew Request Re-Xmit | The total number of renew request retransmit binding updates sent by this system or the specified service.
Dereg Request Xmit | The total number of deregistration request transmit binding updates sent by this system or the specified service.
Dereg Request Re-Xmit | The total number of deregistration request retransmit binding updates sent by this system or the specified service.
Binding Acknowledgement Rcvd
Total | The total number of all binding acknowledgements received by this system or the specified service.
Errors | The total number of all binding acknowledgements, with errors, received by this system or the specified service.
Accepted | The total number of all binding acknowledgements received, and accepted by this system or the specified service.
Denied | The total number of all binding acknowledgements received, but denied by this system or the specified service.
Init Reply Rcvd | The total number of all binding acknowledgements - initial reply received by this system or the specified service.
Renew Reply Rcvd | The total number of all binding acknowledgements - renew reply received by this system or the specified service.
Dereg Reply Rcvd | The total number of all binding acknowledgements - deregistration reply received by this system or the specified service.
Denied by LMA
Insufficient Resources | The total number of binding updates sent by this system or the specified service but denied by the LMA due to insufficient resources.
Mismatched ID | The total number of binding updates sent by this system or the specified service but denied by the LMA due to mismatched IDs.
MN Auth Failure | The total number of binding updates sent by this system or the specified service but denied by the LMA due to mobile node authorization failures.
Admin Prohibited | The total number of binding updates sent by this system or the specified service but denied by the LMA due to admin prohibited conditions.
Msg ID Required | The total number of binding updates sent by this system or the specified service but denied by the LMA due to missing message IDs.
DAD Failed | The total number of binding updates sent by this system or the specified service but denied by the LMA due to DAD failures.
Not Home Subnet | The total number of binding updates sent by this system or the specified service but denied by the LMA due to incorrect home subnet.
Sequence Out Of Window | The total number of binding updates sent by this system or the specified service but denied by the LMA due to sequence out of window conditions.
Reg Type Change Disallowed | The total number of binding updates sent by this system or the specified service but denied by the LMA due to registration type change disallowed.
Unspecified Reason | The total number of binding updates sent by this system or the specified service but denied by the LMA due to unspecified reasons.
Service-Authorization Failed | The total number of binding updates sent by this system or the specified service but denied by the LMA due to failed service authorizations.
Proxy Reg Not Enabled | The total number of binding updates sent by this system or the specified service but denied by the LMA due to proxy registration not being enabled.
Timestamp Mismatch | The total number of binding updates sent by this system or the specified service but denied by the LMA due to timestamp mismatches.
Timestamp Lower Than Expected | The total number of binding updates sent by this system or the specified service but denied by the LMA due to lower than expected timestamps.
Missing MN-ID Option | The total number of binding updates sent by this system or the specified service but denied by the LMA due to missing mobile node ID options.
Missing HNP Option | The total number of binding updates sent by this system or the specified service but denied by the LMA due to missing HNP options.
Missing Access Tech Option | The total number of binding updates sent by this system or the specified service but denied by the LMA due to missing access technology options.
Missing Handoff Ind Option | The total number of binding updates sent by this system or the specified service but denied by the LMA due to missing handoff indication options.
Not Authorized For HNP | The total number of binding updates sent by this system or the specified service but denied by the LMA due to not being authorized for HNP.
Not LMA For Mobile | The total number of binding updates sent by this system or the specified service but denied by the LMA due incorrect LMA for mobility.
Not Authorized For Proxy Reg | The total number of binding updates sent by this system or the specified service but denied by the LMA due to not being authorized for proxy registration.
BCE Prefix Do Not Match | The total number of binding updates sent by this system or the specified service but denied by the LMA due to BCE prefix mismatches.
Binding Acknowledgement Error Reason
Missing HNP | The total number of binding acknowledgements with missing HNP errors received by this system or the specified service.
Missing NAI | The total number of binding acknowledgements with missing NAI errors received by this system or the specified service.
Home Address Conflict | The total number of binding acknowledgements with home address conflict errors received by this system or the specified service.
Matching Request Not Found | The total number of binding acknowledgements with matching requests not found errors received by this system or the specified service.
Badly Formed | The total number of binding acknowledgements with badly formed message errors received by this system or the specified service.
Checksum Error | The total number of binding acknowledgements with checksum errors received by this system or the specified service.
Session Not Found | The total number of binding acknowledgements with session not found errors received by this system or the specified service.
Binding Revocation
Sent | The total number of binding revocations sent by this system or the specified service.
Retries Sent | The total number of binding revocation retries sent by this system or the specified service.
Ack Rcvd | The total number of binding revocation acknowledgements received by this system or the specified service.
Not Acknowledged | The total number of binding revocations sent, but not acknowledged, by this system or the specified service.
Rcvd | The total number of binding revocations received by this system or the specified service.
Ack Sent | The total number of binding revocation acknowledgements sent by this system or the specified service.
Received Binding Revocation Trigger Reasons
Unspecified | The total number of Binding Revocation Indication (BRI) messages received by the MAG with an “Unspecified” revocation trigger reason.
Administrative Reason | The total number of Binding Revocation Indication (BRI) messages received by the MAG with an “Administrative Reason” revocation trigger reason.
Inter-MAG Handoff-Same ATT | The total number of Binding Revocation Indication (BRI) messages received by the MAG with an “Inter-MAG Handoff-Same ATT” revocation trigger reason.
Inter-MAG - Unknown Handoff | The total number of Binding Revocation Indication (BRI) messages received by the MAG with an “Inter-MAG - Unknown Handoff” revocation trigger reason.
Inter-MAG Handoff-Diff ATT | The total number of Binding Revocation Indication (BRI) messages received by the MAG with an “Inter-MAG Handoff-Diff ATT” revocation trigger reason.
Per-Peer Policy | The total number of Binding Revocation Indication (BRI) messages received by the MAG with a “Per-Peer Policy” revocation trigger reason.
Revoking Node Local Policy | The total number of Binding Revocation Indication (BRI) messages received by the MAG with a “Revoking Node Local Policy” revocation trigger reason.
User Initiated Session Term | The total number of Binding Revocation Indication (BRI) messages received by the MAG with a “User Initiated Session Term” revocation trigger reason.
Access Network Session Term | The total number of Binding Revocation Indication (BRI) messages received by the MAG with an “Access Network Session Term” revocation trigger reason.
Out-of Sync BCE State | The total number of Binding Revocation Indication (BRI) messages received by the MAG with an “Out-of Sync BCE State” revocation trigger reason.
Unknown | The total number of Binding Revocation Indication (BRI) messages received by the MAG with an “Unknown” revocation trigger reason.
Sent Revocation ACK Status
Success | The total number of Binding Revocation Acknowledgement (BRA) messages sent by the MAG with a “Success” status.
Partial-Success | The total number of Binding Revocation Acknowledgement (BRA) messages sent by the MAG with a “Partial-Success” status.
Binding-Does-Not-Exist | The total number of Binding Revocation Acknowledgement (BRA) messages sent by the MAG with a “Binding-Does-Not-Exist” status.
No IPv4-HoA-Bind | The total number of Binding Revocation Acknowledgement (BRA) messages sent by the MAG with a “No IPv4-HoA-Bind” status.
Global-Revoc-Not-Authorized | The total number of Binding Revocation Acknowledgement (BRA) messages sent by the MAG with a “Global-Revoc-Not-Authorized” status.
Revoc-MN-ID-Required | The total number of Binding Revocation Acknowledgement (BRA) messages sent by the MAG with a “Revoc-MN-ID-Required” status.
Revoc-Failed-MN-Attached | The total number of Binding Revocation Acknowledgement (BRA) messages sent by the MAG with a “Revoc-Failed-MN-Attached” status.
Trigger-Not-Supported | The total number of Binding Revocation Acknowledgement (BRA) messages sent by the MAG with a “Trigger-Not-Supported” status.
Proxy-Bind-Rev-Not-Supported | The total number of Binding Revocation Acknowledgement (BRA) messages sent by the MAG with a “Proxy-Bind-Rev-Not-Supported” status.
Revoc-Func-Not-Supported | The total number of Binding Revocation Acknowledgement (BRA) messages sent by the MAG with a “Revoc-Func-Not-Supported” status.
Unknown | The total number of Binding Revocation Acknowledgement (BRA) messages sent by the MAG with an “Unknown” status.
Binding Revocation Indication Discarded
Total | The total number of binding revocation acknowledgements received and discarded by this system or the specified service.
Session Not Found | The total number of binding revocation acknowledgements received and discarded, due to a session not found condition, by this system or the specified service.
Badly Formed Request | The total number of binding revocation acknowledgements received and discarded, due to a badly formed request condition, by this system or the specified service.
Decode Error | The total number of binding revocation acknowledgements received and discarded, due to a decode error condition, by this system or the specified service.
Checksum Error | The total number of binding revocation acknowledgements received and discarded, due to a checksum error condition, by this system or the specified service.
Invalid Message Type | The total number of binding revocation acknowledgements received and discarded, due to a invalid memory type condition, by this system or the specified service.
No Memory | The total number of binding revocation acknowledgements received and discarded, due to insufficient memory, by this system or the specified service.
Tunnel Data Received
Total Packets | The total number of tunnel packets received by this system or the specified service.
6in6 4in6 IPv6 GRE (IPv4) IPv6 GRE (IPv6) | The total number of IPv6-in-IPv6 tunnel packets received by this system or the specified service. The total number of IPv4-in-IPv6 tunnel packets received by this system or the specified service. The total number of IPv4-in-IPv6 GRE tunnel packets received by this system or the specified service. The total number of IPv6-in-IPv6 GRE tunnel packets received by this system or the specified service.
Total Bytes | The total number of tunnel bytes received by this system or the specified service.
6in6 4in6 IPv6 GRE (IPv4) IPv6 GRE (IPv6) | The total number of IPv6-in-IPv6 tunnel bytes received by this system or the specified service. The total number of IPv4-in-IPv6 tunnel bytes received by this system or the specified service. The total number of IPv4-in-IPv6 GRE tunnel bytes received by this system or the specified service. The total number of IPv6-in-IPv6 GRE tunnel bytes received by this system or the specified service.
Errors
Protocol Type Error | The total number of protocol type data errors received by this system or the specified service.
Invalid Pkt Length | The total number of invalid packet length data errors received by this system or the specified service.
No Session Found | The total number of no session found data errors received by this system or the specified service.
Tunnel Data Sent
Total Packets | The total number of tunnel packets sent by this system or the specified service.
6in6 4in6 IPv6 GRE (IPv4) IPv6 GRE (IPv6) | The total number of IPv6-in-IPv6 tunnel packets sent by this system or the specified service. The total number of IPv4-in-IPv6 tunnel packets sent by this system or the specified service. The total number of IPv4-in-IPv6 GRE tunnel packets sent by this system or the specified service. The total number of IPv6-in-IPv6 GRE tunnel packets sent by this system or the specified service.
Total Bytes | The total number of tunnel bytes sent by this system or the specified service.
6in6 4in6 IPv6 GRE (IPv4) IPv6 GRE (IPv6) | The total number of IPv6-in-IPv6 tunnel bytes sent by this system or the specified service. The total number of IPv4-in-IPv6 tunnel bytes sent by this system or the specified service. The total number of IPv4-in-IPv6 GRE tunnel bytes sent by this system or the specified service. The total number of IPv6-in-IPv6 GRE tunnel bytes sent by this system or the specified service.
Total Disconnects/Failures
Lifetime expiry | The total number of disconnects due to lifetime expiry initiated by this system or the specified service.
Access Initiated Term | The total number of disconnects due to deregistrations initiated by this system or the specified service.
Admin Drops | The total number of disconnects due to admin drops initiated by this system or the specified service.
Other Reasons | The total number of disconnects due to “other reasons” initiated by this system or the specified service.
LMA Revocations | The total number of disconnects due to LMA revocations received by this system or the specified service.