# show congestion-control

This chapter includes the show congestion-control command output tables.
show congestion-control statistics a11mgr instance
Table 1. show congestion-control statistics a11mgr instance Command Output Descriptions

Field | Description
--- | ---
Current congestion status | The current congestion control state as “Cleared” or “Applied”.
Congestion applied | Displays the number of times the system invoked a congestion control policy for the specified service type.
Congestion Control Resource Limits | Indicates the congestion control threshold that was triggered. For more information, refer to the congestion-control threshold command in the Global Configuration Mode chapter of the Command Line Interface Reference.

show congestion-control statistics asngwmgr instance
Table 2. show congestion-control statistics asngwmgr instance Command Output Descriptions

Field | Description
--- | ---
Current congestion status | The current congestion control state as “Cleared” or “Applied”.
Congestion applied | Displays the number of times the system invoked a congestion control policy for the specified service type.
Congestion Control Resource Limits | Indicates the congestion control threshold that was triggered. For more information, refer to the congestion-control threshold command in the Global Configuration Mode chapter of the Command Line Interface Reference.
system cpu use exceeded | Indicates the number of time the ASNGW Manager exceeded the system CPU usage limit.
service cpu use exceeded | Indicates the number of time the ASNGW Manager exceeded the CPU usage limit specified for this service.
system memory use exceeded | Indicates the number of time the ASNGW Manager exceeded the allocated system memory usage limit.
port rx use exceeded | Indicates the number of time the ASNGW Manager exceeded the Rx port usage limit.
port tx use exceeded | Indicates the number of time the ASNGW Manager exceeded the Tx port usage limit.
port specific rx use exceeded | Indicates the number of time the ASNGW Manager exceeded the Rx port usage limit for a specific port number.
port specific tx use exceeded | Indicates the number of time the ASNGW Manager exceeded the Tx port usage limit for a specific port number.
max sess use exceeded | Indicates the number of time the ASNGW Manager exceeded the maximum session usage limit for a service.
license use exceeded | Indicates the number of time the ASNGW Manager exceeded the maximum license usage limit.
msg queue size use exceeded | Indicates the number of time the ASNGW Manager exceeded the message queue size usage.
msg queue wait time exceeded | Indicates the number of time the ASNGW Manager exceeded the message queue wait time.
license threshold exceeded | Indicates the number of time the ASNGW Manager exceeded the license threshold limit.
max sess threshold exceeded | Indicates the number of time the ASNGW Manager exceeded the maximum session threshold limit.
Sessions disconnected due to overload disconnect | Indicates the total number of sessions disconnected due to overload.