> show ipsg
> This chapter describes the outputs of the show ipsg command.
> show ipsg service all
> show ipsg service all Command Output Descriptions

> Field | Description
> Context | The context in which the IPSG service is configured.
> Bind | The binding status of the service. Defines if the service has been bound to the appropriate interfaces (radius-server mode) or to any interface in the context (radius-snoop mode).
> Max Subscribers | The total number of subscribers allowed for the service. This field displays a configured number or, if not configured, the total amount specified by the IPSG service license.
> Mode | The IPSG service mode type: radius-server or radius-snoop
> Address | The IP address of the interface where RADIUS accounting requests are received.
> Port | The port number of the interface where RADIUS accounting requests are received.
> Source-Context | The source context with the interface where RADIUS accounting requests are received.
> Default Subscriber | Identifies the default subscriber for the context.
> Service Status | The status of the IPSG service. Defines if the service has been started.

> ‌
> show ipsg session all
> show ipsg session all Command Output Descriptions

> Field | Description
> CALLID | The call ID of the session.
> NAI | The subscriber’s Network Address Identifier.
> Home Address | The subscriber’s IP address.

> ‌
> show ipsg statistics
> show ipsg statistics Command Output Descriptions

> Field | Description
> RADIUS Accounting
> Total START Req rcvd | Cumulative RADIUS accounting start requests received since the last system restart or clear command.
> Total START Req (Retransmitted) rcvd | Cumulative retransmitted RADIUS accounting start requests received since the last system restart or clear command.
> Total START Sent | Cumulative RADIUS accounting start responses sent by this system since the last system restart or clear command.
> Total INTERIM Updt rcvd | Cumulative RADIUS accounting interim updates received since the last system restart or clear command.
> Total STOP Req rcvd | Cumulative RADIUS accounting stop requests received since the last system restart or clear command.
> Total ACCESS Req rcvd | Cumulative IPSG RADIUS Access Request messages received since the last system restart or clear command.
> Total ACCESS Req (Retransmitted) rcvd | Cumulative IPSG RADIUS Access Request retransmission messages received since the last system restart or clear command.
> Total ACCESS Accept sent | Cumulative IPSG RADIUS Access Accept messages sent since the last system restart or clear command.
> Total ACCESS Reject sent | Cumulative IPSG RADIUS Access Reject messages sent since the last system restart or clear command.
> Total UNKNOWN req rcvd | Cumulative unknown requests received since the last system restart or clear command.
> Total Response sent | Cumulative RADIUS accounting responses sent since the last system restart or clear command.
> Total Discarded Msgs (Mandatory Attr Missing) | Cumulative messages discarded because of missing mandatory attribute since the last system restart or clear command.
> Total Discarded Msgs (Interim For Non-Existing Session) | Cumulative RADIUS accounting interim packets discarded, when there is no session existing, since the last system restart or clear command.
> Total Discarded Msgs (Stop For Non-Existing Session) | Cumulative RADIUS accounting stop packets discarded, when there is no session existing, since the last system restart or clear command.
> Total Discarded Msgs (Unknown Client) | Cumulative messages discarded when received from an unknown client since the last system restart or clear command.
> Total Discarded Msgs (Interconnect shared secret) | Cumulative RADIUS request messages discarded, because the shared secret was incorrect, since the last system restart or clear command.

> ‌

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883