> Line Configuration Mode Commands
> The Line Configuration Mode is used to manage the terminal line characteristics for output formatting.
> Important: The commands or keywords/variables that are available are dependent on platform type, product version, and installed license(s).
> default
> Restores the default length or width for the output to the display terminal.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> default { length | width }
> length | width
> length: restores the default value for the number of rows (length) of the output for display.
> width: restores the default value for the number of columns (width) of the output for display as the number of characters.
> Usage
> Reset the output display properties if they had been changed during a session.
> Example
> default length
> default width
> end
> Exits the line configuration mode and returns to the Exec mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> end
> Usage
> Change the mode back to the Exec mode.
> exit
> Exits the line configuration mode and returns to the global configuration mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> exit
> Usage
> Return to the global configuration mode.
> length
> Configures the output for the displays length (number of rows).
> Privilege
> Security Administrator, Administrator
> Syntax
> length number
> number
> Specifies the number of rows (lines) of output that can be displayed at one time for the display (output) terminal. number must have a value of 0 or be in the range from 5 through 512 where the special value 0 implies an infinite number of rows.
> Usage
> Set the current session’s display terminal has different display characteristics than the defaults. The special infinite value (0) is typically used when logging the output of a session from a remote machine since this will result in no pagination of output.
> Example
> The following commands set the length of the display to infinite and 33, respectively.
> length 0
> length 33
> width
> Configures the output for the displays width (number of columns/characters wide).
> Privilege
> Security Administrator, Administrator
> Syntax
> width number
> number
> Specifies the number of columns (characters) of output that can be displayed at one time for the display (output) terminal. number must have a value in the range from 5 through 512.
> Usage
> Set the current session’s display terminal has different display characteristics than the defaults.
> Example
> width 160

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883