> show dynamic-policy
> This chapter includes the show dynamic-policy command output tables.
> show dynamic-policy statistics
> show dynamic-policy statistics Command Output Descriptions

> Field | Description
> Dynamic Policy Stats
> PCC rule stats
> Install requests | Total number of Policy Control and Charging (PCC) rule install requests.
> Remove requests | Total number of PCC rule removal requests.
> Installed uplink | Total number of PCC rules installed for uplink direction.
> Installed downlink | Total number of PCC rules installed for downlink direction.
> Activate requests | Total number of PCC rule activate requests.
> Deactivate requests | Total number of PCC rule deactivate requests.
> Activate group | Total number of policy groups activated.
> Deactivate group | Total number of policy groups deactivated.
> PCC rule failure stats
> Install failure | Total number of PCC rule install failures.
> Remove failure | Total number of PCC rule removal failures.
> Activation failure | Total number of PCC rule activation failures.
> Deactivation failure | Total number of PCC rule deactivation failures.
> Group activation failure | Total number of policy group activation failures.
> Group deactivation failure | Total number of policy group deactivation failures.
> Event stats
> Session up | Total number of subscriber sessions up.
> Session down | Total number of subscriber sessions down.
> Handoff | Total number of handoffs occurred.
> RAT change | Total number of Radio Access Type (RAT) changes occurred.
> User location change | Total number of user location changes occurred.
> Default Bearer QoS change | Total number of default bearer QoS changes occurred.
> Flow create | Total number of flows created.
> Flow delete | Total number of flows deleted.
> Bearer loss | Total number of bearer loss.
> Bearer recovery | Total number of bearer recoveries after loss of bearer.
> Update tft | Total number of Traffic Flow Template (TFT) updates.
> Update qos | Total number of QoS updates.
> UE Time Zone change | Total number of UE time zone changes occurred.
> Event failure stats
> Session up | Total number of session up failures.
> Session down | Total number of session down failures.
> Handoff | Total number of handoff failures.
> RAT change | Total number of RAT change failures.
> User location change | Total number of user location change failures.
> Default Bearer QoS change | Total number of default bearer QoS change failures.
> Flow create | Total number of flow creation failures.
> Flow delete | Total number of flow deletion failures.
> Bearer loss | Total number of bearer loss failures.
> Bearer recovery | Total number of bearer recovery failures.
> Update tft | Total number of TFT update failures.
> Update qos | Total number of QoS update failures.
> UE Time Zone change | Total number of UE time zone change failures.
> Auth stats
> Auth request | Total number of authorization requests sent.
> Auth failure | Total number of authorization request failures.
> Reauth request | Total number of re-authorization requests sent.
> Reauth request failure | Total number of re-authorization request failures.
> Terminate request | Total number of terminate requests sent.
> Terminate request failure | Total number of terminate request failures.

> ‌

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883