> CSCF Crypto Template Configuration Mode Commands
> The CSCF Crypto Template Configuration Mode is used to configure a P-CSCF IPsec policy. It includes most of the IPsec parameters and Internet Key Exchange version 1 (IKEv1) parameters for cryptographic and authentication algorithms etc. A P-CSCF service will not support IPSec without a configured crypto template. Only one crypto template can be configured per P-CSCF service.
> Important: The commands or keywords/variables that are available are dependent on platform type, product version, and installed license(s).
> end
> Exits the current mode and returns to the Exec Mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> end
> Usage
> Change the mode back to the Exec Mode.
> exit
> Exits the current mode and returns to the previous mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> exit
> Usage
> Returns to the previous mode.
> ipsec
> Configures parameters for the 3GPP/3GPP2 P-CSCF security associations within this crypto template.
> Product
> SCM
> Privilege
> Security Administrator, Administrator
> Syntax
> ipsec transform-set list list_name
> transform-set list name
> transform-set: Specifies a context-level IPSec security association transform set to be used for deriving 3GPP/3GPP2 P-CSCF security associations from this crypto template.
> list list_name: A space separated list of 3GPP/3GPP2 P-CSCF security association transform sets. list_name must be an existing 3GPP/3GPP2 P-CSCF transform set and be from 1 to 127 alpha and/or numeric characters.
> Important: A minimum of one transform set is required. A maximum of four transform sets may be specified.
> Usage
> Use this command to configure parameters for the 3GPP/3GPP2 P-CSCF security associations within this crypto template.
> Example
> The following command configures the 3GPP/3GPP2 P-CSCF transform set list name to ikev1list1:
> ipsec transform-set list ikev1list1

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883