> SSL Template Configuration Mode Commands
> The SSL Template Configuration Mode is used to configure an SSL cryptographic policy. It includes most of the SSL parameters for cryptographic and authentication algorithms.
> A P-CSCF service for SSL access will not function without a configured SSL template. Only one SSL template can be configured per P-CSCF service.
> Important: The commands or keywords/variables that are available are dependent on platform type, product version, and installed license(s).
> ca-certificate
> Specifies a list of ca-certificates.
> Product
> SCM (P-CSCF, A-BG)
> Privilege
> Administrator
> Syntax
> ca-certificate list name
> list name
> Specifies the name(s) of ca-certificate(s), which can be an alpha and/or numeric string of 1 to 129 characters.
> Usage
> Use this command to specify a list of ca-certificates for the SSL template.
> Example
> The following command specifies the ca-certificate ca_certificate_1 for the SSL template:
> ca-certificate list ca_certificate_1
> certificate
> Used to bind an X.509 trusted certificate to the SSL template.
> Product
> SCM (P-CSCF, A-BG)
> Privilege
> Administrator
> Syntax
> certificate name
> name
> Specifies the name of a certificate, which can be an alpha and/or numeric string of 1 to 127 characters.
> Usage
> Use this command to bind an X.509 certificate to the SSL template.
> Example
> The following command binds the X.509 certificate certificate_1 to the SSL template:
> certificate certificate_1
> cipher-suites
> Specifies a list of SSL cipher suites.
> Product
> SCM (P-CSCF, A-BG)
> Privilege
> Administrator
> Syntax
> cipher-suites list name
> list name
> Specifies the name of an SSL cipher suite, which can be an alpha and/or numeric string of 1 to 127 characters.
> Usage
> Use this command to specify an SSL cipher suite for the SSL template.
> Important: Currently, the system supports only one SSL cipher suite per SSL template.
> Example
> The following command specifies the SSL cipher suite cipher_suite_1 for the SSL template:
> cipher-suites list cipher_suite_1
> end
> Exits the current configuration mode and returns to the Exec mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> end
> Usage
> Use this command to return to the Exec mode.
> exit
> Exits the current mode and returns to the parent configuration mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> exit
> Usage
> Use this command to return to the parent configuration mode.
> version
> Specifies the supported version(s) of SSL protocol on the P-CSCF/A-BG.
> Product
> SCM (P-CSCF, A-BG)
> Privilege
> Administrator
> Syntax
> version list { tlsv1 }
> default version
> list { tlsv1 }
> Specifies the supported version of SSL protocol to be TLS v0.1.
> default
> Sets the supported version of SSL protocol to its default value of TLS v0.1.
> Usage
> Use this command to specify the supported version(s) of SSL protocol on the P-CSCF/A-BG. Currently, there is only one supported version of SSL protocol, which is TLS v0.1.
> Example
> The following command sets the supported version of SSL protocol to TLS v0.1:
> version list tlsv1

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883