> IPCF SSC Application MIB
> The figure that follows illustrates the hierarchical structure of the management information base (MIB) for the Subscriber Service Controller (SSC) application for Cisco PCC solution.
> MIB Textual Conventions
> starentMIB(8164).starentMIBObjects(1). starentSSCMIB(201)
> starentMIB(8164).starentMIBObjects(1).starentSSCMIB(201). starentSSCMIBObjects(1)
> Object
> starSSCTimeTicks
> Object ID
> enterprises.8164.1.201.1
> Description
> This object indicates the time when this notification was generated.
> Syntax
> TimeStamp
> Access
> accessible-for-notify
> Object
> starSSCEntity
> Object ID
> enterprises.8164.1.201.2
> Description
> This object indicates the reference of the SSC entity for which notification was generated.
> Syntax
> DisplayString
> Access
> accessible-for-notify
> Object
> starSSCTaskInfo
> Object ID
> enterprises.8164.1.201.3
> Description
> SSC process facility-name and instance ID.
> Syntax
> DisplayString
> Access
> accessible-for-notify
> Object
> starSSCProcessMaxRestartCnt
> Object ID
> enterprises.8164.1.201.4
> Description
> SSC process maximum restart count.
> Syntax
> Unsigned32
> Access
> Read-only
> Object
> starIPMSProcessRestartWaitTime
> Object ID
> enterprises.8164.1.201.1.5
> Description
> SSC process next restart wait seconds.
> Syntax
> Unsigned32
> Access
> accessible-for-notify
> Object
> starSSCResourceType
> Object ID
> enterprises.8164.1.201.1.6
> Description
> SSC resource type.
> Syntax
> INTEGER { hbd(1), logd(2), sysmgr(3), scheduler(4), shctrl(5), enctrl(6), profilectrl(7), appmgr(8) }
> Access
> accessible-for-notify
> Object
> starSSCResourceInfoState
> Object ID
> enterprises.8164.1.201.1.7
> Description
> SSC resource information status.
> Syntax
> INTEGER { available(1), notavailable(2), unknown(3), invalid(4) }
> Access
> accessible-for-notify
> Object
> starSSCResourceCurrentValue
> Object ID
> enterprises.8164.1.201.1.8
> Description
> The current value of SSC resource (CPU/memory/disk-space). Value is in float so mapping it to string.
> Syntax
> DisplayString
> Access
> accessible-for-notify
> Object
> starSSCResourceConfThreshold
> Object ID
> enterprises.8164.1.201.1.9
> Description
> The configured threshold value for SSC resource (CPU/memory/disk-space). Value is in float so mapping it to string.
> Syntax
> DisplayString
> Access
> accessible-for-notify
> Object
> starSSCPeerName
> Object ID
> enterprises.8164.1.201.1.10
> Description
> SSC Peer name.
> Syntax
> DisplayString
> Access
> accessible-for-notify
> Object
> starSSCPeerIP
> Object ID
> enterprises.8164.1.201.1.11
> Description
> SSC Peer IP.
> Syntax
> DisplayString
> Access
> accessible-for-notify
> Object
> starSSCPeerPort
> Object ID
> enterprises.8164.1.201.1.12
> Description
> SSC Peer port.
> Syntax
> Unsigned32
> Access
> accessible-for-notify
> Object
> starSSCIcmpState
> Object ID
> enterprises.8164.1.201.1.19
> Description
> SSC ICMP State.
> Syntax
> Unsigned32
> Access
> accessible-for-notify
> Object
> starSSCCorbaState
> Object ID
> enterprises.8164.1.201.1.20
> Description
> SSC CORBA State.
> Syntax
> Unsigned32
> Access
> accessible-for-notify
> Object
> starSSCOperState
> Object ID
> enterprises.8164.1.201.1.21
> Description
> SSC Operational State.
> Syntax
> Unsigned32
> Access
> accessible-for-notify
> Object
> starSSCOperStateChangeReason
> Object ID
> enterprises.8164.1.201.1.22
> Description
> SSC Operational State Change Reason.
> Syntax
> Unsigned32
> Access
> accessible-for-notify
> Object
> starSSCFTPServer
> Object ID
> enterprises.8164.1.201.1.23
> Description
> FTP Server for bulk Statistics upload.
> Syntax
> DisplayString
> Access
> accessible-for-notify
> Object
> starSSCFTPUser
> Object ID
> enterprises.8164.1.201.1.24
> Description
> User name for Bulk Statistics FTP Server.
> Syntax
> DisplayString
> Access
> accessible-for-notify
> Object
> starSSCEmailServer
> Object ID
> enterprises.8164.1.201.1.25
> Description
> Email Server.
> Syntax
> DisplayString
> Access
> accessible-for-notify
> Object
> starSSCSmsServer
> Object ID
> enterprises.8164.1.201.1.26
> Description
> SMS Server.
> Syntax
> DisplayString
> Access
> accessible-for-notify
> Object
> starSSCInstanceId
> Object ID
> enterprises.8164.1.201.1.27
> Description
> SSC Instance ID.
> Syntax
> Unsigned32
> Access
> accessible-for-notify
> Object
> starSSCFacilityId
> Object ID
> enterprises.8164.1.201.1.28
> Description
> SSC Facility ID.
> Syntax
> Unsigned32
> Access
> accessible-for-notify
> Object
> starSSCDefault
> Object ID
> enterprises.8164.1.201.1.29
> Description
> SSC Default.
> Syntax
> Unsigned32
> Access
> accessible-for-notify
> Object
> starSSCExisting
> Object ID
> enterprises.8164.1.201.1.30
> Description
> SSC Existing.
> Syntax
> Unsigned32
> Access
> accessible-for-notify
> Object
> starSSCProcessName
> Object ID
> enterprises.8164.1.201.1.31
> Description
> SSC Process Name.
> Syntax
> DisplayString
> Access
> accessible-for-notify
> Object
> starSSCProcessInstance
> Object ID
> enterprises.8164.1.201.1.32
> Description
> SSC Process Instance.
> Syntax
> DisplayString
> Access
> accessible-for-notify
> Object
> starSSCService
> Object ID
> enterprises.8164.1.201.1.33
> Description
> SSC Service.
> Syntax
> DisplayString
> Access
> accessible-for-notify
> Object
> starSSCOperation
> Object ID
> enterprises.8164.1.201.1.34
> Description
> SSC Operation.
> Syntax
> DisplayString
> Access
> accessible-for-notify
> Object
> starSSCSprStatus
> Object ID
> enterprises.8164.1.201.1.35
> Description
> SSC spr status.
> Syntax
> DisplayString
> Access
> accessible-for-notify
> starSSCMIBTraps
> Object
> starSSCEntityStart
> Object ID
> enterprises.8164.1.201.2.1
> Description
> SSC Component started successfully.
> Objects
> starSSCEntity
> Object
> starSSCEntityStop
> Object ID
> enterprises.8164.1.201.2.2
> Description
> SSC Component shutting down.
> Objects
> starSSCEntity
> Object
> starSSCProcessStart
> Object ID
> enterprises.8164.1.201.2.3
> Description
> SSC Process started successfully.
> Objects
> starSSCTaskInfo,
> starSSCEntity
> Object
> starSSCProcessStartFail
> Object ID
> enterprises.8164.1.201.2.4
> Description
> SSC Process failed to start.
> Objects
> starSSCProcessInstance
> starSSCProcessName
> starSSCProcessInstance
> Object
> starSSCProcessRestartFail
> Object ID
> enterprises.8164.1.201.2.5
> Description
> SSC Process max-restart-count reached.
> Objects
> starSSCProcessMaxRestartCnt
> starSSCEntity
> starSSCTaskInfo
> starSSCProcessRestartWaitTime
> Object
> starSSCPeerStateUp
> Object ID
> enterprises.8164.1.201.2.6
> Description
> Generated by SSC when peer (query server/SSC server) changes the state.
> Objects
> starSSCEntity
> starSSCPeerName
> starSSCPeerIP
> starSSCPeerPort
> Object
> starSSCPeerStateDown
> Object ID
> enterprises.8164.1.201.2.7
> Description
> Generated by SSC when peer (query server/SSC server) changes the state.
> Objects
> starSSCEntity
> starSSCPeerName
> starSSCPeerIP
> starSSCPeerPort
> Object
> starSSCFTPServerUnreachable
> Object ID
> enterprises.8164.1.201.2.8
> Description
> Generated by SSC when FTP Server for Bulk Statistics upload is unreachable.
> Objects
> starSSCFTPServer
> starSSCFTPUser
> Object
> starSSCFTPServerReachable
> Object ID
> enterprises.8164.1.201.2.9
> Description
> Generated by SSC when FTP Server for Bulk Statistics upload is reachable
> Objects
> starSSCFTPServer
> starSSCFTPUser
> Object
> starSSCEmailServerUnreachable
> Object ID
> enterprises.8164.1.201.2.10
> Description
> Generated by SSC when Email Notification Server is unreachable.
> Objects
> starSSCEntity
> starSSCEmailServer
> Object
> starSSCEmailServerReachable
> Object ID
> enterprises.8164.1.201.2.11
> Description
> Generated by SSC when Email Notification Server is reachable.
> Objects
> starSSCEntity
> starSSCEmailServer
> Object
> starSSCSmsServerUnreachable
> Object ID
> enterprises.8164.1.201.2.12
> Description
> Generated by SSC when SMS Notification Server is unreachable.
> Objects
> starSSCEntity
> starSSCSmsServer
> Object
> starSSCSmsServerReachable
> Object ID
> enterprises.8164.1.201.2.13
> Description
> Generated by SSC when SMS Notification Server is reachable.
> Objects
> starSSCEntity
> starSSCSmsServer
> Object
> starSSCShCtrlPeerUp
> Object ID
> enterprises.8164.1.201.2.14
> Description
> Generated by SSC when Sh Peer is Up.
> Objects
> starSSCPeerName
> starSSCPeerIP
> starSSCPeerPort
> Object
> starSSCShCtrlPeerDown
> Object ID
> enterprises.8164.1.201.2.15
> Description
> Generated by SSC when Sh Peer is Down.
> Objects
> starSSCPeerName
> starSSCPeerIP
> starSSCPeerPort
> Object
> starSSCEnCtrlPeerUp
> Object ID
> enterprises.8164.1.201.2.16
> Description
> Generated by SSC when EN Peer is Up.
> Objects
> starSSCPeerName
> starSSCPeerIP
> starSSCPeerPort
> Object
> starSSCEnCtrlPeerDown
> Object ID
> enterprises.8164.1.201.2.17
> Description
> Generated by SSC when EN Peer is Down.
> Objects
> starSSCPeerName
> starSSCPeerIP
> starSSCPeerPort
> Object
> starSSCSysMgrFailover
> Object ID
> enterprises.8164.1.201.2.18
> Description
> Generated by SSC when SysMgr fails over.
> Objects
> starSSCDefault
> starSSCOperation
> Object
> starSSCCpuThresholdCrossed
> Object ID
> enterprises.8164.1.201.2.19
> Description
> Generated by SSC when CPU Threshold is crossed.
> Objects
> starSSCDefault
> starSSCExisting
> Object
> starSSCCpuThresholdCleared
> Object ID
> enterprises.8164.1.201.2.20
> Description
> Generated by SSC when CPU Threshold is cleared.
> Objects
> starSSCDefault
> starSSCExisting
> Object
> starSSCSwapThresholdCrossed
> Object ID
> enterprises.8164.1.201.2.21
> Description
> Generated by SSC when Swap memory Threshold is crossed.
> Objects
> starSSCDefault
> starSSCExisting
> Object
> starSSCSwapThresholdCleared
> Object ID
> enterprises.8164.1.201.2.22
> Description
> Generated by SSC when Swap memory Threshold is cleared.
> Objects
> starSSCDefault
> starSSCExisting
> Object
> starSSCEnMgrConnFailed
> Object ID
> enterprises.8164.1.201.2.23
> Description
> Generated by SSC when EnMgr fails to connect to peer.
> Objects
> starSSCPeerIP
> starSSCPeerPort
> Object
> starSSCEnMgrConnEstablished
> Object ID
> enterprises.8164.1.201.2.24
> Description
> Generated by SSC when EnMgr connects to peer.
> Objects
> starSSCPeerIP
> starSSCPeerPort
> Object
> starSSCProcTheshCrossed
> Object ID
> enterprises.8164.1.201.2.25
> Description
> Generated by SSC when CPU threshold for process crossed.
> Objects
> starSSCProcessName,
> starSSCProcessInstance
> starSSCDefault
> starSSCExisting
> Object
> starSSCProcTheshCleared
> Object ID
> enterprises.8164.1.201.2.26
> Description
> Generated by SSC when CPU threshold for process cleared.
> Objects
> starSSCProcessName,
> starSSCProcessInstance
> starSSCDefault
> starSSCExisting
> Object
> starSSCMaxShSessionsCrossed
> Object ID
> enterprises.8164.1.201.2.27
> Description
> Generated by SSC when Max Sh sessions crossed.
> Objects
> starSSCDefault
> starSSCExisting
> Object
> starSSCMaxShSessionsCleared
> Object ID
> enterprises.8164.1.201.2.28
> Description
> Generated by SSC when Max Sh sessions cleared.
> Objects
> starSSCDefault
> starSSCExisting
> Object
> starSSCMaxPendReqAppMgrCrossed
> Object ID
> enterprises.8164.1.201.2.29
> Description
> Generated by SSC when Max pending requests at AppMgr crossed.
> Objects
> starSSCDefault
> starSSCExisting
> Object
> starSSCMaxPendReqAppMgrCleared
> Object ID
> enterprises.8164.1.201.2.30
> Description
> Generated by SSC when Max pending requests at AppMgr cleared.
> Objects
> starSSCDefault
> starSSCExisting
> Object
> starSSCMaxPendReqAppMgrSysCrossed
> Object ID
> enterprises.8164.1.201.2.31
> Description
> Generated by SSC when Max pending requests at AppMgr across system crossed.
> Objects
> starSSCDefault
> starSSCExisting
> Object
> starSSCMaxPendReqAppMgrSysCleared
> Object ID
> enterprises.8164.1.201.2.32
> Description
> Generated by SSC when Max pending requests at AppMgr across system cleared.
> Objects
> starSSCDefault
> starSSCExisting,
> Object
> starSSCSprDown
> Object ID
> enterprises.8164.1.201.2.33
> Description
> Generated by SSC when SPR becomes unusable.
> Objects
> starSSCSprStatus
> Object
> starSSCSprUp
> Object ID
> enterprises.8164.1.201.2.34
> Description
> Generated by SSC when SPR becomes usable.
> Object
> starSSCSprCacheDown
> Object ID
> enterprises.8164.1.201.2.35
> Description
> Generated by SSC when SPR cache becomes unusable.
> Objects
> starSSCSprStatus
> Object
> starSSCSprCacheUp
> Object ID
> enterprises.8164.1.201.2.36
> Description
> Generated by SSC when SPR cache becomes usable.
> Starent Compliances statements
> Object
> starSSCMIBCompliance
> Object ID
> enterprises.8164.1.201.3.1
> Description
> The compliance statements for entities implement the STARENT SSC MIB.
> MANDATORY-GROUPS
> starSSCObjectGroup
> starSSCNotifGroup
> Object
> starSSCObjectGroup
> Object ID
> enterprises.8164.1.201.3.1.1
> Description
> A collection of objects related with notification management on SSC.
> Objects
> starSSCTimeTicks
> starSSCEntity
> starSSCTaskInfo
> starSSCProcessMaxRestartCnt
> starSSCProcessRestartWaitTime
> starSSCResourceType
> starSSCResourceInfoState
> starSSCResourceCurrentValue
> starSSCResourceConfThreshold
> starSSCPeerName
> starSSCPeerIP
> starSSCPeerPort
> starSSCIcmpState
> starSSCCorbaState
> starSSCOperState
> starSSCOperStateChangeReason
> starSSCFTPServer
> starSSCFTPUser
> starSSCEmailServer
> starSSCSmsServer
> starSSCInstanceId
> starSSCFacilityId
> starSSCDefault
> starSSCExisting
> starSSCProcessName
> starSSCProcessInstance
> starSSCService
> starSSCOperation
> starSSCSprStatus
> Object
> starSSCNotifGroup
> Object ID
> enterprises.8164.1.201.3.1.2
> Description
> A collection of SSC notifications.
> Objects
> starSSCEntityStart
> starSSCEntityStop
> starSSCProcessStart
> starSSCProcessStartFail
> starSSCProcessRestartFail
> starSSCPeerStateUp
> starSSCPeerStateDown
> starSSCFTPServerUnreachable
> starSSCFTPServerReachable
> starSSCEmailServerUnreachable
> starSSCEmailServerReachable
> starSSCSmsServerUnreachable
> starSSCSmsServerReachable
> starSSCShCtrlPeerUp
> starSSCShCtrlPeerDown
> starSSCEnCtrlPeerUp
> starSSCEnCtrlPeerDown
> starSSCSysMgrFailover
> starSSCCpuThresholdCrossed
> starSSCCpuThresholdCleared
> starSSCSwapThresholdCrossed
> starSSCSwapThresholdCleared
> starSSCEnMgrConnFailed
> starSSCEnMgrConnEstablished
> starSSCProcTheshCrossed
> starSSCProcTheshCleared
> starSSCMaxShSessionsCrossed
> starSSCMaxShSessionsCleared
> starSSCMaxPendReqAppMgrCrossed
> starSSCMaxPendReqAppMgrCleared
> starSSCMaxPendReqAppMgrSysCrossed
> starSSCMaxPendReqAppMgrSysCleared
> starSSCSprDown
> starSSCSprUp
> starSSCSprCacheDown
> starSSCSprCacheUp

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883