> show pcc-af
> This chapter describes the output of the show pcc-af command.
> show pcc-af service all
> show pcc-af service all Command Output Description

> Variables | Description
> Service Name | The name of the PCC-AF service for which statistics are collected or displayed.
> Context | The name of the context in which PCC-AF service is configured.
> Service State | Indicates the state of PCC-AF service.
> Diameter | This group indicates the Diameter endpoint configuration information for Rx interface.
> Origin | Indicates the name of the Diameter origin endpoint configured for PCC-AF service.
> Dictionary | Indicates the name of the Diameter dictionary configured for Rx interface in PCC-AF service. By default it is “Standard” dictionary.
> Associated PCC-Service | Indicates the name of the PCC-Service associated with PCC-AF service.
> Max Charging Sessions | Indicates the maximum number of charging sessions allowed in this PCC-AF service instance. By default it is 10000.
> Newcall Policy | Indicates the new call policy configured to manage the congestion control on a PCC-AF service.

> ‌
> show pcc-af service statistics
> show pcc-af service statistics Command Output Description

> Variables | Description
> Service Name | The name of the PCC-AF service for which statistics are collected or displayed.
> Inbound Messages | Indicates the total number of Rx messages received.
> AAR Messages | Indicates the total number of Rx AAR messages received.
> STR Messages | Indicates the total number of Rx STR messages received.
> RAR Messages | Indicates the total number of Rx RAR request received.
> ASR Messages | Indicates the total number of Rx ASR request received.
> Outbound Messages | Indicates the total number of Rx messages sent.
> Accepted AAR Messages | Indicates the total number of Rx AAR-Accepted messages sent.
> Accepted STR Messages | Indicates the total number of Rx STR-Accepted messages sent.
> RAA Messages | Indicates the total number of Rx RAA messages sent.
> ASA Messages | Indicates the total number of Rx ASA sent.
> Unknown Messages | Indicates the total number of unknown type of Rx messages received.

> ‌

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883