> PCC-Service-Profile Configuration Mode Commands
> The PCC-Service-Profile Configuration Mode is used to define the business logic used by the operator for managing the policy requirements and objectives for the network specific to a group of subscribers in the network. A PCC-Service-Profile manages multiple PCC-Conditions-Groups and associated PCC-Action-Sets pairs in an ordered manner. A maximum of 32 PCC-Service-Profile can be configured in a PCC-Service instance.
> Important: This configuration mode is supported from StarOS Release 12.1 onward.
> default-rulebase-name
> This command is used to associate the default PCC-Rulebase with a PCC-Service-Profile which is to use in Subscriber profile in PCC-Service instance on IPCF node.
> Product
> IPCF
> Privilege
> Security Administrator, Administrator
> Syntax
> [no] default-rulebase-name rulebase_name
> no
> Removes the configured default PCC-Rulebase from PCC-Service-Profile instance on IPCF node.
> rulebase_name
> This keyword specifies the default PCC-Rulebase name to be associated with PCC-Service-Profile instance.
> rulebase_name is the Rulebase name configured at PCEF and must be an alphanumeric string of 1 through 63 characters.
> Usage
> Use this command to associate the default PCC-Rulebase configured on PCEF with a PCC-Service-Profile which is to use in Subscriber profile in PCC-Service instance on IPCF node.
> Example
> Following command associates the PCC-Rulebase named pcc_rulebase1 for PCC-Profile instance on IPCF node.
> default-rulebase-name pcc_rulebase1
> eval-priority
> This command sets the priority for evaluation of PCC-Condition-Group with corresponding PCC-Action-Set in a PCC-Service-Profile which is to use in Subscriber profile in PCC-Service instance on IPCF node.
> Product
> IPCF
> Privilege
> Security Administrator, Administrator
> Syntax
> [no] eval-priority last action-set actionset_name
> [no] eval-priority priority_value timedef timedef_name [condition-group cond_grp_name] action-set actionset_name
> [no] eval-priority priority_value condition-group cond_grp_name action-set actionset_name
> no
> Removes the configured evaluation priority for PCC-Condition-Group with corresponding PCC-Action-Set from PCC-Service-Profile instance on IPCF node.
> last
> Sets last evaluation priority action-set configured for the PCC-Service-Profile instance.
> no removes the last evaluation priority action-set.
> priority_value
> Specifies the priority to be set for PCC-Condition-Group with corresponding PCC-Action-Set in a PCC-Service-Profile instance.
> priority_value must be an integer from 1 through 1023.
> timedef timedef_name
> Specifies a pre-configured time definition in PCC-Timedef Configuration mode and to be set for evaluation priority in a PCC-Service-Profile instance.
> timedef_name is a pre-configured PCC-Timedef and must be an alphanumerical string of 1 through 63 characters.
> condition-group cond_grp_name
> Specifies a pre-configured PCC-Condition-Group to be set for evaluation priority in a PCC-Service-Profile instance.
> cond_grp_name is a pre-configured PCC-Condition-Group and must be an alphanumerical string of 1 through 63 characters.
> Important: An special PCC-Condition-Group “none” can be used to set the default PCC-Condition-Group for any-match typically used for a default condition for a session which does not match any of the conditions specified with higher evaluation priority.
> action-set actionset_name
> Specifies a pre-configured PCC-Action-Set for PCC-Condition-Group to be set for evaluation priority in a PCC-Service-Profile instance.
> actionset_name is a pre-configured PCC-Action-Set and must be an alphanumerical string of 1 through 63 characters.
> Usage
> Use this command to set the priority for evaluation of PCC-Condition-Group with corresponding PCC-Action-Set in a PCC-Service-Profile which is to use in Subscriber profile in PCC-Service instance on IPCF node.
> Additionally timedef is used to accept the Timedefs to support the time-of-day-based procedures to trigger an evaluation priority. The action is triggered only when the time of session lies in the time span defined in specific PCC-Timedef timedef_name.
> Default eval-priority has the lowest priority in the PCC-Service-Profile and as default eval-priority does not have any PCC-Condition-Group associated with it, all the actions in the action-set always be applied.
> A maximum of 64 PCC-Evaluation-Priorities can be configured in a PCC-Service-Profile.
> Example
> Following command sets the evaluation priority value as 1 for PCC-Condition-Group cond_1 along with PCC-Action-Set act_cond1 for PCC-Service-Profile instance on IPCF node:
> eval-priority 1 condition-group cond_1 action-set act_cond1
> Following command sets the evaluation priority value as 2 for PCC-Condition-Group none for any-match typically used for a default condition for a session which does not match any of the conditions specified with higher evaluation priority.along with PCC-Action-Set act_cond1 for PCC-Service-Profile instance on IPCF node:
> eval-priority 1 condition-group none action-set act_cond1
> service-tag
> This command configures the PCC-Service Tags to be used for PCC-Rulename or PCC-Rule-base in a PCC-Service-Profile which is to use in Subscriber profile in PCC-Service instance on IPCF node.
> Product
> IPCF
> Privilege
> Security Administrator, Administrator
> Syntax
> [no] service-tag svc_tag {rule-name rule_name | rulebase-name rulebase_name}
> no
> Removes the configured PCC-Service Tags for PCC-Rulename and PCC-Rulebase from PCC-Service-Profile instance on IPCF node.
> svc_tag
> Specifies the name of the PCC-Service Tag to be used for PCC-Rulename and PCC-Rulebase in a PCC-Service-Profile instance.
> svc_tag must be an alphanumerical string of 1 through 63 characters.
> rule-name rule_name
> Specifies a pre-defined PCC-Rulename on PCEF to be used with PCC-Service Tag svc_tag in a PCC-Service-Profile instance.
> rule_name is a pre-defined PCC-Rulename on PCEF and must be an alphanumerical string of 1 through 63 characters.
> rulebase-name rulebase_name
> Specifies a pre-defined PCC-Rulebase name pre-defined on PCEF to be used with PCC-Service Tag svc_tag in a PCC-Service-Profile instance.
> rulebase_name is a pre-defined PCC-Rulebase name on PCEF and must be an alphanumerical string of 1 through 63 characters.
> Usage
> Use this command to set the PCC-Service Tag for PCC-Rulename and PCC-Rulebase which are defined on PCEF with a PCC-Service-Profile which is to use in Subscriber profile in PCC-Service instance.
> Example
> Following command sets the PCC-Service Tag named Rule1 for PCC-Rulebase named pcc_rulebase1 for PCC-Service-Profile instance on IPCF node:
> service-tag Rule1 rulebase-name pcc_rulebase1
> Following command sets the PCC-Service Tag named Rule11 for PCC-Rulename pcc_rule1 for PCC-Service-Profile instance on IPCF node:
> service-tag Rule11 rule-name pcc_rule1
> usage-monitor
> This command creates/modifies/deletes the PCC-Usage-Monitor Configuration instance to track the usage volume across the PCC-services based on the usage monitor settings in a PCC-service instance for IPCF configuration.
> Product
> IPCF
> Privilege
> Security Administrator, Administrator
> Syntax
> [no] usage-monitor usage_mon_name [-noconfirm]
> no
> Removes the configured PCC-Usage-Monitor from PCC-Service-Profile instance for IPCF configuration.
> usage_mon_name
> Identifies the name of the PCC-Usage-Monitor instance which is to be created or modified through this command.
> The usage_mon_name must be an alphanumerical string from 1 through 63 characters.
> -noconfirm
> Indicates that the command is to execute without any additional prompt and confirmation from the user.
> Warning: If this keyword option is used with no usage-monitor usage_mon_name command, the PCC-Usage-Monitor instance named usage_mon_name is deleted with all configured parameters without prompting any warning or confirmation.
> Usage
> Use this command to create and configure a PCC-Usage-Monitor for PCC-Service-Profile in a PCC-service instance of IPCF configuration.
> A maximum number of 8 PCC-Usage-Monitors can be configured per PCC-Service-Profile.
> Entering this command results in the following prompt:
> [context_name]hostname(config-pcc-profile-usage-mon)#
> The commands configured in this mode are defined in the PCC-Usage-Monitor Configuration Mode Commands chapter of Command Line Interface Reference.
> Caution: This is a critical configuration. The PCC-Usage-Monitor for volume usage can not be configured without this configuration. Any change to this configuration would lead to removing or disabling configuration parameters defined here.
> Example
> Following command configures the PCC-Usage-Monitor named pcc_usage1 to track the usage of service with in a PCC-Service-Profile instance.
> usage-monitor pcc_usage1
> unknown-services-treatment
> This command configures the PCC-Service for handling of unknown services at IPCF which is to be used in Subscriber profile in PCC-Service instance on IPCF node.
> Product
> IPCF
> Privilege
> Security Administrator, Administrator
> Syntax
> [default] unknown-services-treatment {not-allowed | qos-profile qos_prof_name precedence from start_preced to end_preced order {ascending | descending}}
> default
> Sets the configured PCC-Service for handling of unknown services at IPCF to default value of “Not allowed” which is to be used in Subscriber profile in PCC-Service instance on IPCF node.
> not-allowed
> Sets the PCC-Service-Profile instance to reject the packet filters and does not installs any dynamic rule when IPCF receives any request to authorize Packet Filters from PCEF and no matching service flow is found in data service list.
> qos-profile qos_prof_name
> Specifies a pre-defined PCC-QoS profile name to be used to create dynamic rule when IPCF receives any request to authorize Packet Filters from PCEF and no matching service flow is found in data service list.
> qos_prof_name is a pre-defined PCC-QoS Profile and must be an alphanumerical string of 1 through 63 characters.
> precedence from start_preced to end_preced
> Specifies the precedence parameters to install dynamic rules for selection of QoS profile when QoS profile is configured to create dynamic rule when IPCF receives any request to authorize Packet Filters from PCEF and no matching service flow is found in data service list.
> start_preced is an integer between 1 through 65535 and must be less than end_preced value where end_preced is an integer between 1 through 65535 and must be more than start_preced value
> order {ascending | descending}
> Specifies the order of precedence for QoS profile to be used to install dynamic rule when IPCF receives any request to authorize Packet Filters from PCEF and no matching service flow is found in data service list.

> • | ascending sets the precedence setting in ascending order.

> • | descending sets the precedence setting in descending order.

> Usage
> Use this command to set the PCC-Service Tag for PCC-Rulename and PCC-Rulebase which are defined on PCEF with a PCC-Service-Profile which is to use in Subscriber profile in PCC-Service instance.
> Whenever IPCF receives any request to authorize Packet Filters from PCEF, it does a lookup in data service list to find a match. If No service flow is found matching then the requested filters are treated as unknown service request and handled as per the mentioned configuration.
> When unknown-service-treatment is set to not-allowed, then Packet Filters are rejected and no dynamic rule is installed. Otherwise, dynamic rule is created using the requested packet filters, data rates mentioned in the QoS profile name qos_prof_name and precedence value derived from the configured values.
> The precedence configuration works in following manner:

> • | If precedence limits are configured as 1000 to 2000 with order ascending then precedence of subsequent dynamic rules will go from 1000 to 2000.

> • | If precedence limits are configured as 1000 to 2000 with order descending then precedence of subsequent dynamic rules will go from 2000 to 1000.

> Example
> Following command sets the PCC-Service for handling of unknown services for PCC-Service-Profile instance on IPCF node to default action of not allowed:
> default unknown-services-treatment

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883