> SHAPP Schema Statistics
> The Sh Application (SHAPP) schema provides the following type of statistics:

> • | Counter: A counter records incremental data cumulatively and rolls over when the counter limit is reached. The limit depends upon the counter data type.

> • | Gauge: A gauge statistic indicates a single value representative of a single instance. This type is often used to track particular events in time.

> • | Fixed Value String: A string statistic indicates the name of a service instance or a node.

> Important: The format string syntax is described by Schema Format String Syntax in the Bulk Statistics Overview chapter.
> Important: Unless otherwise indicated all statistics are of proprietary type based on 3GPP standard.
> Important: Unless otherwise indicated, all statistics are counters. For statistics with the Int32 data type, the roll-over to zero limit is 4,294,967,295. For statistics with the Int64 data type, the roll-over to zero limit is 18,446,744,073,709,551,615. All statistics are cumulative and reset only by one of the following methods: roll-over (as described above), after a system restart, or after a clear command is performed. All statistics are considered standards-based unless otherwise noted.
> The following variables are supported:
> SHAPP Schema Statistics

> Statistic | Description | Data Type
> sh_db_query | Indicates total number of database queries made during Sh call processing. Trigger: When DB API is called. Availability: Available across Sh application. | Gauge/ Int64
> db_rid_usage | Indicates current usage count per Rating Id. Trigger: When a given rating id is used. Availability: Available across Sh application. | Gauge/ Int64
> db_umon_usage | Indicates current usage count per usage monitor. Trigger: When a usage monitor is used. Availability: Available across Sh application. | Gauge/ Int64
> db_sess_usage | Indicates current session usage. Trigger: Usage for a given session. Availability: Available across Sh application. | Gauge/ Int64
> db_rid_upd | Indicates total number of updates per rating id. Trigger: When a given rating id is updated. Availability: Available across Sh application. | Gauge/ Int64
> db_umon_upd | Indicates total number of database usage updates, incremented for each database update, each plan in a Profile Update Request.- (PUR). Trigger: When a database usage is updated for PUR. Availability: Available across Sh application. | Gauge/ Int64
> sh_db_err | Indicates total number of database errors encountered in processing of Sh calls. Trigger: When database API has returned an error. Availability: Available across Sh application. | Gauge/ Int64
> sh_notif | Indicates total number of Push Notification Request (PNR) IPC messages sent by application manager to Sh controller. Trigger: When PNR is generated at application manager. Availability: Available across Sh application. | Gauge/ Int64
> sh_db_profile | Indicates requested subscriber profile. Trigger: When a subscriber profile is requested. Availability: Available across Sh application. | Gauge/ Int64
> snr_in | Indicates total number of Subscriber Notification Request (SNRs) messages received. Trigger: When an SNR is received. Availability: Available across Sh application. | Gauge/ Int64
> sna_out | Indicates Subscriber Notification Answer (SNA) Sent. Trigger: When an SNR is sent. Availability: Available across Sh application. | Gauge/ Int64
> pur_in | Indicates total number of Profile Update Request (PUR) messages received. Trigger: When a PUR is received. Availability: Available across Sh application. | Gauge/ Int64
> pua_out | Indicates total number of Profile Update Answer (PUA) replies sent. Trigger: When a PUA is sent. Availability: Available across Sh application. | Gauge/ Int64
> pnr_out | Indicates total number of Push Notification Request (PNR) messages sent. Trigger: When a PNR is sent. Availability: Available across Sh application. | Gauge/ Int64
> pna_in | Indicates Push Notification Answer (PNA) messages received. Trigger: When a PNA is received. Availability: Available across Sh application. | Gauge/ Int64
> ipc_appmgr_req | Indicates total number of IPC requests sent to application manager by Sh controller. Trigger: When an IPC request is sent to application manager by Sh controller. Availability: Available across Sh application. | Gauge/ Int64

> ‌

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883