> Content Filtering Application MIB
> The figure that follows illustrates the hierarchical structure of the management information base (MIB) for the Content Filtering service applications.
> MIB Textual Conventions
> starentMIB(8164).starentMIBObjects(1).starentCFMIB(100).starCfCommonMIB(1)
> starentMIB(8164).starentMIBObjects(1).starentCFMIB(100).starCFCOMMONMIB(1).starCFCOMMONMIBConformances(3)
> starentMIB(8164).starentMIBObjects(1).starentCFMIB(100).starCFCOMMONMIB(1).starCFCOMMONMIBConformances(3).starCFCOMMONMIBCompliances(1)
> Object
> starCFCOMMONMIBCompliance
> Object ID
> enterprises.8164.1.100.1.3.1.1
> Description
> The compliance statements for entities which implement the STARENT CF MIB.
> Objects
> starCFCOMMONNotifMgmtGroup
> starentMIB(8164).starentMIBObjects(1).starentCFMIB(100).starCfCommonMIB(1)
> starentMIB(8164).starentMIBObjects(1).starentCFMIB(100).starCFCOMMONMIB(1).starCFCOMMONMIBConformances(3)
> starentMIB(8164).starentMIBObjects(1).starentCFMIB(100).starCFCOMMONMIB(1).starCFCOMMONMIBConformances(3).starCFCOMMONMIBCompliances(1)
> Object
> starCFCOMMONMIBCompliance
> Object ID
> enterprises.8164.1.100.1.3.1.1
> Description
> The compliance statements for entities which implement the STARENT CF MIB.
> Objects
> starCFCOMMONNotifMgmtGroup
> starentMIB(8164).starentMIBObjects(1).starentCFMIB(100).starCFCOMMONMIB(1).starCFCOMMONMIBConformances(3)
> starentMIB(8164).starentMIBObjects(1).starentCFMIB(100).starCFCOMMONMIB(1).starCFCOMMONMIBConformances(3).starCFCOMMONMIBGroup(2)
> Object Group
> starCFCOMMONNotifMgmtGroup
> Object ID
> enterprises.8164.1.100.1.3.2.1
> Description
> A collection of objects related with notification management on CF-Common.
> Objects
> starCfNotifRaisedTime starCfThresholdConfigured starCfThresholdMeasured starCfIPAddr starCfNotifInfo
> starentMIB(8164).starentMIBObjects(1).starentCFMIB(100).starCFCDPMIB(2)
> starentMIB(8164).starentMIBObjects(1).starentCFMIB(100).starCFCDPMIB(2).starCFCDPMIBTraps(2)
> Object
> starCfCdpStart
> Object ID
> enterprises.8164.1.100.2.2.1
> Description
> This notification is generated when CDP server starts and CF-CDP server process comes up.
> Objects
> starCfNotifRaisedTime starCfNotifInfo
> Object
> starCfCdpStop
> Object ID
> enterprises.8164.1.100.2.2.2
> Description
> This notification is generated when CDP server stops and CF-CDP server process goes down.
> Objects
> starCfNotifRaisedTime starCfNotifInfo
> Object
> starCfCdpRestart
> Object ID
> enterprises.8164.1.100.2.2.3
> Description
> This notification is generated when CDP server restarts and CF-CDP server process again comes up.
> Objects
> starCfNotifRaisedTime starCfNotifInfo
> Object
> starCfCdpProcApiOpFailed
> Object ID
> enterprises.8164.1.100.2.2.4
> Description
> This notification is generated by CF-CDP when the CFLIB API Operation fails.
> Objects
> starCfNotifRaisedTime starCfParseFileName starCfNotifInfo
> Object
> starCfCdpApiVerError
> Object ID
> enterprises.8164.1.100.2.2.5
> Description
> Notification generated by CF-CDP when the CFLIB DB Version Error occurs.
> Objects
> starCfNotifRaisedTime starCfParseFileName starCfNotifInfo
> Object
> starCfCdpThreshCPUUtilization
> Object ID
> enterprises.8164.1.100.2.2.6
> Description
> This notification is generated by CF-System when the CDP process’s CPU usage threshold exceeds the configured limit. The starCfThresholdMeasured indicates the current CDP process’s CPU usage in percentage.
> Objects
> starCfNotifRaisedTime starCfThresholdMeasured
> Object
> starCfCdpClearThreshCPUUtilization
> Object ID
> enterprises.8164.1.100.2.2.7
> Description
> This notification is generated by CF-System when the CDP process’s CPU usage comes back to below the threshold limit. The starCfThresholdMeasured indicates the current CDP process’s CPU usage in percentage.
> Objects
> starCfNotifRaisedTime starCfThresholdMeasured
> Object
> starCfCdpThreshDiskUtilization
> Object ID
> enterprises.8164.1.100.2.2.8
> Description
> This notification is generated by CF-System when the CDP process’s disk usage threshold exceeds the configured limit. The starCfThresholdMeasured indicates the current CDP process’s disk usage in percentage.
> Objects
> starCfNotifRaisedTime starCfThresholdMeasured
> Object
> starCfCdpClearThreshDiskUtilization
> Object ID
> enterprises.8164.1.100.2.2.9
> Description
> This notification is generated by CF-System when the CDP process’s disk usage comes back to below the threshold limit. The starCfThresholdMeasured indicates the current CDP process’s disk usage in percentage.
> Objects
> starCfNotifRaisedTime starCfThresholdMeasured
> Object
> starCfCdpThreshSwapUtilization
> Object ID
> enterprises.8164.1.100.2.2.10
> Description
> This notification is generated by CF-System when the CDP process’s swap usage threshold exceeds the configured limit. The starCfThresholdMeasured indicates the current CDP process’s swap usage in percentage.
> Objects
> starCfNotifRaisedTime starCfThresholdMeasured
> Object
> starCfCdpClearThreshSwapUtilization
> Object ID
> enterprises.8164.1.100.2.2.11
> Description
> This notification is generated by CF-System when the CDP process’s swap usage comes back to below the threshold limit. The starCfThresholdMeasured indicates the current CDP process’s swap usage in percentage.
> Objects
> starCfNotifRaisedTime starCfThresholdMeasured
> Object
> starCfCdpProcReportErrWithMsg
> Object ID
> enterprises.8164.1.100.2.2.12
> Description
> This notification is generated by CF-CDP when any system error is generated by CFLIB API.
> Objects
> starCfNotifRaisedTime, starCfParseFileName, starCfNotifInfo
> Object
> StarCfCdpProcApiCfdcmErrWithMsg
> Object ID
> enterprises.8164.1.100.2.2.13
> Description
> This notification is generated by CFDCM Library when any error other than system error occurs.
> Objects
> starCfNotifRaisedTime, starCfParseFileName, starCfNotifInfo
> starentMIB(8164).starentMIBObjects(1).starentCFMIB(100).starCFCDPMIB(2).starCFCDPMIBConformances(3)
> starentMIB(8164).starentMIBObjects(1).starentCFMIB(100).starCFCDPMIB(2).starCFCDPMIBConformances(3).starCFCDPMIBGroup(2)
> Object Group
> starCFCDPNotifMgmtGroup
> Object ID
> enterprises.8164.1.100.2.3.2.1
> Description
> A collection of objects related with notification management on CF-CDP.
> Objects
> starCfParseFileName
> Object Group
> starCFCDPNotifGroup
> Object ID
> enterprises.8164.1.100.2.3.2.2
> Description
> A collection of CF-CDP notifications.
> Objects
> starCfCdpStart starCfCdpStop starCfCdpRestart starCfCDPApiOpFailed starCfCdpApiVerError starCfCdpThreshCPUUtilization starCfCdpClearThreshCPUUtilization starCfCdpThreshDiskUtilization starCfCdpClearThreshDiskUtilization starCfCdpThreshSwapUtilization starCfCdpClearThreshSwapUtilization starCfCdpProcReportErrWithMsg, StarCfCdpProcApiCfdcmErrWithMsg starCfCdpProcApiPermissionDenied starCfCdpProcApiInvalidAgrs
> starentMIB(8164).starentMIBObjects(1).starentCFMIB(100).starCFCDPMIB(2).starCFCDPMIBConformances(3)
> starentMIB(8164).starentMIBObjects(1).starentCFMIB(100).starCFCDPMIB(2).starCFCDPMIBConformances(3).starCFCDPMIBGroup(2)
> Object Group
> starCFCDPNotifMgmtGroup
> Object ID
> enterprises.8164.1.100.2.3.2.1
> Description
> A collection of objects related with notification management on CF-CDP.
> Objects
> starCfParseFileName
> Object Group
> starCFCDPNotifGroup
> Object ID
> enterprises.8164.1.100.2.3.2.2
> Description
> A collection of CF-CDP notifications.
> Objects
> starCfCdpStart starCfCdpStop starCfCdpRestart starCfCDPApiOpFailed starCfCdpApiVerError starCfCdpThreshCPUUtilization starCfCdpClearThreshCPUUtilization starCfCdpThreshDiskUtilization starCfCdpClearThreshDiskUtilization starCfCdpThreshSwapUtilization starCfCdpClearThreshSwapUtilization starCfCdpProcReportErrWithMsg, StarCfCdpProcApiCfdcmErrWithMsg starCfCdpProcApiPermissionDenied starCfCdpProcApiInvalidAgrs
> starentMIB(8164).starentMIBObjects(1).starentCFMIB(100).starCFREMIB(3)
> starentMIB(8164).starentMIBObjects(1).starentCFMIB(100).starCFREMIB(3).starCFREMIBTraps(2)
> Object
> starCfReStart
> Object ID
> enterprises.8164.1.100.3.2.1
> Description
> This notification is generated when Report Engine starts and CF-RE process comes up.
> Objects
> starCfNotifRaisedTime
> Object
> starCfReStop
> Object ID
> enterprises.8164.1.100.3.2.2
> Description
> This notification is generated when Report Engine stops and CF-RE process goes down.
> Objects
> starCfNotifRaisedTime
> Object
> starCfReRestart
> Object ID
> enterprises.8164.1.100.3.2.3
> Description
> This notification is generated when Report Engine restarts and CF-RE process restart is detected.
> Objects
> starCfNotifRaisedTime
> Object
> starCfReFileParsingAborted
> Object ID
> enterprises.8164.1.100.3.2.4
> Description
> This notification is generated by CF-RE when Report Engine fails to parse EDR.
> Objects
> starCfNotifRaisedTime starCfParseFileName
> Object
> starCfReThreshCPUUtilization
> Object ID
> enterprises.8164.1.100.3.2.5
> Description
> This notification is generated by CF-System when the Report Engine process’s CPU usage threshold exceeds the configured limit. The starCfThresholdMeasured indicates the current Report Engine process’s CPU usage in percentage.
> Objects
> starCfNotifRaisedTime starCfThresholdMeasured
> Object
> starCfReClearThreshCPUUtilization
> Object ID
> enterprises.8164.1.100.3.2.6
> Description
> This notification is generated by CF-System when the Report Engine process’s CPU usage comes back to below the threshold limit. The starCfThresholdMeasured indicates the current Report Engine process’s CPU usage in percentage.
> Objects
> starCfNotifRaisedTime starCfThresholdMeasured
> Object
> starCfReThreshDiskUtilization
> Object ID
> enterprises.8164.1.100.3.2.7
> Description
> This notification is generated by CF-System when the Report Engine process’s disk usage threshold exceeds the configured limit. The starCfThresholdMeasured indicates the current Report Engine process’s disk usage in percentage.
> Objects
> starCfNotifRaisedTime starCfThresholdMeasured
> Object
> starCfReClearThreshDiskUtilization
> Object ID
> enterprises.8164.1.100.3.2.8
> Description
> This notification is generated by CF-System when the Report Engine process’s disk usage comes back to below the threshold limit. The starCfThresholdMeasured indicates the current Report Engine process’s disk usage in percentage.
> Objects
> starCfNotifRaisedTime starCfThresholdMeasured
> Object
> starCfDbThreshCPUUtilization
> Object ID
> enterprises.8164.1.100.3.2.9
> Description
> This notification is generated by CF-System when the Postgres process’s CPU usage threshold exceeds the configured limit. The starCfThresholdMeasured indicates the current Postgres process’s CPU usage in percentage.
> Objects
> starCfNotifRaisedTime starCfThresholdMeasured
> Object
> starCfDbClearThreshCPUUtilization
> Object ID
> enterprises.8164.1.100.3.2.10
> Description
> This notification is generated by CF-System when the Postgres process’s CPU usage comes back to below the threshold limit. The starCfThresholdMeasured indicates the current Postgres process’s CPU usage in percentage.
> Objects
> starCfNotifRaisedTime starCfThresholdMeasured
> Object
> starCfDbThreshDiskUtilization
> Object ID
> enterprises.8164.1.100.3.2.11
> Description
> This notification is generated by CF-System when the Postgres process’s disk usage threshold exceeds the configured limit. The starCfThresholdMeasured indicates the current Postgres process’s disk usage in percentage.
> Objects
> starCfNotifRaisedTime starCfThresholdMeasured
> Object
> starCfDbClearThreshDiskUtilization
> Object ID
> enterprises.8164.1.100.3.2.12
> Description
> This notification is generated by CF-System when the Postgres process’s disk usage comes back to below the threshold limit. The starCfThresholdMeasured indicates the current Postgres process’s disk usage in percentage.
> Objects
> starCfNotifRaisedTime starCfThresholdMeasured
> starentMIB(8164).starentMIBObjects(1).starentCFMIB(100).starCFREMIB(3)
> starentMIB(8164).starentMIBObjects(1).starentCFMIB(100).starCFREMIB(3).starCFREMIBTraps(2)
> Object
> starCfReStart
> Object ID
> enterprises.8164.1.100.3.2.1
> Description
> This notification is generated when Report Engine starts and CF-RE process comes up.
> Objects
> starCfNotifRaisedTime
> Object
> starCfReStop
> Object ID
> enterprises.8164.1.100.3.2.2
> Description
> This notification is generated when Report Engine stops and CF-RE process goes down.
> Objects
> starCfNotifRaisedTime
> Object
> starCfReRestart
> Object ID
> enterprises.8164.1.100.3.2.3
> Description
> This notification is generated when Report Engine restarts and CF-RE process restart is detected.
> Objects
> starCfNotifRaisedTime
> Object
> starCfReFileParsingAborted
> Object ID
> enterprises.8164.1.100.3.2.4
> Description
> This notification is generated by CF-RE when Report Engine fails to parse EDR.
> Objects
> starCfNotifRaisedTime starCfParseFileName
> Object
> starCfReThreshCPUUtilization
> Object ID
> enterprises.8164.1.100.3.2.5
> Description
> This notification is generated by CF-System when the Report Engine process’s CPU usage threshold exceeds the configured limit. The starCfThresholdMeasured indicates the current Report Engine process’s CPU usage in percentage.
> Objects
> starCfNotifRaisedTime starCfThresholdMeasured
> Object
> starCfReClearThreshCPUUtilization
> Object ID
> enterprises.8164.1.100.3.2.6
> Description
> This notification is generated by CF-System when the Report Engine process’s CPU usage comes back to below the threshold limit. The starCfThresholdMeasured indicates the current Report Engine process’s CPU usage in percentage.
> Objects
> starCfNotifRaisedTime starCfThresholdMeasured
> Object
> starCfReThreshDiskUtilization
> Object ID
> enterprises.8164.1.100.3.2.7
> Description
> This notification is generated by CF-System when the Report Engine process’s disk usage threshold exceeds the configured limit. The starCfThresholdMeasured indicates the current Report Engine process’s disk usage in percentage.
> Objects
> starCfNotifRaisedTime starCfThresholdMeasured
> Object
> starCfReClearThreshDiskUtilization
> Object ID
> enterprises.8164.1.100.3.2.8
> Description
> This notification is generated by CF-System when the Report Engine process’s disk usage comes back to below the threshold limit. The starCfThresholdMeasured indicates the current Report Engine process’s disk usage in percentage.
> Objects
> starCfNotifRaisedTime starCfThresholdMeasured
> Object
> starCfDbThreshCPUUtilization
> Object ID
> enterprises.8164.1.100.3.2.9
> Description
> This notification is generated by CF-System when the Postgres process’s CPU usage threshold exceeds the configured limit. The starCfThresholdMeasured indicates the current Postgres process’s CPU usage in percentage.
> Objects
> starCfNotifRaisedTime starCfThresholdMeasured
> Object
> starCfDbClearThreshCPUUtilization
> Object ID
> enterprises.8164.1.100.3.2.10
> Description
> This notification is generated by CF-System when the Postgres process’s CPU usage comes back to below the threshold limit. The starCfThresholdMeasured indicates the current Postgres process’s CPU usage in percentage.
> Objects
> starCfNotifRaisedTime starCfThresholdMeasured
> Object
> starCfDbThreshDiskUtilization
> Object ID
> enterprises.8164.1.100.3.2.11
> Description
> This notification is generated by CF-System when the Postgres process’s disk usage threshold exceeds the configured limit. The starCfThresholdMeasured indicates the current Postgres process’s disk usage in percentage.
> Objects
> starCfNotifRaisedTime starCfThresholdMeasured
> Object
> starCfDbClearThreshDiskUtilization
> Object ID
> enterprises.8164.1.100.3.2.12
> Description
> This notification is generated by CF-System when the Postgres process’s disk usage comes back to below the threshold limit. The starCfThresholdMeasured indicates the current Postgres process’s disk usage in percentage.
> Objects
> starCfNotifRaisedTime starCfThresholdMeasured
> starentMIB(8164).starentMIBObjects(1).starentCFMIB(100).starCFREMIB(3).starCFREMIBConformances(3)
> starentMIB(8164).starentMIBObjects(1).starentCFMIB(100).starCfReMIB(3).starCfReMIBConformances(3).starCfReMIBGroup(2)
> Object Group
> starCFEMSNotifMgmtGroup
> Object ID
> enterprises.8164.1.100.3.3.2.1
> Description
> A collection of objects related with notification management on CF Report Engine.
> Objects
> starCfEmsMcrdbsHostAddress starCfEmsDbType starCfEmsSourceDbFileName starCfEmsCdpHostAddress starCfEmsFromDbType starCfEmsToDbType starCfEmsDestDbFileName
> Object Group
> starCFRENotifGroup
> Object ID
> enterprises.8164.1.100.3.3.2.2
> Description
> A collection of CF-CDP notifications.
> Objects
> starCfReStart starCfReStop starCfReRestart starCfReFileParsingAborted starCfReThreshCPUUtilization starCfReClearThreshCPUUtilization starCfReThreshDiskUtilization starCfReClearThreshDiskUtilization starCfDbThreshCPUUtilization starCfDbClearThreshCPUUtilization starCfDbThreshDiskUtilization starCfDbClearThreshDiskUtilization
> starentMIB(8164).starentMIBObjects(1).starentCFMIB(100).starCFREMIB(3).starCFREMIBConformances(3)
> starentMIB(8164).starentMIBObjects(1).starentCFMIB(100).starCfReMIB(3).starCfReMIBConformances(3).starCfReMIBGroup(2)
> Object Group
> starCFEMSNotifMgmtGroup
> Object ID
> enterprises.8164.1.100.3.3.2.1
> Description
> A collection of objects related with notification management on CF Report Engine.
> Objects
> starCfEmsMcrdbsHostAddress starCfEmsDbType starCfEmsSourceDbFileName starCfEmsCdpHostAddress starCfEmsFromDbType starCfEmsToDbType starCfEmsDestDbFileName
> Object Group
> starCFRENotifGroup
> Object ID
> enterprises.8164.1.100.3.3.2.2
> Description
> A collection of CF-CDP notifications.
> Objects
> starCfReStart starCfReStop starCfReRestart starCfReFileParsingAborted starCfReThreshCPUUtilization starCfReClearThreshCPUUtilization starCfReThreshDiskUtilization starCfReClearThreshDiskUtilization starCfDbThreshCPUUtilization starCfDbClearThreshCPUUtilization starCfDbThreshDiskUtilization starCfDbClearThreshDiskUtilization
> starentMIB(8164).starentMIBObjects(1).starentCFMIB(100).starCFCCIMIB(4)
> starentMIB(8164).starentMIBObjects(1).starentCFMIB(100).starCfCciMIB(4).starCfCciMIBConformances(3).starCfCciMIBGroup(2)
> Object Group
> starCFEMSNotifGroup
> Object ID
> enterprises.8164.1.100.4.3.2.1
> Description
> A collection of CF-CDP notifications.
> Objects
> starCfEmsServerProcStart starCfEmsServerProcStop starCfEmsDbImportFailed starCfEmsDbImportSucceeded starCfEmsDbExportFailed starCFEMSDbExportSucceeded starCfEmsDbConversionFailed starCfEmsDbConversionSucceeded starCfEmsFtpConnetionFailed
> starentMIB(8164).starentMIBObjects(1).starentCFMIB(100).starCFCCIMIB(4)
> starentMIB(8164).starentMIBObjects(1).starentCFMIB(100).starCfCciMIB(4).starCfCciMIBConformances(3).starCfCciMIBGroup(2)
> Object Group
> starCFEMSNotifGroup
> Object ID
> enterprises.8164.1.100.4.3.2.1
> Description
> A collection of CF-CDP notifications.
> Objects
> starCfEmsServerProcStart starCfEmsServerProcStop starCfEmsDbImportFailed starCfEmsDbImportSucceeded starCfEmsDbExportFailed starCFEMSDbExportSucceeded starCfEmsDbConversionFailed starCfEmsDbConversionSucceeded starCfEmsFtpConnetionFailed
> starentMIB(8164).starentMIBObjects(1).starentCFMIB(100).starCFCCIMIB(4)
> starentMIB(8164).starentMIBObjects(1).starentCFMIB(100).starCfCciMIB(4).starCfCciMIBConformances(3).starCfCciMIBGroup(2)
> Object Group
> starCFEMSNotifGroup
> Object ID
> enterprises.8164.1.100.4.3.2.1
> Description
> A collection of CF-CDP notifications.
> Objects
> starCfEmsServerProcStart starCfEmsServerProcStop starCfEmsDbImportFailed starCfEmsDbImportSucceeded starCfEmsDbExportFailed starCFEMSDbExportSucceeded starCfEmsDbConversionFailed starCfEmsDbConversionSucceeded starCfEmsFtpConnetionFailed
> starentMIB(8164).starentMIBObjects(1).starentCFMIB(100).starCFCCIMIB(4)
> starentMIB(8164).starentMIBObjects(1).starentCFMIB(100).starCfCciMIB(4).starCfCciMIBConformances(3).starCfCciMIBGroup(2)
> Object Group
> starCFEMSNotifGroup
> Object ID
> enterprises.8164.1.100.4.3.2.1
> Description
> A collection of CF-CDP notifications.
> Objects
> starCfEmsServerProc
> Start starCfEmsServerProcStop starCfEmsDbImportFailed starCfEmsDbImportSucceeded starCfEmsDbExportFailed starCFEMSDbExportSucceeded starCfEmsDbConversionFailed starCfEmsDbConversionSucceeded starCfEmsFtpConnetionFailed
> starentMIB(8164).starentMIBObjects(1).starentCFMIB(100).starCFMCRDBSMIB(6)
> starentMIB(8164).starentMIBObjects(1).starentCFMIB(100).starCfMcrdbsMIB(6).starCfMcrdbsMIBConformances(3)
> starentMIB(8164).starentMIBObjects(1).starentCFMIB(100).starCFMCRDBSMIB(6).starCFMCRDBSMIBConformances(3).starCFMCRDBSMIBGroup(2)
> Object Group
> starCFMDBNotifMgmtGroup
> Object ID
> enterprises.8164.1.100.6.3.2.1
> Description
> A collection of objects related with notification management on CF-MCRDBS.
> Objects
> starCfParseFileName
> Object Group
> starCFMDBNotifGroup
> Object ID
> enterprises.8164.1.100.6.3.2.2
> Description
> A collection of CF-MCRDBS notifications.
> Objects
> starCfMdbProcStart starCfMdbProcStop starCfMdbProcDbAbsent starCfMdbProcApiOpFailed starCfMdbProcDbParseErrot starCfMdbProcMemUsageOverLimit starCfMdbProcmemUsageNormal starCfMdbProcCpuUsageOverLimit starCfMdbProcCpuUsageNormal starCfMdbProcDiskUsageOverLimit starCfMdbProcDiskUsageNormalstarCfMdbProcInvalidFileName starCfMdbProcReportErrWithMsg starCfMdbProcCfdcmErrWithMsg starCfMdbProcMcrdbsErrWithMsg
> starentMIB(8164).starentMIBObjects(1).starentCFMIB(100).starCFMCRDBSMIB(6)
> starentMIB(8164).starentMIBObjects(1).starentCFMIB(100).starCfMcrdbsMIB(6).starCfMcrdbsMIBConformances(3)
> starentMIB(8164).starentMIBObjects(1).starentCFMIB(100).starCFMCRDBSMIB(6).starCFMCRDBSMIBConformances(3).starCFMCRDBSMIBGroup(2)
> Object Group
> starCFMDBNotifMgmtGroup
> Object ID
> enterprises.8164.1.100.6.3.2.1
> Description
> A collection of objects related with notification management on CF-MCRDBS.
> Objects
> starCfParseFileName
> Object Group
> starCFMDBNotifGroup
> Object ID
> enterprises.8164.1.100.6.3.2.2
> Description
> A collection of CF-MCRDBS notifications.
> Objects
> starCfMdbProcStart starCfMdbProcStop starCfMdbProcDbAbsent starCfMdbProcApiOpFailed starCfMdbProcDbParseErrot starCfMdbProcMemUsageOverLimit starCfMdbProcmemUsageNormal starCfMdbProcCpuUsageOverLimit starCfMdbProcCpuUsageNormal starCfMdbProcDiskUsageOverLimit starCfMdbProcDiskUsageNormalstarCfMdbProcInvalidFileName starCfMdbProcReportErrWithMsg starCfMdbProcCfdcmErrWithMsg starCfMdbProcMcrdbsErrWithMsg
> starentMIB(8164).starentMIBObjects(1).starentCFMIB(100).starCFMCRDBSMIB(6)
> starentMIB(8164).starentMIBObjects(1).starentCFMIB(100).starCfMcrdbsMIB(6).starCfMcrdbsMIBConformances(3)
> starentMIB(8164).starentMIBObjects(1).starentCFMIB(100).starCFMCRDBSMIB(6).starCFMCRDBSMIBConformances(3).starCFMCRDBSMIBGroup(2)
> Object Group
> starCFMDBNotifMgmtGroup
> Object ID
> enterprises.8164.1.100.6.3.2.1
> Description
> A collection of objects related with notification management on CF-MCRDBS.
> Objects
> starCfParseFileName
> Object Group
> starCFMDBNotifGroup
> Object ID
> enterprises.8164.1.100.6.3.2.2
> Description
> A collection of CF-MCRDBS notifications.
> Objects
> starCfMdbProcStart starCfMdbProcStop starCfMdbProcDbAbsent starCfMdbProcApiOpFailed starCfMdbProcDbParseErrot starCfMdbProcMemUsageOverLimit starCfMdbProcmemUsageNormal starCfMdbProcCpuUsageOverLimit starCfMdbProcCpuUsageNormal starCfMdbProcDiskUsageOverLimit starCfMdbProcDiskUsageNormalstarCfMdbProcInvalidFileName starCfMdbProcReportErrWithMsg starCfMdbProcCfdcmErrWithMsg starCfMdbProcMcrdbsErrWithMsg

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883