> ACS Group-of-Prefixed-URLs Configuration Mode Commands
> The ACS Group-of-Prefixed-URLs Configuration Mode is used to create and configure groups of prefixed URLs.
> Important: This configuration mode is customer specific. For more information, please contact your local service representative.
> Important: The commands or keywords/variables that are available are dependent on platform type, product version, and installed license(s).
> end
> Exits the current configuration mode and returns to the Exec mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> end
> Usage
> Use this command to return to the Exec mode.
> exit
> Exits the current mode and returns to the parent configuration mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> exit
> Usage
> Use this command to return to the parent configuration mode.
> prefixed-url
> This command enables adding/removing URLs from the group.
> Important: A maximum of 10 URLs can be added per group.
> Product
> ACS
> Privilege
> Security Administrator, Administrator
> Syntax
> [ no ] prefixed-url url
> no
> Removes the specified URL from the group.
> url
> Specifies the URL.
> url must be an alpha and/or numeric string of 1 through 63 characters in length.
> Usage
> Use this command to add/remove URLs to be filtered from the group.
> Example
> The following command adds the URL http://abc.net to the current group:
> prefixed-url http://abc.net

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883