> CSCF Charging Configuration Mode Commands
> The CSCF Charging Configuration Mode is used to manage CSCF service policy profiles within the system.
> Important: The commands or keywords/variables that are available are dependent on platform type, product version, and installed license(s).
> end
> Exits the current mode and returns to the Exec Mode.
> Product
> All
> Privilege
> Administrator
> Syntax
> end
> Usage
> Change the mode back to the Exec mode.
> exclude
> Configures the service to exclude SIP requests from the Rf charging configuration.
> Product
> SCM
> Privilege
> Administrator
> Syntax
> [ no ] exclude { custom sip_method | invite | message | notify | register | subscribe | update }
> no
> Removes the exclusion of the specified SIP request message type.
> custom sip_method
> Specifies CUSTOM SIP requests that are to be excluded from Rf charging.
> sip_method can be a name of any SIP method and be from 1 to 31 alpha and/or numeric characters.
> invite
> Specifies that INVITE SIP requests are to be excluded from Rf charging.
> message
> Specifies that MESSAGE SIP requests are to be excluded from Rf charging.
> notify
> Specifies that NOTIFY SIP requests are to be excluded from Rf charging.
> register
> Specifies that REGISTER SIP requests are to be excluded from Rf charging.
> subscribe
> Specifies that SUBSCRIBE SIP requests are to be excluded from Rf charging.
> update
> Specifies that UPDATE SIP requests are to be excluded from Rf charging.
> Usage
> Use this command to exclude specific SIP requests from Rf charging.
> Example
> The following command configures the service to exclude SIP REGISTER requests from Rf charging:
> exclude register
> exit
> Exits the current mode and returns to the previous mode.
> Product
> All
> Privilege
> Administrator
> Syntax
> exit
> Usage
> Return to the previous mode.

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883