> Configuring and Maintaining Bulk Statistics
> This chapter provides configuration information for:

> • | Configuring Communication With the Collection Server

> • | Viewing Collected Bulk Statistics Data

> • | Manually Gathering and Transferring Bulk Statistics

> • | Clearing Bulk Statistics Counters and Information

> • | Bulk Statistics Event Log Messages

> Configuring Communication With the Collection Server
> Two configuration methods are available for defining how bulk statistics are collected and managed. A “standard” configuration allows the system to automatically assign a number to the bulk statistic file. Optionally, a number can be specified by an administrator in the optional configuration method. Command details and descriptions of keywords and variables for commands in this chapter are located in the Bulk Statistics Configuration Mode Commands chapter and the Bulk Statistics File Configuration Mode Commands chapter in the Command Line Interface Reference.
> Configuring Standard Settings
> The configuration example in this section defines basic operation of the bulk statistics feature. Use the following example configuration to set up the system to communicate with the statistic collection server:
> configure
> bulkstats mode
> schema <name> format <format_string>
> sample-interval <time_interval>
> transfer-interval <xmit_time_interval>
> limit <mem_limit>
> exit
> bulkstats collection
> end
> Configuring Optional Settings
> This section describes optional commands that can be used within the bulk statistics configuration mode. Specifically, bulk statistic “files” under which to group the bulk statistic configuration are configured using commands in this section. “Files” are used to group bulk statistic schema, delivery options, and receiver configuration. Because multiple “files” can be configured, this functionality provides greater flexibility in that it allows you to configure different schemas to go to different receivers.
> configure
> bulkstats mode
> file <number>
> receiver <ip_address> { primary | secondary } [ mechanism { { { ftp | sftp } login <user_name> [ encrypted ] password <pwd> } | tftp } } ] }
> receiver mode { redundant | secondary-on-failure }
> remotefile format <naming_convention> [ both-receivers | primary-receiver | secondary-receiver ]
> header format <header_format>
> footer format <footer_format>
> exit
> <name> schema format <format_string>
> sample-interval <time_interval>
> transfer-interval <xmit_time_interval>
> limit <mem_limit>
> exit
> bulkstats collection
> end
> Configuring Bulk Statistic Schemas
> In each configuration example described in Configuring Standard Settings and Configuring Optional Settings, the following is the primary command used to configure the type of schema and the statistics collected:
> name schema format format_string
> Refer to the Bulk Statistics Configuration Mode Commands chapter and the Bulk Statistics File Configuration Mode Commands chapter in the Command Line Interface Reference for more information regarding supported schemas, available statistics, and proper command syntax.
> Verifying Your Configuration
> After configuring support for bulk statistics on the system, you can check your settings prior to saving them.
> Follow the instructions in this section to verify your bulk statistic settings. These instructions assume that you are at the root prompt for the Exec mode.
> Check your collection server communication and schema settings by entering the following command:
> show bulkstats schema
> The following is an example command output:
> Bulk Statistics Server Configuration:
> Server State: Enabled
> File Limit: 1000 KB
> Sample Interval: 1 minutes (0D 0H 1M)
> Transfer Interval: 5 minutes (0D 0H 5M)
> Collection Mode: Cumulative
> Receiver Mode: Secondary-on-failure
> Remote File Format: /users/ems/server/data/chicago/bulkstat%date%%time%.txt
> File Header: "CHI_test %time%"
> File Footer: ""
> Local File Storage: None
> Bulk Statistics Server Statistics:
> Records awaiting transmission: 114
> Bytes awaiting transmission: 8092
> Total records collected: 59926
> Total bytes collected: 4190178
> Total records transmitted: 59812
> Total bytes transmitted: 4188512
> Total records discarded: 0
> Total bytes discarded: 0
> Last collection time required: 2 second(s)
> Last transfer time required: 0 second(s)
> Last successful transfer: Wednesday December 7 12:14:30 EDT 2011
> Last successful tx recs: 190
> Last successful tx bytes: 13507
> Last attempted transfer: Wednesday December 7 12:14:30 EDT 2011
> Bulkstats Receivers:
> Primary: 192.168.0.100 using FTP with username administrator
> Type Name Format
> --------- --------- -----------------------------
> port portstats %bcast_inpackets% - %bcast_outpackets%
> Saving Your Configuration
> Save the configuration as described in the Verifying and Saving Your Configuration chapter.
> Viewing Collected Bulk Statistics Data
> The system provides a mechanism for viewing data that has been collected but has not been transferred. This data is referred to as “pending data”.
> View pending bulk statistics data per schema by entering the following:
> show bulkstats data
> The above command also shows the statistics of remote files, if configured in the Configuring Optional Settings subsection of the Configuring Communication With the Collection Server section in this chapter.
> The following is a sample output:
> Bulk Statistics Server Statistics:
> Records awaiting transmission: 1800
> Bytes awaiting transmission: 163687
> Total records collected: 1800
> Total bytes collected: 163687
> Total records transmitted: 0
> Total bytes transmitted: 0
> Total records discarded: 0
> Total bytes discarded: 0
> Last collection time required: 2 second(s)
> Last transfer time required: 0 second(s)
> No successful data transfers
> Last attempted transfer: Monday February 14 15:12:30 EST 2011
> File 1
> Remote File Format: /users/server/data/bulkstat%date%%time%.txt
> File Header: "Format 4.5.3.0"
> File Footer: ""
> Bulkstats Receivers:
> Primary: 192.168.1.200 using FTP with username root
> File Statistics:
> Records awaiting transmission: 1800
> Bytes awaiting transmission: 163687
> Total records collected: 1800
> Total bytes collected: 163687
> Total records transmitted: 0
> Total bytes transmitted: 0
> Total records discarded: 0
> Total bytes discarded: 0
> Last transfer time required: 0 second(s)
> No successful data transfers
> Last attempted transfer: Monday February 14 15:12:30 EST 2011
> File 2 not configured
> File 3 not configured
> File 4 not configured
> Manually Gathering and Transferring Bulk Statistics
> There may be times where it is necessary to gather and transfer bulk statistics outside of the configured intervals. The system provides commands that allow you to manually initiate the gathering and transferring of bulk statistics.
> These commands are issued from the Exec mode.
> To manually initiate the gathering of bulk statistics outside of the configured sampling interval, enter the following command:
> bulkstats force gather
> To manually initiate the transferring of bulk statistics prior to reaching the of the maximum configured storage limit, enter the following command:
> bulkstats force transfer
> Clearing Bulk Statistics Counters and Information
> It may be necessary to periodically clear counters pertaining to bulk statistics in order to gather new information or to remove bulk statistics information that has already been collected. The following command can be used to perform either of these functions:
> clear bulkstats { counters | data }

> Keyword/Variable | Description
> counters | Clears the counters maintained by the system “bulkstats” facility.
> data | Clears any accumulated data that has not been transferred. This includes any "completed" files that haven't been successfully transferred.

> ‌
> Bulk Statistics Event Log Messages
> The stat logging facility captures several events that can be useful for diagnosing errors that could occur with either the creation or writing of a bulk statistic data set to a particular location.
> The following table displays information pertaining to these events.
> Logging Events Pertaining to Bulk Statistics

> Event | Event ID | Severity | Additional Information
> Local File Open Error | 31002 | Warning | "Unable to open local file filename for storing bulkstats data"
> Receiver Open Error | 31018 | Warning | "Unable to open url filename for storing bulkstats data"
> Receiver Write Error | 31019 | Warning | "Unable to write to url filename while storing bulkstats data"
> Receiver Close Error | 31020 | Warning | "Unable to close url filename while storing bulkstats data"

> ‌

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883