> Credit Control Service Configuration Mode Commands
> The Credit Control Service Configuration Mode is used to create and manage Credit Control Service.
> diameter dictionary
> This command configures the Diameter dictionary to be used for this Credit Control Service instance.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> diameter dictionary { custom1 | standard }
> default diameter dictionary
> default
> Configures the default setting.
> dictionary { custom1 | standard }
> Specifies the Diameter dictionary to be used.
> custom1: Specifies the custom dictionary custom1.
> standard: Specifies the standard dictionary.
> Usage
> Use this command to configure the Diameter dictionary to be used for this Credit Control Service instance.
> Example
> The following command configures the standard Diameter dictionary:
> diameter dictionary standard
> diameter endpoint
> This command configures the Diameter Credit Control Interface Endpoint.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> diameter endpoint endpoint_name
> { default | no } diameter endpoint
> default
> Configures the default setting.
> no
> Removes the previous Diameter endpoint configuration.
> endpoint_name
> Specifies the Diameter endpoint name as an alpha and/or numeric string of 1 through 63 characters.
> Usage
> Use this command to configure the Diameter Credit Control Interface Endpoint.
> Example
> The following command configures the Diameter Credit Control Interface Endpoint named test135:
> diameter endpoint test135
> end
> Exits the current configuration mode and returns to the Exec mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> end
> Usage
> Use this command to return to the Exec mode.
> exit
> Exits the current mode and returns to the parent configuration mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> exit
> Usage
> Use this command to return to the parent configuration mode.
> failure-handling
> This command configures the Diameter failure handling behavior.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> failure-handling { initial-request | terminate-request | update-request } { diameter-result-code result_code [ to result_code ] | peer-unavailable | request-timeout } action { continue | retry-and-continue | retry-and-terminate | terminate }
> { default | no } failure-handling { initial-request | terminate-request | update-request } { diameter-result-code result_code [ to result_code ] | peer-unavailable | request-timeout }
> default
> Configures the default setting.
> no
> Removes the previous failure handling configuration.
> initial-request | terminate-request | update-request
> initial-request: Specifies failure handling for Initial Request.
> terminate-request: Specifies failure handling for Terminate Request.
> update-request: Specifies failure handling for Update Request.
> diameter-result-code | peer-unavailable | request-timeout
> diameter-result-code result_code [ to result_code ]: Specifies Diameter result code(s) for failure handling.
> result_code must be an integer from 3000 through 9999.
> to result_code: Specifies the range of Diameter result codes.
> peer-unavailable: Specifies failure handling for peer being unavailable.
> request-timeout: Specifies failure handling for request timeouts.
> action { continue | retry-and-continue | retry-and-terminate | terminate }
> Specifies the failure handling action.
> continue: Continue the session without credit control.
> retry-and-continue: Retry and, even if credit control is not available, continue.
> retry-and-terminate: Retry and then terminate.
> terminate: Terminate the session.
> Usage
> Use this command to configure the Diameter failure handling behavior.
> Example
> The following command configures initial request failure handling behavior for Diameter result codes 3001 to 4001 with terminate action:
> failure-handling initial-request diameter-result-code 3001 to 4001 action terminate
> request timeout
> This command configures the timeout period for Diameter requests.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> request timeout timeout
> { default | no } request timeout
> default
> Configures the default setting.
> no
> Removes the previous request timeout configuration.
> timeout
> Specifies the timeout period in seconds. The value must be an integer from 1 through 300.
> Usage
> Use this command to configure the Diameter request timeout value, after which the request is deemed to have failed. This timeout is an overall timeout, and encompasses all retries with the server(s).
> Example
> The following command configures the timeout period to 150 seconds:
> request timeout 150

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883