> MUR Application MIB
> The following figure illustrates the hierarchical structure of the management information base (MIB) for the MUR application.
> MIB Textual Conventions
> Object
> starMURThreshConfigured
> Object ID
> enterprises.8164.1.103.1.1
> Description
> This object indicates configured value of a thresholded parameter.
> Syntax
> StarMURFloatValue
> Access
> read-only
> Object
> starMURThreshMeasured
> Object ID
> enterprises.8164.1.103.1.2
> Description
> This object indicates measured value of a thresholded parameter.
> Syntax
> StarMURFloatValue
> Access
> read-only
> Object
> starMURDiskPath
> Object ID
> enterprises.8164.1.103.1.3
> Description
> Disk path to be monitored.
> Syntax
> DisplayString (SIZE (1..255))
> Access
> accessible-for-notify
> Object
> starMURAppIdentifier
> Object ID
> enterprises.8164.1.103.1.4
> Description
> Identifier of the MUR application to be monitored.
> Syntax
> INTEGER
> schedulingserver(1), postgresserver(2), apacheserver(3)
> Access
> accessible-for-notify
> Object
> starMURDataIdentifier
> Object ID
> enterprises.8164.1.103.1.5
> Description
> Identifier of the MUR data to be monitored.
> Syntax
> INTEGER { edr(1), cfedr(2), bulkstats(3), httpedr(4)}
> Access
> accessible-for-notify
> Object
> starMURTaskIdentifier
> Object ID
> enterprises.8164.1.103.1.6
> Description
> Name of the task to be monitored.
> Syntax
> INTEGER
> edrnormalization(1), httpedrnormalization(2), cfedrnormalization(3), portaggregation(4), protocolsummary(5), subscriberaggregationminutely(6), subscriberaggregationhourly7), flowcount(8) httphostaggregationminutely(9) httphostaggregationhourly(10) httpcontentsummary(11)
> Access
> accessible-for-notify
> Object
> starMURGatewayIdentifier
> Object ID
> enterprises.8164.1.103.1.7
> Description
> Identifier of the MUR Gateway to be monitored.
> Syntax
> Integer32
> Access
> accessible-for-notify
> Object
> starMURThreshComaparator
> Object ID
> enterprises.8164.1.103.1.8
> Description
> Used as comparator for threshold.
> Syntax
> INTEGER { greaterthanequal(1), lesserthanequal(2) }
> Access
> accessible-for-notify
> Object
> starMURThreshConfiguredString
> Object ID
> enterprises.8164.1.103.1.10
> Description
> This object indicates configured value of a thresholded parameter in string format.
> Syntax
> DisplayString (SIZE (1..32))
> Access
> accessible-for-notify
> Object
> starMURThreshMeasuredString
> Object ID
> enterprises.8164.1.103.1.11
> Description
> This object indicates measured value of a thresholded parameter in string format.
> Syntax
> DisplayString (SIZE (1..32))
> Access
> accessible-for-notify
> Object
> starMURKPITable
> Object ID
> enterprises.8164.1.103.1.1
> Description
> A table containing information of KPI alarms.
> Syntax
> SEQUENCE OF StarMURKPIEntry
> Access
> not-accessible
> Object
> starMURKPIEntry
> Object ID
> enterprises.8164.1.103.1.1.1
> Description
> Information about a particular KPI.
> Syntax
> StarMURKPIEntry
> Access
> not-accessible
> Object
> starMURGatewayName
> Object ID
> enterprises.8164.1.103.1.1.1.1
> Description
> The object indicates the name of the Chassis.
> Syntax
> DisplayString (SIZE (1..255))
> Access
> accessible-for-notify
> Object
> starMURKPIName
> Object ID
> enterprises.8164.1.103.1.1.1.2
> Description
> KPI to be monitored.
> Syntax
> DisplayString (SIZE (1..255))
> Access
> accessible-for-notify
> Object
> starMUREntityName
> Object ID
> enterprises.8164.1.103.1.1.1.3
> Description
> The object instance of the schema, i.e. CARD-0 , CARD-1.
> Syntax
> DisplayString (SIZE (1..64))
> Access
> accessible-for-notify
> Object
> starMURCPUBusy
> Object ID
> enterprises.8164.1.103.2.1
> Description
> MUR application is experiencing high CPU usage. The usage has exceeded an operator-configure value.
> Probable Cause: The amount of information being sent to the MUR application is approaching the MUR application's capacity the MUR application has other tasks running on it which are taking CPU time; a problem with the MUR application is causing the CPU to be abnormally busy.
> Condition Clear Alarm: This condition is cleared by a starMURCPUNormal notification.
> Objects
> starMURThreshConfigured
> starMURThreshMeasured
> Object
> starMURCPUNormal
> Object ID
> enterprises.8164.1.103.2.2
> Description
> MUR application's CPU usage has returned to a normal range.
> Objects
> starMURThreshConfigured
> starMURThreshMeasured
> Object
> starMURDiskSpaceLow
> Object ID
> enterprises.8164.1.103.2.3
> Description
> MUR application is experiencing low available disk space. The available disk space has gone below an operator-configure value.
> Probable Cause: The amount of information being sent to the MUR application is approaching the MUR application's capacity; the MUR application has other information consuming disk space; a problem with the MUR application is causing less disk space to be available then normal.
> Condition Clear Alarm: This condition is cleared by a starMURDiskSpaceNormal notification.
> Objects
> starMURThreshConfigured
> starMURThreshMeasured
> starMURDiskPath
> Object
> starMURDiskSpaceNormal
> Object ID
> enterprises.8164.1.103.2.4
> Description
> MUR application's available disk space has returned to a normal range.
> Objects
> starMURThreshConfigured
> starMURThreshMeasured
> starMURDiskPath
> Object
> starMURMemLow
> Object ID
> enterprises.8164.1.103.2.5
> Description
> MUR application is experiencing a low memory condition. The available amount of memory has gone below an operator-configure value.
> Probable Cause: The MUR application has other tasks consuming memory space; a problem with the MUR application is causing less memory space to be available then normal.
> Condition Clear Alarm: This condition is cleared by a starstarMURMEMNormal notification.
> Object
> starMURMemNormal
> Object ID
> enterprises.8164.1.103.2.6
> Description
> MUR application's available memory space has returned to a normal range.
> Objects
> starMURThreshConfigured
> starMURThreshMeasured
> Object
> starMURAppStart
> Object ID
> enterprises.8164.1.103.2.7
> Description
> One of the processes in MUR application has been started.
> Objects
> starMURAppIdentifier
> Object
> starMURAppStop
> Object ID
> enterprises.8164.1.103.2.8
> Description
> One of the processes in MUR application has been stopped.
> Objects
> starMURAppIdentifier
> Object
> starMURThreshComaparator
> Object
> starMURUnProcessedFiles
> Object ID
> enterprises.8164.1.103.2.9
> Description
> MUR application reports that there are too many unprocessed data files. Number of unprocessed data files are greater than an operator-configured value.
> Probable Cause: No action has been taken long for the data files received by MUR application.
> Condition Clear Alarm: This condition is cleared by a starMURUnProcessedFilesNormal notification.
> Object
> starMURUnProcessedFilesNormal
> Object ID
> enterprises.8164.1.103.2.10
> Description
> MUR application reports that number of unprocessed data files are less than an operator-configured value.
> Objects
> starMURThreshConfigured
> starMURThreshMeasured
> starMURDataIdentifier
> starMURGatewayIdentifier
> Object
> starMURErroneousFiles
> Object ID
> enterprises.8164.1.103.2.11
> Description
> MUR application reports that there are too many errorneous data files. Number of errorneous data files are greater than an operator-configured value.
> Probable Cause: Corrupted files.
> Objects
> starMURThreshConfigured
> starMURThreshMeasured
> starMURDataIdentifier
> starMURGatewayIdentifier
> Object
> starMURErrorneousRecords
> Object ID
> enterprises.8164.1.103.2.12
> Description
> MUR application reports that there are too many errorneous records. Number of errorneous records are greater than an operator-configured value.
> Probable Cause: Corrupted records or mismatch of records.
> Objects
> starMURThreshConfigured
> starMURThreshMeasured
> starMURDataIdentifier
> starMURGatewayIdentifier
> Object
> starMURRecordProcessingTaskLag
> Object ID
> enterprises.8164.1.103.2.13
> Description
> MUR application reports that one of the data processing task stakes more than stipulated time for processing.
> Probable Cause: The amount of information being sent to the MUR application is approaching the MUR application's capacity; the MUR application has other tasks running on it which are taking CPU time; a problem with the MUR application
> Condition Clear Alarm: This condition is cleared by a starMURRecordProcessingTaskLagNormal notification.
> Objects
> starMURThreshConfigured
> starMURThreshMeasured
> starMURTaskIdentifier
> Object
> starMURRecordProcessingTaskLagNormal
> Object ID
> enterprises.8164.1.103.2.14
> Description
> MUR application's reports that processing time of one of the data processing tasks has returned to a normal range.
> Objects
> starMURThreshConfigured
> starMURThreshMeasured
> starMURTaskIdentifier
> Object
> starMURKPIThreshCritical
> Object ID
> enterprises.8164.1.103.2.15
> Description
> PI threshold Critical alarm indicates for which gateway, KPI and entity the alarm is generated and also its configured and measured threshold value.
> Objects
> starMURKPIName
> starMURThreshComaparator
> starMURThreshConfiguredString
> starMURThreshMeasuredString
> starMURGatewayName
> starMUREntityName
> Object
> starMURKPIThreshCriticalClear
> Object ID
> enterprises.8164.1.103.2.16
> Description
> KPI threshold Critical Clear alarm indicates for which gateway, KPI and entity the alarm is generated and also its configured and measured threshold value.
> Objects
> starMURKPIName
> starMURThreshComaparator
> starMURThreshConfiguredString
> starMURThreshMeasuredString
> starMURGatewayName
> starMUREntityName
> Object
> starMURKPIThreshMajor
> Object ID
> enterprises.8164.1.103.2.17
> Description
> KPI threshold Major alarm indicates for which gateway,KPI and entity the alarm is generated and also its configured and measured threshold value.
> Objects
> starMURKPIName
> starMURThreshComaparator
> starMURThreshConfiguredString
> starMURThreshMeasuredString
> starMURGatewayName
> starMUREntityName
> Object
> starMURKPIThreshMajorClear
> Object ID
> enterprises.8164.1.103.2.18
> Description
> KPI threshold Major clear alarm indicates for which gateway, KPI and entity the alarm is generated and also its configured and measured threshold value
> Objects
> starMURKPIName
> starMURThreshComaparator
> starMURThreshConfiguredString
> starMURThreshMeasuredString
> starMURGatewayName
> starMUREntityName
> Object
> starMURKPIThreshMinor
> Object ID
> enterprises.8164.1.103.2.19
> Description
> KPI threshold minor alarm indicates for which gateway, KPI and entity the alarm is generated and also its configured and measured threshold value.
> Objects
> starMURKPIName
> starMURThreshComaparator
> starMURThreshConfiguredString
> starMURThreshMeasuredString
> starMURGatewayName
> starMUREntityName
> Object
> starMURKPIThreshMinorClear
> Object ID
> enterprises.8164.1.103.2.20
> Description
> KPI threshold minor clear alarm indicates for which gateway, KPI and entity the alarm is generated and also its configured and measured threshold value.
> Objects
> starMURKPIName
> starMURThreshComaparator
> starMURThreshConfiguredString
> starMURThreshMeasuredString
> starMURGatewayName
> starMUREntityName
> Object
> starMURKPIThreshWarning
> Object ID
> enterprises.8164.1.103.2.21
> Description
> KPI threshold warning alarm indicates for which gateway, KPI and entity the alarm is generated and also its configured and measured threshold value.
> Objects
> starMURKPIName
> starMURThreshComaparator
> starMURThreshConfiguredString
> starMURThreshMeasuredString
> starMURGatewayName
> starMUREntityName
> Object
> starMURKPIThreshWarningClear
> Object ID
> enterprises.8164.1.103.2.22
> Description
> KPI threshold warning clear alarm indicates for which gateway ,KPI and entity the alarm is generated and also its configured and measured threshold value.
> Objects
> starMURKPIName
> starMURThreshComaparator
> starMURThreshConfiguredString
> starMURThreshMeasuredString
> starMURGatewayName
> starMUREntityName
> starMURMIBConformances(3)
> Object
> starMURMIBCompliance
> Object ID
> enterprises.8164.1.103.3.1
> Description
> The compliance statements for entities which implement the STARENT MUR MIB.
> Object
> starMURNotifMgmtGroup
> Object ID
> enterprises.8164.1.103.3.1.1
> Description
> A collection of objects related with notification management on MUR.
> Objects
> starMURThreshConfigured
> starMURThreshMeasured
> starMURDiskPath
> starMURAppIdentifier
> starMURDataIdentifier
> starMURTaskIdentifier
> starMURGatewayIdentifier
> starMURGatewayName
> starMUREntityName
> starMURKPIName
> starMURThreshComaparator
> starMURThreshConfiguredString
> starMURThreshMeasuredString
> Object
> starMURNotifGroup
> Object ID
> enterprises.8164.1.103.3.1.2
> Description
> A collection of notifications.
> Objects
> starMURCPUBusy
> starMURCPUNormal
> starMURDiskSpaceLow
> starMURDiskSpaceNormal
> starMURMemLow
> starMURMemNormal
> starMURAppStart
> starMURAppStop
> starMURUnProcessedFiles
> starMURUnProcessedFilesNormal
> starMURErroneousFiles
> starMURErrorneousRecords
> starMURRecordProcessingTaskLag
> starMURRecordProcessingTaskLagNormal
> starMURKPIThreshCritical
> starMURKPIThreshCriticalClear
> starMURKPIThreshMajor
> starMURKPIThreshMajorClear
> starMURKPIThreshMinor
> starMURKPIThreshMinorClear
> starMURKPIThreshWarning
> starMURKPIThreshWarningClear

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883