> MSEG Global Configuration Mode Commands
> The MSEG Global Configuration Mode is used to configure global Mobile Service Edge Gateway (MSEG) parameters.
> Important: This configuration mode is not supported in this release. For more information please contact your Cisco account representative.
> apn-profile
> This command allows you to create/configure/delete MSEG APN profiles.
> Important: This command is not supported in this release. For more information please contact your Cisco account representative.
> Product
> MSEG
> Privilege
> Security Administrator, Administrator
> Syntax
> apn-profile mseg_apn_profile_name [ -noconfirm ]
> no apn-profile mseg_apn_profile_name
> no
> Deletes the specified MSEG APN profile.
> mseg_apn_profile_name
> Specifies the APN profile to add/configure/delete.
> mseg_apn_profile_name must be the name of an MSEG APN profile, and must be an alphanumeric string of 1 through 63 characters.
> If the named APN profile does not exist, it is created, and the CLI mode changes to the MSEG APN Profile Configuration Mode wherein the APN profile can be configured.
> If the named APN profile already exists, the CLI mode changes to the MSEG APN Profile Configuration mode for that APN profile.
> -noconfirm
> Executes the command without prompting for confirmation.
> Usage
> Use this command to create/configure/delete MSEG APN profiles.
> Entering this command results in the following prompt:
> [context_name]hostname(config-mseg-apn-profile)#
> MSEG APN Profile configuration commands are described in the MSEG APN Profile Configuration Mode Commands chapter.
> Example
> The following command creates an APN profile named test, and changes to the MSEG APN Profile Configuration Mode:
> apn-profile test
> associated-services-profile
> This command allows you to create/configure/delete MSEG associated-services profiles.
> Important: This command is not supported in this release. For more information please contact your Cisco account representative.
> Product
> MSEG
> Privilege
> Security Administrator, Administrator
> Syntax
> associated-services-profile mseg_as_profile_name [ -noconfirm ]
> no associated-services-profile mseg_as_profile_name
> no
> Deletes the specified MSEG associated-services profile.
> mseg_as_profile_name
> Specifies the MSEG associated services profile to add/configure/delete.
> mseg_as_profile_name must be the name of an MSEG associated-services profile, and must be an alphanumeric string of 1 through 63 characters.
> If the named associated-services profile does not exist, it is created, and the CLI mode changes to the MSEG Associated Services Profile Configuration Mode wherein the profile can be configured.
> If the named associated-services profile already exists, the CLI mode changes to the MSEG Associated Services Profile Configuration Mode for that profile.
> -noconfirm
> Executes the command without prompting for confirmation.
> Usage
> Use this command to create/configure/delete MSEG associated-services profiles.
> Entering this command results in the following prompt:
> [context_name]hostname(config-mseg-as-profile)#
> MSEG associated-services profile configuration commands are described in the MSEG Associated Services Profile Configuration Mode Commands chapter. This mode contains configurations for all the associated services such as NAT, accounting context, destination context, and so on, from other parts of the system, that are to be applied to an offloaded session once it is set up.
> Example
> The following command creates an associated-services profile named test, and changes to the MSEG Associated Services Profile Configuration Mode:
> associated-services-profile test
> end
> Exits the current configuration mode and returns to the Exec mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> end
> Usage
> Use this command to return to the Exec mode.
> exit
> Exits the current mode and returns to the parent configuration mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> exit
> Usage
> Use this command to return to the parent configuration mode.
> imei-profile
> This command allows you to create/configure/delete MSEG IMEI profiles.
> Important: This command is not supported in this release. For more information please contact your Cisco account representative.
> Product
> MSEG
> Privilege
> Security Administrator, Administrator
> Syntax
> imei-profile mseg_imei_profile_name [ -noconfirm ]
> no imei-profile mseg_imei_profile_name
> no
> Deletes the specified MSEG IMEI profile.
> mseg_imei_profile_name
> Specifies the MSEG IMEI profile to add/configure/delete.
> mseg_imei_profile_name must be the name of an MSEG IMEI profile, and must be an alphanumeric string of 1 through 63 characters.
> If the named IMEI profile does not exist, it is created, and the CLI mode changes to the MSEG IMEI Profile Configuration Mode wherein the IMEI profile can be configured.
> If the named IMEI profile already exists, the CLI mode changes to the MSEG IMEI Profile Configuration Mode for that IMEI profile.
> -noconfirm
> Executes the command without prompting for confirmation.
> Usage
> Use this command to create/configure/delete MSEG IMEI profiles.
> Entering this command results in the following prompt:
> [context_name]hostname(config-mseg-imei-profile)#
> MSEG IMEI Profile configuration commands are described in the MSEG IMEI Profile Configuration Mode Commands chapter.
> Example
> The following command creates an IMEI profile named test, and changes to the MSEG IMEI Profile Configuration Mode:
> imei-profile test
> imsi-profile
> This command allows you to create/configure/delete MSEG IMSI profiles.
> Important: This command is not supported in this release. For more information please contact your Cisco account representative.
> Product
> MSEG
> Privilege
> Security Administrator, Administrator
> Syntax
> imsi-profile mseg_imsi_profile_name [ -noconfirm ]
> no imsi-profile mseg_imsi_profile_name
> no
> Deletes the specified MSEG IMSI profile.
> mseg_imsi_profile_name
> Specifies the MSEG IMSI profile to add/configure/delete.
> mseg_imsi_profile_name must be the name of an MSEG IMSI profile, and must be an alphanumeric string of 1 through 63 characters.
> If the named IMSI profile does not exist, it is created, and the CLI mode changes to the MSEG IMSI Profile Configuration Mode wherein the IMSI profile can be configured.
> If the named IMSI profile already exists, the CLI mode changes to the MSEG IMSI Profile Configuration Mode for that IMSI profile.
> -noconfirm
> Executes the command without prompting for confirmation.
> Usage
> Use this command to create/configure/delete MSEG IMSI profiles.
> Entering this command results in the following prompt:
> [context_name]hostname(config-mseg-imsi-profile)#
> MSEG IMSI Profile configuration commands are described in the MSEG IMSI Profile Configuration Mode Commands chapter.
> Example
> The following command creates an IMSI profile named test, and changes to the MSEG IMSI Profile Configuration Mode:
> imsi-profile test
> mseg-criteria
> This command allows you to create/configure/delete MSEG criteria.
> Important: This command is not supported in this release. For more information please contact your Cisco account representative.
> Product
> MSEG
> Privilege
> Security Administrator, Administrator
> Syntax
> mseg-criteria mseg_criteria_name [ -noconfirm ]
> no mseg-criteria mseg_criteria_name
> no
> Deletes the specified MSEG criteria.
> mseg_criteria_name
> Specifies the MSEG criteria to add/configure/delete.
> mseg_criteria_name must be the name of the MSEG criteria, and must be an alphanumeric string of 1 through 63 characters.
> If the named MSEG criteria does not exist, it is created, and the CLI mode changes to the MSEG Criteria Configuration Mode wherein the MSEG criteria set can be configured.
> If the named MSEG criteria already exists, the CLI mode changes to the MSEG Criteria Configuration Mode for that MSEG criteria.
> -noconfirm
> Executes the command without prompting for confirmation.
> Usage
> Use this command to create/configure/delete an MSEG criteria — a set of filters that are applied by an MSEG service. There can be multiple MSEG criteria configured though only one can be associated with an MSEG service at any given time.
> Entering this command results in the following prompt:
> [context_name]hostname(config-mseg-criteria)#
> MSEG criteria configuration commands are described in the MSEG Criteria Configuration Mode Commands chapter.
> Example
> The following command creates an MSEG criteria named test, and changes to the MSEG Criteria Configuration Mode:
> mseg-criteria test
> mseg-ruleset
> This command allows you to create/configure/delete MSEG rules.
> Important: This command is not supported in this release. For more information please contact your Cisco account representative.
> Product
> MSEG
> Privilege
> Security Administrator, Administrator
> Syntax
> mseg-ruleset mseg_ruleset_name [ -noconfirm ]
> no mseg-ruleset mseg_ruleset_name
> no
> Deletes the specified MSEG ruleset.
> mseg_ruleset_name
> Specifies the MSEG ruleset to add/configure/delete.
> mseg_ruleset_name must be the name of an MSEG ruleset, and must be an alphanumeric string of 1 through 63 characters.
> If the named MSEG ruleset does not exist, it is created, and the CLI mode changes to the MSEG Ruleset Configuration Mode wherein the MSEG ruleset can be configured.
> If the named MSEG ruleset already exists, the CLI mode changes to the MSEG Ruleset Configuration Mode for that MSEG ruleset.
> -noconfirm
> Executes the command without prompting for confirmation.
> Usage
> Use this command to create/configure/delete MSEG rulesets — filter combinations to be applied while evaluating whether a session should be offloaded or not.
> Entering this command results in the following prompt:
> [context_name]hostname(config-mseg-ruleset)#
> MSEG ruleset configuration commands are described in the MSEG Ruleset Configuration Mode Commands chapter.
> Example
> The following command creates an MSEG ruleset named test, and changes to the MSEG Ruleset Configuration Mode:
> mseg-ruleset test
> peer-mseg-profile
> This command allows you to create/configure/delete MSEG peer profiles.
> Important: This command is not supported in this release. For more information please contact your Cisco account representative.
> Product
> MSEG
> Privilege
> Security Administrator, Administrator
> Syntax
> peer-mseg-profile mseg_peer_profile_name [ -noconfirm ]
> no peer-mseg-profile mseg_peer_profile_name
> no
> Deletes the specified MSEG peer profile.
> mseg_peer_profile_name
> Specifies the MSEG peer profile to add/configure/delete.
> mseg_peer_profile_name must be the name of an MSEG peer profile, and must be an alphanumeric string of 1 through 63 characters.
> If the named MSEG peer profile does not exist, it is created, and the CLI mode changes to the MSEG Peer Profile Configuration Mode wherein the MSEG peer profile can be configured.
> If the named MSEG peer profile already exists, the CLI mode changes to the MSEG Peer Profile Configuration Mode for that peer profile.
> -noconfirm
> Specifies that the command must execute without prompting for confirmation.
> Usage
> Use this command to create/configure/delete MSEG peer profiles. Configuration of all non-local MSEG instances in the network. Multiple MSEG peer profiles can be configured.
> Entering this command results in the following prompt:
> [context_name]hostname(config-mseg-profile)#
> MSEG peer profile configuration commands are described in the MSEG Peer Profile Configuration Mode Commands chapter.
> Example
> The following command creates a peer profile named test, and changes to the MSEG Peer Profile Configuration Mode:
> peer-mseg-profile test
> rnc-profile
> This command allows you to create/configure/delete MSEG Radio Network Controller (RNC) profiles.
> Important: This command is not supported in this release. For more information please contact your Cisco account representative.
> Product
> MSEG
> Privilege
> Security Administrator, Administrator
> Syntax
> rnc-profile mseg_rnc_profile_name [ -noconfirm ]
> no rnc-profile mseg_rnc_profile_name
> no
> Deletes the specified MSEG RNC profile.
> mseg_rnc_profile_name
> Specifies the MSEG RNC profile to add/configure/delete.
> mseg_rnc_profile_name must be the name of an MSEG RNC profile, and must be an alphanumeric string of 1 through 63 characters.
> If the named RNC profile does not exist, it is created, and the CLI mode changes to the MSEG RNC Profile Configuration Mode wherein the RNC profile can be configured.
> If the named RNC profile already exists, the CLI mode changes to the MSEG RNC Profile Configuration Mode for that RNC profile.
> -noconfirm
> Executes the command without prompting for confirmation.
> Usage
> Use this command to create/configure/delete MSEG RNC profiles. Multiple RNC profiles can be configured.
> Entering this command results in the following prompt:
> [context_name]hostname(config-mseg-rnc-profile)#
> MSEG RNC Profile configuration commands are described in the MSEG RNC Profile Configuration Mode Commands chapter.
> Example
> The following command creates an RNC profile named test, and changes to the MSEG RNC Profile Configuration Mode:
> rnc-profile test

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883