# Monitoring the Service

This chapter provides information for monitoring service status and performance using the show commands found in the Command Line Interface (CLI). These command have many related keywords that allow them to provide useful information on all aspects of the system ranging from current software configuration through call activity and status.

The selection of keywords described in this chapter is intended to provided the most useful and in-depth information for monitoring the system. For additional information on these and other show command keywords, refer to the CDMA Command Line Interface Reference.

In addition to the CLI, the system supports the sending of Simple Network Management Protocol (SNMP) traps that indicate status and alarm conditions. Refer to the SNMP MIB Reference Guide for a detailed listing of these traps.

Monitoring System Status and Performance

This section contains commands used to monitor the status of tasks, managers, applications and other software components in the system. Output descriptions for most of the commands are located in the Statistics and Counters Reference.
Table 1. System Status and Performance Monitoring Commands

To do this: | Enter this command:
--- | ---
View Congestion-Control Statistics | .
View Congestion-Control Statistics | show congestion-control statistics { a11mgr | gtpcmgr | hamgr | l2tpmgr }
View Subscriber Information | .
View session resource status | show resources session
Display Subscriber Configuration Information | .
View locally configured subscriber profile settings (must be in context where subscriber resides) | show subscribers configuration username subscriber_name
View remotely configured subscriber profile settings | show subscribers aaa-configuration username subscriber_name
View Subscribers Currently Accessing the System | .
View a listing of subscribers currently accessing the system | show subscribers all
Display PCF-Summary Session Counters | .
View PCF-summary session counters | show session counters pcf-summary
Display Session State Statistics | .
View session state statistics | show session progress
Display Session State PCF Statistics | .
View session state PCF statistics | show session progress pcf all
Display Session Subsystem and Task Statistics IMPORTANT: Refer to the System Software Task and Subsystem Descriptions appendix in the System Administration Guide for additional information on the Session subsystem and its various manager tasks. | .
View A11 Manager statistics | show session subsystem facility a11mgr all
View AAA Manager statistics | show session subsystem facility aaamgr all
View FA Manager statistics | show session subsystem facility famgr all
View L2TP demux manager statistics | show session subsystem facility l2tpdemux all
View L2TP Manager statistics | show session subsystem facility l2tpmgr all
View Session Manager statistics | show session subsystem facility sessmgr all
View Session Recovery Status | .
View session recovery status | show session recovery status [verbose]
Display Session Disconnect Reasons | .
View session disconnect reasons with verbose output | show session disconnect-reasons
View Point-to-Point Protocol Statistics | .
Display a Summary of PPP Counter Status | .
View cumulative subscriber session PPP counters | show ppp
Display PPP Counters for a Specific Subscriber | .
View individual subscriber session PPP counters | show ppp username subscriber_name
View individual subscriber session PPP error and data counters | show ppp counters username subscriber_name
View individual subscriber session detailed PPP counters | show ppp full username subscriber_name
Display PPP Statistics for PDSN Services | .
Views PPP statistics for a all PDSN services | show ppp statistics pdsn-service
Views PPP statistics for a specific PDSN service | show ppp statistics pdsn-service service_name
View R-P Interface Statistics | .
Display a Summary of R-P Interface Counter Status | .
View cumulative R-P interface counters for every subscriber session currently in progress | show rp
Display R-P Interface Counters for a Specific Subscriber | .
View R-P interface counters for a specific subscriber | show rp full username subscriber_name
Display R-P Interface Statistics for PDSN Services | .
View R-P interface statistics for all PDSN services | show rp statistics pdsn-service
View R-P interface statistics for a specific PDSN service | show rp statistics pdsn-service service_name
View Mobile IP Foreign Agent Statistics | .
Display Mobile IP FA Information for a Specific Subscriber | .
View Mobile IP FA counters for a specific subscriber | show mipfa full username subscriber_name
Display Mobile IP Statistics for FA Services | .
View statistics for a specific FA service | show mipfa statistics fa-service service_name
Display Mobile IP FA Counters | .
View Mobile IP FA counters for individual subscriber sessions | show mipfa counters
Display RADIUS Server States IMPORTANT: These commands can display 10 state transition histories of RADIUS accounting and authentication servers (Active/Not responding/Down States). For a complete explanation of RADIUS server states, refer to the RADIUS Server State Behavior appendix in the AAA Administration and Reference. | .
View RADIUS authentication server group server states for a specific group | show radius authentication servers radius group group_name detail
View RADIUS accounting server group server states for a specific group | show radius accounting servers radius group group_name detail
Display RADIUS Protocol Counters | .
View cumulative RADIUS protocol counters | show radius counters all
View RADIUS protocol counter summary of RADIUS authentication and accounting | show radius counters summary
View L2TP Information | .
Display L2TP Session Information | .
View cumulative statistics for all sessions processed within the current context IMPORTANT: If this command is executed from within the localout-of-band context, cumulative session information is displayed for all contexts. | show l2tp sessions
View all information pertaining to the L2TP session of a specific subscriber | show l2tp session full username subscriber_name
Display L2TP Statistics | .
View statistics for a specific LAC service IMPORTANT: If this command is executed from within the localout-of-band context, cumulative session information is displayed for all contexts. | show l2tp statistics lac-service service_name
Display L2TP Tunnel Information | .
View all tunnels currently being facilitated by LAC services within a specific context | show l2tp tunnels all
Display IPSec Security Association Statistics | .
View IPSec security association statistics for crypto maps in the current context | show crypto ipsec security-associations statistics
Display Pre-shared ISAKMP Keys | .
View pre-shared keys received from peer security gateways as part of the Diffie-Hellman exchange | show crypto isakmp keys
Display IPSec Statistics | .
View cumulative IPSec statistics for the current context | show crypto statistics

Clearing Statistics and Counters

It may be necessary to periodically clear statistics and counters in order to gather new information. The system provides the ability to clear statistics and counters based on their grouping (PPP, MIPHA, MIPFA, etc.).

Statistics and counters can be cleared using the CLI clear command. Refer to the CDMA Command Line Interface Reference for detailed information on using this command.