# P-GW Node Level Schema Statistics

The P-GW schema provides operational statistics that can be used for monitoring and troubleshooting the following products: P-GW
This schema provides the following types of statistics:

- Counter: A counter records incremental data cumulatively and rolls over when the counter limit is reached. All counter statistics are cumulative and reset only by one of the following methods: roll-over when limit is reached, after a system restart, or after a clear command is performed. The limit depends upon the data type.
- Gauge: A gauge statistic indicates a single value; a snapshot representation of a single point in time within a defined time frame. The gauge changes to a new value with each snapshot though a value may repeat from one period to the next. The limit depends upon the data type.
- Information: This type of statistic provides information, often intended to differentiate sets of statistics; for example, a VPN name or IP address. The type of information provided depends upon the data type.

The data type defines the format of the data for the value provided by the statistic. The following data types are used in statistics for this schema:

- Int32/Int64: An integer, either 32-bit or 64-bit: For statistics with the Int32 data type, the roll-over to zero limit is 4,294,967,295. For statistics with the Int64 data type, the roll-over to zero limit is 18,446,744,073,709,551,615.
- Float: A numeric value that can be represented fractionally; for example, 1.345.
- String: A series of ASCII alphanumeric characters in a single grouping, usually pre-configured.

IMPORTANT:

Unless otherwise indicated, all statistics are counters and all statistics are standards-based.

Key Variables: Every schema has some variables which are typically referred to as 'key variables'. These key variables provide index markers to identify which object the statistics apply to. For example, in the card schema, the card number (variable %card%) uniquely identifies a card. For an HA service, the keys would be "%vpnname%" plus "%servname%", as the combination uniquely identifies an HA service. So, in a given measurement interval, one row of statistics will be generated per unique key. The schema keys are identified in the Description section of the table.
Table 1. Bulk Statistic Variables in the P-GW Service Schema

Variables | Description | Data Type
--- | --- | ---
vpnname | The name of the context configured on the system that is currently facilitating the P-GW service. This is a key variable. Type: Information | String
vpnid | The identification number of the context configured on the system that is currently facilitating the P-GW service. This is an internal reference number. This is a key variable. Type: Information | Int32
servname | Displays the name of the P-GW service for which the statistics are displayed. This is a key variable. Type: Information | String
servid | The identification number of the service configured on the system that is currently facilitating the P-GW service. This is an internal reference number. This is a key variable. Type: Information | Int32
sess-cur | The total number of sessions currently established on this system. Type: Gauge | Int32
ue-active | The total number of active subscribers. Type: Gauge | Int32
sessstat-bearact-def | Session Statistics - Total default bearers active Type: Gauge | Int32
sessstat-bearact-emergency-def | Session Statistics - Total emergency default bearers active Type: Gauge | Int32
sessstat-bearact-emergency-auth-imsi-def | Session Statistics - Total emergency default bearers (Auth-IMSI) active Type: Gauge | Int32
sessstat-bearact-emergency-unauth-imsi-def | Session Statistics - Total emergency default bearers (Unauth-IMSI) active Type: Gauge | Int32
sessstat-bearact-emergency-only-imei-def | Session Statistics - Total emergency default bearers (Only IMEI) active Type: Gauge | Int32
sessstat-bearact-ded | Session Statistics - Total dedicated bearers active Type: Gauge | Int32
sessstat-bearact-ue-init-ded | Session Statistics - Total bearers active - UE-initiated Type: Gauge | Int32
sessstat-bearact-nw-init-ded | Session Statistics - Total bearers active - Network-initiated Type: Gauge | Int32
sessstat-bearact-emergency-ded | Session Statistics - Total emergency dedicated bearers active Type: Gauge | Int32
sessstat-bearact-emergency-auth-imsi-ded | Session Statistics - Total emergency dedicated bearers (Auth-IMSI) active Type: Gauge | Int32
sessstat-bearact-emergency-unauth-imsi-ded | Session Statistics - Total emergency dedicated bearers (Unauth-IMSI) active Type: Gauge | Int32
sessstat-bearact-emergency-only-imei-ded | Session Statistics - Total emergency dedicated bearers (Only IMEI) active Type: Gauge | Int32
sessstat-bearact-nw-init-ded-att | Session Statistics - Total bearers active - Network-initiated dedicated bearers Type: Gauge | Int32
sessstat-bearsetup-def | Session Statistics - Total default bearers setup Type: Counter | Int32
sessstat-bearsetup-emergency-def | Session Statistics - Total emergency default bearers setup Type: Counter | Int32
sessstat-bearsetup-emergency-auth-imsi-def | Session Statistics - Total emergency default bearers (Auth-IMSI) setup Type: Counter | Int32
sessstat-bearsetup-emergency-unauth-imsi-def | Session Statistics - Total emergency default bearers (Unauth-IMSI) setup Type: Counter | Int32
sessstat-bearsetup-emergency-only-imei-def | Session Statistics - Total emergency default bearers (Only IMEI) setup Type: Counter | Int32
sessstat-bearsetup-ded | Session Statistics - Total dedicated bearers setup Type: Counter | Int32
sessstat-bearsetup-ue-init-ded | Session Statistics - Total bearers rejected - Network-req reject - No Resource Type: Counter | Int32
sessstat-bearsetup-nw-init-ded | Session Statistics - Total bearers setup - Dedicated bearers - Network-initiated Type: Counter | Int32
sessstat-bearsetup-emergency-ded | Session Statistics - Total emergency dedicated bearers setup Type: Counter | Int32
sessstat-bearsetup-emergency-auth-imsi-ded | Session Statistics - Total emergency dedicated bearers (Auth-IMSI) setup Type: Counter | Int32
sessstat-bearsetup-emergency-unauth-imsi-ded | Session Statistics - Total emergency dedicated bearers (Unauth-IMSI) setup Type: Counter | Int32
sessstat-bearsetup-emergency-only-imei-ded | Session Statistics - Total emergency dedicated bearers (Only IMEI) setup Type: Counter | Int32
sessstat-bearrel-def | Session Statistics - Total default bearers released Type: Counter | Int32
sessstat-bearrel-ded | Session Statistics - Total dedicated bearers released Type: Counter | Int32
sessstat-bearrel-nwdefadmin | Session Statistics - Total bearers released - Network Default Admin disconnect Type: Counter | Int32
sessstat-bearrel-nwdefgtp | Session Statistics - Total bearers released - Network Default GTP-U error ind Type: Counter | Int32
sessstat-bearrel-nwdefsgw | Session Statistics - Total bearers released - Network Default S-GW Path failure Type: Counter | Int32
sessstat-bearrel-nwdefmme | Session Statistics - Total bearers released - Network Default MME initiated release Type: Counter | Int32
sessstat-bearrel-nwdedadmin | Session Statistics - Total bearers released - Network Dedicated Admin disconnect Type: Counter | Int32
sessstat-bearrel-nwdedgtp | Session Statistics - Total bearers released - Network Dedicated GTP-U error ind Type: Counter | Int32
sessstat-bearrel-nwdedmme | Session Statistics - Total bearers released - Network Dedicated MME initiated release Type: Counter | Int32
sessstat-bearrel-nwdeddefbear | Session Statistics - Total bearers released - Network Dedicated Default bearer release Type: Counter | Int32
sessstat-bearrel-nwdedgxdisc | Session Statistics - Total bearers released - Network Dedicated GX Disconnect Type: Counter | Int32
sessstat-bearrelfail-def | Session Statistics - Total bearers release failure - Default bearers Type: Counter | Int32
sessstat-bearrelfail-ded | Session Statistics - Total bearers release failure - Dedicated bearers Type: Counter | Int32
sessstat-bearrej-def | Session Statistics - Total bearers rejected - Default bearers Type: Counter | Int32
sessstat-bearrej-ded | Session Statistics - Total bearers rejected - Dedicated bearers Type: Counter | Int32
sessstat-bearrej-emergency-def | Session Statistics - Total bearers rejected - Emergency default bearers Type: Counter | Int32
sessstat-bearrej-emergency-ded | Session Statistics - Total bearers rejected - Emergency dedicated bearers Type: Counter | Int32
sessstat-bearrej-nores | Session Statistics - Total bearers rejected - No Resource Type: Counter | Int32
sessstat-bearrej-uereq | Session Statistics - Total bearers rejected - UE-req reject Type: Counter | Int32
sessstat-bearrej-uereq-nores | Session Statistics - Total bearers rejected - UE-req reject - No Resource Type: Counter | Int32
sessstat-bearrej-misapn | Session Statistics - Total bearers rejected - Missing or unknown APN Type: Counter | Int32
sessstat-bearrej-nwreq | Session Statistics - Total bearers rejected - Network-req reject Type: Counter | Int32
sessstat-bearrej-nwreq-nores | Session Statistics - Total bearers rejected - Network-req reject - No Resource Type: Counter | Int32
sessstat-bearrej-nwreq-nomem | Session Statistics - Total bearers rejected - Network-req reject - No memory available Type: Counter | Int32
sessstat-bearrej-nwreq-sysfail | Session Statistics - Total bearers rejected - Network-req reject - System failure Type: Counter | Int32
sessstat-bearrej-apnmode | Session Statistics - Total bearers rejected - APN selection -Mode mismatch Type: Counter | Int32
sessstat-bearrej-pdn | Session Statistics - Total bearers rejected - Pref PDN -Type not supported Type: Counter | Int32
sessstat-bearrej-apnrestr | Session Statistics - Total bearers rejected - APN restr violation Type: Counter | Int32
sessstat-bearrej-subsauth | Session Statistics - Total bearers rejected - Subs auth failed Type: Counter | Int32
sessstat-bearrej-subsaddrnotallow | Session Statistics - Total bearers rejected - Subscriber’s static address not allowed Type: Counter | Int32
sessstat-bearrej-subsaddrnotalloc | Session Statistics - Total bearers rejected - Subscriber’s static address not allocated Type: Counter | Int32
sessstat-bearrej-dynaddrnotalloc | Session Statistics - Total bearers rejected - Dynamic address not allocated Type: Counter | Int32
sessstat-bearrej-subsaddrnotpres | Session Statistics - Total bearers rejected - Subscriber’s static address not present Type: Counter | Int32
sessstat-bearmod-ueinit | Session Statistics - Total bearers modified - UE-initiated modification Type: Counter | Int32
sessstat-bearmod-nwinit | Session Statistics - Total bearers modified - Network-initiated modification Type: Counter | Int32
sessstat-bearmod-ueqos | Session Statistics - Total bearers modified - UE-initiated quality of service (QoS) modification Type: Counter | Int32
sessstat-bearmod-uetft | Session Statistics - Total bearers modified - UE-initiated TFT modification Type: Counter | Int32
sessstat-bearmod-nwqos | Session Statistics - Total bearers modified - Network-initiated QoS modification Type: Counter | Int32
sessstat-bearmod-nwtft | Session Statistics - Total bearers modified - Network-initiated TFT modification Type: Counter | Int32
sessstat-bearmodfail-ueinit | Session Statistics - Total bearers modification failure - UE-initiated modification failed Type: Counter | Int32
sessstat-bearmodfail-nwinit | Session Statistics - Total bearers modification failure - Network-initiated modification failed Type: Counter | Int32
sessstat-bearmodfail-uenores | Session Statistics - Total bearers modification failure - UE-initiated No res available Type: Counter | Int32
sessstat-bearmodfail-uesemtft | Session Statistics - Total bearers modification failure - UE-initiated Semantic error in TFT oper Type: Counter | Int32
sessstat-bearmodfail-uesyntft | Session Statistics - Total bearers modification failure - UE-initiated Syntax error in TFT oper Type: Counter | Int32
sessstat-bearmodfail-uesempkt | Session Statistics - Total bearers modification failure - UE-initiated Semantic error in packet filter Type: Counter | Int32
sessstat-bearmodfail-uesynpkt | Session Statistics - Total bearers modification failure - UE-initiated syntax error in packet filter Type: Counter | Int32
sessstat-bearmodfail-nwnores | Session Statistics - Total bearers modification failure - Network-initiated - No res available Type: Counter | Int32
sessstat-bearmodfail-nwnomem | Session Statistics - Total bearers modification failure - Network-initiated - No memory available Type: Counter | Int32
sessstat-bearmodfail-nwsysfail | Session Statistics - Total bearers modification failure - Network-initiated - System failure Type: Counter | Int32
sessstat-bearmodfail-nwsemtft | Session Statistics - Total bearers modification failure - Network-initiated Semantic error in TFT oper Type: Counter | Int32
sessstat-bearmodfail-nwsyntft | Session Statistics - Total bearers modification failure - Network-initiated syntax error in TFT oper Type: Counter | Int32
sessstat-bearmodfail-nwsempkt | Session Statistics - Total bearers modification failure - Network-initiated Semantic error in packet filter Type: Counter | Int32
sessstat-bearmodfail-nwsynpkt | Session Statistics - Total bearers modification failure - Network-initiated syntax error in packet filter Type: Counter | Int32
sessstat-bearmodfail-qos-uenores | Session Statistics - Total bearer modification failures - User equipment quality of service no response errors Type: Counter | Int32
sessstat-bearmodfail-qos-uesemtft | Session Statistics - Total bearer modification failures - User equipment quality of service TFT semantics errors Type: Counter | Int32
sessstat-bearmodfail-qos-uesyntft | Session Statistics - Total bearer modification failures - User equipment quality of service TFT syntax errors Type: Counter | Int32
sessstat-bearmodfail-qos-uesempkt | Session Statistics - Total bearer modification failures - User equipment quality of service packet semantics errors Type: Counter | Int32
sessstat-bearmodfail-qos-uesynpkt | Session Statistics - Total bearer modification failures - User equipment quality of service packet syntax errors Type: Counter | Int32
sessstat-bearmodfail-qos-nwnores | Session Statistics - Total bearer modification failures - Network-initiated quality of service no response Type: Counter | Int32
sessstat-bearmodfail-qos-nwnomem | Session Statistics - Total bearer modification failures - Network-initiated quality of service no memory Type: Counter | Int32
sessstat-bearmodfail-qos-nwsysfail | Session Statistics - Total bearer modification failures - Network-initiated quality of service system failures Type: Counter | Int32
sessstat-bearmodfail-qos-nwsemtft | Session Statistics - Total bearer modification failures - Network-initiated quality of service semantics of TFT Type: Counter | Int32
sessstat-bearmodfail-qos-nwsyntft | Session Statistics - Total modified bearer failures - Network-initiated TFT syntax Type: Counter | Int32
sessstat-bearmodfail-qos-nwsempkt | Session Statistics - Total modified bearer failures - Network quality of service semantics packets Type: Counter | Int32
sessstat-bearmodfail-qos-nwsynpkt | Session Statistics - Total modified bearer failures - Network quality of service syntax of packets Type: Counter | Int32
sessstat-beardel-ded | Session Statistics - Total deleted dedicated bearers Type: Counter | Int32
sessstat-nw-init-qos-update-att | Session Statistics - Total bearers modified - Network initiated - quality of service (QoS) modifications attempted Type: Counter | Int32
sessstat-nw-init-no-qos-update-att | Session Statistics - Total bearers modified - Network initiated - no quality of service (QoS) modifications attempted Type: Counter | Int32
sessstat-nw-init-bearer-fail-cause | Session Statistics - Total bearers modification failure - Network-initiated Syntax error in packet filter Type: Counter | Int32
sessstat-pdn-ipv4active | Session Statistics - Total PDN-Type Statistics - IPv4 Active Type: Gauge | Int32
sessstat-pdn-ipv4setup | Session Statistics - Total PDN-Type Statistics - IPv4 Setup Type: Counter | Int32
sessstat-pdn-ipv4rel | Session Statistics - Total PDN-Type Statistics - IPv4 Released Type: Counter | Int32
sessstat-pdn-ipv6active | Session Statistics - Total PDN-Type Statistics - IPv6 Active Type: Gauge | Int32
sessstat-pdn-ipv6setup | Session Statistics - Total PDN-Type Statistics - IPv6 Setup Type: Counter | Int32
sessstat-pdn-ipv6rel | Session Statistics - Total PDN-Type Statistics - IPv6 Released Type: Counter | Int32
sessstat-pdn-ipv4v6active | Session Statistics - Total PDN-Type Statistics - IPv4v6 Active Type: Gauge | Int32
sessstat-pdn-ipv4v6setup | Session Statistics - Total PDN-Type Statistics - IPv4v6 Setup Type: Counter | Int32
sessstat-pdn-ipv4v6rel | Session Statistics - Total PDN-Type Statistics - IPv4v6 Released Type: Counter | Int32
sessstat-ipv4addaloc | Session Statistics - IPv4 address allocation Type: Counter | Int32
sessstat-ipaddaloc-ipv4loacalpool | Session Statistics - IP address allocation Statistics - IPv4 Local pool address assign Type: Counter | Int32
sessstat-ipaddaloc-ipv4staticaddr | Session Statistics - IP address allocation Statistics - IPv4 Static address assign Type: Counter | Int32
sessstat-ipaddaloc-ipv4radaddr | Session Statistics - IP address allocation Statistics - IPv4 Radius provided address assign Type: Counter | Int32
sessstat-ipv6addaloc | Session Statistics - IPv6 address allocation Type: Counter | Int32
sessstat-ipaddaloc-ipv6auto | Session Statistics - IP address allocation Statistics - IPv6 Stateless auto config Type: Counter | Int32
subplmnstat-homesubact | Subscriber PLMN Statistics - Home subscribers sessions active Type: Gauge | Int32
subplmnstat-homesubsetup | Subscriber PLMN Statistics - Home subscribers sessions setup Type: Counter | Int32
subplmnstat-homesubrel | Subscriber PLMN Statistics - Home subscribers sessions released Type: Counter | Int32
subplmnstat-roamsubact | Subscriber PLMN Statistics - Roaming subscribers sessions active Type: Gauge | Int32
subplmnstat-roamsubsetup | Subscriber PLMN Statistics - Roaming subscribers sessions setup Type: Counter | Int32
subplmnstat-roamsubrel | Subscriber PLMN Statistics - Roaming subscribers sessions released Type: Counter | Int32
subplmnstat-visitsubact | Subscriber PLMN Statistics - Visiting subscribers sessions active Type: Gauge | Int32
subplmnstat-visitsubsetup | Subscriber PLMN Statistics - Visiting subscribers sessions setup Type: Counter | Int32
subplmnstat-visitsubrel | Subscriber PLMN Statistics - Visiting subscribers sessions released Type: Counter | Int32
sgitunstat-ipv4sessact | SGi tunneling Statistics - IPv4 IP-in-IP tunnel sessions active Type: Gauge | Int32
sgitunstat-ipv4sesssetup | SGi tunneling Statistics - IPv4 IP-in-IP tunnel sessions setup Type: Counter | Int32
sgitunstat-ipv4sessrel | SGi tunneling Statistics - IPv4 IP-in-IP tunnel sessions released Type: Counter | Int32
sgitunstat-ipv4gresessact | SGi tunneling Statistics - IPv4 GRE tunnel sessions active Type: Gauge | Int32
sgitunstat-ipv4gresesssetup | SGi tunneling Statistics - IPv4 GRE tunnel sessions setup Type: Counter | Int32
sgitunstat-ipv4gresessrel | SGi tunneling Statistics - IPv4 GRE tunnel sessions released Type: Counter | Int32
sgitunstat-ipv6sessact | SGi tunneling Statistics - IPv6 6to4 tunnel sessions active Type: Gauge | Int32
sgitunstat-ipv6sesssetup | SGi tunneling Statistics - IPv6 6to4 tunnel sessions setup Type: Counter | Int32
sgitunstat-ipv6sessrel | SGi tunneling Statistics - IPv6 6to4 tunnel sessions released Type: Counter | Int32
handoverstat-intersgsnatt | Handover Statistics - Total number of inter-SGSN handover attempts Type: Counter | Int32
handoverstat-intersgsnsucc | Handover Statistics - Total number of successful inter-SGSN handovers Type: Counter | Int32
handoverstat-intersgsnfail | Handover Statistics - Total number of failed inter-SGSN handovers Type: Counter | Int32
handoverstat-intersgwatt | Handover Statistics - Total number of inter-SGW handover attempts Type: Counter | Int32
handoverstat-intersgwsucc | Handover Statistics - Total number of successful inter-SGW handovers Type: Counter | Int32
handoverstat-intersgwfail | Handover Statistics - Total number of failed inter-SGW handovers Type: Counter | Int32
handoverstat-interhsgwatt | Handover Statistics - Total number of inter-HSGW handover attempts Type: Counter | Int32
handoverstat-interhsgwsucc | Handover Statistics - Total number of successful inter-HSGW handovers Type: Counter | Int32
handoverstat-interhsgwfail | Handover Statistics - Total number of failed inter-HSGW handovers Type: Counter | Int32
handoverstat-gngptolteatt | Handover Statistics - Number of Gn/Gp to LTE attempted handovers Type: Counter | Int32
handoverstat-gngptoltesucc | Handover Statistics - Number of Gn/Gp to LTE successful handovers Type: Counter | Int32
handoverstat-gngptoltefail | Handover Statistics - Number of Gn/Gp to LTE failed handovers Type: Counter | Int32
handoverstat-ltetogngpatt | Handover Statistics - Number of LTE to Gn/Gp attempted handovers Type: Counter | Int32
handoverstat-ltetogngpsucc | Handover Statistics - Number of LTE to Gn/Gp successful handovers Type: Counter | Int32
handoverstat-ltetogngpfail | Handover Statistics - Number of LTE to Gn/Gp failed handovers Type: Counter | Int32
handoverstat-ltetoehrpdatt | Handover Statistics -Number of LTE to eHPRD attempted handovers Type: Counter | Int32
handoverstat-ltetoehrpdsucc | Handover Statistics - Number of LTE to eHPRD successful handovers Type: Counter | Int32
handoverstat-ltetoehrpdfail | Handover Statistics - Number of LTE to eHRPD failed handovers Type: Counter | Int32
handoverstat-ehrpdtolteatt | Handover Statistics - Number of eHPRD to LTE attempted handovers Type: Counter | Int32
handoverstat-ehrpdtoltesucc | Handover Statistics - Number of eHPRD to LTE successful handovers Type: Counter | Int32
handoverstat-ehrpdtoltefail | Handover Statistics - Number of eHPRD to LTE failed handovers Type: Counter | Int32
subqosstat-bearact-qci1 | Subscriber QoS Statistics - Total bearers active - QCI 1 Type: Gauge | Int32
subqosstat-bearact-qci2 | Subscriber QoS Statistics - Total bearers active - QCI 2 Type: Gauge | Int32
subqosstat-bearact-qci3 | Subscriber QoS Statistics - Total bearers active - QCI 3 Type: Gauge | Int32
subqosstat-bearact-qci4 | Subscriber QoS Statistics - Total bearers active - QCI 4 Type: Gauge | Int32
subqosstat-bearact-qci5 | Subscriber QoS Statistics - Total bearers active - QCI 5 Type: Gauge | Int32
subqosstat-bearact-qci6 | Subscriber QoS Statistics - Total bearers active - QCI 6 Type: Gauge | Int32
subqosstat-bearact-qci7 | Subscriber QoS Statistics - Total bearers active - QCI 7 Type: Gauge | Int32
subqosstat-bearact-qci8 | Subscriber QoS Statistics - Total bearers active - QCI 8 Type: Gauge | Int32
subqosstat-bearact-qci9 | Subscriber QoS Statistics - Total bearers active - QCI 9 Type: Gauge | Int32
subqosstat-bearact-qcinongbr | Subscriber QoS Statistics - Total bearers active - Non-Standard QCI (Non-GBR) Type: Gauge | Int32
subqosstat-bearact-qcigbr | Subscriber QoS Statistics - Total bearers active - Non-Standard QCI (GBR) Type: Gauge | Int32
subqosstat-bearsetup-qci1 | Subscriber QoS Statistics - Total bearers setup - QCI 1 Type: Counter | Int32
subqosstat-bearsetup-qci2 | Subscriber QoS Statistics - Total bearers setup - QCI 2 Type: Counter | Int32
subqosstat-bearsetup-qci3 | Subscriber QoS Statistics - Total bearers setup - QCI 3 Type: Counter | Int32
subqosstat-bearsetup-qci4 | Subscriber QoS Statistics - Total bearers setup - QCI 4 Type: Counter | Int32
subqosstat-bearsetup-qci5 | Subscriber QoS Statistics - Total bearers setup - QCI 5 Type: Counter | Int32
subqosstat-bearsetup-qci6 | Subscriber QoS Statistics - Total bearers setup - QCI 6 Type: Counter | Int32
subqosstat-bearsetup-qci7 | Subscriber QoS Statistics - Total bearers setup - QCI 7 Type: Counter | Int32
subqosstat-bearsetup-qci8 | Subscriber QoS Statistics - Total bearers setup - QCI 8 Type: Counter | Int32
subqosstat-bearsetup-qci9 | Subscriber QoS Statistics - Total bearers setup - QCI 9 Type: Counter | Int32
subqosstat-bearsetup-qcinongbr | Subscriber QoS Statistics - Total bearers setup - Non-Standard QCI (Non-GBR) Type: Counter | Int32
subqosstat-bearsetup-qcigbr | Subscriber QoS Statistics - Total bearers setup - Non-Standard QCI (GBR) Type: Counter | Int32
subqosstat-bearrel-qci1 | Subscriber QoS Statistics - Total bearers released - QCI 1 Type: Counter | Int32
subqosstat-bearrel-qci2 | Subscriber QoS Statistics - Total bearers released - QCI 2 Type: Counter | Int32
subqosstat-bearrel-qci3 | Subscriber QoS Statistics - Total bearers released - QCI 3 Type: Counter | Int32
subqosstat-bearrel-qci4 | Subscriber QoS Statistics - Total bearers released - QCI 4 Type: Counter | Int32
subqosstat-bearrel-qci5 | Subscriber QoS Statistics - Total bearers released - QCI 5 Type: Counter | Int32
subqosstat-bearrel-qci6 | Subscriber QoS Statistics - Total bearers released - QCI 6 Type: Counter | Int32
subqosstat-bearrel-qci7 | Subscriber QoS Statistics - Total bearers released - QCI 7 Type: Counter | Int32
subqosstat-bearrel-qci8 | Subscriber QoS Statistics - Total bearers released - QCI 8 Type: Counter | Int32
subqosstat-bearrel-qci9 | Subscriber QoS Statistics - Total bearers released - QCI 9 Type: Counter | Int32
subqosstat-bearrel-qcinongbr | Subscriber QoS Statistics - Total bearers released - Non-Standard QCI (Non-GBR) Type: Counter | Int32
subqosstat-bearrel-qcigbr | Subscriber QoS Statistics - Total bearers released - Non-Standard QCI (GBR) Type: Counter | Int32
subdatastat-totuppktfwd | Subscriber Data Statistics - Total Uplink packets forwarded Type: Counter | Int32
subdatastat-uppktfwd-qci1 | Subscriber Data Statistics -Uplink packets forwarded - QCI 1 Type: Counter | Int32
subdatastat-uppktfwd-qci2 | Subscriber Data Statistics -Uplink packets forwarded - QCI 2 Type: Counter | Int32
subdatastat-uppktfwd-qci3 | Subscriber Data Statistics -Uplink packets forwarded - QCI 3 Type: Counter | Int32
subdatastat-uppktfwd-qci4 | Subscriber Data Statistics -Uplink packets forwarded - QCI 4 Type: Counter | Int32
subdatastat-uppktfwd-qci5 | Subscriber Data Statistics -Uplink packets forwarded - QCI 5 Type: Counter | Int32
subdatastat-uppktfwd-qci6 | Subscriber Data Statistics -Uplink packets forwarded - QCI 6 Type: Counter | Int32
subdatastat-uppktfwd-qci7 | Subscriber Data Statistics -Uplink packets forwarded - QCI 7 Type: Counter | Int32
subdatastat-uppktfwd-qci8 | Subscriber Data Statistics -Uplink packets forwarded - QCI 8 Type: Counter | Int32
subdatastat-uppktfwd-qci9 | Subscriber Data Statistics -Uplink packets forwarded - QCI 9 Type: Counter | Int32
subdatastat-uppktfwd-stdqcinongbr | Subscriber Data Statistics - Uplink packets forwarded - Standard QCI (Non-GBR) Type: Counter | Int32
subdatastat-uppktfwd-stdqcigbr | Subscriber Data Statistics - Uplink packets forwarded - Standard QCI (GBR) Type: Counter | Int32
subdatastat-uppktfwd-qcinongbr | Subscriber Data Statistics - Uplink packets forwarded - Non-Standard QCI (Non-GBR) Type: Counter | Int32
subdatastat-uppktfwd-qcigbr | Subscriber Data Statistics - Uplink packets forwarded - Non-Standard QCI (GBR) Type: Counter | Int32
subdatastat-uppktfwd-totgbr | Subscriber Data Statistics - Uplink packets forwarded - Total GBR Type: Counter | Int32
subdatastat-uppktfwd-totnongbr | Subscriber Data Statistics - Uplink packets forwarded - Total Non-GBR Type: Counter | Int32
subdatastat-totupbytefwd | Subscriber Data Statistics - Total Uplink bytes forwarded Type: Counter | Int64
subdatastat-upbytefwd-qci1 | Subscriber Data Statistics - Uplink bytes forwarded - QCI 1 Type: Counter | Int64
subdatastat-upbytefwd-qci2 | Subscriber Data Statistics - Uplink bytes forwarded - QCI 2 Type: Counter | Int64
subdatastat-upbytefwd-qci3 | Subscriber Data Statistics - Uplink bytes forwarded - QCI 3 Type: Counter | Int64
subdatastat-upbytefwd-qci4 | Subscriber Data Statistics - Uplink bytes forwarded - QCI 4 Type: Counter | Int64
subdatastat-upbytefwd-qci5 | Subscriber Data Statistics - Uplink bytes forwarded - QCI 5 Type: Counter | Int64
subdatastat-upbytefwd-qci6 | Subscriber Data Statistics - Uplink bytes forwarded - QCI 6 Type: Counter | Int64
subdatastat-upbytefwd-qci7 | Subscriber Data Statistics - Uplink bytes forwarded - QCI 7 Type: Counter | Int64
subdatastat-upbytefwd-qci8 | Subscriber Data Statistics - Uplink bytes forwarded - QCI 8 Type: Counter | Int64
subdatastat-upbytefwd-qci9 | Subscriber Data Statistics - Uplink bytes forwarded - QCI 9 Type: Counter | Int64
subdatastat-upbytefwd-stdqcinongbr | Subscriber Data Statistics - Uplink bytes forwarded - Standard QCI (Non-GBR) Type: Counter | Int64
subdatastat-upbytefwd-stdqcigbr | Subscriber Data Statistics - Uplink bytes forwarded - Standard QCI (GBR) Type: Counter | Int64
subdatastat-upbytefwd-qcinongbr | Subscriber Data Statistics - Uplink bytes forwarded - Non-Standard QCI (Non-GBR) Type: Counter | Int64
subdatastat-upbytefwd-qcigbr | Subscriber Data Statistics - Uplink bytes forwarded - Non-Standard QCI (GBR) Type: Counter | Int64
subdatastat-upbytefwd-totgbr | Subscriber Data Statistics - Uplink bytes forwarded - Total GBR Type: Counter | Int64
subdatastat-upbytefwd-totnongbr | Subscriber Data Statistics - Uplink bytes forwarded - Total NON-GBR Type: Counter | Int64
subdatastat-totdownpktfwd | Subscriber Data Statistics - Total Downlink packets forwarded Type: Counter | Int32
subdatastat-downpktfwd-qci1 | Subscriber Data Statistics - Downlink packets forwarded - QCI 1 Type: Counter | Int32
subdatastat-downpktfwd-qci2 | Subscriber Data Statistics - Downlink packets forwarded - QCI 2 Type: Counter | Int32
subdatastat-downpktfwd-qci3 | Subscriber Data Statistics - Downlink packets forwarded - QCI 3 Type: Counter | Int32
subdatastat-downpktfwd-qci4 | Subscriber Data Statistics - Downlink packets forwarded - QCI 4 Type: Counter | Int32
subdatastat-downpktfwd-qci5 | Subscriber Data Statistics - Downlink packets forwarded - QCI 5 Type: Counter | Int32
subdatastat-downpktfwd-qci6 | Subscriber Data Statistics - Downlink packets forwarded - QCI 6 Type: Counter | Int32
subdatastat-downpktfwd-qci7 | Subscriber Data Statistics - Downlink packets forwarded - QCI 7 Type: Counter | Int32
subdatastat-downpktfwd-qci8 | Subscriber Data Statistics - Downlink packets forwarded - QCI 8 Type: Counter | Int32
subdatastat-downpktfwd-qci9 | Subscriber Data Statistics - Downlink packets forwarded - QCI 9 Type: Counter | Int32
subdatastat-downpktfwd-stdqcinongbr | Subscriber Data Statistics - Downlink packets forwarded - Standard QCI (Non-GBR) Type: Counter | Int32
subdatastat-downpktfwd-stdqcigbr | Subscriber Data Statistics - Downlink packets forwarded - Standard QCI (GBR) Type: Counter | Int32
subdatastat-downpktfwd-qcinongbr | Subscriber Data Statistics - Downlink packets forwarded - Non-Standard QCI (Non-GBR) Type: Counter | Int32
subdatastat-downpktfwd-qcigbr | Subscriber Data Statistics - Downlink packets forwarded - Non-Standard QCI (GBR) Type: Counter | Int32
subdatastat-downpktfwd-totgbr | Subscriber Data Statistics - Downlink packets forwarded - Total GBR Type: Counter | Int32
subdatastat-downpktfwd-totnongbr | Subscriber Data Statistics - Downlink packets forwarded - Total Non-GBR Type: Counter | Int32
subdatastat-totdownbytefwd | Subscriber Data Statistics - Total Downlink bytes forwarded Type: Counter | Int64
subdatastat-downbytefwd-qci1 | Subscriber Data Statistics - Downlink bytes forwarded - QCI 1 Type: Counter | Int64
subdatastat-downbytefwd-qci2 | Subscriber Data Statistics - Downlink bytes forwarded - QCI 2 Type: Counter | Int64
subdatastat-downbytefwd-qci3 | Subscriber Data Statistics - Downlink bytes forwarded - QCI 3 Type: Counter | Int64
subdatastat-downbytefwd-qci4 | Subscriber Data Statistics - Downlink bytes forwarded - QCI 4 Type: Counter | Int64
subdatastat-downbytefwd-qci5 | Subscriber Data Statistics - Downlink bytes forwarded - QCI 5 Type: Counter | Int64
subdatastat-downbytefwd-qci6 | Subscriber Data Statistics - Downlink bytes forwarded - QCI 6 Type: Counter | Int64
subdatastat-downbytefwd-qci7 | Subscriber Data Statistics - Downlink bytes forwarded - QCI 7 Type: Counter | Int64
subdatastat-downbytefwd-qci8 | Subscriber Data Statistics - Downlink bytes forwarded - QCI 8 Type: Counter | Int64
subdatastat-downbytefwd-qci9 | Subscriber Data Statistics - Downlink bytes forwarded - QCI 9 Type: Counter | Int64
subdatastat-downbytefwd-stdqcinongbr | Subscriber Data Statistics - Downlink bytes forwarded - Standard QCI (Non-GBR) Type: Counter | Int64
subdatastat-downbytefwd-stdqcigbr | Subscriber Data Statistics - Downlink bytes forwarded - Standard QCI (GBR) Type: Counter | Int64
subdatastat-downbytefwd-qcinongbr | Subscriber Data Statistics - Downlink bytes forwarded - Non-Standard QCI (Non-GBR) Type: Counter | Int64
subdatastat-downbytefwd-qcigbr | Subscriber Data Statistics - Downlink bytes forwarded - Non-Standard QCI (GBR) Type: Counter | Int64
subdatastat-downbytefwd-totgbr | Subscriber Data Statistics - Downlink bytes forwarded - Total GBR Type: Counter | Int64
subdatastat-downbytefwd-totnongbr | Subscriber Data Statistics - Downlink bytes forwarded - Total Non-GBR Type: Counter | Int64
subdatastat-totuppktdrop | Subscriber Data Statistics - Total Uplink packets dropped Type: Counter | Int32
subdatastat-uppktdrop-qci1 | Subscriber Data Statistics -Uplink packets dropped - QCI 1 Type: Counter | Int32
subdatastat-uppktdrop-qci2 | Subscriber Data Statistics -Uplink packets dropped - QCI 2 Type: Counter | Int32
subdatastat-uppktdrop-qci3 | Subscriber Data Statistics -Uplink packets dropped - QCI 3 Type: Counter | Int32
subdatastat-uppktdrop-qci4 | Subscriber Data Statistics -Uplink packets dropped - QCI 4 Type: Counter | Int32
subdatastat-uppktdrop-qci5 | Subscriber Data Statistics -Uplink packets dropped - QCI 5 Type: Counter | Int32
subdatastat-uppktdrop-qci6 | Subscriber Data Statistics -Uplink packets dropped - QCI 6 Type: Counter | Int32
subdatastat-uppktdrop-qci7 | Subscriber Data Statistics -Uplink packets dropped - QCI 7 Type: Counter | Int32
subdatastat-uppktdrop-qci8 | Subscriber Data Statistics -Uplink packets dropped - QCI 8 Type: Counter | Int32
subdatastat-uppktdrop-qci9 | Subscriber Data Statistics -Uplink packets dropped - QCI 9 Type: Counter | Int32
subdatastat-uppktdrop-stdqcinongbr | Subscriber Data Statistics - Uplink packets dropped - Standard QCI (Non-GBR) Type: Counter | Int32
subdatastat-uppktdrop-stdqcigbr | Subscriber Data Statistics - Uplink packets dropped - Standard QCI (GBR) Type: Counter | Int32
subdatastat-uppktdrop-qcinongbr | Subscriber Data Statistics - Uplink packets dropped - Non-Standard QCI (Non-GBR) Type: Counter | Int32
subdatastat-uppktdrop-qcigbr | Subscriber Data Statistics - Uplink packets dropped - Non-Standard QCI (GBR) Type: Counter | Int32
subdatastat-uppktdrop-totgbr | Subscriber Data Statistics - Uplink packets dropped - Total GBR Type: Counter | Int32
subdatastat-uppktdrop-totnongbr | Subscriber Data Statistics - Uplink packets dropped - Total Non-GBR Type: Counter | Int32
subdatastat-totupbytedrop | Subscriber Data Statistics - Total Uplink bytes dropped Type: Counter | Int64
subdatastat-upbytedrop-qci1 | Subscriber Data Statistics - Uplink bytes dropped - QCI 1 Type: Counter | Int64
subdatastat-upbytedrop-qci2 | Subscriber Data Statistics - Uplink bytes dropped - QCI 2 Type: Counter | Int64
subdatastat-upbytedrop-qci3 | Subscriber Data Statistics - Uplink bytes dropped - QCI 3 Type: Counter | Int64
subdatastat-upbytedrop-qci4 | Subscriber Data Statistics - Uplink bytes dropped - QCI 4 Type: Counter | Int64
subdatastat-upbytedrop-qci5 | Subscriber Data Statistics - Uplink bytes dropped - QCI 5 Type: Counter | Int64
subdatastat-upbytedrop-qci6 | Subscriber Data Statistics - Uplink bytes dropped - QCI 6 Type: Counter | Int64
subdatastat-upbytedrop-qci7 | Subscriber Data Statistics - Uplink bytes dropped - QCI 7 Type: Counter | Int64
subdatastat-upbytedrop-qci8 | Subscriber Data Statistics - Uplink bytes dropped - QCI 8 Type: Counter | Int64
subdatastat-upbytedrop-qci9 | Subscriber Data Statistics - Uplink bytes dropped - QCI 9 Type: Counter | Int64
subdatastat-upbytedrop-stdqcinongbr | Subscriber Data Statistics - Uplink bytes dropped - Standard QCI (Non-GBR) Type: Counter | Int64
subdatastat-upbytedrop- stdqcigbr | Subscriber Data Statistics - Uplink bytes dropped - Standard QCI (GBR) Type: Counter | Int64
subdatastat-upbytedrop-qcinongbr | Subscriber Data Statistics - Uplink bytes dropped - Non-Standard QCI (Non-GBR) Type: Counter | Int64
subdatastat-upbytedrop-qcigbr | Subscriber Data Statistics - Uplink bytes dropped - Non-Standard QCI (GBR) Type: Counter | Int64
subdatastat-upbytedrop-totgbr | Subscriber Data Statistics - Uplink bytes dropped - Total GBR Type: Counter | Int64
subdatastat-upbytedrop-totnongbr | Subscriber Data Statistics - Uplink bytes dropped - Total Non-GBR Type: Counter | Int64
subdatastat-totdownpktdrop | Subscriber Data Statistics - Total Downlink packets dropped Type: Counter | Int32
subdatastat-downpktdrop-qci1 | Subscriber Data Statistics - Downlink packets dropped - QCI 1 Type: Counter | Int32
subdatastat-downpktdrop-qci2 | Subscriber Data Statistics - Downlink packets dropped - QCI 2 Type: Counter | Int32
subdatastat-downpktdrop-qci3 | Subscriber Data Statistics - Downlink packets dropped - QCI 3 Type: Counter | Int32
subdatastat-downpktdrop-qci4 | Subscriber Data Statistics - Downlink packets dropped - QCI 4 Type: Counter | Int32
subdatastat-downpktdrop-qci5 | Subscriber Data Statistics - Downlink packets dropped - QCI 5 Type: Counter | Int32
subdatastat-downpktdrop-qci6 | Subscriber Data Statistics - Downlink packets dropped - QCI 6 Type: Counter | Int32
subdatastat-downpktdrop-qci7 | Subscriber Data Statistics - Downlink packets dropped - QCI 7 Type: Counter | Int32
subdatastat-downpktdrop-qci8 | Subscriber Data Statistics - Downlink packets dropped - QCI 8 Type: Counter | Int32
subdatastat-downpktdrop-qci9 | Subscriber Data Statistics - Downlink packets dropped - QCI 9 Type: Counter | Int32
subdatastat-downpktdrop-stdqcinongbr | Subscriber Data Statistics - Downlink packets dropped - Standard QCI (Non-GBR) Type: Counter | Int32
subdatastat-downpktdrop-stdqcigbr | Subscriber Data Statistics - Downlink packets dropped - Standard QCI (GBR) Type: Counter | Int32
subdatastat-downpktdrop-qcinongbr | Subscriber Data Statistics - Downlink packets dropped - Non-Standard QCI (Non-GBR) Type: Counter | Int32
subdatastat-downpktdrop-qcigbr | Subscriber Data Statistics - Downlink packets dropped - Non-Standard QCI (GBR) Type: Counter | Int32
subdatastat-downpktdrop-totgbr | Subscriber Data Statistics - Downlink packets dropped - Total GBR Type: Counter | Int32
subdatastat-downpktdrop-totnongbr | Subscriber Data Statistics - Downlink packets dropped - Total Non-GBR Type: Counter | Int32
subdatastat-totdownbytedrop | Subscriber Data Statistics - Total Downlink bytes dropped Type: Counter | Int64
subdatastat-downbytedrop-qci1 | Subscriber Data Statistics - Downlink bytes dropped - QCI 1 Type: Counter | Int64
subdatastat-downbytedrop-qci2 | Subscriber Data Statistics - Downlink bytes dropped - QCI 2 Type: Counter | Int64
subdatastat-downbytedrop-qci3 | Subscriber Data Statistics - Downlink bytes dropped - QCI 3 Type: Counter | Int64
subdatastat-downbytedrop-qci4 | Subscriber Data Statistics - Downlink bytes dropped - QCI 4 Type: Counter | Int64
subdatastat-downbytedrop-qci5 | Subscriber Data Statistics - Downlink bytes dropped - QCI 5 Type: Counter | Int64
subdatastat-downbytedrop-qci6 | Subscriber Data Statistics - Downlink bytes dropped - QCI 6 Type: Counter | Int64
subdatastat-downbytedrop-qci7 | Subscriber Data Statistics - Downlink bytes dropped - QCI 7 Type: Counter | Int64
subdatastat-downbytedrop-qci8 | Subscriber Data Statistics - Downlink bytes dropped - QCI 8 Type: Counter | Int64
subdatastat-downbytedrop-qci9 | Subscriber Data Statistics - Downlink bytes dropped - QCI 9 Type: Counter | Int64
subdatastat-downbytedrop-stdqcinongbr | Subscriber Data Statistics - Downlink bytes dropped - Standard QCI (Non-GBR) Type: Counter | Int64
subdatastat-downbytedrop-stdqcigbr | Subscriber Data Statistics - Downlink bytes dropped - Standard QCI (GBR) Type: Counter | Int64
subdatastat-downbytedrop-qcinongbr | Subscriber Data Statistics - Downlink bytes dropped - Non-Standard QCI (Non-GBR) Type: Counter | Int64
subdatastat-downbytedrop-qcigbr | Subscriber Data Statistics - Downlink bytes dropped - Non-Standard QCI (GBR) Type: Counter | Int64
subdatastat-downbytedrop-totgbr | Subscriber Data Statistics - Downlink bytes dropped - Total GBR Type: Counter | Int64
subdatastat-downbytedrop-totnongbr | Subscriber Data Statistics - Downlink bytes dropped - Total Non-GBR Type: Counter | Int64
subdatastat-totuppktdropmbrexc | Subscriber Data Statistics - Total Uplink packets Drop mbr exceed Type: Counter | Int32
subdatastat-uppktdropmbrexc-qci1 | Subscriber Data Statistics - Uplink packets Drop mbr exceed - QCI 1 Type: Counter | Int32
subdatastat-uppktdropmbrexc-qci2 | Subscriber Data Statistics - Uplink packets Drop mbr exceed - QCI 2 Type: Counter | Int32
subdatastat-uppktdropmbrexc-qci3 | Subscriber Data Statistics - Uplink packets Drop mbr exceed- QCI 3 Type: Counter | Int32
subdatastat-uppktdropmbrexc-qci4 | Subscriber Data Statistics - Uplink packets Drop mbr exceed - QCI 4 Type: Counter | Int32
subdatastat-uppktdropmbrexc-qci5 | Subscriber Data Statistics - Uplink packets Drop mbr exceed- QCI 5 Type: Counter | Int32
subdatastat-uppktdropmbrexc-qci6 | Subscriber Data Statistics - Uplink packets Drop mbr exceed - QCI 6 Type: Counter | Int32
subdatastat-uppktdropmbrexc-qci7 | Subscriber Data Statistics - Uplink packets Drop mbr exceed - QCI 7 Type: Counter | Int32
subdatastat-uppktdropmbrexc-qci8 | Subscriber Data Statistics - Uplink packets Drop mbr exceed - QCI 8 Type: Counter | Int32
subdatastat-uppktdropmbrexc-qci9 | Subscriber Data Statistics - Uplink packets Drop mbr exceed - QCI 9 Type: Counter | Int32
subdatastat-uppktdropmbrexc-stdqcinongbr | Subscriber Data Statistics - Uplink packets Drop mbr exceed - Standard QCI (Non-GBR Type: Counter | Int32
subdatastat-uppktdropmbrexc-stdqcigbr | Subscriber Data Statistics - Uplink packets Drop mbr exceed - Standard QCI (GBR) Type: Counter | Int32
subdatastat-uppktdropmbrexc-qcinongbr | Subscriber Data Statistics - Uplink packets Drop mbr exceed - Non-Standard QCI (Non-GBR) Type: Counter | Int32
subdatastat-uppktdropmbrexc-qcigbr | Subscriber Data Statistics - Uplink packets Drop mbr exceed - Non-Standard QCI (GBR) Type: Counter | Int32
subdatastat-uppktdropmbrexc-totgbr | Subscriber Data Statistics - Uplink packets Drop mbr exceed - Total GBR Type: Counter | Int32
subdatastat-uppktdropmbrexc-totnongbr | Subscriber Data Statistics - Uplink packets Drop mbr exceed - Total Non-GBR Type: Counter | Int32
subdatastat-totupbytedropmbrexc | Subscriber Data Statistics - Total Uplink bytes Drop mbr exceed Type: Counter | Int64
subdatastat-upbytedropmbrexc-qci1 | Subscriber Data Statistics - Uplink bytes Drop mbr exceed - QCI 1 Type: Counter | Int64
subdatastat-upbytedropmbrexc-qci2 | Subscriber Data Statistics - Uplink bytes Drop mbr exceed - QCI 2 Type: Counter | Int64
subdatastat-upbytedropmbrexc-qci3 | Subscriber Data Statistics - Uplink bytes Drop mbr exceed- QCI 3 Type: Counter | Int64
subdatastat-upbytedropmbrexc-qci4 | Subscriber Data Statistics - Uplink bytes Drop mbr exceed - QCI 4 Type: Counter | Int64
subdatastat-upbytedropmbrexc-qci5 | Subscriber Data Statistics - Uplink bytes Drop mbr exceed- QCI 5 Type: Counter | Int64
subdatastat-upbytedropmbrexc-qci6 | Subscriber Data Statistics - Uplink bytes Drop mbr exceed - QCI 6 Type: Counter | Int64
subdatastat-upbytedropmbrexc-qci7 | Subscriber Data Statistics - Uplink bytes Drop mbr exceed - QCI 7 Type: Counter | Int64
subdatastat-upbytedropmbrexc-qci8 | Subscriber Data Statistics - Uplink bytes Drop mbr exceed - QCI 8 Type: Counter | Int64
subdatastat-upbytedropmbrexc-qci9 | Subscriber Data Statistics - Uplink bytes Drop mbr exceed - QCI 9 Type: Counter | Int64
subdatastat-upbytedropmbrexc-stdqcinongbr | Subscriber Data Statistics - Uplink bytes Drop mbr exceed - Standard QCI (Non-GBR Type: Counter | Int64
subdatastat-upbytedropmbrexc-stdqcigbr | Subscriber Data Statistics - Uplink bytes Drop mbr exceed - Standard QCI (GBR) Type: Counter | Int64
subdatastat-upbytedropmbrexc-qcinongbr | Subscriber Data Statistics - Uplink bytes Drop mbr exceed - Non-Standard QCI (Non-GBR) Type: Counter | Int64
subdatastat-upbytedropmbrexc-qcigbr | Subscriber Data Statistics - Uplink bytes Drop mbr exceed - Non-Standard QCI (GBR) Type: Counter | Int64
subdatastat-upbytedropmbrexc-totgbr | Subscriber Data Statistics - Uplink bytes Drop mbr exceed - Total GBR Type: Counter | Int64
subdatastat-upbytedropmbrexc-totnongbr | Subscriber Data Statistics - Uplink bytes Drop mbr exceed - Total NON-GBR Type: Counter | Int64
subdatastat-totdownpktdropmbrexc | Subscriber Data Statistics - Total Downlink packets Drop mbr exceed Type: Counter | Int32
subdatastat-downpktdropmbrexc-qci1 | Subscriber Data Statistics - Downlink packets Drop mbr exceed - QCI 1 Type: Counter | Int32
subdatastat-downpktdropmbrexc-qci2 | Subscriber Data Statistics - Downlink packets Drop mbr exceed - QCI 2 Type: Counter | Int32
subdatastat-downpktdropmbrexc-qci3 | Subscriber Data Statistics - Downlink packets Drop mbr exceed- QCI 3 Type: Counter | Int32
subdatastat-downpktdropmbrexc-qci4 | Subscriber Data Statistics - Downlink packets Drop mbr exceed - QCI 4 Type: Counter | Int32
subdatastat-downpktdropmbrexc-qci5 | Subscriber Data Statistics - Downlink packets Drop mbr exceed- QCI 5 Type: Counter | Int32
subdatastat-downpktdropmbrexc-qci6 | Subscriber Data Statistics - Downlink packets Drop mbr exceed - QCI 6 Type: Counter | Int32
subdatastat-downpktdropmbrexc-qci7 | Subscriber Data Statistics - Downlink packets Drop mbr exceed - QCI 7 Type: Counter | Int32
subdatastat-downpktdropmbrexc-qci8 | Subscriber Data Statistics - Downlink packets Drop mbr exceed - QCI 8 Type: Counter | Int32
subdatastat-downpktdropmbrexc-qci9 | Subscriber Data Statistics - Downlink packets Drop mbr exceed - QCI 9 Type: Counter | Int32
subdatastat-downpktdropmbrexc-stdqcinongbr | Subscriber Data Statistics - Downlink packets Drop mbr exceed - Standard QCI (Non-GBR Type: Counter | Int32
subdatastat-downpktdropmbrexc-stdqcigbr | Subscriber Data Statistics - Downlink packets Drop mbr exceed - Standard QCI (GBR) Type: Counter | Int32
subdatastat-downpktdropmbrexc-qcinongbr | Subscriber Data Statistics - Downlink packets Drop mbr exceed - Non-Standard QCI (Non-GBR) Type: Counter | Int32
subdatastat-downpktdropmbrexc-qcigbr | Subscriber Data Statistics - Downlink packets Drop mbr exceed - Non-Standard QCI (GBR) Type: Counter | Int32
subdatastat-downpktdropmbrexc-totgbr | Subscriber Data Statistics - Downlink packets Drop mbr exceed - Total GBR Type: Counter | Int32
subdatastat-downpktdropmbrexc-totnongbr | Subscriber Data Statistics - Downlink packets Drop mbr exceed - Total NON-GBR Type: Counter | Int32
subdatastat-totdownbytedropmbrexc | Subscriber Data Statistics - Total Downlink bytes Drop mbr exceed Type: Counter | Int64
subdatastat-downbytedropmbrexc-qci1 | Subscriber Data Statistics - Downlink bytes Drop mbr exceed - QCI 1 Type: Counter | Int64
subdatastat-downbytedropmbrexc-qci2 | Subscriber Data Statistics - Downlink bytes Drop mbr exceed - QCI 2 Type: Counter | Int64
subdatastat-downbytedropmbrexc-qci3 | Subscriber Data Statistics - Downlink bytes Drop mbr exceed- QCI 3 Type: Counter | Int64
subdatastat-downbytedropmbrexc-qci4 | Subscriber Data Statistics - Downlink bytes Drop mbr exceed - QCI 4 Type: Counter | Int64
subdatastat-downbytedropmbrexc-qci5 | Subscriber Data Statistics - Downlink bytes Drop mbr exceed- QCI 5 Type: Counter | Int64
subdatastat-downbytedropmbrexc-qci6 | Subscriber Data Statistics - Downlink bytes Drop mbr exceed - QCI 6 Type: Counter | Int64
subdatastat-downbytedropmbrexc-qci7 | Subscriber Data Statistics - Downlink bytes Drop mbr exceed - QCI 7 Type: Counter | Int64
subdatastat-downbytedropmbrexc-qci8 | Subscriber Data Statistics - Downlink bytes Drop mbr exceed - QCI 8 Type: Counter | Int64
subdatastat-downbytedropmbrexc-qci9 | Subscriber Data Statistics - Downlink bytes Drop mbr exceed - QCI 9 Type: Counter | Int64
subdatastat-downbytedropmbrexc-stdqcinongbr | Subscriber Data Statistics - Downlink bytes Drop mbr exceed - Standard QCI (Non-GBR) Type: Counter | Int64
subdatastat-downbytedropmbrexc-stdqcigbr | Subscriber Data Statistics - Downlink bytes Drop mbr exceed - Standard QCI (GBR) Type: Counter | Int64
subdatastat-downbytedropmbrexc-qcinongbr | Subscriber Data Statistics - Downlink bytes Drop mbr exceed - Non-Standard QCI (Non-GBR) Type: Counter | Int64
subdatastat-downbytedropmbrexc-qcigbr | Subscriber Data Statistics - Downlink bytes Drop mbr exceed - Non-Standard QCI (GBR) Type: Counter | Int64
subdatastat-downbytedropmbrexc-totgbr | Subscriber Data Statistics - Downlink bytes Drop mbr exceed - Total GBR Type: Counter | Int64
subdatastat-downbytedropmbrexc-totnongbr | Subscriber Data Statistics - Downlink bytes Drop mbr exceed - Total NON-GBR Type: Counter | Int64
apnambrratelimit-uppktdrop | APN AMBR Rate Limiting Statistics - Uplink packets dropped Type: Counter | Int32
apnambrratelimit-downpktdrop | APN AMBR Rate Limiting Statistics - Downlink packets dropped Type: Counter | Int32
apnambrratelimit-upbytedrop | APN AMBR Rate Limiting Statistics - Uplink bytes dropped Type: Counter | Int64
apnambrratelimit-downbytedrop | APN AMBR Rate Limiting Statistics - Downlink bytes dropped Type: Counter | Int64
ipv4-pdn-to-user-pkt | Subscriber Data Statistics - IPv4 PDN to user packets Type: Counter | Int64
ipv4-pdn-to-user-byte | Subscriber Data Statistics - IPv4 PDN to user bytes Type: Counter | Int64
ipv4-pdn-from-user-pkt | Subscriber Data Statistics - IPv4 PDN from user packets Type: Counter | Int64
ipv4-pdn-from-user-byte | Subscriber Data Statistics - IPv4 PDN from user bytes Type: Counter | Int64
ipv6-pdn-to-user-pkt | Subscriber Data Statistics - IPv6 PDN to user packets Type: Counter | Int64
ipv6-pdn-to-user-byte | Subscriber Data Statistics - IPv6 PDN to user bytes Type: Counter | Int64
ipv6-pdn-from-user-pkt | Subscriber Data Statistics - IPv6 PDN from user packets Type: Counter | Int64
ipv6-pdn-from-user-byte | Subscriber Data Statistics - IPv6 PDN from user bytes Type: Counter | Int64
ipv4v6-pdn-ipv4-to-user-pkt | Subscriber Data Statistics - IPv4v6 PDN IPv4 to user packets Type: Counter | Int64
ipv4v6-pdn-ipv4-to-user-byte | Subscriber Data Statistics - IPv4v6 PDN IPv4 to user bytes Type: Counter | Int64
ipv4v6-pdn-ipv4-from-user-pkt | Subscriber Data Statistics - IPv4v6 PDN IPv4 from user packets Type: Counter | Int64
ipv4v6-pdn-ipv4-from-user-byte | Subscriber Data Statistics - IPv4v6 PDN IPv4 from user bytes Type: Counter | Int64
ipv4v6-pdn-ipv6-to-user-pkt | Subscriber Data Statistics - IPv4v6 PDN IPv6 to user packets Type: Counter | Int64
ipv4v6-pdn-ipv6-to-user-byte | Subscriber Data Statistics - IPv4v6 PDN IPv6 to user bytes Type: Counter | Int64
ipv4v6-pdn-ipv6-from-user-pkt | Subscriber Data Statistics - IPv4v6 PDN IPv6 from user packets Type: Counter | Int64
ipv4v6-pdn-ipv6-from-user-byte | Subscriber Data Statistics - IPv4v6 PDN IPv6 from user bytes Type: Counter | Int64
IMPORTANT: For information on statistics that are common to all schema see the Statistics and Counters Overview chapter.