# show gmb

This chapter includes the show gmb command output tables.

show gmb statistics

Table 1. show gmb statistics Command Output Descriptions

Field | Description
--- | ---
MBMS Context Stats
Total Current | Total number of MBMS contexts currently in active status on Gmb interface.
Total Setup | Total number of MBMS contexts are in setup status on Gmb interface.
Total Released | Total number of MBMS contexts release on Gmb interface.
Total Denied | Total number of MBMS contexts requests denied on Gmb interface.
MBMS UE | Total number of UEs in active/setup status or released/denied on this Gmb interface for MBMS service.
MBMS Mcast Bearer | Total number of multicast bearers in active/setup status or released/denied on this Gmb interface for MBMS service.
MBMS Bcast Bearer | Total number of broadcast bearers in active/setup status or released/denied on this Gmb interface for MBMS service.
MBMS UE Context Management Stats
MBMS UE Auth | Total number of UE Auth Request messages received on this Gmb interface for MBMS service.
Accepted | Total number of UE Auth Request messages received and accepted on this Gmb interface for MBMS service.
Denied | Total number of UE Auth Request messages received and denied on this Gmb interface for MBMS service.
MBMS UE Update | Total number of UE Update Request messages received on this Gmb interface for MBMS service.
Accepted | Total number of UE Update Request messages received and accepted on this Gmb interface for MBMS service.
Denied | Total number of UE Update Request messages received and denied on this Gmb interface for MBMS service.
MBMS UE Delete Tx | Total number of UE Delete Request messages transmitted on this Gmb interface for MBMS service.
Accepted | Total number of UE Delete Request messages transmitted and accepted on this Gmb interface for MBMS service.
Denied | Total number of UE Delete Request messages transmitted and denied on this Gmb interface for MBMS service.
MBMS UE Delete Rx | Total number of UE Delete Request messages received on this Gmb interface for MBMS service.
Accepted | Total number of UE Delete Request messages received and accepted on this Gmb interface for MBMS service.
Denied | Total number of UE Delete Request messages received and denied on this Gmb interface for MBMS service.
Discarded | Total number of UE Delete Request messages received but discarded on this Gmb interface for MBMS service.
MBMS Bearer (Multicast) Context Management Stats
MBMS Bearer Reg | Total number of Multicast Bearer Context Register request messages received on this Gmb interface for MBMS service.
Accepted | Total number of Multicast Bearer Context Register request messages received and accepted on this Gmb interface for MBMS service.
Denied | Total number of Multicast Bearer Context Register request messages received and denied on this Gmb interface for MBMS service.
MBMS Bearer Dereg TX | Total number of Multicast Bearer Context Dereg Request messages transmitted on this Gmb interface for MBMS service.
Accepted | Total number of Multicast Bearer Context Dereg Request messages transmitted and accepted on this Gmb interface for MBMS service.
Denied | Total number of Multicast Bearer Context Dereg Request messages transmitted and denied on this Gmb interface for MBMS service.
MBMS Bearer Dereg RX | Total number of Multicast Bearer Context Dereg messages received on this Gmb interface for MBMS service.
Accepted | Total number of Multicast Bearer Context Dereg Request messages received and accepted on this Gmb interface for MBMS service.
Denied | Total number of Multicast Bearer Context Dereg Request messages received and denied on this Gmb interface for MBMS service.
Discarded | Total number of Multicast Bearer Context Dereg Request messages received but discarded on this Gmb interface for MBMS service.
MBMS Mcast Sess Start | Total number of Multicast Session Start Request messages received on this Gmb interface for MBMS service.
Accepted | Total number of Multicast Session Start Request messages received and accepted on this Gmb interface for MBMS service.
Denied | Total number of Multicast Session Start Request messages received and denied on this Gmb interface for MBMS service.
Discarded | Total number of Multicast Session Start Request messages received but discarded on this Gmb interface for MBMS service.
MBMS Mcast Sess Stop | Total number of Multicast Session Stop Request messages received on this Gmb interface for MBMS service.
Accepted | Total number of Multicast Session Stop Request messages received and accepted on this Gmb interface for MBMS service.
Denied | Total number of Multicast Session Stop Request messages received and denied on this Gmb interface for MBMS service.
Discarded | Total number of Multicast Session Stop Request messages received but discarded on this Gmb interface for MBMS service.
MBMS Mcast Sess Update | Total number of Multicast Session Update Request messages received on this Gmb interface for MBMS service.
Accepted | Total number of Multicast Session Update Request messages received and accepted on this Gmb interface for MBMS service.
Denied | Total number of Multicast Session Update Request messages received and denied on this Gmb interface for MBMS service.
Discarded | Total number of Multicast Session Update Request messages received but discarded on this Gmb interface for MBMS service.
MBMS Bearer (Broadcast) Context Management Stats
MBMS Bcast Sess Start | Total number of Broadcast Session Start Request messages received on this Gmb interface for MBMS service.
Accepted | Total number of Broadcast Session Start Request messages received and accepted on this Gmb interface for MBMS service.
Denied | Total number of Broadcast Session Start Request messages received and denied on this Gmb interface for MBMS service.
Discarded | Total number of Broadcast Session Start Request messages received but discarded on this Gmb interface for MBMS service.
MBMS Bcast Sess Stop | Total number of Broadcast Session Stop messages received on this Gmb interface for MBMS service.
Accepted | Total number of Broadcast Session Stop Request messages received and accepted on this Gmb interface for MBMS service.
Denied | Total number of Broadcast Session Stop Request messages received and denied on this Gmb interface for MBMS service.
Discarded | Total number of Broadcast Session Stop Request messages received but discarded on this Gmb interface for MBMS service.
MBMS Bcast Sess Update | Total number of Broadcast Session Update messages received on this Gmb interface for MBMS service.
Accepted | Total number of Broadcast Session Update Request messages received and accepted on this Gmb interface for MBMS service.
Denied | Total number of Broadcast Session Update Request messages received and denied on this Gmb interface for MBMS service.
Discarded | Total number of Broadcast Session Update Request messages received but discarded on this Gmb interface for MBMS service.
MBMS Bearer (Unknown Service Type) Stats
MBMS Unknown Sess Start denied | Total number of unknown type of Session Start messages received and denied on this Gmb interface for MBMS service.
MBMS Unknown Sess Stop denied | Total number of unknown type of Session Stop messages received and denied on this Gmb interface for MBMS service.
MBMS Unknown Sess Update denied | Total number of unknown type of Session Update messages received and denied on this Gmb interface for MBMS service.