> CSCF ISC Template Configuration Mode Commands
> The CSCF ISC Template Configuration Mode is used to configure the IMS Service Control (ISC) interface within the system.
> Important: The commands or keywords/variables that are available are dependent on platform type, product version, and installed license(s).
> cnsa
> Core Network Service Authorization (CNSA) related commands used to create media profile and service ids.
> Product
> SCM (S-CSCF)
> Privilege
> Administrator
> Syntax
> cnsa { media-profile-id profile_id | service-id service_id [ service_id ]...[ service_id ] }
> no cnsa { media-profile-id | service-id [ service_id ] [ service_id ]...[ service_id ] }
> media-profile profile_id
> Specifies the cnsa media profile id.
> profile_id must be an integer from 0 to 10.
> The media profile id is assigned to a service policy using the cnsa-media-profile command under CSCF Service configuration.
> Important: You can only create one media profile id per ISC template.
> service-id service_id
> Specifies the cnsa service id(s). These ids represent URN parameters which are ICSI (IMS Communication Service Identifier) values that are mapped to a service profile through a media profile id.
> service_id must be from 1 to 79 alpha and/or numeric characters.
> no cnsa { media-profile-id | service-id [ service_id ] [ service_id ]... [ service_id ] }
> Removes a media profile or service id(s).
> Usage
> Use this command to configure cnsa media profile ids and service ids. Information for core network authorization is received from HSS. It contains a list of service ids and a media profile id. Since the media profile id is an integer value, the S-CSCF needs to have a static database that contains the mapping between the integer value and the subscribed media profile. The media profile id is assigned to this service policy using the cnsa-media-profile command under CSCF Service configuration.
> The S-CSCF selects the service profile based on the media profile id set and the policies, such as enforce-codec-policy and video-sessions, will be matched with the incoming request. Other policies, if configured, will be ignored in this scenario.
> Example
> The following command defines the media profile id as 2:
> cnsa media-profile-id 2
> The following command defines several service ids:
> cnsa service-id xxx:exampletelephony.version1 xxx:abc.com
> end
> Exits the current mode and returns to the Exec Mode.
> Product
> All
> Privilege
> Administrator
> Syntax
> end
> Usage
> Change the mode back to the Exec mode.
> exit
> Exits the current mode and returns to the previous mode.
> Product
> All
> Privilege
> Administrator
> Syntax
> exit
> Usage
> Return to the previous mode.
> filter-criteria
> Configure the filter criteria to be used by this template.
> Product
> SCM (S-CSCF)
> Privilege
> Administrator
> Syntax
> [ no ] filter-criteria name criteria_name
> no
> Removes the specified filter criteria.
> name criteria_name
> Specifies the name of existing filter criteria to be used by this template. The particular criteria applied to a subscriber will be based on the priority parameter.
> criteria_name must be from 1 to 39 alpha and/or numeric characters in length.
> Important: Filter criteria can be assigned to more than one ISC template.
> Usage
> Use this command to configure the filter criteria to be used by this template.
> Example
> The following command identifies the filter criteria criteria1:
> filter-criteria name criteria1

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883