> show diameter
> This chapter includes the show diameter command output tables.
> show diameter aaa-statistics
> show diameter aaa-statistics Command Output Descriptions

> Field | Description
> Authentication Servers Summary
> Message Stats | Total Diameter session message statistics.
> Total MA Requests | Total number of Multimedia-Auth-Requests.
> Total MA Answers | Total number of Multimedia-Auth-Answers.
> MAR - Retries | Total number of Multimedia-Auth-Request retries.
> MAA Timeouts | Total number of Multimedia-Auth-Answer timeouts.
> MAA - Dropped | Total number of Multimedia-Auth-Answer dropped.
> Total SA Requests | Total number of Server-Assignment-Requests.
> Total SA Answers | Total number of Server-Assignment-Answers.
> SAR - Retries | Total number of Server-Assignment-Request retries.
> SAA Timeouts | Total number of Server-Assignment-Answer timeouts.
> SAA - Dropped | Total number of Server-Assignment-Answers dropped.
> Total UA Requests | Total number of User-Authorization-Requests.
> Total UA Answers | Total number of User-Authorization-Answers.
> UAR - Retries | Total number of User-Authorization-Request retries.
> UAA Timeouts | Total number of User-Authorization-Answer timeouts.
> UAA - Dropped | Total number of User-Authorization-Answers dropped.
> Total LI Requests | Total number of Location-Info-Requests.
> Total LI Answers | Total number of Location-Info-Answers.
> LIR - Retries | Total number of Location-Info-Request retries.
> LIA Timeouts | Total number of Location-Info-Answer timeouts.
> LIA - Dropped | Total number of Location-Info-Answers dropped.
> Total RT Requests | Total number of Registration-Termination-Requests.
> Total RT Answers | Total number of Registration-Termination-Answers.
> RTR - Rejected | Total number of Registration-Termination-Requests rejected.
> Total PP Requests | Total number of Push-Profile-Requests.
> Total PP Answers | Total number of Push-Profile-Answers.
> PPR - Rejected | Total number of Push-Profile-Requests rejected.
> Total DE Requests | Total number of Diameter-EAP-Requests.
> Total DE Answers | Total number of Diameter-EAP-Answers.
> DEA - Accept | Total number of Diameter-EAP-Answers accepted.
> DEA - Reject | Total number of Diameter-EAP-Answers rejected.
> DER - Retries | Total number of Diameter-EAP-Request retries.
> DEA Timeouts | Total number of Diameter-EAP-Answer timeouts.
> DEA - Dropped | Total number of Diameter-EAP-Answer dropped.
> Total AA Requests | Indicates the total number of AA (Authentication and/or Authorization) Request messages sent by P-GW on S6b interface to AAA Server/Proxy.
> Total AA Answers | Indicates the total number of AA (Authentication and/or Authorization) Answer messages received by P-GW on S6b interface from AAA Server/Proxy.
> AAR - Retries | Indicates the total number of AAR (AA Request) messages retransmitted by P-GW on S6b interface to AAA Server/Proxy.
> AAA Timeouts | Indicates the total number of AAA (AA Answer) messages timed-out due to no response from AAA Server/Proxy.
> AAA - Dropped | Indicates the total number of AAA (AA Answer) messages dropped due any reason from AAA Server/Proxy.
> ASR | Total number of Abort-Session-Requests.
> ASA | Total number of Abort-Session-Answers.
> RAR | Total number of Re-Auth-Requests.
> RAA | Total number of Re-Auth-Answers.
> STR | Total number of Session-Termination-Requests.
> STA | Total number of Session-Termination-Answers.
> STR - Retries | Total number of Session-Termination-Request retries.
> DE Message Error Stats
> Diameter Protocol Errs | Total number of Diameter protocol errors.
> Bad Answers | Total number of bad answers.
> Unknown Session Reqs | Total number of unknown session requests.
> Unknown Command Code | Total number of unknown command codes.
> Request Timeouts | Total number of request timeouts.
> Parse Errors | Total number of parse errors.
> Request Retries | Total number of request retries.
> Session Stats | Diameter Session Statistics.
> Total Sessions | Total number of sessions.
> Freed Sessions | Total number of freed sessions.
> Session Timeouts | Total number of session timeouts.
> Active Sessions | Total number of active sessions.
> STR Termination Cause Stats | Session-Termination-Request termination cause statistics.
> Diameter Logout | Total number of Session-Termination-Request terminations due to Diameter logouts.
> Service Not Provided | Total number of Session-Termination-Request terminations due to service not provided.
> Bad Answer | Total number of Session-Termination-Request terminations due to bad answers.
> Administrative | Total number of Session-Termination-Request terminations due to administrative reasons.
> Link Broken | Total number of Session-Termination-Request terminations due to links broken.
> Auth Expired | Total number of Session-Termination-Request terminations due to auth expiry.
> User Moved | Total number of Session-Termination-Request terminations due to user moves.
> Session Timeout | Total number of Session-Termination-Request terminations due to session timeouts.
> User Request | Total number of Session-Termination-Request terminations due to user requests.
> Lost Carrier | Total number of Session-Termination-Request terminations due to lost carriers.
> Lost Service | Total number of Session-Termination-Request terminations due to lost service.
> Idle Timeout | Total number of Session-Termination-Request terminations due to idle timeouts.
> NAS Session Timeout | Total number of Session-Termination-Request terminations due to NAS session timeouts.
> Admin Reset | Total number of Session-Termination-Request terminations due to admin resetting.
> Admin Reboot | Total number of Session-Termination-Request terminations due to admin reboots.
> Port Error | Total number of Session-Termination-Request terminations due to port errors.
> NAS Error | Total number of Session-Termination-Request terminations due to NAS errors.
> NAS Request | Total number of Session-Termination-Request terminations due to NAS requests.
> NAS Reboot | Total number of Session-Termination-Request terminations due to NAS reboots.
> Port Unneeded | Total number of Session-Termination-Request terminations due to unneeded ports.
> Port Preempted | Total number of Session-Termination-Request terminations due to preempted ports.
> Port Suspended | Total number of Session-Termination-Request terminations due to suspended ports.
> Service Unavailable | Total number of Session-Termination-Request terminations due to unavailable service.
> Callback | Total number of Session-Termination-Request terminations due to callback.
> User Error | Total number of Session-Termination-Request terminations due to user errors.
> Host Request | Total number of Session-Termination-Request terminations due to host requests.
> Accounting Servers Summary
> Message Stats | Accounting message statistics.
> Total AC Requests | Total number of AC-Requests.
> Total AC Answers | Total number of AC-Answers.
> ACR-Start | Total number of AC-Request starts.
> ACA-Start | Total number of AC-Answer starts.
> ACR-Start Retries | Total number of AC-Request start retries.
> ACA-Start Timeouts | Total number of AC-Answer timeouts.
> ACR-Interim | Total number of AC-Request interim.
> ACA-Interim | Total number of AC-Answer interim.
> ACR-Interim Retries | Total number of AC-Request interim retries.
> ACA-Interim Timeouts | Total number of AC-Answer interim timeouts.
> ACR-Event | Total number of AC-Request events.
> ACA-Event | Total number of AC-Answer events.
> ACR-Stop | Total number of AC-Request stops.
> ACA-Stop | Total number of AC-Answer stops.
> ACR-Stop Retries | Total number of AC-Request stop retries.
> ACA-Stop Timeouts | Total number of AC-Answer stop timeouts.
> ACA-Dropped | Total number of AC-Answers dropped.
> AC Message Error Stats | Accounting message error statistics.
> Diameter Protocol Errs | Total number of Diameter protocol errors.
> Bad Answers | Total number of bad answers.
> Unknown Session Reqs | Total number of unknown session requests.
> Unknown Command Code | Total number of unknown command codes.
> Request Timeouts | Total number of request timeouts.
> Parse Errors | Total number of parse errors.
> Request Retries | Total number of request retries.

> ‌
> show diameter authentication servers
> show diameter authentication servers Command Output Descriptions

> Field | Description
> Context Name | Name of the context in which the Diameter servers are configured.
> AAA Group | Name of the AAA group.
> Endpoint | Name of the Diameter endpoint.
> Peer | Name of the Diameter server host.
> No of Instance in UP state | The number of instances between Diameter server and AAA Manager in up state.
> No of Instance in DOWN state | The number of instances between Diameter server and AAA Manager in down state.
> Priority | The relative priority of this server considered when the system is selecting which Diameter server to use. Lower number has higher priority.
> Message Sent/Queued | The number of messages sent/queued from Diameter server to AAA Manager.

> ‌
> show diameter endpoints all
> show diameter endpoints all Command Output Descriptions

> Field | Description
> Context | Name of the configured context.
> Endpoint | Name of the endpoint.
> Realm | Domain (Realm) name for subscriber.
> Task | Task running on ACSMgr or AAAMgr.
> CPU | Indicates the Card and CPU number.
> Application | Indicates the application running on ACSMgr or AAAMgr.
> Total endpoints matching specified criteria | Indicates the total number of matching endpoints.

> ‌
> show diameter message-queue counters outbound endpoint
> show diameter message-queue counters outbound endpoint Command Output Descriptions

> Field | Description
> Context | Name of the configured context.
> Endpoint | Name of the endpoint.
> Peer Host | Name of the peer host.
> Peer Realm | Name of the peer realm.
> Accounting-Answer | The number of outbound Accounting-Answer messages for the specified endpoint.
> Accounting-Request | The number of outbound Accounting-Request messages for the specified endpoint.
> Abort-Session-Answer | The number of outbound Abort-Session-Answer messages for the specified endpoint.
> Abort-Session-Request | The number of outbound Abort-Session-Request messages for the specified endpoint.
> Authorization-Authentication-Ans | The number of outbound Authorization-Authentication-Ans messages for the specified endpoint.
> Authorization-Authentication-Req | The number of outbound Authorization-Authentication-Req messages for the specified endpoint.
> Capabilities-Exchange-Answer | The number of outbound Capabilities-Exchange-Answer messages for the specified endpoint.
> Capabilities-Exchange-Request | The number of outbound Capabilities-Exchange-Request messages for the specified endpoint.
> Credit-Control-Answer | The number of outbound Credit-Control-Answer messages for the specified endpoint.
> Credit-Control-Request | The number of outbound Credit-Control-Request messages for the specified endpoint.
> Device-Watchdog-Answer | The number of outbound Device-Watchdog-Answer messages for the specified endpoint.
> Device-Watchdog-Request | The number of outbound Device-Watchdog-Request messages for the specified endpoint.
> Diameter-EAP-Answer | The number of outbound Diameter-EAP-Answer messages for the specified endpoint.
> Diameter-EAP-Request | The number of outbound Diameter-EAP-Request messages for the specified endpoint.
> Disconnect-Peer-Answer | The number of outbound Disconnect-Peer-Answer messages for the specified endpoint.
> Disconnect-Peer-Request | The number of outbound Disconnect-Peer-Request messages for the specified endpoint.
> Location-Info-Answer | The number of outbound Location-Info-Answer messages for the specified endpoint.
> Location-Info-Request | The number of outbound Location-Info-Request messages for the specified endpoint.
> Multimedia-Auth-Answer | The number of outbound Multimedia-Auth-Answer messages for the specified endpoint.
> Multimedia-Auth-Request | The number of outbound Multimedia-Auth-Request messages for the specified endpoint.
> Profile-Update-Answer | The number of outbound Profile-Update-Answer messages for the specified endpoint.
> Profile-Update-Request | The number of outbound Profile-Update-Request messages for the specified endpoint.
> Push-Profile-Answer | The number of outbound Push-Profile-Answer messages for the specified endpoint.
> Push-Profile-Request | The number of outbound Push-Profile-Request messages for the specified endpoint.
> Re-Auth-Answer | The number of outbound Re-Auth-Answer messages for the specified endpoint.
> Re-Auth-Request | The number of outbound Re-Auth-Request messages for the specified endpoint.
> Registration-Termination-Answer | The number of outbound Registration-Termination-Answer messages for the specified endpoint.
> Registration-Termination-Request | The number of outbound Registration-Termination-Request messages for the specified endpoint.
> Server-Assignment-Answer | The number of outbound Server-Assignment-Answer messages for the specified endpoint.
> Server-Assignment-Request | The number of outbound Server-Assignment-Request messages for the specified endpoint.
> Session-Termination-Answer | The number of outbound Session-Termination-Answer messages for the specified endpoint.
> Session-Termination-Request | The number of outbound Session-Termination-Request messages for the specified endpoint.
> User-Authorization-Answer | The number of outbound User-Authorization-Answer messages for the specified endpoint.
> User-Authorization-Request | The number of outbound User-Authorization-Request messages for the specified endpoint.
> User-Data-Answer | The number of outbound User-Data-Answer messages for the specified endpoint.
> User-Data-Request | The number of outbound User-Data-Request messages for the specified endpoint.
> Total peers matching specified criteria | Indicates the total number of matching peers.

> ‌
> show diameter peers full all
> show diameter peers full all Command Output Descriptions

> Field | Description
> Context | Name of the context.
> Endpoint | Name of the endpoint.
> Inbound listening sockets | Displays listening Diameter interface:ports information when origin-host is configured as of “accept-inbound” connection type. If no inbound sockets are present these fields are not displayed.
> Local Host | Name of the local host.
> Local Address | IP address and port number of the local host.
> Endpoint | Name of the endpoint.
> Task | The task instance running on ACSMgr or AAAMgr.
> Peer Hostname | Name of the peer host.
> Local Hostname | Name of the local host.
> Peer Realm | Peer domain (realm) name for Subscriber.
> Local Realm | Local domain (realm) name for Subscriber.
> Peer Address | Address of peer domain (realm).
> Local Address | Address of local domain (realm).
> State | Indicates the connection status.
> CPU | The Card and CPU number.
> Messages Out/Queued | The number of messages sent out/queued.
> Task | The task running on ACSMgr or AAAMgr.
> Supported Vendor IDs | The supported vendor IDs.
> Admin Status | Indicates the admin status. Whether the user can administratively disable a peer while still preserving its configuration.
> DPR Disconnect | Disconnect-Peer-Request disconnect cause.
> Total peers matching specified criteria | The total number of peers matching the criteria.

> ‌
> show diameter statistics
> show diameter statistics Command Output Descriptions

> Field | Description
> Connection statistics
> Connection attempts | The total number of connections attempted.
> Connection failures | The total number of connections failed.
> Connection reads | The total number of connections read.
> Connection starts | The total number of connections started.
> Connection disconnects | The total number of connections disconnected
> Connection closes | The total number of connections closes.
> Connection DHOST requests | The total number of connections with DHOST requested.
> Connection DHOST removes | The total number of connections with DHOST removed.
> Connection Timeouts | The total number of connections timed out.
> Tc Expire Connection Attempts | The total number of connections attempted due to Tc timer expired. Note: The Tc timer controls the frequency that transport connection attempts are done to a peer with whom no active transport connection exists.
> Tw Expire Connection Closes | The total number of connections closed due to Tw timer expired.
> Connection failure statistics
> Connection bind errors | The total number of connections failed during binding errors.
> Connection connect errors | The total number of connections failed during connect errors.
> Connection address errors | The total number of connections failed due to address errors.
> Connection misc errors | The total number of connections failed due to other errors not mentioned in output.
> Connection DHOST errors | The total number of connections failed due to DHOST errors.
> Capabilities Exchange Request and Answers statistics
> Connection CER sent | The total number of Capabilities Exchange Request (CER) messages sent for connection.
> Connection CER send errors | The total number of connections failed due to errors during CER messages sent.
> CERs received | The total number of CER messages received.
> Connection CER create failures | The total number of connections failed during CER message creation.
> CEAs received | The total number of Capabilities Exchange Answer (CEA) messages received.
> CEA AVPs unknown | The total number of unknown Attribute Value Pairs (AVPs) related to CEA message.
> CEA Application ID mismatch | The total number of CEA Application ID mismatch.
> Read CEA Messages | The total number of READ messages for CEA.
> Read CEA Messages Unexpected | The total number of unexpected READ messages for CEA.
> Read CEA Missing | The total number of missing READ messages for CEA.
> Read CEA Negotiation Failure | The total number of failures in READ messages negotiation for CEA.
> Read CER Messages | The total number of READ messages for CER.
> Read CER Messages Unexpected | The total number of unexpected READ messages for CER.
> Read CER Missing | The total number of missing READ messages for CER.
> Tw Expire Waiting for CEA | The total number of CEAs waiting for answer due to Tw timer expired. Note: The Tw timer controls the changing of a peer to the SUSPECT state when no answer is received to a watchdog request.
> Device Watchdog Requests and Answers statistics
> DWA attempts | The total number of attempts for Device Watchdog Answer (DWA).
> DWA handle allocation failures | The total number of failures to handle allocation of DWA .
> DWAs sent | The total number of DWA messages sent.
> DWR send errors | The total number of errors while sending DWR messages.
> Read DWA Messages | The total number of READ messages for DWA.
> Read DWA Messages Unexpected | The total number of unexpected READ messages for DWA.
> Read DWR Messages | The total number of missing READ messages for DWR.
> Tw Expire Send DWR | The total number of DWRs sent due to Tw timer expired.
> Send DWR Attempts | The total number of attempts to send ‘DWR Sent’ messages.
> Send DWR Send Errors | The total number of errors while sending ‘DWR Sent’ messages.
> Send DWR Calls | The total number of calls for ‘DWR Sent’ messages.
> Send DWR MH Errors | The total number of message handling errors for ‘DWR Sent’ messages.
> Create Messages statistics
> Create Message Calls | The total number of calls for ‘Create’ message.
> Create Message Success | The total number of messages successful for ‘Create’ message.
> Create Message Routed | The total number of messages routed for ‘Create’ message.
> Create Message Directed | The total number of messages directed for ‘Create’ message.
> Create Message Buffer Errors | The total number of errors for ‘Create’ message buffer.
> Create Message Peer Never Up Errors | The total number of errors due to peer failure for ‘Create’ message.
> Create Message Window Errors | The total number of errors due to ‘Create’ message window.
> Create Message Unsupported Application Errors | The total number of errors due to unsupported applications for ‘Create’ message.
> Message Parse statistics
> Message Pool Expand Attempts | The total number of attempts for message pool expansion.
> Buffer Expand Attempts | The total number of attempts for buffer expansion.
> Message Parse Calls | The total number of calls for message parsing.
> Message Parse Too Many AVP Errors | The total number of message parsed having excessive AVP errors.
> Message Parse Header Errors | The total number of message parsed having header errors.
> Message Parse AVP Unknown Errors | The total number of message parsed having unknown AVP errors (errors not listed here).
> Message Parse Runt Errors | The total number of message parsed having runtime errors.
> Message Parse AVP Header Errors | The total number of message parsed having AVP header errors.
> Message Protocol Error | The total number of message parsed having protocol errors.
> Message Parse Mand AVP Unknown Errors | The total number of message parsed having unknown errors for mandatory AVP.
> Message aborts | The total number of message aborted during parsing.
> Send Message statistics
> Send Message Calls | The total number of calls for ‘Send’ message.
> Send Message Truncated Errors | The total number of truncated errors for ‘Send’ message.
> Read Statistics
> Read Bytes | The total number of bytes read.
> Read Messages Total | The total number of ‘Read’ messages.
> Requests Read | The total number of requests for ‘Read’ messages.
> Requests Timed Out | The total number of requests timed out for ‘Read’ messages.
> Answers Read | The total number of answers read for ‘Read’ messages.
> Answers Timed Out | The total number of answers timed out for ‘Read’ messages.
> Read Application Messages | The total number of ‘Read application’ messages.
> Unexpected Answers Read | The total number of unexpected answers for ‘Read’ messages.
> Read Parse statistics
> Read Parse Begin | The total number of parsing begins for ‘Read’ message.
> Read Parse E2E Errors | The total number of End-to-End (E2E) errors during parsing of ‘Read’ message.
> Read Parse Success | The total number of successful parsing of ‘Read’ message.
> Read Parse Application ID Errors | The total number of errors with Application Id during parsing of ‘Read’ message.
> Read Parse Command/Flag Errors | The total number of command or flag errors during parsing of ‘Read’ message.
> Read Parse Diameter Protocol Errors | The total number of Diameter protocol errors during parsing of ‘Read’ message.
> Read Parse Errors | The total number of errors during parsing of ‘Read’ message.
> Read Parse Length Padding Errors | The total number of ‘Length Padding’ errors during parsing of ‘Read’ message.
> Read Parse H2H Errors | The total number of Host-to-Host (H2H) errors during parsing of ‘Read’ message.
> Read Parse Length Too Long | The total number of message parsed having excessive length of ‘Read’ message.
> Read Parse Command Unknown | The total number of message parsed having unknown command in ‘Read’ message.
> Read Parse Length Sanity Errors | The total number of message parsed having invalid length of ‘Read’ message.
> Read Parse Length-v-SCTP EOR Errors | The total number of “Length-v-SCTP EOR” errors during parsing of “Read” message.
> Read Parse SCTP Missing EOR Errors | The total number of “SCTP Missing EOR” errors during parsing of “Read” message.
> Write statistics
> Write calls total | The total number of calls for ‘Write’ message.
> Write calls while OPEN | The total number of calls for ‘Write’ message while connection is OPEN.
> Write calls while IDLE | The total number of calls for ‘Write’ message while connection is IDLE.
> Write calls in other states | The total number of calls for ‘Write’ message while connection state is other than OPEN or IDLE state.
> Write backpressure events | The total number of Write messages over the maximum number of outstanding messages to queue.
> Written bytes | The total number of bytes written.
> Write iterations | The total number of write iterations.
> Written messages | The total number of messages written.
> Write EOFs | The total number of ‘Write’ messages with End-of-File (EOFs).
> Write errors | The total number of ‘Write’ message with errors.
> Peer Calls statistics
> Peer Open Calls | The total number of calls to open a peer.
> Peer Close Calls | The total number of calls to close a peer.
> Peer Open New Peer | The total number of calls to open a new peer.
> Peer Open Unknown Peer Errors | The total number of calls to open an unknown peer.
> Peer Open Misses | The total number of missed attempts to open a peer.
> Route statistics
> Route Adds | The total number of routes added.
> Route Expires | The total number of routes expired.
> Route Hits | The total number of hits to a route.
> Routes Misses | The total number of routes missed.
> Route Indirects | The total number of indirect route.
> Redirect Installs | The total number of redirected routes installed.
> Latency statistics
> Last Round Trip Time (ms) | The last round trip time, in milliseconds.
> Average Round Trip Time (ms) | The average round trip time in milliseconds.
> Redirect Host Usage:
> Redirected Host | The number of times the host is redirected.
> Redirect Not Cached | The number of times the redirected host is not cached.
> Redirect All Session | The number of times all messages within the session are sent to Redirect-Host.
> Redirect All Realm | The number of times all messages destined to Realm are sent to Redirect-Host.
> Redirect Realm and Application | The number of times the messages for application requested to Realm are sent to Redirect-Host.
> Redirect All Application | The number of times all messages for application are sent to Redirect-Host.
> Redirect All Host | The number of times the messages sent to Redirect-Host AVP value instead of Redirect-Host value sent by the host.
> Redirect All User | The number of times the message for user sent to Redirect-Host value.

> ‌

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883