> CSCF IFC SPT Group Mode Commands
> The CSCF iFC SPT Group Configuration Mode is used to associate individual SPT conditions with an Initial Filter Criteria (iFC) Service Point Trigger (SPT) group.
> Important: The commands or keywords/variables that are available are dependent on platform type, product version, and installed license(s).
> end
> Exits the current mode and returns to the Exec Mode.
> Product
> All
> Privilege
> Administrator
> Syntax
> end
> Usage
> Change the mode back to the Exec mode.
> exit
> Exits the current mode and returns to the previous mode.
> Product
> All
> Privilege
> Administrator
> Syntax
> exit
> Usage
> Return to the previous mode.
> spt-condition
> Assigns iFC SPT conditions to an existing iFC SPT group.
> Product
> SCM (S-CSCF, SIP Proxy)
> Privilege
> Administrator
> Syntax
> [ no ] spt-condition name cond_name
> no
> Removes the specified CSCF iFC SPT condition from the iFC SPT group.
> spt-condition name cond_name
> Specifies the name of an existing iFC SPT condition.
> cond_name must be from 1 to 39 alpha and/or numeric characters in length.
> Usage
> Use this command to associate individual SPT conditions with an iFC SPT group.
> Important: An iFC SPT group may be associated with multiple SPT conditions.
> Example
> The following command assigns cond2 to an iFC SPT group:
> spt-condition name cond2

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883